WB32L003 Standard Peripherals Firmware Library

Data Fields
SYSCON_TypeDef Struct Reference
CMSIS » Wb32l003 » Device_Peripheral_peripherals

## Data Fields
__IOM uint32_t | CFGR0
__IOM uint32_t | PORTINTCR
__IOM uint32_t | PORTCR
__IOM uint32_t | PCACR
__IOM uint32_t | TIM1CR
__IOM uint32_t | TIM2CR
__IM uint32_t | RESERVED0 [14]
__IOM uint32_t | UNLOCK

## Field Documentation

## ◆ CFGR0

__IOM uint32_t CFGR0

SYSCON setting register 0, Address offset: 0x000

## ◆ PCACR

__IOM uint32_t PCACR

SYSCON pca capture channel source select register, Address offset: 0x00C

## ◆ PORTCR

__IOM uint32_t PORTCR

SYSCON port control register, Address offset: 0x008

## ◆ PORTINTCR

__IOM uint32_t PORTINTCR

SYSCON port interrupt mode setting register, Address offset: 0x004

## ◆ RESERVED0

__IM uint32_t RESERVED0[14]

Address offset: 0x018

## ◆ TIM1CR

__IOM uint32_t TIM1CR

SYSCON tim1 channel source select register, Address offset: 0x010

## ◆ TIM2CR

__IOM uint32_t TIM2CR

SYSCON tim2 channel source select register, Address offset: 0x014

## ◆ UNLOCK

__IOM uint32_t UNLOCK

SYSCON write enable register, Address offset: 0x050

The documentation for this struct was generated from the following file:

- wb32l003.h