WB32L003 Standard Peripherals Firmware Library

Data Fields
VCMP_InitTypeDef Struct Reference
WB32L003_StdPeriph_Driver » VCMP

VCMP Init structure definition. More...

`#include <wb32l003_vcmp.h>`

## Data Fields
uint32_t | VcapDiv
uint32_t | NegPinSel
uint32_t | PosPinSel
uint32_t | Filter_Enable
uint32_t | Filter_Clk
uint32_t | Fliter_Num

## Detailed Description

VCMP Init structure definition.

## Field Documentation

## ◆ Filter_Clk

uint32_t Filter_Clk

Filter clk select, VCMP_Filter_Clock_Selection

## ◆ Filter_Enable

uint32_t Filter_Enable

Filter counter Enable or Disable, VCMP_Filter_Function_Selection

## ◆ Fliter_Num

uint32_t Fliter_Num

Filter counter number. Min_Data >= 0x00 and Max_Data = 0xFFFF

## ◆ NegPinSel

uint32_t NegPinSel

Negative input select, VCMP_InPut_Selection

## ◆ PosPinSel

uint32_t PosPinSel

Positive input select, VCMP_InPut_Selection

## ◆ VcapDiv

uint32_t VcapDiv

Specifies the VCMP VCAPDIV divider, VCMP_VCAP_Division_Slection

The documentation for this struct was generated from the following file:

- wb32l003_vcmp.h