WB32L003 Standard Peripherals Firmware Library

宏定义
Flags Definitions
WB32L003_StdPeriph_Driver » RTC » RTC_Exported_Constants

## 宏定义
#define | RTC_FLAG_ALR2F RTC_ISR_ALM2_F /* Alarm 2 flag */
#define | RTC_FLAG_ALR1F RTC_ISR_ALM1_F /* Alarm 1 flag */
#define | RTC_FLAG_RSF RTC_ISR_RSF /* Registers Synchronized flag */
#define | RTC_FLAG_WAITF RTC_ISR_WAITF /* Initialization mode flag */
#define | RTC_FLAG_WAIT RTC_ISR_WAIT /* Shift operation pending flag */
#define | IS_RTC_GET_FLAG(FLAG)

## 详细描述

## 宏定义说明

## ◆ IS_RTC_GET_FLAG

#define IS_RTC_GET_FLAG | ( |  | FLAG | ) |

值:
(((FLAG) == RTC_FLAG_ALR2F) || \
((FLAG) == RTC_FLAG_ALR1F) || \
((FLAG) == RTC_FLAG_RSF) || \
((FLAG) == RTC_FLAG_WAITF) || \
((FLAG) == RTC_FLAG_WAIT))