WB32L003 Standard Peripherals Firmware Library

成员变量
APSR_Type联合体 参考
Defines and Type Definitions » Status and Control Registers

Union type to access the Application Program Status Register (APSR). 更多...

`#include <core_cm0plus.h>`

## 成员变量
struct {
uint32_t _reserved0:28
uint32_t V:1
uint32_t C:1
uint32_t Z:1
uint32_t N:1
} | b
uint32_t | w

## 详细描述

Union type to access the Application Program Status Register (APSR).

## 结构体成员变量说明

## ◆ _reserved0

uint32_t _reserved0

bit: 0..27 Reserved

## ◆ b

struct { ... } b

Structure used for bit access

## ◆ C

uint32_t C

bit: 29 Carry condition code flag

## ◆ N

uint32_t N

bit: 31 Negative condition code flag

## ◆ V

uint32_t V

bit: 28 Overflow condition code flag

## ◆ w

uint32_t w

Type used for word access

## ◆ Z

uint32_t Z

bit: 30 Zero condition code flag

该联合体的文档由以下文件生成:

- core_cm0plus.h