/**
  @page SYSTICK_Example SYSTICK_Example example
  
  @verbatim
  ****************** (C) COPYRIGHT 2023 ESMT Technology *******************
  * @file    SYSTICK/SYSTICK_Example/readme.txt 
  * @author  ESMT Application Team
  * @version V0.0.4
  * @date    23-April-2023
  * @brief   Description of the SYSTICK SYSTICK_Example example.
  ******************************************************************************
  * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
  * TIME. AS A RESULT, ESMT SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
  * INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM
  * THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
  * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
  ******************************************************************************
   @endverbatim

@par 例程描述 

本例程演示如何配置SysTick以生成1ms的时基。

本例程系统时钟工作在24Mhz。


@par 目录内容 

  - SYSTICK/SYSTICK_Example/SYSTICK_Example.uvprojx      MDK5工程文件
  - SYSTICK/SYSTICK_Example/SYSTICK_Example.uvoptx       MDK5工程配置文件
  - SYSTICK/SYSTICK_Example/JLinkSettings.ini            Jlink配置文件
  - SYSTICK/SYSTICK_Example/main.c                       主程序


@par 硬件和软件环境 

  - 硬件平台搭建
    - 芯片管脚连接如下：
      - PD4 管脚连接到 LED1

@par 如何使用？ 

为了使程序工作，您必须执行以下操作 :
 - 使用 MDK5 打开此例程文件夹中的 SYSTICK_Example.uvprojx 工程
 - 重新编译该工程并下载到目标存储器中
 - 运行此例程
   
 * <h3><center>&copy; COPYRIGHT 2023 ESMT Technology</center></h3>
 */
