WB32L003 Standard Peripherals Firmware Library

ADC get internal VCAP example

      ****************** (C) COPYRIGHT 2023 Westberry Technology *******************
      * @file    ADC/ADC_GetVCAP/readme.txt
      * @author  Westberry Application Team
      * @version V0.0.4
      * @date    23-April-2023
      * @brief   Description of the ADC ADC_GetVCAP example.
      ******************************************************************************
      * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
      * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
      * TIME. AS A RESULT, WESTBERRY SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
      * INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM
      * THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
      * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
      ******************************************************************************

Example Description

This example describes how to get internal VCAP.

In this example, Main clock is configured at 24MHz.

The UART1 is configured as follow:

- BaudRate: 115200
- Word Length: 8

Directory contents

- ADC/ADC_GetVCAP/ADC_GetVCAP.uvprojx MDK5 project file
- ADC/ADC_GetVCAP/ADC_GetVCAP.uvoptx MDK5 project options file
- ADC/ADC_GetVCAP/JLinkSettings.ini Jlink settings file
- ADC/ADC_GetVCAP/main.c Main program

Hardware and Software environment

- Hardware environment
  - The chip pins are connected as follows：
    - UART1 (PD5, PD6) is connected to PC serial port.

How to use it ?

In order to make the program work, you must do the following :

- Open ADC_GetVCAP.uvprojx from this example folder by Keil MDK5
- Rebuild all files and load your image into target memory

- Run the example

  ###
  © COPYRIGHT 2023 Westberry Technology