WB32L003 Standard Peripherals Firmware Library

Data Fields
UART_InitTypeDef Struct Reference
WB32L003_StdPeriph_Driver » UART

UART Init Structure definition. More...

`#include <wb32l003_uart.h>`

## Data Fields
uint32_t | UART_BandDouble
uint32_t | UART_BaudRateMode
uint32_t | UART_BaudRate
uint8_t | UART_WordLength

## Detailed Description

UART Init Structure definition.

## Field Documentation

## ◆ UART_BandDouble

uint32_t UART_BandDouble

Specifies doubled baudrate Enable or Disable This parameter can be a value of UART_BandDouble

## ◆ UART_BaudRate

uint32_t UART_BaudRate

This member configures the UART communication baud rate.

## ◆ UART_BaudRateMode

uint32_t UART_BaudRateMode

Specifies the baud rate configuration source for the UART This parameter can be a value of UART_BaudRate_Mode

## ◆ UART_WordLength

uint8_t UART_WordLength

Specifies the number of data bits transmitted or received in a frame. This parameter can be a value of UART_Word_Length

The documentation for this struct was generated from the following file:

- wb32l003_uart.h