WB32L003 Standard Peripherals Firmware Library

宏定义
TIM_Internal_Trigger_Selection
WB32L003_StdPeriph_Driver » BASETIM WB32L003_StdPeriph_Driver » | TIM » TIM_Exported_constants

## 宏定义
#define | TIM_TS_ITR0 ((uint16_t)0x0000)
#define | TIM_TS_ITR1 ((uint16_t)0x0010)
#define | TIM_TS_ITR2 ((uint16_t)0x0020)
#define | TIM_TS_ITR3 ((uint16_t)0x0030)
#define | TIM_TS_TI1F_ED ((uint16_t)0x0040)
#define | TIM_TS_TI1FP1 ((uint16_t)0x0050)
#define | TIM_TS_TI2FP2 ((uint16_t)0x0060)
#define | TIM_TS_ETRF ((uint16_t)0x0070)
#define | IS_TIM_TRIGGER_SELECTION(SELECTION)
#define | IS_TIM_INTERNAL_TRIGGER_SELECTION(SELECTION)

## 详细描述

## 宏定义说明

## ◆ IS_TIM_INTERNAL_TRIGGER_SELECTION

#define IS_TIM_INTERNAL_TRIGGER_SELECTION | ( |  | SELECTION | ) |

值:
(((SELECTION) == TIM_TS_ITR0) || \
((SELECTION) == TIM_TS_ITR1) || \
((SELECTION) == TIM_TS_ITR2) || \
((SELECTION) == TIM_TS_ITR3))

## ◆ IS_TIM_TRIGGER_SELECTION

#define IS_TIM_TRIGGER_SELECTION | ( |  | SELECTION | ) |

值:
(((SELECTION) == TIM_TS_ITR0) || \
((SELECTION) == TIM_TS_ITR1) || \
((SELECTION) == TIM_TS_ITR2) || \
((SELECTION) == TIM_TS_ITR3) || \
((SELECTION) == TIM_TS_TI1F_ED) || \
((SELECTION) == TIM_TS_TI1FP1) || \
((SELECTION) == TIM_TS_TI2FP2) || \
((SELECTION) == TIM_TS_ETRF))