WB32L003 Standard Peripherals Firmware Library

模块 | 宏定义 | 类型定义 | 枚举
Wb32l003
CMSIS

## 模块
| Device_Peripheral_peripherals
| Exported_macro

## 宏定义
#define | HSE_VALUE (24000000)
| In the following line adjust the value of External High Speed oscillator (HSE) used in your application. 更多...
#define | LSE_VALUE (32768)
| In the following line adjust the value of External High Speed oscillator (LSE) used in your application. 更多...
#define | HSI_VALUE (24000000)
| In the following line adjust the value of External High Speed oscillator (HSI) used in your application. 更多...
#define | LSI_VALUE (32768)
| In the following line adjust the value of External High Speed oscillator (LSI) used in your application. 更多...
#define | __CM0PLUS_REV 0x0001U /* Core revision r0p1 */
#define | __MPU_PRESENT 0U /* MPU present or not */
#define | __VTOR_PRESENT 1U /* VTOR present or not */
#define | __NVIC_PRIO_BITS 2U /* Number of Bits used for Priority Levels */
#define | __Vendor_SysTickConfig 0U /* Set to 1 if different SysTick Config is used */
#define | IS_FUNCTIONAL_STATE(STATE) (((STATE) == DISABLE) || ((STATE) == ENABLE))
#define | FLASH_MEMORY_BASE ((uint32_t)0x00000000UL)
#define | SRAM_MEMORY_BASE ((uint32_t)0x20000000UL)
#define | PERIPH_BASE ((uint32_t)0x40000000UL)
#define | UID_BASE ((uint32_t)0x180000F0UL)
#define | SCR_BASE ((uint32_t)0xE000ED10UL)
#define | APBPERIPH_BASE (PERIPH_BASE + 0x00000UL)
#define | AHBPERIPH_BASE (PERIPH_BASE + 0x20000UL)
#define | RCC_BASE (AHBPERIPH_BASE + 0x0000)
#define | FLASH_BASE (AHBPERIPH_BASE + 0x0400)
#define | CRC_BASE (AHBPERIPH_BASE + 0x0800)
#define | GPIOA_BASE (AHBPERIPH_BASE + 0x1000)
#define | GPIOB_BASE (AHBPERIPH_BASE + 0x1400)
#define | GPIOC_BASE (AHBPERIPH_BASE + 0x1800)
#define | GPIOD_BASE (AHBPERIPH_BASE + 0x1C00)
#define | UART1_BASE (APBPERIPH_BASE + 0x0000)
#define | UART2_BASE (APBPERIPH_BASE + 0x0400)
#define | SPI_BASE (APBPERIPH_BASE + 0x0800)
#define | I2C_BASE (APBPERIPH_BASE + 0x0C00)
#define | TIM1_BASE (APBPERIPH_BASE + 0x1000)
#define | PCA_BASE (APBPERIPH_BASE + 0x1400)
#define | TIM10_BASE (APBPERIPH_BASE + 0x1800)
#define | TIM11_BASE (APBPERIPH_BASE + 0x1900)
#define | SYSCON_BASE (APBPERIPH_BASE + 0x1C00)
#define | WWDG_BASE (APBPERIPH_BASE + 0x2000)
#define | IWDG_BASE (APBPERIPH_BASE + 0x2400)
#define | AWK_BASE (APBPERIPH_BASE + 0x2800)
#define | ADC_BASE (APBPERIPH_BASE + 0x2C00)
#define | RTC_BASE (APBPERIPH_BASE + 0x3000)
#define | CLKTRIM_BASE (APBPERIPH_BASE + 0x3400)
#define | OWIRE_BASE (APBPERIPH_BASE + 0x3800)
#define | TIM2_BASE (APBPERIPH_BASE + 0x3C00)
#define | LVD_BASE (APBPERIPH_BASE + 0x4000)
#define | VCMP_BASE (APBPERIPH_BASE + 0x4080)
#define | LPTIM_BASE (APBPERIPH_BASE + 0x4400)
#define | BEEP_BASE (APBPERIPH_BASE + 0x4800)
#define | DBG_BASE (APBPERIPH_BASE + 0x4C00)
#define | LPUART_BASE (APBPERIPH_BASE + 0x5000)
#define | VCMP (( VCMP_TypeDef*) VCMP_BASE)
#define | LVD (( LVD_TypeDef*) LVD_BASE)
#define | ADC (( ADC_TypeDef*) ADC_BASE)
#define | RTC (( RTC_TypeDef*) RTC_BASE)
#define | CLKTRIM (( CLKTRIM_TypeDef*) CLKTRIM_BASE)
#define | OWIRE (( OWIRE_TypeDef*) OWIRE_BASE)
#define | SPI (( SPI_TypeDef*) SPI_BASE)
#define | I2C (( I2C_TypeDef*) I2C_BASE)
#define | LPUART (( LPUART_TypeDef*) LPUART_BASE)
#define | UART1 (( UART_TypeDef*) UART1_BASE)
#define | UART2 (( UART_TypeDef*) UART2_BASE)
#define | WWDG (( WWDG_TypeDef*) WWDG_BASE)
#define | IWDG (( IWDG_TypeDef*) IWDG_BASE)
#define | BEEP (( BEEP_TypeDef*) BEEP_BASE)
#define | AWK (( AWK_TypeDef*) AWK_BASE)
#define | LPTIM (( LPTIM_TypeDef*) LPTIM_BASE)
#define | TIM10 (( BASETIM_TypeDef*) TIM10_BASE)
#define | TIM11 (( BASETIM_TypeDef*) TIM11_BASE)
#define | PCA (( PCA_TypeDef*) PCA_BASE)
#define | TIM1 (( TIM_TypeDef*) TIM1_BASE)
#define | TIM2 (( TIM_TypeDef*) TIM2_BASE)
#define | CRC (( CRC_TypeDef*) CRC_BASE)
#define | FLASH (( FLASH_TypeDef*) FLASH_BASE)
#define | GPIOA (( GPIO_TypeDef*) GPIOA_BASE)
#define | GPIOB (( GPIO_TypeDef*) GPIOB_BASE)
#define | GPIOC (( GPIO_TypeDef*) GPIOC_BASE)
#define | GPIOD (( GPIO_TypeDef*) GPIOD_BASE)
#define | SYSCON (( SYSCON_TypeDef*) SYSCON_BASE)
#define | RCC (( RCC_TypeDef*) RCC_BASE)
#define | DBG (( DBG_TypeDef *) DBG_BASE)
#define | DBG_APBFZ_TIM10DBGSTOP_Pos (0UL)
#define | DBG_APBFZ_TIM10DBGSTOP_Msk (0x1UL)
#define | DBG_APBFZ_TIM11DBGSTOP_Pos (1UL)
#define | DBG_APBFZ_TIM11DBGSTOP_Msk (0x1UL)
#define | DBG_APBFZ_LPTIMDBGSTOP_Pos (2UL)
#define | DBG_APBFZ_LPTIMDBGSTOP_Msk (0x1UL)
#define | DBG_APBFZ_PCADBGSTOP_Pos (4UL)
#define | DBG_APBFZ_PCADBGSTOP_Msk (0x1UL)
#define | DBG_APBFZ_TIM1DBGSTOP_Pos (5UL)
#define | DBG_APBFZ_TIM1DBGSTOP_Msk (0x1UL)
#define | DBG_APBFZ_RTCDBGSTOP_Pos (6UL)
#define | DBG_APBFZ_RTCDBGSTOP_Msk (0x1UL)
#define | DBG_APBFZ_BEEPDBGSTOP_Pos (8UL)
#define | DBG_APBFZ_BEEPDBGSTOP_Msk (0x1UL)
#define | DBG_APBFZ_IWDGDBGSTOP_Pos (9UL)
#define | DBG_APBFZ_IWDGDBGSTOP_Msk (0x1UL)
#define | DBG_APBFZ_WWDGDBGSTOP_Pos (10UL)
#define | DBG_APBFZ_WWDGDBGSTOP_Msk (0x1UL)
#define | DBG_APBFZ_TIM2DBGSTOP_Pos (11UL)
#define | DBG_APBFZ_TIM2DBGSTOP_Msk (0x1UL)
#define | DBG_APBFZ_KEY_Pos (16UL)
#define | DBG_APBFZ_KEY_Msk (0xFFUL)
#define | VCMP_CR0_PINSEL_Pos (0UL)
#define | VCMP_CR0_PINSEL_Msk (0x3UL)
#define | VCMP_CR0_NINSEL_Pos (2UL)
#define | VCMP_CR0_NINSEL_Msk (0xCUL)
#define | VCMP_CR0_VCAPDIV_Pos (4UL)
#define | VCMP_CR0_VCAPDIV_Msk (0x30UL)
#define | VCMP_CR0_VCAPDIV_EN_Pos (6UL)
#define | VCMP_CR0_VCAPDIV_EN_Msk (0x40UL)
#define | VCMP_CR0_VCAPDIV_EN VCMP_CR0_VCAPDIV_EN_Msk
#define | VCMP_CR1_VCEN_Pos (0UL)
#define | VCMP_CR1_VCEN_Msk (0x1UL)
#define | VCMP_CR1_VCEN VCMP_CR1_VCEN_Msk
#define | VCMP_CR1_VCMP_FLTCLK_SEL_Pos (2UL)
#define | VCMP_CR1_VCMP_FLTCLK_SEL_Msk (0xCUL)
#define | VCMP_CR1_VCMP_FLTCLK_SEL VCMP_CR1_VCMP_FLTCLK_SEL_Msk
#define | VCMP_CR1_FLTEN_Pos (8UL)
#define | VCMP_CR1_FLTEN_Msk (0x100UL)
#define | VCMP_CR1_FLTEN VCMP_CR1_FLTEN_Msk
#define | VCMP_CR1_FALLINTEN_Pos (12UL)
#define | VCMP_CR1_FALLINTEN_Msk (0x1000UL)
#define | VCMP_CR1_FALLINTEN VCMP_CR1_FALLINTEN_Msk
#define | VCMP_CR1_RISEINTEN_Pos (13UL)
#define | VCMP_CR1_RISEINTEN_Msk (0x2000UL)
#define | VCMP_CR1_RISEINTEN VCMP_CR1_RISEINTEN_Msk
#define | VCMP_CR1_HIGHINTEN_Pos (14UL)
#define | VCMP_CR1_HIGHINTEN_Msk (0x4000UL)
#define | VCMP_CR1_HIGHINTEN VCMP_CR1_HIGHINTEN_Msk
#define | VCMP_CR1_INT_EN_Pos (15UL)
#define | VCMP_CR1_INT_EN_Msk (0x8000UL)
#define | VCMP_CR1_INT_EN VCMP_CR1_INT_EN_Msk
#define | VCMP_CR1_FLT_NUM_Pos (16UL)
#define | VCMP_CR1_FLT_NUM_Msk (0xFFFF0000UL)
#define | VCMP_OUTCFG_INV_TIMX_Pos (0UL)
#define | VCMP_OUTCFG_INV_TIMX_Msk (0x1UL)
#define | VCMP_OUTCFG_TIM10_EN_Pos (1UL)
#define | VCMP_OUTCFG_TIM10_EN_Msk (0x2UL)
#define | VCMP_OUTCFG_TIM11_EN_Pos (2UL)
#define | VCMP_OUTCFG_TIM11_EN_Msk (0x4UL)
#define | VCMP_OUTCFG_LPTIM_EN_Pos (4UL)
#define | VCMP_OUTCFG_LPTIM_EN_Msk (0x10UL)
#define | VCMP_OUTCFG_LPTIMEXT_EN_Pos (5UL)
#define | VCMP_OUTCFG_LPTIMEXT_EN_Msk (0x20UL)
#define | VCMP_OUTCFG_INV_PCA_Pos (6UL)
#define | VCMP_OUTCFG_INV_PCA_Msk (0x40UL)
#define | VCMP_OUTCFG_PCACAP0_EN_Pos (7UL)
#define | VCMP_OUTCFG_PCACAP0_EN_Msk (0x80UL)
#define | VCMP_OUTCFG_PCAECI_EN_Pos (8UL)
#define | VCMP_OUTCFG_PCAECI_EN_Msk (0x100UL)
#define | VCMP_OUTCFG_INV_TIM1CH1_Pos (9UL)
#define | VCMP_OUTCFG_INV_TIM1CH1_Msk (0x200UL)
#define | VCMP_OUTCFG_TIM1CH1_EN_Pos (10UL)
#define | VCMP_OUTCFG_TIM1CH1_EN_Msk (0x400UL)
#define | VCMP_OUTCFG_INV_TIM1CH2_Pos (11UL)
#define | VCMP_OUTCFG_INV_TIM1CH2_Msk (0x800UL)
#define | VCMP_OUTCFG_TIM1CH2_EN_Pos (12UL)
#define | VCMP_OUTCFG_TIM1CH2_EN_Msk (0x1000UL)
#define | VCMP_OUTCFG_INV_TIM1CH3_Pos (13UL)
#define | VCMP_OUTCFG_INV_TIM1CH3_Msk (0x2000UL)
#define | VCMP_OUTCFG_TIM1CH3_EN_Pos (14UL)
#define | VCMP_OUTCFG_TIM1CH3_EN_Msk (0x4000UL)
#define | VCMP_OUTCFG_INV_TIM1CH4_Pos (15UL)
#define | VCMP_OUTCFG_INV_TIM1CH4_Msk (0x8000UL)
#define | VCMP_OUTCFG_TIM1CH4_EN_Pos (16UL)
#define | VCMP_OUTCFG_TIM1CH4_EN_Msk (0x10000UL)
#define | VCMP_OUTCFG_TIM1BKE_Pos (17UL)
#define | VCMP_OUTCFG_TIM1BKE_Msk (0x20000UL)
#define | VCMP_OUTCFG_INV_PAD_Pos (18UL)
#define | VCMP_OUTCFG_INV_PAD_Msk (0x40000UL)
#define | VCMP_SR_INTF_Pos (0UL)
#define | VCMP_SR_INTF_Msk (0x1UL)
#define | VCMP_SR_INTF VCMP_SR_INTF_Msk
#define | VCMP_SR_VCMP_FLOUT_Pos (1UL)
#define | VCMP_SR_VCMP_FLOUT_Msk (0x2UL)
#define | VCMP_SR_VCMP_FLOUT VCMP_SR_VCMP_FLOUT_Msk
#define | LVD_CR_DIV_SEL_Pos (0UL)
#define | LVD_CR_DIV_SEL_Msk (0xFUL)
#define | LVD_CR_DIV_SEL LVD_CR_DIV_SEL_Msk
#define | LVD_CR_DIV_SEL_0 (0x1 << LVD_CR_DIV_SEL_Pos)
#define | LVD_CR_DIV_SEL_1 (0x2 << LVD_CR_DIV_SEL_Pos)
#define | LVD_CR_DIV_SEL_2 (0x4 << LVD_CR_DIV_SEL_Pos)
#define | LVD_CR_DIV_SEL_3 (0x8 << LVD_CR_DIV_SEL_Pos)
#define | LVD_CR_LVDEN_Pos (5UL)
#define | LVD_CR_LVDEN_Msk (0x20UL)
#define | LVD_CR_LVDEN LVD_CR_LVDEN_Msk
#define | LVD_CR_ACT_Pos (6UL)
#define | LVD_CR_ACT_Msk (0x40UL)
#define | LVD_CR_ACT LVD_CR_ACT_Msk
#define | LVD_CR_FLTEN_Pos (7UL)
#define | LVD_CR_FLTEN_Msk (0x80UL)
#define | LVD_CR_FLTEN LVD_CR_FLTEN_Msk
#define | LVD_CR_FLTCLK_SEL_Pos (8UL)
#define | LVD_CR_FLTCLK_SEL_Msk (0x300UL)
#define | LVD_CR_FLTCLK_SEL LVD_CR_FLTCLK_SEL_Msk
#define | LVD_CR_FLTCLK_SEL_0 (0x1 << LVD_CR_FLTCLK_SEL_Pos)
#define | LVD_CR_FLTCLK_SEL_1 (0x2 << LVD_CR_FLTCLK_SEL_Pos)
#define | LVD_CR_FALLINTEN_Pos (12UL)
#define | LVD_CR_FALLINTEN_Msk (0x1000UL)
#define | LVD_CR_FALLINTEN LVD_CR_FALLINTEN_Msk
#define | LVD_CR_RISEINTEN_Pos (13UL)
#define | LVD_CR_RISEINTEN_Msk (0x2000UL)
#define | LVD_CR_RISEINTEN LVD_CR_RISEINTEN_Msk
#define | LVD_CR_HIGHINTEN_Pos (14UL)
#define | LVD_CR_HIGHINTEN_Msk (0x4000UL)
#define | LVD_CR_HIGHINTEN LVD_CR_HIGHINTEN_Msk
#define | LVD_CR_INT_EN_Pos (15UL)
#define | LVD_CR_INT_EN_Msk (0x8000UL)
#define | LVD_CR_INT_EN LVD_CR_INT_EN_Msk
#define | LVD_CR_FLT_NUM_Pos (16UL)
#define | LVD_CR_FLT_NUM_Msk (0xFFFF0000UL)
#define | LVD_CR_FLT_NUM LVD_CR_FLT_NUM_Msk
#define | LVD_CR_ALL_Msk (0xFFFFF3EFUL)
#define | LVD_SR_INTF_Pos (0UL)
#define | LVD_SR_INTF_Msk (0x1UL)
#define | LVD_SR_INTF LVD_SR_INTF_Msk
#define | ADC_CR0_ADCEN_Pos (0UL)
#define | ADC_CR0_ADCEN_Msk (0x1UL)
#define | ADC_CR0_ADCEN ADC_CR0_ADCEN_Msk
#define | ADC_CR0_START_Pos (1UL)
#define | ADC_CR0_START_Msk (0x2UL)
#define | ADC_CR0_START ADC_CR0_START_Msk
#define | ADC_CR0_CLKSEL_Pos (4UL)
#define | ADC_CR0_CLKSEL_Msk (0x70UL)
#define | ADC_CR0_CLKSEL ADC_CR0_CLKSEL_Msk
#define | ADC_CR0_CLKSEL_0 (0x1 << ADC_CR0_CLKSEL_Pos)
#define | ADC_CR0_CLKSEL_1 (0x2 << ADC_CR0_CLKSEL_Pos)
#define | ADC_CR0_CLKSEL_2 (0x4 << ADC_CR0_CLKSEL_Pos)
#define | ADC_CR0_SEL_Pos (8UL)
#define | ADC_CR0_SEL3_Pos (7UL)
#define | ADC_CR0_SEL_Msk (0x700UL | 0x80UL)
#define | ADC_CR0_SEL ADC_CR0_SEL_Msk
#define | ADC_CR0_SEL_0 (0x1 << ADC_CR0_SEL_Pos)
#define | ADC_CR0_SEL_1 (0x2 << ADC_CR0_SEL_Pos)
#define | ADC_CR0_SEL_2 (0x4 << ADC_CR0_SEL_Pos)
#define | ADC_CR0_SEL_3 (0x1 << ADC_CR0_SEL3_Pos)
#define | ADC_CR0_SAM_Pos (11UL)
#define | ADC_CR0_SAM_Msk (0x800UL)
#define | ADC_CR0_SAM ADC_CR0_SAM_Msk
#define | ADC_CR0_STATERST_Pos (15UL)
#define | ADC_CR0_STATERST_Msk (0x8000UL)
#define | ADC_CR0_STATERST ADC_CR0_STATERST_Msk
#define | ADC_CR1_TRIGS0_Pos (0UL)
#define | ADC_CR1_TRIGS0_Msk (0x1001FUL)
#define | ADC_CR1_TRIGS0 ADC_CR1_TRIGS0_Msk
#define | ADC_CR1_TRIGS0_0 (0x1 << ADC_CR1_TRIGS0_Pos)
#define | ADC_CR1_TRIGS0_1 (0x2 << ADC_CR1_TRIGS0_Pos)
#define | ADC_CR1_TRIGS0_2 (0x4 << ADC_CR1_TRIGS0_Pos)
#define | ADC_CR1_TRIGS0_3 (0x8 << ADC_CR1_TRIGS0_Pos)
#define | ADC_CR1_TRIGS0_4 (0x10 << ADC_CR1_TRIGS0_Pos)
#define | ADC_CR1_TRIGS0_5 (0x1 << 16)
#define | ADC_CR1_TRIGS1_Pos (5UL)
#define | ADC_CR1_TRIGS1_Msk (0x203E0UL)
#define | ADC_CR1_TRIGS1 ADC_CR1_TRIGS1_Msk
#define | ADC_CR1_TRIGS1_0 (0x1 << ADC_CR1_TRIGS1_Pos)
#define | ADC_CR1_TRIGS1_1 (0x2 << ADC_CR1_TRIGS1_Pos)
#define | ADC_CR1_TRIGS1_2 (0x4 << ADC_CR1_TRIGS1_Pos)
#define | ADC_CR1_TRIGS1_3 (0x8 << ADC_CR1_TRIGS1_Pos)
#define | ADC_CR1_TRIGS1_4 (0x10 << ADC_CR1_TRIGS1_Pos)
#define | ADC_CR1_TRIGS1_5 (0x1 << 17)
#define | ADC_CR1_CT_Pos (10UL)
#define | ADC_CR1_CT_Msk (0x400UL)
#define | ADC_CR1_CT ADC_CR1_CT_Msk
#define | ADC_CR1_RACC_EN_Pos (11UL)
#define | ADC_CR1_RACC_EN_Msk (0x800UL)
#define | ADC_CR1_RACC_EN ADC_CR1_RACC_EN_Msk
#define | ADC_CR1_LTCMP_Pos (12UL)
#define | ADC_CR1_LTCMP_Msk (0x1000UL)
#define | ADC_CR1_LTCMP ADC_CR1_LTCMP_Msk
#define | ADC_CR1_HTCMP_Pos (13UL)
#define | ADC_CR1_HTCMP_Msk (0x2000UL)
#define | ADC_CR1_HTCMP ADC_CR1_HTCMP_Msk
#define | ADC_CR1_REGCMP_Pos (14UL)
#define | ADC_CR1_REGCMP_Msk (0x4000UL)
#define | ADC_CR1_REGCMP ADC_CR1_REGCMP_Msk
#define | ADC_CR1_RACC_CLR_Pos (15UL)
#define | ADC_CR1_RACC_CLR_Msk (0x8000UL)
#define | ADC_CR1_RACC_CLR ADC_CR1_RACC_CLR_Msk
#define | ADC_CR2_CHEN_Pos (0UL)
#define | ADC_CR2_CH15_8EN_Pos (20UL)
#define | ADC_CR2_CHEN_Msk (0xFFUL | (0xFF00000UL))
#define | ADC_CR2_CHEN ADC_CR2_CHEN_Msk
#define | ADC_CR2_CHEN_0 (0x1 << ADC_CR2_CHEN_Pos)
#define | ADC_CR2_CHEN_1 (0x2 << ADC_CR2_CHEN_Pos)
#define | ADC_CR2_CHEN_2 (0x4 << ADC_CR2_CHEN_Pos)
#define | ADC_CR2_CHEN_3 (0x8 << ADC_CR2_CHEN_Pos)
#define | ADC_CR2_CHEN_4 (0x10 << ADC_CR2_CHEN_Pos)
#define | ADC_CR2_CHEN_5 (0x20 << ADC_CR2_CHEN_Pos)
#define | ADC_CR2_CHEN_6 (0x40 << ADC_CR2_CHEN_Pos)
#define | ADC_CR2_CHEN_7 (0x80 << ADC_CR2_CHEN_Pos)
#define | ADC_CR2_CHEN_8 (0x1 << ADC_CR2_CH15_8EN_Pos)
#define | ADC_CR2_CHEN_9 (0x2 << ADC_CR2_CH15_8EN_Pos)
#define | ADC_CR2_CHEN_10 (0x4 << ADC_CR2_CH15_8EN_Pos)
#define | ADC_CR2_CHEN_11 (0x8 << ADC_CR2_CH15_8EN_Pos)
#define | ADC_CR2_CHEN_12 (0x10 << ADC_CR2_CH15_8EN_Pos)
#define | ADC_CR2_CHEN_13 (0x20 << ADC_CR2_CH15_8EN_Pos)
#define | ADC_CR2_CHEN_14 (0x40 << ADC_CR2_CH15_8EN_Pos)
#define | ADC_CR2_CHEN_15 (0x80 << ADC_CR2_CH15_8EN_Pos)
#define | ADC_CR2_ADCCNT_Pos (8UL)
#define | ADC_CR2_ADCCNT_Msk (0xFF00UL)
#define | ADC_CR2_ADCCNT ADC_CR2_ADCCNT_Msk
#define | ADC_CR2_CIRCLE_MODE_Pos (16UL)
#define | ADC_CR2_CIRCLE_MODE_Msk (0x10000UL)
#define | ADC_CR2_CIRCLE_MODE ADC_CR2_CIRCLE_MODE_Msk
#define | ADC_RESULT0_Result0_Pos (0UL)
#define | ADC_RESULT0_Result0_Msk (0xFFFUL)
#define | ADC_RESULT1_Result1_Pos (0UL)
#define | ADC_RESULT1_Result1_Msk (0xFFFFFFUL)
#define | ADC_RESULT2_Result2_Pos (0UL)
#define | ADC_RESULT2_Result2_Msk (0xFFFUL)
#define | ADC_RESULT3_Result3_Pos (0UL)
#define | ADC_RESULT3_Result3_Msk (0xFFFUL)
#define | ADC_RESULT4_Result4_Pos (0UL)
#define | ADC_RESULT4_Result4_Msk (0xFFFUL)
#define | ADC_RESULT5_Result5_Pos (0UL)
#define | ADC_RESULT5_Result5_Msk (0xFFFUL)
#define | ADC_RESULT6_Result6_Pos (0UL)
#define | ADC_RESULT6_Result6_Msk (0xFFFUL)
#define | ADC_RESULT7_Result7_Pos (0UL)
#define | ADC_RESULT7_Result7_Msk (0xFFFUL)
#define | ADC_RESULT8_Result8_Pos (0UL)
#define | ADC_RESULT8_Result8_Msk (0xFFFUL)
#define | ADC_RESULT9_Result9_Pos (0UL)
#define | ADC_RESULT9_Result9_Msk (0xFFFUL)
#define | ADC_RESULT10_Result10_Pos (0UL)
#define | ADC_RESULT10_Result10_Msk (0xFFFUL)
#define | ADC_RESULT11_Result11_Pos (0UL)
#define | ADC_RESULT11_Result11_Msk (0xFFFUL)
#define | ADC_RESULT12_Result12_Pos (0UL)
#define | ADC_RESULT12_Result12_Msk (0xFFFUL)
#define | ADC_RESULT13_Result13_Pos (0UL)
#define | ADC_RESULT13_Result13_Msk (0xFFFUL)
#define | ADC_RESULT14_Result14_Pos (0UL)
#define | ADC_RESULT14_Result14_Msk (0xFFFUL)
#define | ADC_RESULT15_Result15_Pos (0UL)
#define | ADC_RESULT15_Result15_Msk (0xFFFUL)
#define | ADC_RESULT_RESULT_Pos (0UL)
#define | ADC_RESULT_RESULT_Msk (0xFFFUL)
#define | ADC_RESULT_ACC_HT_Pos (0UL)
#define | ADC_RESULT_ACC_HT_Msk (0xFFFUL)
#define | ADC_HT_HT_Pos (0UL)
#define | ADC_HT_HT_Msk (0xFFFUL)
#define | ADC_LT_LT_Pos (0UL)
#define | ADC_LT_LT_Msk (0xFFFUL)
#define | ADC_INTEN_ADCXIEN_Pos (0UL)
#define | ADC_INTEN_ADC15_8XIEN_Pos (12UL)
#define | ADC_INTEN_ADCXIEN_Msk (0xFFUL | 0xFF000UL)
#define | ADC_INTEN_ADCXIEN ADC_INTEN_ADCXIEN_Msk
#define | ADC_INTEN_ADCXIEN_0 (0x1 << ADC_INTEN_ADCXIEN_Pos)
#define | ADC_INTEN_ADCXIEN_1 (0x2 << ADC_INTEN_ADCXIEN_Pos)
#define | ADC_INTEN_ADCXIEN_2 (0x4 << ADC_INTEN_ADCXIEN_Pos)
#define | ADC_INTEN_ADCXIEN_3 (0x8 << ADC_INTEN_ADCXIEN_Pos)
#define | ADC_INTEN_ADCXIEN_4 (0x10 << ADC_INTEN_ADCXIEN_Pos)
#define | ADC_INTEN_ADCXIEN_5 (0x20 << ADC_INTEN_ADCXIEN_Pos)
#define | ADC_INTEN_ADCXIEN_6 (0x40 << ADC_INTEN_ADCXIEN_Pos)
#define | ADC_INTEN_ADCXIEN_7 (0x80 << ADC_INTEN_ADCXIEN_Pos)
#define | ADC_INTEN_ADCXIEN_8 (0x1 << ADC_INTEN_ADC15_8XIEN_Pos)
#define | ADC_INTEN_ADCXIEN_9 (0x2 << ADC_INTEN_ADC15_8XIEN_Pos)
#define | ADC_INTEN_ADCXIEN_10 (0x4 << ADC_INTEN_ADC15_8XIEN_Pos)
#define | ADC_INTEN_ADCXIEN_11 (0x8 << ADC_INTEN_ADC15_8XIEN_Pos)
#define | ADC_INTEN_ADCXIEN_12 (0x10 << ADC_INTEN_ADC15_8XIEN_Pos)
#define | ADC_INTEN_ADCXIEN_13 (0x20 << ADC_INTEN_ADC15_8XIEN_Pos)
#define | ADC_INTEN_ADCXIEN_14 (0x40 << ADC_INTEN_ADC15_8XIEN_Pos)
#define | ADC_INTEN_ADCXIEN_15 (0x80 << ADC_INTEN_ADC15_8XIEN_Pos)
#define | ADC_INTEN_LLT_IEN_Pos (8UL)
#define | ADC_INTEN_LLT_IEN_Msk (0x100UL)
#define | ADC_INTEN_LLT_IEN ADC_INTEN_LLT_IEN_Msk
#define | ADC_INTEN_HHT_IEN_Pos (9UL)
#define | ADC_INTEN_HHT_IEN_Msk (0x200UL)
#define | ADC_INTEN_HHT_IEN ADC_INTEN_HHT_IEN_Msk
#define | ADC_INTEN_REG_IEN_Pos (10UL)
#define | ADC_INTEN_REG_IEN_Msk (0x400UL)
#define | ADC_INTEN_REG_IEN ADC_INTEN_REG_IEN_Msk
#define | ADC_INTEN_CONT_IEN_Pos (11UL)
#define | ADC_INTEN_CONT_IEN_Msk (0x800UL)
#define | ADC_INTEN_CONT_IEN ADC_INTEN_CONT_IEN_Msk
#define | ADC_INTEN_CONT_ALL (0xFFFUL)
#define | ADC_INTCLR_ADCICLR_Pos (0UL)
#define | ADC_INTCLR_ADC15_8ICLR_Pos (12UL)
#define | ADC_INTCLR_ADCICLR_Msk (0xFFUL | 0xFF000UL)
#define | ADC_INTCLR_ADCICLR ADC_INTCLR_ADCICLR_Msk
#define | ADC_INTCLR_ADCICLR_0 (0x1 << ADC_INTCLR_ADCICLR_Pos)
#define | ADC_INTCLR_ADCICLR_1 (0x2 << ADC_INTCLR_ADCICLR_Pos)
#define | ADC_INTCLR_ADCICLR_2 (0x4 << ADC_INTCLR_ADCICLR_Pos)
#define | ADC_INTCLR_ADCICLR_3 (0x8 << ADC_INTCLR_ADCICLR_Pos)
#define | ADC_INTCLR_ADCICLR_4 (0x10 << ADC_INTCLR_ADCICLR_Pos)
#define | ADC_INTCLR_ADCICLR_5 (0x20 << ADC_INTCLR_ADCICLR_Pos)
#define | ADC_INTCLR_ADCICLR_6 (0x40 << ADC_INTCLR_ADCICLR_Pos)
#define | ADC_INTCLR_ADCICLR_7 (0x80 << ADC_INTCLR_ADCICLR_Pos)
#define | ADC_INTCLR_ADCICLR_8 (0x1 << ADC_INTCLR_ADC15_8ICLR_Pos)
#define | ADC_INTCLR_ADCICLR_9 (0x2 << ADC_INTCLR_ADC15_8ICLR_Pos)
#define | ADC_INTCLR_ADCICLR_10 (0x4 << ADC_INTCLR_ADC15_8ICLR_Pos)
#define | ADC_INTCLR_ADCICLR_11 (0x8 << ADC_INTCLR_ADC15_8ICLR_Pos)
#define | ADC_INTCLR_ADCICLR_12 (0x10 << ADC_INTCLR_ADC15_8ICLR_Pos)
#define | ADC_INTCLR_ADCICLR_13 (0x20 << ADC_INTCLR_ADC15_8ICLR_Pos)
#define | ADC_INTCLR_ADCICLR_14 (0x40 << ADC_INTCLR_ADC15_8ICLR_Pos)
#define | ADC_INTCLR_ADCICLR_15 (0x80 << ADC_INTCLR_ADC15_8ICLR_Pos)
#define | ADC_INTCLR_LLT_INTC_Pos (8UL)
#define | ADC_INTCLR_LLT_INTC_Msk (0x100UL)
#define | ADC_INTCLR_LLT_INTC ADC_INTCLR_LLT_INTC_Msk
#define | ADC_INTCLR_HHT_INTC_Pos (9UL)
#define | ADC_INTCLR_HHT_INTC_Msk (0x200UL)
#define | ADC_INTCLR_HHT_INTC ADC_INTCLR_HHT_INTC_Msk
#define | ADC_INTCLR_REG_INTC_Pos (10UL)
#define | ADC_INTCLR_REG_INTC_Msk (0x400UL)
#define | ADC_INTCLR_REG_INTC ADC_INTCLR_REG_INTC_Msk
#define | ADC_INTCLR_CONT_INTC_Pos (11UL)
#define | ADC_INTCLR_CONT_INTC_Msk (0x800UL)
#define | ADC_INTCLR_CONT_INTC ADC_INTCLR_CONT_INTC_Msk
#define | ADC_RAWINTSR_ADCRIS_Pos (0UL)
#define | ADC_RAWINTSR_ADC15_8RIS_Pos (12UL)
#define | ADC_RAWINTSR_ADCRIS_Msk (0xFFUL | 0xFF000UL)
#define | ADC_RAWINTSR_ADCRIS ADC_RAWINTSR_ADCRIS_Msk
#define | ADC_RAWINTSR_ADCRIS_0 (0x1 << ADC_RAWINTSR_ADCRIS_Pos)
#define | ADC_RAWINTSR_ADCRIS_1 (0x2 << ADC_RAWINTSR_ADCRIS_Pos)
#define | ADC_RAWINTSR_ADCRIS_2 (0x4 << ADC_RAWINTSR_ADCRIS_Pos)
#define | ADC_RAWINTSR_ADCRIS_3 (0x8 << ADC_RAWINTSR_ADCRIS_Pos)
#define | ADC_RAWINTSR_ADCRIS_4 (0x10 << ADC_RAWINTSR_ADCRIS_Pos)
#define | ADC_RAWINTSR_ADCRIS_5 (0x20 << ADC_RAWINTSR_ADCRIS_Pos)
#define | ADC_RAWINTSR_ADCRIS_6 (0x40 << ADC_RAWINTSR_ADCRIS_Pos)
#define | ADC_RAWINTSR_ADCRIS_7 (0x80 << ADC_RAWINTSR_ADCRIS_Pos)
#define | ADC_RAWINTSR_ADCRIS_8 (0x1 << ADC_RAWINTSR_ADC15_8RIS_Pos)
#define | ADC_RAWINTSR_ADCRIS_9 (0x2 << ADC_RAWINTSR_ADC15_8RIS_Pos)
#define | ADC_RAWINTSR_ADCRIS_10 (0x4 << ADC_RAWINTSR_ADC15_8RIS_Pos)
#define | ADC_RAWINTSR_ADCRIS_11 (0x8 << ADC_RAWINTSR_ADC15_8RIS_Pos)
#define | ADC_RAWINTSR_ADCRIS_12 (0x10 << ADC_RAWINTSR_ADC15_8RIS_Pos)
#define | ADC_RAWINTSR_ADCRIS_13 (0x20 << ADC_RAWINTSR_ADC15_8RIS_Pos)
#define | ADC_RAWINTSR_ADCRIS_14 (0x40 << ADC_RAWINTSR_ADC15_8RIS_Pos)
#define | ADC_RAWINTSR_ADCRIS_15 (0x80 << ADC_RAWINTSR_ADC15_8RIS_Pos)
#define | ADC_RAWINTSR_LLT_INTF_Pos (8UL)
#define | ADC_RAWINTSR_LLT_INTF_Msk (0x100UL)
#define | ADC_RAWINTSR_LLT_INTF ADC_RAWINTSR_LLT_INTF_Msk
#define | ADC_RAWINTSR_HHT_INTF_Pos (9UL)
#define | ADC_RAWINTSR_HHT_INTF_Msk (0x200UL)
#define | ADC_RAWINTSR_HHT_INTF ADC_RAWINTSR_HHT_INTF_Msk
#define | ADC_RAWINTSR_REG_INTF_Pos (10UL)
#define | ADC_RAWINTSR_REG_INTF_Msk (0x400UL)
#define | ADC_RAWINTSR_REG_INTF ADC_RAWINTSR_REG_INTF_Msk
#define | ADC_RAWINTSR_CONT_INTF_Pos (11UL)
#define | ADC_RAWINTSR_CONT_INTF_Msk (0x800UL)
#define | ADC_RAWINTSR_CONT_INTF ADC_RAWINTSR_CONT_INTF_Msk
#define | ADC_MSKINTSR_ADCMIS_Pos (0UL)
#define | ADC_MSKINTSR_ADC15_8MIS_Pos (12UL)
#define | ADC_MSKINTSR_ADCMIS_Msk (0xFFUL | 0xFF000UL)
#define | ADC_MSKINTSR_ADCMIS ADC_MSKINTSR_ADCMIS_Msk
#define | ADC_MSKINTSR_ADCMIS_0 (0x1 << ADC_MSKINTSR_ADCMIS_Pos)
#define | ADC_MSKINTSR_ADCMIS_1 (0x2 << ADC_MSKINTSR_ADCMIS_Pos)
#define | ADC_MSKINTSR_ADCMIS_2 (0x4 << ADC_MSKINTSR_ADCMIS_Pos)
#define | ADC_MSKINTSR_ADCMIS_3 (0x8 << ADC_MSKINTSR_ADCMIS_Pos)
#define | ADC_MSKINTSR_ADCMIS_4 (0x10 << ADC_MSKINTSR_ADCMIS_Pos)
#define | ADC_MSKINTSR_ADCMIS_5 (0x20 << ADC_MSKINTSR_ADCMIS_Pos)
#define | ADC_MSKINTSR_ADCMIS_6 (0x40 << ADC_MSKINTSR_ADCMIS_Pos)
#define | ADC_MSKINTSR_ADCMIS_7 (0x80 << ADC_MSKINTSR_ADCMIS_Pos)
#define | ADC_MSKINTSR_ADCMIS_8 (0x1 << ADC_MSKINTSR_ADC15_8MIS_Pos)
#define | ADC_MSKINTSR_ADCMIS_9 (0x2 << ADC_MSKINTSR_ADC15_8MIS_Pos)
#define | ADC_MSKINTSR_ADCMIS_10 (0x4 << ADC_MSKINTSR_ADC15_8MIS_Pos)
#define | ADC_MSKINTSR_ADCMIS_11 (0x8 << ADC_MSKINTSR_ADC15_8MIS_Pos)
#define | ADC_MSKINTSR_ADCMIS_12 (0x10 << ADC_MSKINTSR_ADC15_8MIS_Pos)
#define | ADC_MSKINTSR_ADCMIS_13 (0x20 << ADC_MSKINTSR_ADC15_8MIS_Pos)
#define | ADC_MSKINTSR_ADCMIS_14 (0x40 << ADC_MSKINTSR_ADC15_8MIS_Pos)
#define | ADC_MSKINTSR_ADCMIS_15 (0x80 << ADC_MSKINTSR_ADC15_8MIS_Pos)
#define | ADC_MSKINTSR_LLT_MIF_Pos (8UL)
#define | ADC_MSKINTSR_LLT_MIF_Msk (0x100UL)
#define | ADC_MSKINTSR_LLT_MIF ADC_MSKINTSR_LLT_MIF_Msk
#define | ADC_MSKINTSR_HHT_MIF_Pos (9UL)
#define | ADC_MSKINTSR_HHT_MIF_Msk (0x200UL)
#define | ADC_MSKINTSR_HHT_MIF ADC_MSKINTSR_HHT_MIF_Msk
#define | ADC_MSKINTSR_REG_MIF_Pos (10UL)
#define | ADC_MSKINTSR_REG_MIF_Msk (0x400UL)
#define | ADC_MSKINTSR_REG_MIF ADC_MSKINTSR_REG_MIF_Msk
#define | ADC_MSKINTSR_CONT_MIF_Pos (11UL)
#define | ADC_MSKINTSR_CONT_MIF_Msk (0x800UL)
#define | ADC_MSKINTSR_CONT_MIF ADC_MSKINTSR_CONT_MIF_Msk
#define | RTC_CR_BYPSHAD_Pos (0UL)
#define | RTC_CR_BYPSHAD_Msk (0x1UL)
#define | RTC_CR_BYPSHAD RTC_CR_BYPSHAD_Msk
#define | RTC_CR_RTC1HZOE_Pos (1UL)
#define | RTC_CR_RTC1HZOE_Msk (0x2UL)
#define | RTC_CR_RTC1HZOE RTC_CR_RTC1HZOE_Msk
#define | RTC_CR_FMT_Pos (2UL)
#define | RTC_CR_FMT_Msk (0x4UL)
#define | RTC_CR_FMT RTC_CR_FMT_Msk
#define | RTC_CR_ALM1_INTEN_Pos (4UL)
#define | RTC_CR_ALM1_INTEN_Msk (0x10UL)
#define | RTC_CR_ALM1_INTEN RTC_CR_ALM1_INTEN_Msk
#define | RTC_CR_ALM2_INTEN_Pos (5UL)
#define | RTC_CR_ALM2_INTEN_Msk (0x20UL)
#define | RTC_CR_ALM2_INTEN RTC_CR_ALM2_INTEN_Msk
#define | RTC_CR_ALM1EN_Pos (6UL)
#define | RTC_CR_ALM1EN_Msk (0x40UL)
#define | RTC_CR_ALM1EN RTC_CR_ALM1EN_Msk
#define | RTC_CR_START_Pos (8UL)
#define | RTC_CR_START_Msk (0x100UL)
#define | RTC_CR_START RTC_CR_START_Msk
#define | RTC_CLKCR_HSEDIV_Pos (0UL)
#define | RTC_CLKCR_HSEDIV_Msk (0x3FFUL)
#define | RTC_CLKCR_HSEDIV RTC_CLKCR_HSEDIV_Msk
#define | RTC_CLKCR_RTCCKSEL_Pos (16UL)
#define | RTC_CLKCR_RTCCKSEL_Msk (0x30000UL)
#define | RTC_CLKCR_RTCCKEN_Pos (20UL)
#define | RTC_CLKCR_RTCCKEN_Msk (0x100000UL)
#define | RTC_CLKCR_RTCCKEN RTC_CLKCR_RTCCKEN_Msk
#define | RTC_TIME_SEC_Pos (0UL)
#define | RTC_TIME_SEC_Msk (0x7FUL)
#define | RTC_TIME_SEC RTC_TIME_SEC_Msk
#define | RTC_TIME_MIN_Pos (8UL)
#define | RTC_TIME_MIN_Msk (0x7F00UL)
#define | RTC_TIME_MIN RTC_TIME_MIN_Msk
#define | RTC_TIME_HOUR19_Pos (16UL)
#define | RTC_TIME_HOUR19_Msk (0x1F0000UL)
#define | RTC_TIME_HOUR19 RTC_TIME_HOUR19_Msk
#define | RTC_TIME_H20_PA_Pos (21UL)
#define | RTC_TIME_H20_PA_Msk (0x200000UL)
#define | RTC_TIME_H20_PA RTC_TIME_H20_PA_Msk
#define | RTC_TIME_WEEK_Pos (24UL)
#define | RTC_TIME_WEEK_Msk (0x7000000UL)
#define | RTC_TIME_WEEK RTC_TIME_WEEK_Msk
#define | RTC_DATE_DAY_Pos (0UL)
#define | RTC_DATE_DAY_Msk (0x3FUL)
#define | RTC_DATE_DAY RTC_DATE_DAY_Msk
#define | RTC_DATE_MONTH_Pos (8UL)
#define | RTC_DATE_MONTH_Msk (0x1F00UL)
#define | RTC_DATE_MONTH RTC_DATE_MONTH_Msk
#define | RTC_DATE_CEN_Pos (15UL)
#define | RTC_DATE_CEN_Msk (0x8000UL)
#define | RTC_DATE_CEN RTC_DATE_CEN_Msk
#define | RTC_DATE_YEAR_Pos (16UL)
#define | RTC_DATE_YEAR_Msk (0xFF0000UL)
#define | RTC_DATE_YEAR RTC_DATE_YEAR_Msk
#define | RTC_ALM1TIME_ALSEC_Pos (0UL)
#define | RTC_ALM1TIME_ALSEC_Msk (0x7FUL)
#define | RTC_ALM1TIME_ALMIN_Pos (8UL)
#define | RTC_ALM1TIME_ALMIN_Msk (0x7F00UL)
#define | RTC_ALM1TIME_ALHOUR19_Pos (16UL)
#define | RTC_ALM1TIME_ALHOUR19_Msk (0x1F0000UL)
#define | RTC_ALM1TIME_ALH20_PA_Pos (21UL)
#define | RTC_ALM1TIME_ALH20_PA_Msk (0x200000UL)
#define | RTC_ALM1TIME_ALWEEK_Pos (24UL)
#define | RTC_ALM1TIME_ALWEEK_Msk (0x7000000UL)
#define | RTC_ALM1DATE_ALDAY_Pos (0UL)
#define | RTC_ALM1DATE_ALDAY_Msk (0x3FUL)
#define | RTC_ALM1DATE_ALMONTH_Pos (8UL)
#define | RTC_ALM1DATE_ALMONTH_Msk (0x1F00UL)
#define | RTC_ALM1DATE_ALCEN_Pos (15UL)
#define | RTC_ALM1DATE_ALCEN_Msk (0x8000UL)
#define | RTC_ALM1DATE_ALYEAR_Pos (16UL)
#define | RTC_ALM1DATE_ALYEAR_Msk (0xFF0000UL)
#define | RTC_ALM1DATE_ALYEAR RTC_ALM1DATE_ALYEAR_Msk
#define | RTC_ALM1DATE_ALMSECEN_Pos (24UL)
#define | RTC_ALM1DATE_ALMSECEN_Msk (0x1000000UL)
#define | RTC_ALM1DATE_ALMSECEN RTC_ALM1DATE_ALMSECEN_Msk
#define | RTC_ALM1DATE_ALMMINEN_Pos (25UL)
#define | RTC_ALM1DATE_ALMMINEN_Msk (0x2000000UL)
#define | RTC_ALM1DATE_ALMMINEN RTC_ALM1DATE_ALMMINEN_Msk
#define | RTC_ALM1DATE_ALMHOUREN_Pos (26UL)
#define | RTC_ALM1DATE_ALMHOUREN_Msk (0x4000000UL)
#define | RTC_ALM1DATE_ALMHOUREN RTC_ALM1DATE_ALMHOUREN_Msk
#define | RTC_ALM1DATE_ALMWEEKEN_Pos (27UL)
#define | RTC_ALM1DATE_ALMWEEKEN_Msk (0x8000000UL)
#define | RTC_ALM1DATE_ALMWEEKEN RTC_ALM1DATE_ALMWEEKEN_Msk
#define | RTC_ALM1DATE_ALMDAYEN_Pos (28UL)
#define | RTC_ALM1DATE_ALMDAYEN_Msk (0x10000000UL)
#define | RTC_ALM1DATE_ALMDAYEN RTC_ALM1DATE_ALMDAYEN_Msk
#define | RTC_ALM1DATE_ALMMONEN_Pos (29UL)
#define | RTC_ALM1DATE_ALMMONEN_Msk (0x20000000UL)
#define | RTC_ALM1DATE_ALMMONEN RTC_ALM1DATE_ALMMONEN_Msk
#define | RTC_ALM1DATE_ALMYEAREN_Pos (30UL)
#define | RTC_ALM1DATE_ALMYEAREN_Msk (0x40000000UL)
#define | RTC_ALM1DATE_ALMYEAREN RTC_ALM1DATE_ALMYEAREN_Msk
#define | RTC_ALM2PRD_ALM2PR_CNT_Pos (0UL)
#define | RTC_ALM2PRD_ALM2PR_CNT_Msk (0xFUL)
#define | RTC_CLKTRIM_TRIM_Pos (0UL)
#define | RTC_CLKTRIM_TRIM_Msk (0xFFUL)
#define | RTC_CLKTRIM_MODE_1_0_Pos (8UL)
#define | RTC_CLKTRIM_MODE_1_0_Msk (0x100UL)
#define | RTC_ISR_WAIT_Pos (0UL)
#define | RTC_ISR_WAIT_Msk (0x1UL)
#define | RTC_ISR_WAIT RTC_ISR_WAIT_Msk
#define | RTC_ISR_WAITF_Pos (1UL)
#define | RTC_ISR_WAITF_Msk (0x2UL)
#define | RTC_ISR_WAITF RTC_ISR_WAITF_Msk
#define | RTC_ISR_RSF_Pos (2UL)
#define | RTC_ISR_RSF_Msk (0x4UL)
#define | RTC_ISR_RSF RTC_ISR_RSF_Msk
#define | RTC_ISR_ALM1_F_Pos (4UL)
#define | RTC_ISR_ALM1_F_Msk (0x10UL)
#define | RTC_ISR_ALM1_F RTC_ISR_ALM1_F_Msk
#define | RTC_ISR_ALM2_F_Pos (5UL)
#define | RTC_ISR_ALM2_F_Msk (0x20UL)
#define | RTC_ISR_ALM2_F RTC_ISR_ALM2_F_Msk
#define | RTC_INTCLR_ALM1_CLR_Pos (4UL)
#define | RTC_INTCLR_ALM1_CLR_Msk (0x10UL)
#define | RTC_INTCLR_ALM1_CLR RTC_INTCLR_ALM1_CLR_Msk
#define | RTC_INTCLR_ALM2_CLR_Pos (5UL)
#define | RTC_INTCLR_ALM2_CLR_Msk (0x20UL)
#define | RTC_INTCLR_ALM2_CLR RTC_INTCLR_ALM2_CLR_Msk
#define | RTC_WPR_WPR_Pos (0UL)
#define | RTC_WPR_WPR_Msk (0xFFUL)
#define | CLKTRIM_CR_TRIM_START_Pos (0UL)
#define | CLKTRIM_CR_TRIM_START_Msk (0x1UL)
#define | CLKTRIM_CR_TRIM_START CLKTRIM_CR_TRIM_START_Msk
#define | CLKTRIM_CR_REFCLK_SEL_Pos (1UL)
#define | CLKTRIM_CR_REFCLK_SEL_Msk (0xEUL)
#define | CLKTRIM_CR_REFCLK_SEL CLKTRIM_CR_REFCLK_SEL_Msk
#define | CLKTRIM_CR_REFCLK_SEL_0 (0x1 << CLKTRIM_CR_REFCLK_SEL_Pos)
#define | CLKTRIM_CR_REFCLK_SEL_1 (0x2 << CLKTRIM_CR_REFCLK_SEL_Pos)
#define | CLKTRIM_CR_REFCLK_SEL_2 (0x4 << CLKTRIM_CR_REFCLK_SEL_Pos)
#define | CLKTRIM_CR_CALCLK_SEL_Pos (4UL)
#define | CLKTRIM_CR_CALCLK_SEL_Msk (0x30UL)
#define | CLKTRIM_CR_CALCLK_SEL CLKTRIM_CR_CALCLK_SEL_Msk
#define | CLKTRIM_CR_CALCLK_SEL_0 (0x1 << CLKTRIM_CR_CALCLK_SEL_Pos)
#define | CLKTRIM_CR_CALCLK_SEL_1 (0x2 << CLKTRIM_CR_CALCLK_SEL_Pos)
#define | CLKTRIM_CR_CALCLK_SEL_2 (0x4 << CLKTRIM_CR_CALCLK_SEL_Pos)
#define | CLKTRIM_CR_MON_EN_Pos (6UL)
#define | CLKTRIM_CR_MON_EN_Msk (0x40UL)
#define | CLKTRIM_CR_MON_EN CLKTRIM_CR_MON_EN_Msk
#define | CLKTRIM_CR_IE_Pos (7UL)
#define | CLKTRIM_CR_IE_Msk (0x80UL)
#define | CLKTRIM_CR_IE CLKTRIM_CR_IE_Msk
#define | CLKTRIM_CR_CLKEN_Pos (8UL)
#define | CLKTRIM_CR_CLKEN_Msk (0x100UL)
#define | CLKTRIM_CR_CLKEN CLKTRIM_CR_CLKEN_Msk
#define | CLKTRIM_CR_ALL_Msk (0x1FFUL)
#define | CLKTRIM_REFCON_RCNTVAL_Pos (0UL)
#define | CLKTRIM_REFCON_RCNTVAL_Msk (0xFFFFFFFFUL)
#define | CLKTRIM_REFCON_RCNTVAL CLKTRIM_REFCON_RCNTVAL_Msk
#define | CLKTRIM_REFCNT_REFCNT_Pos (0UL)
#define | CLKTRIM_REFCNT_REFCNT_Msk (0xFFFFFFFFUL)
#define | CLKTRIM_REFCNT_REFCNT CLKTRIM_REFCNT_REFCNT_Msk
#define | CLKTRIM_CALCNT_CALCNT_Pos (0UL)
#define | CLKTRIM_CALCNT_CALCNT_Msk (0xFFFFFFFFUL)
#define | CLKTRIM_CALCNT_CALCNT CLKTRIM_CALCNT_CALCNT_Msk
#define | CLKTRIM_IFR_STOP_Pos (0UL)
#define | CLKTRIM_IFR_STOP_Msk (0x1UL)
#define | CLKTRIM_IFR_STOP CLKTRIM_IFR_STOP_Msk
#define | CLKTRIM_IFR_CALCNT_OVF_Pos (1UL)
#define | CLKTRIM_IFR_CALCNT_OVF_Msk (0x2UL)
#define | CLKTRIM_IFR_CALCNT_OVF CLKTRIM_IFR_CALCNT_OVF_Msk
#define | CLKTRIM_IFR_LSE_FAULT_Pos (2UL)
#define | CLKTRIM_IFR_LSE_FAULT_Msk (0x4UL)
#define | CLKTRIM_IFR_LSE_FAULT CLKTRIM_IFR_LSE_FAULT_Msk
#define | CLKTRIM_IFR_HSE_FAULT_Pos (3UL)
#define | CLKTRIM_IFR_HSE_FAULT_Msk (0x8UL)
#define | CLKTRIM_IFR_HSE_FAULT CLKTRIM_IFR_HSE_FAULT_Msk
#define | CLKTRIM_ICLR_LSE_FAULT_CLR_Pos (2UL)
#define | CLKTRIM_ICLR_LSE_FAULT_CLR_Msk (0x4UL)
#define | CLKTRIM_ICLR_LSE_FAULT_CLR CLKTRIM_ICLR_LSE_FAULT_CLR_Msk
#define | CLKTRIM_ICLR_HSE_FAULT_CLR_Pos (3UL)
#define | CLKTRIM_ICLR_HSE_FAULT_CLR_Msk (0x8UL)
#define | CLKTRIM_ICLR_HSE_FAULT_CLR CLKTRIM_ICLR_HSE_FAULT_CLR_Msk
#define | CLKTRIM_CALCON_CALOVCNT_Pos (0UL)
#define | CLKTRIM_CALCON_CALOVCNT_Msk (0xFFFFUL)
#define | CLKTRIM_CALCON_CALOVCNT CLKTRIM_CALCON_CALOVCNT_Msk
#define | OWIRE_CR_CLKDIV_Pos (0UL)
#define | OWIRE_CR_CLKDIV_Msk (0x3UL)
#define | OWIRE_CR_SIZE_Pos (4UL)
#define | OWIRE_CR_SIZE_Msk (0x10UL)
#define | OWIRE_CR_EN_Pos (5UL)
#define | OWIRE_CR_EN_Msk (0x20UL)
#define | OWIRE_CR_MSBFIRST_Pos (6UL)
#define | OWIRE_CR_MSBFIRST_Msk (0x40UL)
#define | OWIRE_CR_RDMODE_Pos (7UL)
#define | OWIRE_CR_RDMODE_Msk (0x80UL)
#define | OWIRE_NFCR_NFDIV_Pos (0UL)
#define | OWIRE_NFCR_NFDIV_Msk (0x3UL)
#define | OWIRE_NFCR_NFEN_Pos (4UL)
#define | OWIRE_NFCR_NFEN_Msk (0x10UL)
#define | OWIRE_RSTCNT_RSTCNT_Pos (0UL)
#define | OWIRE_RSTCNT_RSTCNT_Msk (0xFFFFUL)
#define | OWIRE_PRESCNT_PRESCNT_Pos (0UL)
#define | OWIRE_PRESCNT_PRESCNT_Msk (0x1FFFUL)
#define | OWIRE_BITRATECNT_BITRATECNT_Pos (0UL)
#define | OWIRE_BITRATECNT_BITRATECNT_Msk (0xFFFUL)
#define | OWIRE_DRVCNT_DRVCNT_Pos (0UL)
#define | OWIRE_DRVCNT_DRVCNT_Msk (0x1FFUL)
#define | OWIRE_RDSMPCNT_RDSMPCNT_Pos (0UL)
#define | OWIRE_RDSMPCNT_RDSMPCNT_Msk (0x1FFUL)
#define | OWIRE_RECCNT_RECCNT_Pos (0UL)
#define | OWIRE_RECCNT_RECCNT_Msk (0x7FFUL)
#define | OWIRE_DATA_DRVCNT_Pos (0UL)
#define | OWIRE_DATA_DRVCNT_Msk (0xFFUL)
#define | OWIRE_CMD_CMD_Pos (0UL)
#define | OWIRE_CMD_CMD_Msk (0x3UL)
#define | OWIRE_INTEN_ACKERREN_Pos (0UL)
#define | OWIRE_INTEN_ACKERREN_Msk (0x1UL)
#define | OWIRE_INTEN_INITEN_Pos (1UL)
#define | OWIRE_INTEN_INITEN_Msk (0x2UL)
#define | OWIRE_INTEN_TXDONEEN_Pos (2UL)
#define | OWIRE_INTEN_TXDONEEN_Msk (0x4UL)
#define | OWIRE_INTEN_RXDONEEN_Pos (3UL)
#define | OWIRE_INTEN_RXDONEEN_Msk (0x8UL)
#define | OWIRE_SR_ACKERR_Pos (0UL)
#define | OWIRE_SR_ACKERR_Msk (0x1UL)
#define | OWIRE_SR_INITDONE_Pos (1UL)
#define | OWIRE_SR_INITDONE_Msk (0x2UL)
#define | OWIRE_SR_TXDONE_Pos (2UL)
#define | OWIRE_SR_TXDONE_Msk (0x4UL)
#define | OWIRE_SR_RXDONE_Pos (3UL)
#define | OWIRE_SR_RXDONE_Msk (0x8UL)
#define | OWIRE_INTCLR_ACKERRCLR_Pos (0UL)
#define | OWIRE_INTCLR_ACKERRCLR_Msk (0x1UL)
#define | OWIRE_INTCLR_INTDONCECLR_Pos (1UL)
#define | OWIRE_INTCLR_INTDONCECLR_Msk (0x2UL)
#define | OWIRE_INTCLR_TXDONECLR_Pos (2UL)
#define | OWIRE_INTCLR_TXDONECLR_Msk (0x4UL)
#define | OWIRE_INTCLR_RXDONECLR_Pos (3UL)
#define | OWIRE_INTCLR_RXDONECLR_Msk (0x8UL)
#define | SPI_CR_SPR0_Pos (0UL)
#define | SPI_CR_SPR0_Msk (0x1UL)
#define | SPI_CR_SPR0 SPI_CR_SPR0_Msk
#define | SPI_CR_SPR1_Pos (1UL)
#define | SPI_CR_SPR1_Msk (0x2UL)
#define | SPI_CR_SPR1 SPI_CR_SPR1_Msk
#define | SPI_CR_CPHA_Pos (2UL)
#define | SPI_CR_CPHA_Msk (0x4UL)
#define | SPI_CR_CPHA SPI_CR_CPHA_Msk
#define | SPI_CR_CPOL_Pos (3UL)
#define | SPI_CR_CPOL_Msk (0x8UL)
#define | SPI_CR_CPOL SPI_CR_CPOL_Msk
#define | SPI_CR_MSTR_Pos (4UL)
#define | SPI_CR_MSTR_Msk (0x10UL)
#define | SPI_CR_MSTR SPI_CR_MSTR_Msk
#define | SPI_CR_SPEN_Pos (6UL)
#define | SPI_CR_SPEN_Msk (0x40UL)
#define | SPI_CR_SPEN SPI_CR_SPEN_Msk
#define | SPI_CR_SPR2_Pos (7UL)
#define | SPI_CR_SPR2_Msk (0x80UL)
#define | SPI_CR_SPR2 SPI_CR_SPR2_Msk
#define | SPI_SSN_SSN_Pos (0UL)
#define | SPI_SSN_SSN_Msk (0x1UL)
#define | SPI_SSN_SSN SPI_SSN_SSN_Msk
#define | SPI_SR_MDF_Pos (4UL)
#define | SPI_SR_MDF_Msk (0x10UL)
#define | SPI_SR_MDF SPI_SR_MDF_Msk
#define | SPI_SR_SSERR_Pos (5UL)
#define | SPI_SR_SSERR_Msk (0x20UL)
#define | SPI_SR_SSERR SPI_SR_SSERR_Msk
#define | SPI_SR_WCOL_Pos (6UL)
#define | SPI_SR_WCOL_Msk (0x40UL)
#define | SPI_SR_WCOL SPI_SR_WCOL_Msk
#define | SPI_SR_SPIF_Pos (7UL)
#define | SPI_SR_SPIF_Msk (0x80UL)
#define | SPI_SR_SPIF SPI_SR_SPIF_Msk
#define | SPI_DATA_SPDATA_Pos (0UL)
#define | SPI_DATA_SPDATA_Msk (0xFFUL)
#define | I2C_CR_H1M_Pos (0UL)
#define | I2C_CR_H1M_Msk (0x1UL)
#define | I2C_CR_H1M I2C_CR_H1M_Msk
#define | I2C_CR_AA_Pos (2UL)
#define | I2C_CR_AA_Msk (0x4UL)
#define | I2C_CR_AA I2C_CR_AA_Msk
#define | I2C_CR_SI_Pos (3UL)
#define | I2C_CR_SI_Msk (0x8UL)
#define | I2C_CR_SI I2C_CR_SI_Msk
#define | I2C_CR_STO_Pos (4UL)
#define | I2C_CR_STO_Msk (0x10UL)
#define | I2C_CR_STO I2C_CR_STO_Msk
#define | I2C_CR_STA_Pos (5UL)
#define | I2C_CR_STA_Msk (0x20UL)
#define | I2C_CR_STA I2C_CR_STA_Msk
#define | I2C_CR_ENS_Pos (6UL)
#define | I2C_CR_ENS_Msk (0x40UL)
#define | I2C_CR_ENS I2C_CR_ENS_Msk
#define | I2C_DATA_DAT_Pos (0UL)
#define | I2C_DATA_DAT_Msk (0xFFUL)
#define | I2C_ADDR_GC_Pos (0UL)
#define | I2C_ADDR_GC_Msk (0x1UL)
#define | I2C_ADDR_GC I2C_ADDR_GC_Msk
#define | I2C_ADDR_I2CADR_Pos (1UL)
#define | I2C_ADDR_I2CADR_Msk (0xFEUL)
#define | I2C_SR_I2CSTA_Pos (0UL)
#define | I2C_SR_I2CSTA_Msk (0xFFUL)
#define | I2C_TIMRUN_TME_Pos (0UL)
#define | I2C_TIMRUN_TME_Msk (0x1UL)
#define | I2C_TIMRUN_TME I2C_TIMRUN_TME_Msk
#define | I2C_BAUDCR_TM_Pos (0UL)
#define | I2C_BAUDCR_TM_Msk (0xFFUL)
#define | I2C_BAUDCR_TM I2C_BAUDCR_TM_Msk
#define | LPUART_SBUF_SBUF_Pos (0UL)
#define | LPUART_SBUF_SBUF_Msk (0xFFUL)
#define | LPUART_SBUF_SBUF LPUART_SBUF_SBUF_Msk
#define | LPUART_SADDR_SADDR_Pos (0UL)
#define | LPUART_SADDR_SADDR_Msk (0xFFUL)
#define | LPUART_SADDR_SADDR LPUART_SADDR_SADDR_Msk
#define | LPUART_SADEN_SADEN_Pos (0UL)
#define | LPUART_SADEN_SADEN_Msk (0xFFUL)
#define | LPUART_SADEN_SADEN LPUART_SADEN_SADEN_Msk
#define | LPUART_INTSR_RI_Pos (0UL)
#define | LPUART_INTSR_RI_Msk (0x1UL)
#define | LPUART_INTSR_RI LPUART_INTSR_RI_Msk
#define | LPUART_INTSR_TI_Pos (1UL)
#define | LPUART_INTSR_TI_Msk (0x2UL)
#define | LPUART_INTSR_TI LPUART_INTSR_TI_Msk
#define | LPUART_INTSR_FE_Pos (2UL)
#define | LPUART_INTSR_FE_Msk (0x4UL)
#define | LPUART_INTSR_FE LPUART_INTSR_FE_Msk
#define | LPUART_SCON_RIEN_Pos (0UL)
#define | LPUART_SCON_RIEN_Msk (0x1UL)
#define | LPUART_SCON_RIEN LPUART_SCON_RIEN_Msk
#define | LPUART_SCON_TIEN_Pos (1UL)
#define | LPUART_SCON_TIEN_Msk (0x2UL)
#define | LPUART_SCON_TIEN LPUART_SCON_TIEN_Msk
#define | LPUART_SCON_RB8_Pos (2UL)
#define | LPUART_SCON_RB8_Msk (0x4UL)
#define | LPUART_SCON_RB8 LPUART_SCON_RB8_Msk
#define | LPUART_SCON_TB8_Pos (3UL)
#define | LPUART_SCON_TB8_Msk (0x8UL)
#define | LPUART_SCON_TB8 LPUART_SCON_TB8_Msk
#define | LPUART_SCON_REN_Pos (4UL)
#define | LPUART_SCON_REN_Msk (0x10UL)
#define | LPUART_SCON_REN LPUART_SCON_REN_Msk
#define | LPUART_SCON_SM2_Pos (5UL)
#define | LPUART_SCON_SM2_Msk (0x20UL)
#define | LPUART_SCON_SM2 LPUART_SCON_SM2_Msk
#define | LPUART_SCON_SM0_SM1_Pos (6UL)
#define | LPUART_SCON_SM0_SM1_Msk (0x40UL)
#define | LPUART_SCON_SM0_SM1 LPUART_SCON_SM0_SM1_Msk
#define | LPUART_SCON_SM0_SM1_1 (0x1 << LPUART_SCON_SM0_SM1_Pos)
#define | LPUART_SCON_SM0_SM1_0 (0x2 << LPUART_SCON_SM0_SM1_Pos)
#define | LPUART_SCON_TEEN_Pos (8UL)
#define | LPUART_SCON_TEEN_Msk (0x100UL)
#define | LPUART_SCON_TEEN LPUART_SCON_TEEN_Msk
#define | LPUART_SCON_DBAUD_Pos (9UL)
#define | LPUART_SCON_DBAUD_Msk (0x200UL)
#define | LPUART_SCON_DBAUD LPUART_SCON_DBAUD_Msk
#define | LPUART_SCON_LPMODE_Pos (10UL)
#define | LPUART_SCON_LPMODE_Msk (0x400UL)
#define | LPUART_SCON_LPMODE LPUART_SCON_LPMODE_Msk
#define | LPUART_SCON_SCLKSEL_Pos (11UL)
#define | LPUART_SCON_SCLKSEL_Msk (0x1800UL)
#define | LPUART_SCON_SCLKSEL LPUART_SCON_SCLKSEL_Msk
#define | LPUART_SCON_SCLKSEL_0 (0x1 << LPUART_SCON_SCLKSEL_Pos)
#define | LPUART_SCON_SCLKSEL_1 (0x2 << LPUART_SCON_SCLKSEL_Pos)
#define | LPUART_SCON_PRSC_Pos (13UL)
#define | LPUART_SCON_PRSC_Msk (0xE000UL)
#define | LPUART_SCON_PRSC LPUART_SCON_PRSC_Msk
#define | LPUART_SCON_PRSC_0 (0x1 << LPUART_SCON_PRSC_Pos)
#define | LPUART_SCON_PRSC_1 (0x2 << LPUART_SCON_PRSC_Pos)
#define | LPUART_SCON_PRSC_2 (0x4 << LPUART_SCON_PRSC_Pos)
#define | LPUART_SCON_EN_Pos (16UL)
#define | LPUART_SCON_EN_Msk (0x10000UL)
#define | LPUART_SCON_EN LPUART_SCON_EN_Msk
#define | LPUART_INTCLR_RICLR_Pos (0UL)
#define | LPUART_INTCLR_RICLR_Msk (0x1UL)
#define | LPUART_INTCLR_RICLR LPUART_INTCLR_RICLR_Msk
#define | LPUART_INTCLR_TICLR_Pos (1UL)
#define | LPUART_INTCLR_TICLR_Msk (0x2UL)
#define | LPUART_INTCLR_TICLR LPUART_INTCLR_TICLR_Msk
#define | LPUART_INTCLR_FECLR_Pos (2UL)
#define | LPUART_INTCLR_FECLR_Msk (0x4UL)
#define | LPUART_INTCLR_FECLR LPUART_INTCLR_FECLR_Msk
#define | LPUART_BAUDCR_BRG_Pos (0UL)
#define | LPUART_BAUDCR_BRG_Msk (0xFFFFUL)
#define | LPUART_BAUDCR_BRG LPUART_BAUDCR_BRG_Msk
#define | LPUART_BAUDCR_SELF_BRG_Pos (16UL)
#define | LPUART_BAUDCR_SELF_BRG_Msk (0x10000UL)
#define | LPUART_BAUDCR_SELF_BRG LPUART_BAUDCR_SELF_BRG_Msk
#define | UART_SCON_RIEN_Pos (0UL)
#define | UART_SCON_RIEN_Msk (0x1UL)
#define | UART_SCON_RIEN UART_SCON_RIEN_Msk
#define | UART_SCON_TIEN_Pos (1UL)
#define | UART_SCON_TIEN_Msk (0x2UL)
#define | UART_SCON_TIEN UART_SCON_TIEN_Msk
#define | UART_SCON_RB8_Pos (2UL)
#define | UART_SCON_RB8_Msk (0x4UL)
#define | UART_SCON_RB8 UART_SCON_RB8_Msk
#define | UART_SCON_TB8_Pos (3UL)
#define | UART_SCON_TB8_Msk (0x8UL)
#define | UART_SCON_TB8 UART_SCON_TB8_Msk
#define | UART_SCON_REN_Pos (4UL)
#define | UART_SCON_REN_Msk (0x10UL)
#define | UART_SCON_REN UART_SCON_REN_Msk
#define | UART_SCON_SM2_Pos (5UL)
#define | UART_SCON_SM2_Msk (0x20UL)
#define | UART_SCON_SM2 UART_SCON_SM2_Msk
#define | UART_SCON_SM0_SM1_Pos (6UL)
#define | UART_SCON_SM0_SM1_Msk (0xC0UL)
#define | UART_SCON_SM0_SM1 UART_SCON_SM0_SM1_Msk
#define | UART_SCON_FEEN_Pos (8UL)
#define | UART_SCON_FEEN_Msk (0x100UL)
#define | UART_SCON_FEEN UART_SCON_FEEN_Msk
#define | UART_SCON_DBAUD_Pos (9UL)
#define | UART_SCON_DBAUD_Msk (0x200UL)
#define | UART_SCON_DBAUD UART_SCON_DBAUD_Msk
#define | UART_SBUF_SBUF_Pos (0UL)
#define | UART_SBUF_SBUF_Msk (0xFFUL)
#define | UART_SBUF_SBUF UART_SBUF_SBUF_Msk
#define | UART_SADDR_SADDR_Pos (0UL)
#define | UART_SADDR_SADDR_Msk (0xFFUL)
#define | UART_SADEN_SADEN_Pos (0UL)
#define | UART_SADEN_SADEN_Msk (0xFFUL)
#define | UART_INTSR_RI_Pos (0UL)
#define | UART_INTSR_RI_Msk (0x1UL)
#define | UART_INTSR_RI UART_INTSR_RI_Msk
#define | UART_INTSR_TI_Pos (1UL)
#define | UART_INTSR_TI_Msk (0x2UL)
#define | UART_INTSR_TI UART_INTSR_TI_Msk
#define | UART_INTSR_FE_Pos (2UL)
#define | UART_INTSR_FE_Msk (0x4UL)
#define | UART_INTSR_FE UART_INTSR_FE_Msk
#define | UART_INTCLR_RICLR_Pos (0UL)
#define | UART_INTCLR_RICLR_Msk (0x1UL)
#define | UART_INTCLR_TICLR_Pos (1UL)
#define | UART_INTCLR_TICLR_Msk (0x2UL)
#define | UART_INTCLR_FECLR_Pos (2UL)
#define | UART_INTCLR_FECLR_Msk (0x4UL)
#define | UART_BAUDCR_BRG_Pos (0UL)
#define | UART_BAUDCR_BRG_Msk (0xFFFFUL)
#define | UART_BAUDCR_BRG UART_BAUDCR_BRG_Msk
#define | UART_BAUDCR_SELF_BRG_Pos (16UL)
#define | UART_BAUDCR_SELF_BRG_Msk (0x10000UL)
#define | UART_BAUDCR_SELF_BRG UART_BAUDCR_SELF_BRG_Msk
#define | UART_BAUDCR_NOREF_Pos (31UL)
#define | UART_BAUDCR_NOREF_Msk (0x80000000UL)
#define | UART_IRDACR_PSC_Pos (0UL)
#define | UART_IRDACR_PSC_Msk (0xFFUL)
#define | UART_IRDACR_IREN_Pos (8UL)
#define | UART_IRDACR_IREN_Msk (0x100UL)
#define | UART_IRDACR_IRTXINV_Pos (9UL)
#define | UART_IRDACR_IRTXINV_Msk (0x200UL)
#define | UART_IRDACR_IRRXINV_Pos (10UL)
#define | UART_IRDACR_IRRXINV_Msk (0x400UL)
#define | UART_IRDACR_IRLPMODE_Pos (11UL)
#define | UART_IRDACR_IRLPMODE_Msk (0x800UL)
#define | WWDG_RLOAD_RLOAD_Pos (0UL)
#define | WWDG_RLOAD_RLOAD_Msk (0xFFUL)
#define | WWDG_RLOAD_RLOAD WWDG_RLOAD_RLOAD_Msk
#define | WWDG_CR_WINCMP_Pos (0UL)
#define | WWDG_CR_WINCMP_Msk (0xFFUL)
#define | WWDG_CR_WINCMP WWDG_CR_WINCMP_Msk
#define | WWDG_CR_PRSC_Pos (8UL)
#define | WWDG_CR_PRSC_Msk (0xFFFFF00UL)
#define | WWDG_CR_PRSC WWDG_CR_PRSC_Msk
#define | WWDG_CR_WWDGEN_Pos (28UL)
#define | WWDG_CR_WWDGEN_Msk (0x10000000UL)
#define | WWDG_CR_WWDGEN WWDG_CR_WWDGEN_Msk
#define | WWDG_INTEN_WWDGIEN_Pos (0UL)
#define | WWDG_INTEN_WWDGIEN_Msk (0x1UL)
#define | WWDG_INTEN_WWDGIEN WWDG_INTEN_WWDGIEN_Msk
#define | WWDG_SR_WWDGIF_Pos (0UL)
#define | WWDG_SR_WWDGIF_Msk (0x1UL)
#define | WWDG_SR_WWDGIF WWDG_SR_WWDGIF_Msk
#define | WWDG_INTCLR_INTCLR_Pos (0UL)
#define | WWDG_INTCLR_INTCLR_Msk (0x1UL)
#define | WWDG_INTCLR_INTCLR WWDG_INTCLR_INTCLR_Msk
#define | WWDG_CNTVAL_WWDGCNT_Pos (0UL)
#define | WWDG_CNTVAL_WWDGCNT_Msk (0xFFUL)
#define | WWDG_CNTVAL_WWDGCNT WWDG_CNTVAL_WWDGCNT_Msk
#define | IWDG_CMDCR_CMD_Pos (0UL)
#define | IWDG_CMDCR_CMD_Msk (0xFFUL)
#define | IWDG_CFGR_IWDGMODE_Pos (0UL)
#define | IWDG_CFGR_IWDGMODE_Msk (0x1UL)
#define | IWDG_CFGR_IWDGMODE IWDG_CFGR_IWDGMODE_Msk
#define | IWDG_CFGR_IWDGINTMSK_Pos (1UL)
#define | IWDG_CFGR_IWDGINTMSK_Msk (0x2UL)
#define | IWDG_CFGR_IWDGINTMSK IWDG_CFGR_IWDGINTMSK_Msk
#define | IWDG_CFGR_IWDGRUNF_Pos (2UL)
#define | IWDG_CFGR_IWDGRUNF_Msk (0x4UL)
#define | IWDG_RLOAD_IWDGRLOAD_Pos (0UL)
#define | IWDG_RLOAD_IWDGRLOAD_Msk (0xFFFFFUL)
#define | IWDG_RLOAD_IWDGRLOAD IWDG_RLOAD_IWDGRLOAD_Msk
#define | IWDG_CNTVAL_IWDGCNT_Pos (0UL)
#define | IWDG_CNTVAL_IWDGCNT_Msk (0xFFFFFUL)
#define | IWDG_CNTVAL_IWDGCNT IWDG_CNTVAL_IWDGCNT_Msk
#define | IWDG_SR_IWDGOVF_Pos (0UL)
#define | IWDG_SR_IWDGOVF_Msk (0x1UL)
#define | IWDG_INTCLR_IWDGINTCLR_Pos (0UL)
#define | IWDG_INTCLR_IWDGINTCLR_Msk (0x1UL)
#define | IWDG_UNLOCK_IWDGREN_Pos (0UL)
#define | IWDG_UNLOCK_IWDGREN_Msk (0x1UL)
#define | BEEP_CSR_BEEPDIV_Pos (0UL)
#define | BEEP_CSR_BEEPDIV_Msk (0xFFFUL)
#define | BEEP_CSR_BEEPDIV BEEP_CSR_BEEPDIV_Msk
#define | BEEP_CSR_BEEPSEL_Pos (16UL)
#define | BEEP_CSR_BEEPSEL_Msk (0x30000UL)
#define | BEEP_CSR_BEEPSEL BEEP_CSR_BEEPSEL_Msk
#define | BEEP_CSR_BEEPSEL_0 (0x1 << BEEP_CSR_BEEPSEL_Pos)
#define | BEEP_CSR_BEEPSEL_1 (0x2 << BEEP_CSR_BEEPSEL_Pos)
#define | BEEP_CSR_BEEPEN_Pos (18UL)
#define | BEEP_CSR_BEEPEN_Msk (0x40000UL)
#define | BEEP_CSR_BEEPEN BEEP_CSR_BEEPEN_Msk
#define | BEEP_CSR_CLKSEL_Pos (20UL)
#define | BEEP_CSR_CLKSEL_Msk (0x300000UL)
#define | BEEP_CSR_CLKSEL BEEP_CSR_CLKSEL_Msk
#define | BEEP_CSR_CLKSEL_0 (0x1 << BEEP_CSR_CLKSEL_Pos)
#define | BEEP_CSR_CLKSEL_1 (0x2 << BEEP_CSR_CLKSEL_Pos)
#define | BEEP_CSR_CLKSEL_2 (0x4 << BEEP_CSR_CLKSEL_Pos)
#define | BEEP_CSR_ALL_Msk (BEEP_CSR_BEEPDIV_Msk | BEEP_CSR_BEEPSEL_Msk | BEEP_CSR_BEEPEN_Msk | BEEP_CSR_CLKSEL_Msk)
#define | AWK_CR_DIVSEL_Pos (0UL)
#define | AWK_CR_DIVSEL_Msk (0xFUL)
#define | AWK_CR_DIVSEL AWK_CR_DIVSEL_Msk
#define | AWK_CR_DIVSEL_0 (0x1 << AWK_CR_DIVSEL_Pos)
#define | AWK_CR_DIVSEL_1 (0x2 << AWK_CR_DIVSEL_Pos)
#define | AWK_CR_DIVSEL_2 (0x4 << AWK_CR_DIVSEL_Pos)
#define | AWK_CR_DIVSEL_3 (0x8 << AWK_CR_DIVSEL_Pos)
#define | AWK_CR_AWKEN_Pos (4UL)
#define | AWK_CR_AWKEN_Msk (0x10UL)
#define | AWK_CR_AWKEN AWK_CR_AWKEN_Msk
#define | AWK_CR_TCLKSEL_Pos (5UL)
#define | AWK_CR_TCLKSEL_Msk (0x60UL)
#define | AWK_CR_TCLKSEL AWK_CR_TCLKSEL_Msk
#define | AWK_CR_TCLKSEL_0 (0x1 << AWK_CR_TCLKSEL_Pos)
#define | AWK_CR_TCLKSEL_1 (0x2 << AWK_CR_TCLKSEL_Pos)
#define | AWK_CR_HXPRSC_Pos (8UL)
#define | AWK_CR_HXPRSC_Msk (0x7FFF00UL)
#define | AWK_CR_HXPRSC AWK_CR_HXPRSC_Msk
#define | AWK_RLOAD_RLDVAL_Pos (0UL)
#define | AWK_RLOAD_RLDVAL_Msk (0xFFUL)
#define | AWK_RLOAD_RLDVAL AWK_RLOAD_RLDVAL_Msk
#define | AWK_SR_AWUF_Pos (0UL)
#define | AWK_SR_AWUF_Msk (0x1UL)
#define | AWK_SR_AWUF AWK_SR_AWUF_Msk
#define | AWK_INTCLR_INTCLR_Pos (0UL)
#define | AWK_INTCLR_INTCLR_Msk (0x1UL)
#define | AWK_INTCLR_INTCLR AWK_INTCLR_INTCLR_Msk
#define | LPTIM_CNTVAL_LPT_CNT_Pos (0UL)
#define | LPTIM_CNTVAL_LPT_CNT_Msk (0x1UL)
#define | LPTIM_CR_TIM_RUN_Pos (0UL)
#define | LPTIM_CR_TIM_RUN_Msk (0x1UL)
#define | LPTIM_CR_TIM_RUN LPTIM_CR_TIM_RUN_Msk
#define | LPTIM_CR_MODE_Pos (1UL)
#define | LPTIM_CR_MODE_Msk (0x2UL)
#define | LPTIM_CR_MODE LPTIM_CR_MODE_Msk
#define | LPTIM_CR_CT_SEL_Pos (2UL)
#define | LPTIM_CR_CT_SEL_Msk (0x4UL)
#define | LPTIM_CR_CT_SEL LPTIM_CR_CT_SEL_Msk
#define | LPTIM_CR_TOG_EN_Pos (3UL)
#define | LPTIM_CR_TOG_EN_Msk (0x8UL)
#define | LPTIM_CR_TOG_EN LPTIM_CR_TOG_EN_Msk
#define | LPTIM_CR_TCK_SEL_Pos (4UL)
#define | LPTIM_CR_TCK_SEL_Msk (0x30UL)
#define | LPTIM_CR_TCK_SEL LPTIM_CR_TCK_SEL_Msk
#define | LPTIM_CR_TCK_SEL_0 (0x1 << LPTIM_CR_TCK_SEL_Pos)
#define | LPTIM_CR_TCK_SEL_1 (0x2 << LPTIM_CR_TCK_SEL_Pos)
#define | LPTIM_CR_GATE_EN_Pos (6UL)
#define | LPTIM_CR_GATE_EN_Msk (0x40UL)
#define | LPTIM_CR_GATE_EN LPTIM_CR_GATE_EN_Msk
#define | LPTIM_CR_GATE_P_Pos (7UL)
#define | LPTIM_CR_GATE_P_Msk (0x80UL)
#define | LPTIM_CR_GATE_P LPTIM_CR_GATE_P_Msk
#define | LPTIM_CR_INT_EN_Pos (8UL)
#define | LPTIM_CR_INT_EN_Msk (0x100UL)
#define | LPTIM_CR_INT_EN LPTIM_CR_INT_EN_Msk
#define | LPTIM_CR_TCK_EN_Pos (9UL)
#define | LPTIM_CR_TCK_EN_Msk (0x200UL)
#define | LPTIM_CR_TCK_EN LPTIM_CR_TCK_EN_Msk
#define | LPTIM_CR_WT_FLAG_Pos (16UL)
#define | LPTIM_CR_WT_FLAG_Msk (0x10000UL)
#define | LPTIM_CR_WT_FLAG LPTIM_CR_WT_FLAG_Msk
#define | LPTIM_CR_ALL_Msk (0x3FFUL)
#define | LPTIM_LOAD_LOAD_Pos (0UL)
#define | LPTIM_LOAD_LOAD_Msk (0xFFFFUL)
#define | LPTIM_LOAD_LOAD LPTIM_LOAD_LOAD_Msk
#define | LPTIM_INTSR_INTF_Pos (0UL)
#define | LPTIM_INTSR_INTF_Msk (0x01UL)
#define | LPTIM_INTSR_INTF LPTIM_INTSR_INTF_Msk
#define | LPTIM_INTCLR_ICLR_Pos (0UL)
#define | LPTIM_INTCLR_ICLR_Msk (0x1UL)
#define | LPTIM_INTCLR_ICLR LPTIM_INTCLR_ICLR_Msk
#define | LPTIM_BGLOAD_BGLOAD_Pos (0UL)
#define | LPTIM_BGLOAD_BGLOAD_Msk (0xFFFFUL)
#define | LPTIM_BGLOAD_BGLOAD LPTIM_BGLOAD_BGLOAD_Msk
#define | BASETIM_CR_TMR_PRSC_Pos (0UL)
#define | BASETIM_CR_TMR_PRSC_Msk (0x7UL)
#define | BASETIM_CR_TMR_PRSC BASETIM_CR_TMR_PRSC_Msk
#define | BASETIM_CR_TMR_PRSC_0 (0x1 << BASETIM_CR_TMR_PRSC_Pos)
#define | BASETIM_CR_TMR_PRSC_1 (0x2 << BASETIM_CR_TMR_PRSC_Pos)
#define | BASETIM_CR_TMR_PRSC_2 (0x4 << BASETIM_CR_TMR_PRSC_Pos)
#define | BASETIM_CR_ONESHOT_Pos (3UL)
#define | BASETIM_CR_ONESHOT_Msk (0x8UL)
#define | BASETIM_CR_ONESHOT BASETIM_CR_ONESHOT_Msk
#define | BASETIM_CR_TMR_SIZE_Pos (4UL)
#define | BASETIM_CR_TMR_SIZE_Msk (0x10UL)
#define | BASETIM_CR_TMR_SIZE BASETIM_CR_TMR_SIZE_Msk
#define | BASETIM_CR_INTEN_Pos (5UL)
#define | BASETIM_CR_INTEN_Msk (0x20UL)
#define | BASETIM_CR_INTEN BASETIM_CR_INTEN_Msk
#define | BASETIM_CR_MODE_Pos (6UL)
#define | BASETIM_CR_MODE_Msk (0x40UL)
#define | BASETIM_CR_MODE BASETIM_CR_MODE_Msk
#define | BASETIM_CR_TR_Pos (7UL)
#define | BASETIM_CR_TR_Msk (0x80UL)
#define | BASETIM_CR_TR BASETIM_CR_TR_Msk
#define | BASETIM_CR_CT_SEL_Pos (8UL)
#define | BASETIM_CR_CT_SEL_Msk (0x100UL)
#define | BASETIM_CR_CT_SEL BASETIM_CR_CT_SEL_Msk
#define | BASETIM_CR_TOG_EN_Pos (9UL)
#define | BASETIM_CR_TOG_EN_Msk (0x200UL)
#define | BASETIM_CR_TOG_EN BASETIM_CR_TOG_EN_Msk
#define | BASETIM_CR_GATE_EN_Pos (10UL)
#define | BASETIM_CR_GATE_EN_Msk (0x400UL)
#define | BASETIM_CR_GATE_EN BASETIM_CR_GATE_EN_Msk
#define | BASETIM_CR_GATE_P_Pos (11UL)
#define | BASETIM_CR_GATE_P_Msk (0x800UL)
#define | BASETIM_CR_GATE_P BASETIM_CR_GATE_P_Msk
#define | BASETIM_CR_ALL_Msk (0xFFFUL)
#define | BASETIM_LOAD_LOAD_Pos (0UL)
#define | BASETIM_LOAD_LOAD_Msk (0xFFFFFFFFUL)
#define | BASETIM_LOAD_LOAD BASETIM_LOAD_LOAD_Msk
#define | BASETIM_CNT_CNT_Pos (0UL)
#define | BASETIM_CNT_CNT_Msk (0xFFFFFFFFUL)
#define | BASETIM_RAWINTSR_RIS_Pos (0UL)
#define | BASETIM_RAWINTSR_RIS_Msk (0x1UL)
#define | BASETIM_RAWINTSR_RIS BASETIM_RAWINTSR_RIS_Msk
#define | BASETIM_MSKINTSR_TF_Pos (0UL)
#define | BASETIM_MSKINTSR_TF_Msk (0x1UL)
#define | BASETIM_MSKINTSR_TF BASETIM_MSKINTSR_TF_Msk
#define | BASETIM_INTCLR_INTCLR_Pos (0UL)
#define | BASETIM_INTCLR_INTCLR_Msk (0x1UL)
#define | BASETIM_INTCLR_INTCLR BASETIM_INTCLR_INTCLR_Msk
#define | BASETIM_BGLOAD_BGLOAD_Pos (0UL)
#define | BASETIM_BGLOAD_BGLOAD_Msk (0xFFFFFFFFUL)
#define | BASETIM_BGLOAD_BGLOAD BASETIM_BGLOAD_BGLOAD_Msk
#define | PCA_CR_CCF0_Pos (0UL)
#define | PCA_CR_CCF0_Msk (0x1UL)
#define | PCA_CR_CCF0 PCA_CR_CCF0_Msk
#define | PCA_CR_CCF1_Pos (1UL)
#define | PCA_CR_CCF1_Msk (0x2UL)
#define | PCA_CR_CCF1 PCA_CR_CCF1_Msk
#define | PCA_CR_CCF2_Pos (2UL)
#define | PCA_CR_CCF2_Msk (0x4UL)
#define | PCA_CR_CCF2 PCA_CR_CCF2_Msk
#define | PCA_CR_CCF3_Pos (3UL)
#define | PCA_CR_CCF3_Msk (0x8UL)
#define | PCA_CR_CCF3 PCA_CR_CCF3_Msk
#define | PCA_CR_CCF4_Pos (4UL)
#define | PCA_CR_CCF4_Msk (0x10UL)
#define | PCA_CR_CCF4 PCA_CR_CCF4_Msk
#define | PCA_CR_CR_Pos (6UL)
#define | PCA_CR_CR_Msk (0x40UL)
#define | PCA_CR_CR PCA_CR_CR_Msk
#define | PCA_CR_CF_Pos (7UL)
#define | PCA_CR_CF_Msk (0x80UL)
#define | PCA_CR_CF PCA_CR_CF_Msk
#define | PCA_MOD_CFIE_Pos (0UL)
#define | PCA_MOD_CFIE_Msk (0x1UL)
#define | PCA_MOD_CFIE PCA_MOD_CFIE_Msk
#define | PCA_MOD_CPS_Pos (1UL)
#define | PCA_MOD_CPS_Msk (0xEUL)
#define | PCA_MOD_CPS PCA_MOD_CPS_Msk
#define | PCA_MOD_CPS_0 (0x01 << PCA_MOD_CPS_Pos)
#define | PCA_MOD_CPS_1 (0x02 << PCA_MOD_CPS_Pos)
#define | PCA_MOD_CPS_2 (0x04 << PCA_MOD_CPS_Pos)
#define | PCA_MOD_CIDL_Pos (7UL)
#define | PCA_MOD_CIDL_Msk (0x80UL)
#define | PCA_MOD_CIDL PCA_MOD_CIDL_Msk
#define | PCA_CNT_CNT_Pos (0UL)
#define | PCA_CNT_CNT_Msk (0xFFUL)
#define | PCA_INTCLR_CCF0_Pos (0UL)
#define | PCA_INTCLR_CCF0_Msk (0x1UL)
#define | PCA_INTCLR_CCF1_Pos (1UL)
#define | PCA_INTCLR_CCF1_Msk (0x2UL)
#define | PCA_INTCLR_CCF2_Pos (2UL)
#define | PCA_INTCLR_CCF2_Msk (0x4UL)
#define | PCA_INTCLR_CCF3_Pos (3UL)
#define | PCA_INTCLR_CCF3_Msk (0x8UL)
#define | PCA_INTCLR_CCF4_Pos (4UL)
#define | PCA_INTCLR_CCF4_Msk (0x10UL)
#define | PCA_INTCLR_CF_Pos (7UL)
#define | PCA_INTCLR_CF_Msk (0x80UL)
#define | PCA_CCAPM0_ECOM_Pos (6UL)
#define | PCA_CCAPM0_ECOM_Msk (0x40UL)
#define | PCA_CCAPM0_ECOM PCA_CCAPM0_ECOM_Msk
#define | PCA_CCAPM0_CAPP_Pos (5UL)
#define | PCA_CCAPM0_CAPP_Msk (0x20UL)
#define | PCA_CCAPM0_CAPP PCA_CCAPM0_CAPP_Msk
#define | PCA_CCAPM0_CAPN_Pos (4UL)
#define | PCA_CCAPM0_CAPN_Msk (0x10UL)
#define | PCA_CCAPM0_CAPN PCA_CCAPM0_CAPN_Msk
#define | PCA_CCAPM0_MAT_Pos (3UL)
#define | PCA_CCAPM0_MAT_Msk (0x8UL)
#define | PCA_CCAPM0_MAT PCA_CCAPM0_MAT_Msk
#define | PCA_CCAPM0_TOG_Pos (2UL)
#define | PCA_CCAPM0_TOG_Msk (0x4UL)
#define | PCA_CCAPM0_TOG PCA_CCAPM0_TOG_Msk
#define | PCA_CCAPM0_PWM_Pos (1UL)
#define | PCA_CCAPM0_PWM_Msk (0x2UL)
#define | PCA_CCAPM0_PWM PCA_CCAPM0_PWM_Msk
#define | PCA_CCAPM0_CCIE_Pos (0UL)
#define | PCA_CCAPM0_CCIE_Msk (0x1UL)
#define | PCA_CCAPM0_CCIE PCA_CCAPM0_CCIE_Msk
#define | PCA_CCAPM1_ECOM_Pos (6UL)
#define | PCA_CCAPM1_ECOM_Msk (0x40UL)
#define | PCA_CCAPM1_ECOM PCA_CCAPM1_ECOM_Msk
#define | PCA_CCAPM1_CAPP_Pos (5UL)
#define | PCA_CCAPM1_CAPP_Msk (0x20UL)
#define | PCA_CCAPM1_CAPP PCA_CCAPM1_CAPP_Msk
#define | PCA_CCAPM1_CAPN_Pos (4UL)
#define | PCA_CCAPM1_CAPN_Msk (0x10UL)
#define | PCA_CCAPM1_CAPN PCA_CCAPM1_CAPN_Msk
#define | PCA_CCAPM1_MAT_Pos (3UL)
#define | PCA_CCAPM1_MAT_Msk (0x8UL)
#define | PCA_CCAPM1_MAT PCA_CCAPM1_MAT_Msk
#define | PCA_CCAPM1_TOG_Pos (2UL)
#define | PCA_CCAPM1_TOG_Msk (0x4UL)
#define | PCA_CCAPM1_TOG PCA_CCAPM1_TOG_Msk
#define | PCA_CCAPM1_PWM_Pos (1UL)
#define | PCA_CCAPM1_PWM_Msk (0x2UL)
#define | PCA_CCAPM1_PWM PCA_CCAPM1_PWM_Msk
#define | PCA_CCAPM1_CCIE_Pos (0UL)
#define | PCA_CCAPM1_CCIE_Msk (0x1UL)
#define | PCA_CCAPM1_CCIE PCA_CCAPM1_CCIE_Msk
#define | PCA_CCAPM2_ECOM_Pos (6UL)
#define | PCA_CCAPM2_ECOM_Msk (0x40UL)
#define | PCA_CCAPM2_ECOM PCA_CCAPM2_ECOM_Msk
#define | PCA_CCAPM2_CAPP_Pos (5UL)
#define | PCA_CCAPM2_CAPP_Msk (0x20UL)
#define | PCA_CCAPM2_CAPP PCA_CCAPM2_CAPP_Msk
#define | PCA_CCAPM2_CAPN_Pos (4UL)
#define | PCA_CCAPM2_CAPN_Msk (0x10UL)
#define | PCA_CCAPM2_CAPN PCA_CCAPM2_CAPN_Msk
#define | PCA_CCAPM2_MAT_Pos (3UL)
#define | PCA_CCAPM2_MAT_Msk (0x8UL)
#define | PCA_CCAPM2_MAT PCA_CCAPM2_MAT_Msk
#define | PCA_CCAPM2_TOG_Pos (2UL)
#define | PCA_CCAPM2_TOG_Msk (0x4UL)
#define | PCA_CCAPM2_TOG PCA_CCAPM2_TOG_Msk
#define | PCA_CCAPM2_PWM_Pos (1UL)
#define | PCA_CCAPM2_PWM_Msk (0x2UL)
#define | PCA_CCAPM2_PWM PCA_CCAPM2_PWM_Msk
#define | PCA_CCAPM2_CCIE_Pos (0UL)
#define | PCA_CCAPM2_CCIE_Msk (0x1UL)
#define | PCA_CCAPM2_CCIE PCA_CCAPM2_CCIE_Msk
#define | PCA_CCAPM3_ECOM_Pos (6UL)
#define | PCA_CCAPM3_ECOM_Msk (0x40UL)
#define | PCA_CCAPM3_ECOM PCA_CCAPM3_ECOM_Msk
#define | PCA_CCAPM3_CAPP_Pos (5UL)
#define | PCA_CCAPM3_CAPP_Msk (0x20UL)
#define | PCA_CCAPM3_CAPP PCA_CCAPM3_CAPP_Msk
#define | PCA_CCAPM3_CAPN_Pos (4UL)
#define | PCA_CCAPM3_CAPN_Msk (0x10UL)
#define | PCA_CCAPM3_CAPN PCA_CCAPM3_CAPN_Msk
#define | PCA_CCAPM3_MAT_Pos (3UL)
#define | PCA_CCAPM3_MAT_Msk (0x8UL)
#define | PCA_CCAPM3_MAT PCA_CCAPM3_MAT_Msk
#define | PCA_CCAPM3_TOG_Pos (2UL)
#define | PCA_CCAPM3_TOG_Msk (0x4UL)
#define | PCA_CCAPM3_TOG PCA_CCAPM3_TOG_Msk
#define | PCA_CCAPM3_PWM_Pos (1UL)
#define | PCA_CCAPM3_PWM_Msk (0x2UL)
#define | PCA_CCAPM3_PWM PCA_CCAPM3_PWM_Msk
#define | PCA_CCAPM3_CCIE_Pos (0UL)
#define | PCA_CCAPM3_CCIE_Msk (0x1UL)
#define | PCA_CCAPM3_CCIE PCA_CCAPM3_CCIE_Msk
#define | PCA_CCAPM4_ECOM_Pos (6UL)
#define | PCA_CCAPM4_ECOM_Msk (0x40UL)
#define | PCA_CCAPM4_ECOM PCA_CCAPM4_ECOM_Msk
#define | PCA_CCAPM4_CAPP_Pos (5UL)
#define | PCA_CCAPM4_CAPP_Msk (0x20UL)
#define | PCA_CCAPM4_CAPP PCA_CCAPM4_CAPP_Msk
#define | PCA_CCAPM4_CAPN_Pos (4UL)
#define | PCA_CCAPM4_CAPN_Msk (0x10UL)
#define | PCA_CCAPM4_CAPN PCA_CCAPM4_CAPN_Msk
#define | PCA_CCAPM4_MAT_Pos (3UL)
#define | PCA_CCAPM4_MAT_Msk (0x8UL)
#define | PCA_CCAPM4_MAT PCA_CCAPM4_MAT_Msk
#define | PCA_CCAPM4_TOG_Pos (2UL)
#define | PCA_CCAPM4_TOG_Msk (0x4UL)
#define | PCA_CCAPM4_TOG PCA_CCAPM4_TOG_Msk
#define | PCA_CCAPM4_PWM_Pos (1UL)
#define | PCA_CCAPM4_PWM_Msk (0x2UL)
#define | PCA_CCAPM4_PWM PCA_CCAPM4_PWM_Msk
#define | PCA_CCAPM4_CCIE_Pos (0UL)
#define | PCA_CCAPM4_CCIE_Msk (0x1UL)
#define | PCA_CCAPM4_CCIE PCA_CCAPM4_CCIE_Msk
#define | PCA_CCAP0L_CCAP0_Pos (0UL)
#define | PCA_CCAP0L_CCAP0_Msk (0xFFUL)
#define | PCA_CCAP0H_CCAP0_Pos (8UL)
#define | PCA_CCAP0H_CCAP0_Msk (0xFF00UL)
#define | PCA_CCAP1L_CCAP1_Pos (0UL)
#define | PCA_CCAP1L_CCAP1_Msk (0xFFUL)
#define | PCA_CCAP1H_CCAP1_Pos (8UL)
#define | PCA_CCAP1H_CCAP1_Msk (0xFF00UL)
#define | PCA_CCAP2L_CCAP2_Pos (0UL)
#define | PCA_CCAP2L_CCAP2_Msk (0xFFUL)
#define | PCA_CCAP2H_CCAP2_Pos (0UL)
#define | PCA_CCAP2H_CCAP2_Msk (0xFFUL)
#define | PCA_CCAP3L_CCAP3_Pos (0UL)
#define | PCA_CCAP3L_CCAP3_Msk (0xFFUL)
#define | PCA_CCAP3H_CCAP3_Pos (8UL)
#define | PCA_CCAP3H_CCAP3_Msk (0xFF00UL)
#define | PCA_CCAP4L_CCAP4_Pos (0UL)
#define | PCA_CCAP4L_CCAP4_Msk (0xFFUL)
#define | PCA_CCAP4H_CCAP4_Pos (8UL)
#define | PCA_CCAP4H_CCAP4_Msk (0xFF00UL)
#define | PCA_CCAPO_CCAPO4_Pos (4UL)
#define | PCA_CCAPO_CCAPO4_Msk (0x10UL)
#define | PCA_CCAPO_CCAPO3_Pos (3UL)
#define | PCA_CCAPO_CCAPO3_Msk (0x8UL)
#define | PCA_CCAPO_CCAPO2_Pos (2UL)
#define | PCA_CCAPO_CCAPO2_Msk (0x4UL)
#define | PCA_CCAPO_CCAPO1_Pos (1UL)
#define | PCA_CCAPO_CCAPO1_Msk (0x2UL)
#define | PCA_CCAPO_CCAPO0_Pos (0UL)
#define | PCA_CCAPO_CCAPO0_Msk (0x1UL)
#define | PCA_POCR_POINV4_Pos (12UL)
#define | PCA_POCR_POINV4_Msk (0x1000UL)
#define | PCA_POCR_POINV3_Pos (11UL)
#define | PCA_POCR_POINV3_Msk (0x800UL)
#define | PCA_POCR_POINV2_Pos (10UL)
#define | PCA_POCR_POINV2_Msk (0x400UL)
#define | PCA_POCR_POINV1_Pos (9UL)
#define | PCA_POCR_POINV1_Msk (0x200UL)
#define | PCA_POCR_POINV0_Pos (8UL)
#define | PCA_POCR_POINV0_Msk (0x100UL)
#define | PCA_POCR_POE4_Pos (4UL)
#define | PCA_POCR_POE4_Msk (0x10UL)
#define | PCA_POCR_POE4 PCA_POCR_POE4_Msk
#define | PCA_POCR_POE3_Pos (3UL)
#define | PCA_POCR_POE3_Msk (0x8UL)
#define | PCA_POCR_POE3 PCA_POCR_POE3_Msk
#define | PCA_POCR_POE2_Pos (2UL)
#define | PCA_POCR_POE2_Msk (0x4UL)
#define | PCA_POCR_POE2 PCA_POCR_POE2_Msk
#define | PCA_POCR_POE1_Pos (1UL)
#define | PCA_POCR_POE1_Msk (0x2UL)
#define | PCA_POCR_POE1 PCA_POCR_POE1_Msk
#define | PCA_POCR_POE0_Pos (0UL)
#define | PCA_POCR_POE0_Msk (0x1UL)
#define | PCA_POCR_POE0 PCA_POCR_POE0_Msk
#define | PCA_CCAP0_CCAP0_Pos (0UL)
#define | PCA_CCAP0_CCAP0_Msk (0xFFFFUL)
#define | PCA_CCAP1_CCAP1_Pos (0UL)
#define | PCA_CCAP1_CCAP1_Msk (0xFFFFUL)
#define | PCA_CCAP2_CCAP2_Pos (0UL)
#define | PCA_CCAP2_CCAP2_Msk (0xFFFFUL)
#define | PCA_CCAP3_CCAP3_Pos (0UL)
#define | PCA_CCAP3_CCAP3_Msk (0x7FFFUL)
#define | PCA_CCAP4_CCAP4_Pos (0UL)
#define | PCA_CCAP4_CCAP4_Msk (0xFFFFUL)
#define | TIM_CR1_CEN_Pos (0UL)
#define | TIM_CR1_CEN_Msk (0x1UL)
#define | TIM_CR1_CEN TIM_CR1_CEN_Msk
#define | TIM_CR1_UDIS_Pos (1UL)
#define | TIM_CR1_UDIS_Msk (0x2UL)
#define | TIM_CR1_UDIS TIM_CR1_UDIS_Msk
#define | TIM_CR1_URS_Pos (2UL)
#define | TIM_CR1_URS_Msk (0x4UL)
#define | TIM_CR1_URS TIM_CR1_URS_Msk
#define | TIM_CR1_OPM_Pos (3UL)
#define | TIM_CR1_OPM_Msk (0x8UL)
#define | TIM_CR1_OPM TIM_CR1_OPM_Msk
#define | TIM_CR1_DIR_Pos (4UL)
#define | TIM_CR1_DIR_Msk (0x10UL)
#define | TIM_CR1_DIR TIM_CR1_DIR_Msk
#define | TIM_CR1_CMS_Pos (5UL)
#define | TIM_CR1_CMS_Msk (0x60UL)
#define | TIM_CR1_CMS TIM_CR1_CMS_Msk
#define | TIM_CR1_ARPE_Pos (7UL)
#define | TIM_CR1_ARPE_Msk (0x80UL)
#define | TIM_CR1_ARPE TIM_CR1_ARPE_Msk
#define | TIM_CR1_CKD_Pos (8UL)
#define | TIM_CR1_CKD_Msk (0x300UL)
#define | TIM_CR1_CKD TIM_CR1_CKD_Msk
#define | TIM_CR2_CCPC_Pos (0UL)
#define | TIM_CR2_CCPC_Msk (0x1UL)
#define | TIM_CR2_CCPC TIM_CR2_CCPC_Msk
#define | TIM_CR2_CCUS_Pos (2UL)
#define | TIM_CR2_CCUS_Msk (0x4UL)
#define | TIM_CR2_CCUS TIM_CR2_CCUS_Msk
#define | TIM_CR2_MMS_Pos (4UL)
#define | TIM_CR2_MMS_Msk (0x70UL)
#define | TIM_CR2_MMS TIM_CR2_MMS_Msk
#define | TIM_CR2_TI1S_Pos (7UL)
#define | TIM_CR2_TI1S_Msk (0x80UL)
#define | TIM_CR2_TI1S TIM_CR2_TI1S_Msk
#define | TIM_CR2_OIS1_Pos (8UL)
#define | TIM_CR2_OIS1_Msk (0x100UL)
#define | TIM_CR2_OIS1 TIM_CR2_OIS1_Msk
#define | TIM_CR2_OIS1N_Pos (9UL)
#define | TIM_CR2_OIS1N_Msk (0x200UL)
#define | TIM_CR2_OIS1N TIM_CR2_OIS1N_Msk
#define | TIM_CR2_OIS2_Pos (10UL)
#define | TIM_CR2_OIS2_Msk (0x400UL)
#define | TIM_CR2_OIS2 TIM_CR2_OIS2_Msk
#define | TIM_CR2_OIS2N_Pos (11UL)
#define | TIM_CR2_OIS2N_Msk (0x800UL)
#define | TIM_CR2_OIS2N TIM_CR2_OIS2N_Msk
#define | TIM_CR2_OIS3_Pos (12UL)
#define | TIM_CR2_OIS3_Msk (0x1000UL)
#define | TIM_CR2_OIS3 TIM_CR2_OIS3_Msk
#define | TIM_CR2_OIS3N_Pos (13UL)
#define | TIM_CR2_OIS3N_Msk (0x2000UL)
#define | TIM_CR2_OIS3N TIM_CR2_OIS3N_Msk
#define | TIM_CR2_OIS4_Pos (14UL)
#define | TIM_CR2_OIS4_Msk (0x4000UL)
#define | TIM_CR2_OIS4 TIM_CR2_OIS4_Msk
#define | TIM_SMCR_SMS_Pos (0UL)
#define | TIM_SMCR_SMS_Msk (0x7UL)
#define | TIM_SMCR_SMS TIM_SMCR_SMS_Msk
#define | TIM_SMCR_TS_Pos (4UL)
#define | TIM_SMCR_TS_Msk (0x70UL)
#define | TIM_SMCR_TS TIM_SMCR_TS_Msk
#define | TIM_SMCR_TS_0 (0x1U << TIM_SMCR_TS_Pos)
#define | TIM_SMCR_TS_1 (0x2U << TIM_SMCR_TS_Pos)
#define | TIM_SMCR_TS_2 (0x4U << TIM_SMCR_TS_Pos)
#define | TIM_SMCR_MSM_Pos (7UL)
#define | TIM_SMCR_MSM_Msk (0x80UL)
#define | TIM_SMCR_MSM TIM_SMCR_MSM_Msk
#define | TIM_SMCR_ETF_Pos (8UL)
#define | TIM_SMCR_ETF_Msk (0xF00UL)
#define | TIM_SMCR_ETF TIM_SMCR_ETF_Msk
#define | TIM_SMCR_ETPS_Pos (12UL)
#define | TIM_SMCR_ETPS_Msk (0x3000UL)
#define | TIM_SMCR_ETPS TIM_SMCR_ETPS_Msk
#define | TIM_SMCR_ETPS_0 (0x1U << TIM_SMCR_ETPS_Pos)
#define | TIM_SMCR_ETPS_1 (0x2U << TIM_SMCR_ETPS_Pos)
#define | TIM_SMCR_ECE_Pos (14UL)
#define | TIM_SMCR_ECE_Msk (0x4000UL)
#define | TIM_SMCR_ECE TIM_SMCR_ECE_Msk
#define | TIM_SMCR_ETP_Pos (15UL)
#define | TIM_SMCR_ETP_Msk (0x8000UL)
#define | TIM_SMCR_ETP TIM_SMCR_ETP_Msk
#define | TIM_DIER_UIE_Pos (0UL)
#define | TIM_DIER_UIE_Msk (0x1UL)
#define | TIM_DIER_UIE TIM_DIER_UIE_Msk
#define | TIM_DIER_CC1IE_Pos (1UL)
#define | TIM_DIER_CC1IE_Msk (0x2UL)
#define | TIM_DIER_CC1IE TIM_DIER_CC1IE_Msk
#define | TIM_DIER_CC2IE_Pos (2UL)
#define | TIM_DIER_CC2IE_Msk (0x4UL)
#define | TIM_DIER_CC2IE TIM_DIER_CC2IE_Msk
#define | TIM_DIER_CC3IE_Pos (3UL)
#define | TIM_DIER_CC3IE_Msk (0x8UL)
#define | TIM_DIER_CC3IE TIM_DIER_CC3IE_Msk
#define | TIM_DIER_CC4IE_Pos (4UL)
#define | TIM_DIER_CC4IE_Msk (0x10UL)
#define | TIM_DIER_CC4IE TIM_DIER_CC4IE_Msk
#define | TIM_DIER_COMIE_Pos (5UL)
#define | TIM_DIER_COMIE_Msk (0x20UL)
#define | TIM_DIER_COMIE TIM_DIER_COMIE_Msk
#define | TIM_DIER_TIE_Pos (6UL)
#define | TIM_DIER_TIE_Msk (0x40UL)
#define | TIM_DIER_TIE TIM_DIER_TIE_Msk
#define | TIM_DIER_BIE_Pos (7UL)
#define | TIM_DIER_BIE_Msk (0x80UL)
#define | TIM_DIER_BIE TIM_DIER_BIE_Msk
#define | TIM_SR_CC4OF_Pos (12UL)
#define | TIM_SR_CC4OF_Msk (0x1000UL)
#define | TIM_SR_CC4OF TIM_SR_CC4OF_Msk
#define | TIM_SR_CC3OF_Pos (11UL)
#define | TIM_SR_CC3OF_Msk (0x800UL)
#define | TIM_SR_CC3OF TIM_SR_CC3OF_Msk
#define | TIM_SR_CC2OF_Pos (10UL)
#define | TIM_SR_CC2OF_Msk (0x400UL)
#define | TIM_SR_CC2OF TIM_SR_CC2OF_Msk
#define | TIM_SR_CC1OF_Pos (9UL)
#define | TIM_SR_CC1OF_Msk (0x200UL)
#define | TIM_SR_CC1OF TIM_SR_CC1OF_Msk
#define | TIM_SR_BIF_Pos (7UL)
#define | TIM_SR_BIF_Msk (0x80UL)
#define | TIM_SR_BIF TIM_SR_BIF_Msk
#define | TIM_SR_TIF_Pos (6UL)
#define | TIM_SR_TIF_Msk (0x40UL)
#define | TIM_SR_TIF TIM_SR_TIF_Msk
#define | TIM_SR_COMIF_Pos (5UL)
#define | TIM_SR_COMIF_Msk (0x20UL)
#define | TIM_SR_COMIF TIM_SR_COMIF_Msk
#define | TIM_SR_CC4IF_Pos (4UL)
#define | TIM_SR_CC4IF_Msk (0x10UL)
#define | TIM_SR_CC4IF TIM_SR_CC4IF_Msk
#define | TIM_SR_CC3IF_Pos (3UL)
#define | TIM_SR_CC3IF_Msk (0x8UL)
#define | TIM_SR_CC3IF TIM_SR_CC3IF_Msk
#define | TIM_SR_CC2IF_Pos (2UL)
#define | TIM_SR_CC2IF_Msk (0x4UL)
#define | TIM_SR_CC2IF TIM_SR_CC2IF_Msk
#define | TIM_SR_CC1IF_Pos (1UL)
#define | TIM_SR_CC1IF_Msk (0x2UL)
#define | TIM_SR_CC1IF TIM_SR_CC1IF_Msk
#define | TIM_SR_UIF_Pos (0UL)
#define | TIM_SR_UIF_Msk (0x1UL)
#define | TIM_SR_UIF TIM_SR_UIF_Msk
#define | TIM_EGR_BG_Pos (7UL)
#define | TIM_EGR_BG_Msk (0x80UL)
#define | TIM_EGR_TG_Pos (6UL)
#define | TIM_EGR_TG_Msk (0x40UL)
#define | TIM_EGR_COMG_Pos (5UL)
#define | TIM_EGR_COMG_Msk (0x20UL)
#define | TIM_EGR_CC4G_Pos (4UL)
#define | TIM_EGR_CC4G_Msk (0x10UL)
#define | TIM_EGR_CC3G_Pos (3UL)
#define | TIM_EGR_CC3G_Msk (0x8UL)
#define | TIM_EGR_CC2G_Pos (2UL)
#define | TIM_EGR_CC2G_Msk (0x4UL)
#define | TIM_EGR_CC1G_Pos (1UL)
#define | TIM_EGR_CC1G_Msk (0x2UL)
#define | TIM_EGR_UG_Pos (0UL)
#define | TIM_EGR_UG_Msk (0x1UL)
#define | TIM_EGR_UG TIM_EGR_UG_Msk
#define | TIM_CCMR1_OC2CE_Pos (15UL)
#define | TIM_CCMR1_OC2CE_Msk (0x8000UL)
#define | TIM_CCMR1_OC2CE TIM_CCMR1_OC2CE_Msk
#define | TIM_CCMR1_OC2M_Pos (12UL)
#define | TIM_CCMR1_OC2M_Msk (0x7000UL)
#define | TIM_CCMR1_OC2M TIM_CCMR1_OC2M_Msk
#define | TIM_CCMR1_OC2M_0 (0x1U << TIM_CCMR1_OC2M_Pos)
#define | TIM_CCMR1_OC2M_1 (0x2U << TIM_CCMR1_OC2M_Pos)
#define | TIM_CCMR1_OC2M_2 (0x4U << TIM_CCMR1_OC2M_Pos)
#define | TIM_CCMR1_OC2PE_Pos (11UL)
#define | TIM_CCMR1_OC2PE_Msk (0x800UL)
#define | TIM_CCMR1_OC2PE TIM_CCMR1_OC2PE_Msk
#define | TIM_CCMR1_OC2FE_Pos (10UL)
#define | TIM_CCMR1_OC2FE_Msk (0x400UL)
#define | TIM_CCMR1_OC2FE TIM_CCMR1_OC2FE_Msk
#define | TIM_CCMR1_CC2S_Pos (8UL)
#define | TIM_CCMR1_CC2S_Msk (0x300UL)
#define | TIM_CCMR1_CC2S TIM_CCMR1_CC2S_Msk
#define | TIM_CCMR1_CC2S_0 (0x1U << TIM_CCMR1_CC2S_Pos)
#define | TIM_CCMR1_CC2S_1 (0x2U << TIM_CCMR1_CC2S_Pos)
#define | TIM_CCMR1_OC1CE_Pos (7UL)
#define | TIM_CCMR1_OC1CE_Msk (0x80UL)
#define | TIM_CCMR1_OC1CE TIM_CCMR1_OC1CE_Msk
#define | TIM_CCMR1_OC1M_Pos (4UL)
#define | TIM_CCMR1_OC1M_Msk (0x70UL)
#define | TIM_CCMR1_OC1M TIM_CCMR1_OC1M_Msk
#define | TIM_CCMR1_OC1M_0 (0x1U << TIM_CCMR1_OC1M_Pos)
#define | TIM_CCMR1_OC1M_1 (0x2U << TIM_CCMR1_OC1M_Pos)
#define | TIM_CCMR1_OC1M_2 (0x4U << TIM_CCMR1_OC1M_Pos)
#define | TIM_CCMR1_OC1PE_Pos (3UL)
#define | TIM_CCMR1_OC1PE_Msk (0x8UL)
#define | TIM_CCMR1_OC1PE TIM_CCMR1_OC1PE_Msk
#define | TIM_CCMR1_OC1FE_Pos (2UL)
#define | TIM_CCMR1_OC1FE_Msk (0x4UL)
#define | TIM_CCMR1_OC1FE TIM_CCMR1_OC1FE_Msk
#define | TIM_CCMR1_CC1S_Pos (0UL)
#define | TIM_CCMR1_CC1S_Msk (0x3UL)
#define | TIM_CCMR1_CC1S TIM_CCMR1_CC1S_Msk
#define | TIM_CCMR1_CC1S_0 (0x1U << TIM_CCMR1_CC1S_Pos)
#define | TIM_CCMR1_CC1S_1 (0x2U << TIM_CCMR1_CC1S_Pos)
#define | TIM_CCMR1_IC1PSC_Pos (2UL)
#define | TIM_CCMR1_IC1PSC_Msk (0x0000000CUL)
#define | TIM_CCMR1_IC1PSC TIM_CCMR1_IC1PSC_Msk
#define | TIM_CCMR1_IC1PSC_0 (0x00000004UL)
#define | TIM_CCMR1_IC1PSC_1 (0x00000008UL)
#define | TIM_CCMR1_IC1F_Pos (4UL)
#define | TIM_CCMR1_IC1F_Msk (0x000000F0UL)
#define | TIM_CCMR1_IC1F TIM_CCMR1_IC1F_Msk
#define | TIM_CCMR1_IC1F_0 (0x00000010UL)
#define | TIM_CCMR1_IC1F_1 (0x00000020UL)
#define | TIM_CCMR1_IC1F_2 (0x00000040UL)
#define | TIM_CCMR1_IC1F_3 (0x00000080UL)
#define | TIM_CCMR1_IC2PSC_Pos (10UL)
#define | TIM_CCMR1_IC2PSC_Msk (0x00000C00UL)
#define | TIM_CCMR1_IC2PSC TIM_CCMR1_IC2PSC_Msk
#define | TIM_CCMR1_IC2PSC_0 (0x00000400UL)
#define | TIM_CCMR1_IC2PSC_1 (0x00000800UL)
#define | TIM_CCMR1_IC2F_Pos (12U)
#define | TIM_CCMR1_IC2F_Msk (0x0000F000UL)
#define | TIM_CCMR1_IC2F TIM_CCMR1_IC2F_Msk
#define | TIM_CCMR1_IC2F_0 (0x00001000UL)
#define | TIM_CCMR1_IC2F_1 (0x00002000UL)
#define | TIM_CCMR1_IC2F_2 (0x00004000UL)
#define | TIM_CCMR1_IC2F_3 (0x00008000UL)
#define | TIM_CCMR2_OC4CE_Pos (15UL)
#define | TIM_CCMR2_OC4CE_Msk (0x8000UL)
#define | TIM_CCMR2_OC4CE TIM_CCMR2_OC4CE_Msk
#define | TIM_CCMR2_OC4M_Pos (12UL)
#define | TIM_CCMR2_OC4M_Msk (0x7000UL)
#define | TIM_CCMR2_OC4M TIM_CCMR2_OC4M_Msk
#define | TIM_CCMR2_OC4PE_Pos (11UL)
#define | TIM_CCMR2_OC4PE_Msk (0x800UL)
#define | TIM_CCMR2_OC4PE TIM_CCMR2_OC4PE_Msk
#define | TIM_CCMR2_OC4FE_Pos (10UL)
#define | TIM_CCMR2_OC4FE_Msk (0x400UL)
#define | TIM_CCMR2_OC4FE TIM_CCMR2_OC4FE_Msk
#define | TIM_CCMR2_CC4S_Pos (8UL)
#define | TIM_CCMR2_CC4S_Msk (0x300UL)
#define | TIM_CCMR2_CC4S TIM_CCMR2_CC4S_Msk
#define | TIM_CCMR2_OC3CE_Pos (7UL)
#define | TIM_CCMR2_OC3CE_Msk (0x80UL)
#define | TIM_CCMR2_OC3CE TIM_CCMR2_OC3CE_Msk
#define | TIM_CCMR2_OC3M_Pos (4UL)
#define | TIM_CCMR2_OC3M_Msk (0x70UL)
#define | TIM_CCMR2_OC3M TIM_CCMR2_OC3M_Msk
#define | TIM_CCMR2_OC3PE_Pos (3UL)
#define | TIM_CCMR2_OC3PE_Msk (0x8UL)
#define | TIM_CCMR2_OC3PE TIM_CCMR2_OC3PE_Msk
#define | TIM_CCMR2_OC3FE_Pos (2UL)
#define | TIM_CCMR2_OC3FE_Msk (0x4UL)
#define | TIM_CCMR2_OC3FE TIM_CCMR2_OC3FE_Msk
#define | TIM_CCMR2_CC3S_Pos (0UL)
#define | TIM_CCMR2_CC3S_Msk (0x3UL)
#define | TIM_CCMR2_CC3S TIM_CCMR2_CC3S_Msk
#define | TIM_CCMR2_IC3PSC_Pos (2UL)
#define | TIM_CCMR2_IC3PSC_Msk (0x0000000CUL)
#define | TIM_CCMR2_IC3PSC TIM_CCMR2_IC3PSC_Msk
#define | TIM_CCMR2_IC3PSC_0 (0x00000004UL)
#define | TIM_CCMR2_IC3PSC_1 (0x00000008UL)
#define | TIM_CCMR2_IC3F_Pos (4UL)
#define | TIM_CCMR2_IC3F_Msk (0x000000F0UL)
#define | TIM_CCMR2_IC3F TIM_CCMR2_IC3F_Msk
#define | TIM_CCMR2_IC3F_0 (0x00000010UL)
#define | TIM_CCMR2_IC3F_1 (0x00000020UL)
#define | TIM_CCMR2_IC3F_2 (0x00000040UL)
#define | TIM_CCMR2_IC3F_3 (0x00000080UL)
#define | TIM_CCMR2_IC4PSC_Pos (10UL)
#define | TIM_CCMR2_IC4PSC_Msk (0x00000C00UL)
#define | TIM_CCMR2_IC4PSC TIM_CCMR2_IC4PSC_Msk
#define | TIM_CCMR2_IC4PSC_0 (0x00000400UL)
#define | TIM_CCMR2_IC4PSC_1 (0x00000800UL)
#define | TIM_CCMR2_IC4F_Pos (12UL)
#define | TIM_CCMR2_IC4F_Msk (0x0000F000UL)
#define | TIM_CCMR2_IC4F TIM_CCMR2_IC4F_Msk
#define | TIM_CCMR2_IC4F_0 (0x00001000UL)
#define | TIM_CCMR2_IC4F_1 (0x00002000UL)
#define | TIM_CCMR2_IC4F_2 (0x00004000UL)
#define | TIM_CCMR2_IC4F_3 (0x00008000UL)
#define | TIM_CCER_CC4P_Pos (13UL)
#define | TIM_CCER_CC4P_Msk (0x2000UL)
#define | TIM_CCER_CC4P TIM_CCER_CC4P_Msk
#define | TIM_CCER_CC4E_Pos (12UL)
#define | TIM_CCER_CC4E_Msk (0x1000UL)
#define | TIM_CCER_CC4E TIM_CCER_CC4E_Msk
#define | TIM_CCER_CC3NP_Pos (11UL)
#define | TIM_CCER_CC3NP_Msk (0x800UL)
#define | TIM_CCER_CC3NP TIM_CCER_CC3NP_Msk
#define | TIM_CCER_CC3NE_Pos (10UL)
#define | TIM_CCER_CC3NE_Msk (0x400UL)
#define | TIM_CCER_CC3NE TIM_CCER_CC3NE_Msk
#define | TIM_CCER_CC3P_Pos (9UL)
#define | TIM_CCER_CC3P_Msk (0x200UL)
#define | TIM_CCER_CC3P TIM_CCER_CC3P_Msk
#define | TIM_CCER_CC3E_Pos (8UL)
#define | TIM_CCER_CC3E_Msk (0x100UL)
#define | TIM_CCER_CC3E TIM_CCER_CC3E_Msk
#define | TIM_CCER_CC2NP_Pos (7UL)
#define | TIM_CCER_CC2NP_Msk (0x80UL)
#define | TIM_CCER_CC2NP TIM_CCER_CC2NP_Msk
#define | TIM_CCER_CC2NE_Pos (6UL)
#define | TIM_CCER_CC2NE_Msk (0x40UL)
#define | TIM_CCER_CC2NE TIM_CCER_CC2NE_Msk
#define | TIM_CCER_CC2P_Pos (5UL)
#define | TIM_CCER_CC2P_Msk (0x20UL)
#define | TIM_CCER_CC2P TIM_CCER_CC2P_Msk
#define | TIM_CCER_CC2E_Pos (4UL)
#define | TIM_CCER_CC2E_Msk (0x10UL)
#define | TIM_CCER_CC2E TIM_CCER_CC2E_Msk
#define | TIM_CCER_CC1NP_Pos (3UL)
#define | TIM_CCER_CC1NP_Msk (0x8UL)
#define | TIM_CCER_CC1NP TIM_CCER_CC1NP_Msk
#define | TIM_CCER_CC1NE_Pos (2UL)
#define | TIM_CCER_CC1NE_Msk (0x4UL)
#define | TIM_CCER_CC1NE TIM_CCER_CC1NE_Msk
#define | TIM_CCER_CC1P_Pos (1UL)
#define | TIM_CCER_CC1P_Msk (0x2UL)
#define | TIM_CCER_CC1P TIM_CCER_CC1P_Msk
#define | TIM_CCER_CC1E_Pos (0UL)
#define | TIM_CCER_CC1E_Msk (0x1UL)
#define | TIM_CCER_CC1E TIM_CCER_CC1E_Msk
#define | TIM_CNT_CNT_Pos (0UL)
#define | TIM_CNT_CNT_Msk (0xFFFFUL)
#define | TIM_PSC_PSC_Pos (0UL)
#define | TIM_PSC_PSC_Msk (0xFFFFUL)
#define | TIM_ARR_ARR_Pos (0UL)
#define | TIM_ARR_ARR_Msk (0xFFFFUL)
#define | TIM_RCR_REP_Pos (0UL)
#define | TIM_RCR_REP_Msk (0xFFUL)
#define | TIM_CCR1_CCR1_Pos (0UL)
#define | TIM_CCR1_CCR1_Msk (0xFFFFUL)
#define | TIM_CCR2_CCR2_Pos (0UL)
#define | TIM_CCR2_CCR2_Msk (0xFFFFUL)
#define | TIM_CCR3_CCR3_Pos (0UL)
#define | TIM_CCR3_CCR3_Msk (0xFFFFUL)
#define | TIM_CCR4_CCR4_Pos (0UL)
#define | TIM_CCR4_CCR4_Msk (0xFFFFUL)
#define | TIM_BDTR_DTG_Pos (0UL)
#define | TIM_BDTR_DTG_Msk (0xFFUL)
#define | TIM_BDTR_DTG TIM_BDTR_DTG_Msk
#define | TIM_BDTR_DTG_0 (0x01U << TIM_BDTR_DTG_Pos)
#define | TIM_BDTR_DTG_1 (0x02U << TIM_BDTR_DTG_Pos)
#define | TIM_BDTR_DTG_2 (0x04U << TIM_BDTR_DTG_Pos)
#define | TIM_BDTR_DTG_3 (0x08U << TIM_BDTR_DTG_Pos)
#define | TIM_BDTR_DTG_4 (0x10U << TIM_BDTR_DTG_Pos)
#define | TIM_BDTR_DTG_5 (0x20U << TIM_BDTR_DTG_Pos)
#define | TIM_BDTR_DTG_6 (0x40U << TIM_BDTR_DTG_Pos)
#define | TIM_BDTR_DTG_7 (0x80U << TIM_BDTR_DTG_Pos)
#define | TIM_BDTR_LOCK_Pos (8UL)
#define | TIM_BDTR_LOCK_Msk (0x300UL)
#define | TIM_BDTR_LOCK TIM_BDTR_LOCK_Msk
#define | TIM_BDTR_LOCK_0 (0x1U << TIM_BDTR_LOCK_Pos)
#define | TIM_BDTR_LOCK_1 (0x2U << TIM_BDTR_LOCK_Pos)
#define | TIM_BDTR_OSSI_Pos (10UL)
#define | TIM_BDTR_OSSI_Msk (0x400UL)
#define | TIM_BDTR_OSSI TIM_BDTR_OSSI_Msk
#define | TIM_BDTR_OSSR_Pos (11UL)
#define | TIM_BDTR_OSSR_Msk (0x800UL)
#define | TIM_BDTR_OSSR TIM_BDTR_OSSR_Msk
#define | TIM_BDTR_BKE_Pos (12UL)
#define | TIM_BDTR_BKE_Msk (0x1000UL)
#define | TIM_BDTR_BKE TIM_BDTR_BKE_Msk
#define | TIM_BDTR_BKP_Pos (13UL)
#define | TIM_BDTR_BKP_Msk (0x2000UL)
#define | TIM_BDTR_BKP TIM_BDTR_BKP_Msk
#define | TIM_BDTR_AOE_Pos (14UL)
#define | TIM_BDTR_AOE_Msk (0x4000UL)
#define | TIM_BDTR_AOE TIM_BDTR_AOE_Msk
#define | TIM_BDTR_MOE_Pos (15UL)
#define | TIM_BDTR_MOE_Msk (0x8000UL)
#define | TIM_BDTR_MOE TIM_BDTR_MOE_Msk
#define | CRC_RESULT_RESULT_Pos (0UL)
#define | CRC_RESULT_RESULT_Msk (0xFFFFUL)
#define | CRC_RESULT_RESULT CRC_RESULT_RESULT_Msk
#define | CRC_RESULT_FLAG_Pos (16UL)
#define | CRC_RESULT_FLAG_Msk (0x10000UL)
#define | CRC_RESULT_FLAG CRC_RESULT_FLAG_Msk
#define | FLASH_CR_OP_Pos (0UL)
#define | FLASH_CR_OP_Msk (0x3UL)
#define | FLASH_CR_OP FLASH_CR_OP_Msk
#define | FLASH_CR_OP_0 (0x1 << FLASH_CR_OP_Pos)
#define | FLASH_CR_OP_1 (0x2 << FLASH_CR_OP_Pos)
#define | FLASH_CR_BUSY_Pos (2UL)
#define | FLASH_CR_BUSY_Msk (0x4UL)
#define | FLASH_CR_BUSY FLASH_CR_BUSY_Msk
#define | FLASH_CR_IE_Pos (3UL)
#define | FLASH_CR_IE_Msk (0x18UL)
#define | FLASH_CR_IE FLASH_CR_IE_Msk
#define | FLASH_CR_IE_0 (0x1 << FLASH_CR_IE_Pos)
#define | FLASH_CR_IE_1 (0x2 << FLASH_CR_IE_Pos)
#define | FLASH_IFR_IF1_Pos (1UL)
#define | FLASH_IFR_IF1_Msk (0x2UL)
#define | FLASH_IFR_IF1 FLASH_IFR_IF1_Msk
#define | FLASH_IFR_IF0_Pos (0UL)
#define | FLASH_IFR_IF0_Msk (0x1UL)
#define | FLASH_IFR_IF0 FLASH_IFR_IF0_Msk
#define | FLASH_ICLR_ICLR1_Pos (1UL)
#define | FLASH_ICLR_ICLR1_Msk (0x2UL)
#define | FLASH_ICLR_ICLR1 FLASH_ICLR_ICLR1_Msk
#define | FLASH_ICLR_ICLR0_Pos (0UL)
#define | FLASH_ICLR_ICLR0_Msk (0x1UL)
#define | FLASH_ICLR_ICLR0 FLASH_ICLR_ICLR0_Msk
#define | FLASH_BYPASS_BYPASSSEQ_Pos (0UL)
#define | FLASH_BYPASS_BYPASSSEQ_Msk (0xFFFFUL)
#define | FLASH_SLOCK0_SLOCK0_31_Pos (31UL)
#define | FLASH_SLOCK0_SLOCK0_31_Msk (0x80000000UL)
#define | FLASH_SLOCK0_SLOCK0_30_Pos (30UL)
#define | FLASH_SLOCK0_SLOCK0_30_Msk (0x40000000UL)
#define | FLASH_SLOCK0_SLOCK0_29_Pos (29UL)
#define | FLASH_SLOCK0_SLOCK0_29_Msk (0x20000000UL)
#define | FLASH_SLOCK0_SLOCK0_28_Pos (28UL)
#define | FLASH_SLOCK0_SLOCK0_28_Msk (0x10000000UL)
#define | FLASH_SLOCK0_SLOCK0_27_Pos (27UL)
#define | FLASH_SLOCK0_SLOCK0_27_Msk (0x8000000UL)
#define | FLASH_SLOCK0_SLOCK0_26_Pos (26UL)
#define | FLASH_SLOCK0_SLOCK0_26_Msk (0x4000000UL)
#define | FLASH_SLOCK0_SLOCK0_25_Pos (25UL)
#define | FLASH_SLOCK0_SLOCK0_25_Msk (0x2000000UL)
#define | FLASH_SLOCK0_SLOCK0_24_Pos (24UL)
#define | FLASH_SLOCK0_SLOCK0_24_Msk (0x1000000UL)
#define | FLASH_SLOCK0_SLOCK0_23_Pos (23UL)
#define | FLASH_SLOCK0_SLOCK0_23_Msk (0x800000UL)
#define | FLASH_SLOCK0_SLOCK0_22_Pos (22UL)
#define | FLASH_SLOCK0_SLOCK0_22_Msk (0x400000UL)
#define | FLASH_SLOCK0_SLOCK0_21_Pos (21UL)
#define | FLASH_SLOCK0_SLOCK0_21_Msk (0x200000UL)
#define | FLASH_SLOCK0_SLOCK0_20_Pos (20UL)
#define | FLASH_SLOCK0_SLOCK0_20_Msk (0x100000UL)
#define | FLASH_SLOCK0_SLOCK0_19_Pos (19UL)
#define | FLASH_SLOCK0_SLOCK0_19_Msk (0x80000UL)
#define | FLASH_SLOCK0_SLOCK0_18_Pos (18UL)
#define | FLASH_SLOCK0_SLOCK0_18_Msk (0x40000UL)
#define | FLASH_SLOCK0_SLOCK0_17_Pos (17UL)
#define | FLASH_SLOCK0_SLOCK0_17_Msk (0x20000UL)
#define | FLASH_SLOCK0_SLOCK0_16_Pos (16UL)
#define | FLASH_SLOCK0_SLOCK0_16_Msk (0x10000UL)
#define | FLASH_SLOCK0_SLOCK0_15_Pos (15UL)
#define | FLASH_SLOCK0_SLOCK0_15_Msk (0x8000UL)
#define | FLASH_SLOCK0_SLOCK0_14_Pos (14UL)
#define | FLASH_SLOCK0_SLOCK0_14_Msk (0x4000UL)
#define | FLASH_SLOCK0_SLOCK0_13_Pos (13UL)
#define | FLASH_SLOCK0_SLOCK0_13_Msk (0x2000UL)
#define | FLASH_SLOCK0_SLOCK0_12_Pos (12UL)
#define | FLASH_SLOCK0_SLOCK0_12_Msk (0x1000UL)
#define | FLASH_SLOCK0_SLOCK0_11_Pos (11UL)
#define | FLASH_SLOCK0_SLOCK0_11_Msk (0x800UL)
#define | FLASH_SLOCK0_SLOCK0_10_Pos (10UL)
#define | FLASH_SLOCK0_SLOCK0_10_Msk (0x400UL)
#define | FLASH_SLOCK0_SLOCK0_9_Pos (9UL)
#define | FLASH_SLOCK0_SLOCK0_9_Msk (0x200UL)
#define | FLASH_SLOCK0_SLOCK0_8_Pos (8UL)
#define | FLASH_SLOCK0_SLOCK0_8_Msk (0x100UL)
#define | FLASH_SLOCK0_SLOCK0_7_Pos (7UL)
#define | FLASH_SLOCK0_SLOCK0_7_Msk (0x80UL)
#define | FLASH_SLOCK0_SLOCK0_6_Pos (6UL)
#define | FLASH_SLOCK0_SLOCK0_6_Msk (0x40UL)
#define | FLASH_SLOCK0_SLOCK0_5_Pos (5UL)
#define | FLASH_SLOCK0_SLOCK0_5_Msk (0x20UL)
#define | FLASH_SLOCK0_SLOCK0_4_Pos (4UL)
#define | FLASH_SLOCK0_SLOCK0_4_Msk (0x10UL)
#define | FLASH_SLOCK0_SLOCK0_3_Pos (3UL)
#define | FLASH_SLOCK0_SLOCK0_3_Msk (0x8UL)
#define | FLASH_SLOCK0_SLOCK0_2_Pos (2UL)
#define | FLASH_SLOCK0_SLOCK0_2_Msk (0x4UL)
#define | FLASH_SLOCK0_SLOCK0_1_Pos (1UL)
#define | FLASH_SLOCK0_SLOCK0_1_Msk (0x2UL)
#define | FLASH_SLOCK0_SLOCK0_0_Pos (0UL)
#define | FLASH_SLOCK0_SLOCK0_0_Msk (0x1UL)
#define | FLASH_SLOCK1_SLOCK1_31_Pos (31UL)
#define | FLASH_SLOCK1_SLOCK1_31_Msk (0x80000000UL)
#define | FLASH_SLOCK1_SLOCK1_30_Pos (30UL)
#define | FLASH_SLOCK1_SLOCK1_30_Msk (0x40000000UL)
#define | FLASH_SLOCK1_SLOCK1_29_Pos (29UL)
#define | FLASH_SLOCK1_SLOCK1_29_Msk (0x20000000UL)
#define | FLASH_SLOCK1_SLOCK1_28_Pos (28UL)
#define | FLASH_SLOCK1_SLOCK1_28_Msk (0x10000000UL)
#define | FLASH_SLOCK1_SLOCK1_27_Pos (27UL)
#define | FLASH_SLOCK1_SLOCK1_27_Msk (0x8000000UL)
#define | FLASH_SLOCK1_SLOCK1_26_Pos (26UL)
#define | FLASH_SLOCK1_SLOCK1_26_Msk (0x4000000UL)
#define | FLASH_SLOCK1_SLOCK1_25_Pos (25UL)
#define | FLASH_SLOCK1_SLOCK1_25_Msk (0x2000000UL)
#define | FLASH_SLOCK1_SLOCK1_24_Pos (24UL)
#define | FLASH_SLOCK1_SLOCK1_24_Msk (0x1000000UL)
#define | FLASH_SLOCK1_SLOCK1_23_Pos (23UL)
#define | FLASH_SLOCK1_SLOCK1_23_Msk (0x800000UL)
#define | FLASH_SLOCK1_SLOCK1_22_Pos (22UL)
#define | FLASH_SLOCK1_SLOCK1_22_Msk (0x400000UL)
#define | FLASH_SLOCK1_SLOCK1_21_Pos (21UL)
#define | FLASH_SLOCK1_SLOCK1_21_Msk (0x200000UL)
#define | FLASH_SLOCK1_SLOCK1_20_Pos (20UL)
#define | FLASH_SLOCK1_SLOCK1_20_Msk (0x100000UL)
#define | FLASH_SLOCK1_SLOCK1_19_Pos (19UL)
#define | FLASH_SLOCK1_SLOCK1_19_Msk (0x80000UL)
#define | FLASH_SLOCK1_SLOCK1_18_Pos (18UL)
#define | FLASH_SLOCK1_SLOCK1_18_Msk (0x40000UL)
#define | FLASH_SLOCK1_SLOCK1_17_Pos (17UL)
#define | FLASH_SLOCK1_SLOCK1_17_Msk (0x20000UL)
#define | FLASH_SLOCK1_SLOCK1_16_Pos (16UL)
#define | FLASH_SLOCK1_SLOCK1_16_Msk (0x10000UL)
#define | FLASH_SLOCK1_SLOCK1_15_Pos (15UL)
#define | FLASH_SLOCK1_SLOCK1_15_Msk (0x8000UL)
#define | FLASH_SLOCK1_SLOCK1_14_Pos (14UL)
#define | FLASH_SLOCK1_SLOCK1_14_Msk (0x4000UL)
#define | FLASH_SLOCK1_SLOCK1_13_Pos (13UL)
#define | FLASH_SLOCK1_SLOCK1_13_Msk (0x2000UL)
#define | FLASH_SLOCK1_SLOCK1_12_Pos (12UL)
#define | FLASH_SLOCK1_SLOCK1_12_Msk (0x1000UL)
#define | FLASH_SLOCK1_SLOCK1_11_Pos (11UL)
#define | FLASH_SLOCK1_SLOCK1_11_Msk (0x800UL)
#define | FLASH_SLOCK1_SLOCK1_10_Pos (10UL)
#define | FLASH_SLOCK1_SLOCK1_10_Msk (0x400UL)
#define | FLASH_SLOCK1_SLOCK1_9_Pos (9UL)
#define | FLASH_SLOCK1_SLOCK1_9_Msk (0x200UL)
#define | FLASH_SLOCK1_SLOCK1_8_Pos (8UL)
#define | FLASH_SLOCK1_SLOCK1_8_Msk (0x100UL)
#define | FLASH_SLOCK1_SLOCK1_7_Pos (7UL)
#define | FLASH_SLOCK1_SLOCK1_7_Msk (0x80UL)
#define | FLASH_SLOCK1_SLOCK1_6_Pos (6UL)
#define | FLASH_SLOCK1_SLOCK1_6_Msk (0x40UL)
#define | FLASH_SLOCK1_SLOCK1_5_Pos (5UL)
#define | FLASH_SLOCK1_SLOCK1_5_Msk (0x20UL)
#define | FLASH_SLOCK1_SLOCK1_4_Pos (4UL)
#define | FLASH_SLOCK1_SLOCK1_4_Msk (0x10UL)
#define | FLASH_SLOCK1_SLOCK1_3_Pos (3UL)
#define | FLASH_SLOCK1_SLOCK1_3_Msk (0x8UL)
#define | FLASH_SLOCK1_SLOCK1_2_Pos (2UL)
#define | FLASH_SLOCK1_SLOCK1_2_Msk (0x4UL)
#define | FLASH_SLOCK1_SLOCK1_1_Pos (1UL)
#define | FLASH_SLOCK1_SLOCK1_1_Msk (0x2UL)
#define | FLASH_SLOCK1_SLOCK1_0_Pos (0UL)
#define | FLASH_SLOCK1_SLOCK1_0_Msk (0x1UL)
#define | FLASH_ISPCON_ISP_CON_Pos (0UL)
#define | FLASH_ISPCON_ISP_CON_Msk (0x1UL)
#define | GPIO_DIRCR_PxDIR7_Pos (7UL)
#define | GPIO_DIRCR_PxDIR7_Msk (0x80UL)
#define | GPIO_DIRCR_PxDIR6_Pos (6UL)
#define | GPIO_DIRCR_PxDIR6_Msk (0x40UL)
#define | GPIO_DIRCR_PxDIR5_Pos (5UL)
#define | GPIO_DIRCR_PxDIR5_Msk (0x20UL)
#define | GPIO_DIRCR_PxDIR4_Pos (4UL)
#define | GPIO_DIRCR_PxDIR4_Msk (0x10UL)
#define | GPIO_DIRCR_PxDIR3_Pos (3UL)
#define | GPIO_DIRCR_PxDIR3_Msk (0x8UL)
#define | GPIO_DIRCR_PxDIR2_Pos (2UL)
#define | GPIO_DIRCR_PxDIR2_Msk (0x4UL)
#define | GPIO_DIRCR_PxDIR1_Pos (1UL)
#define | GPIO_DIRCR_PxDIR1_Msk (0x2UL)
#define | GPIO_DIRCR_PxDIR0_Pos (0UL)
#define | GPIO_DIRCR_PxDIR0_Msk (0x1UL)
#define | GPIO_DIRCR_PxDIR0 GPIO_DIRCR_PxDIR0_Msk
#define | GPIO_OTYPER_PxOTYP7_Pos (7UL)
#define | GPIO_OTYPER_PxOTYP7_Msk (0x80UL)
#define | GPIO_OTYPER_PxOTYP6_Pos (6UL)
#define | GPIO_OTYPER_PxOTYP6_Msk (0x40UL)
#define | GPIO_OTYPER_PxOTYP5_Pos (5UL)
#define | GPIO_OTYPER_PxOTYP5_Msk (0x20UL)
#define | GPIO_OTYPER_PxOTYP4_Pos (4UL)
#define | GPIO_OTYPER_PxOTYP4_Msk (0x10UL)
#define | GPIO_OTYPER_PxOTYP3_Pos (3UL)
#define | GPIO_OTYPER_PxOTYP3_Msk (0x8UL)
#define | GPIO_OTYPER_PxOTYP2_Pos (2UL)
#define | GPIO_OTYPER_PxOTYP2_Msk (0x4UL)
#define | GPIO_OTYPER_PxOTYP1_Pos (1UL)
#define | GPIO_OTYPER_PxOTYP1_Msk (0x2UL)
#define | GPIO_OTYPER_PxOTYP0_Pos (0UL)
#define | GPIO_OTYPER_PxOTYP0_Msk (0x1UL)
#define | GPIO_ODR_PxOD7_Pos (7UL)
#define | GPIO_ODR_PxOD7_Msk (0x80UL)
#define | GPIO_ODR_PxOD6_Pos (6UL)
#define | GPIO_ODR_PxOD6_Msk (0x40UL)
#define | GPIO_ODR_PxOD5_Pos (5UL)
#define | GPIO_ODR_PxOD5_Msk (0x20UL)
#define | GPIO_ODR_PxOD4_Pos (4UL)
#define | GPIO_ODR_PxOD4_Msk (0x10UL)
#define | GPIO_ODR_PxOD3_Pos (3UL)
#define | GPIO_ODR_PxOD3_Msk (0x8UL)
#define | GPIO_ODR_PxOD2_Pos (2UL)
#define | GPIO_ODR_PxOD2_Msk (0x4UL)
#define | GPIO_ODR_PxOD1_Pos (1UL)
#define | GPIO_ODR_PxOD1_Msk (0x2UL)
#define | GPIO_ODR_PxOD0_Pos (0UL)
#define | GPIO_ODR_PxOD0_Msk (0x1UL)
#define | GPIO_IDR_PxID7_Pos (7UL)
#define | GPIO_IDR_PxID7_Msk (0x80UL)
#define | GPIO_IDR_PxID6_Pos (6UL)
#define | GPIO_IDR_PxID6_Msk (0x40UL)
#define | GPIO_IDR_PxID5_Pos (5UL)
#define | GPIO_IDR_PxID5_Msk (0x20UL)
#define | GPIO_IDR_PxID4_Pos (4UL)
#define | GPIO_IDR_PxID4_Msk (0x10UL)
#define | GPIO_IDR_PxID3_Pos (3UL)
#define | GPIO_IDR_PxID3_Msk (0x8UL)
#define | GPIO_IDR_PxID2_Pos (2UL)
#define | GPIO_IDR_PxID2_Msk (0x4UL)
#define | GPIO_IDR_PxID1_Pos (1UL)
#define | GPIO_IDR_PxID1_Msk (0x2UL)
#define | GPIO_IDR_PxID0_Pos (0UL)
#define | GPIO_IDR_PxID0_Msk (0x1UL)
#define | GPIO_INTEN_PxIEN7_Pos (7UL)
#define | GPIO_INTEN_PxIEN7_Msk (0x80UL)
#define | GPIO_INTEN_PxIEN6_Pos (6UL)
#define | GPIO_INTEN_PxIEN6_Msk (0x40UL)
#define | GPIO_INTEN_PxIEN5_Pos (5UL)
#define | GPIO_INTEN_PxIEN5_Msk (0x20UL)
#define | GPIO_INTEN_PxIEN4_Pos (4UL)
#define | GPIO_INTEN_PxIEN4_Msk (0x10UL)
#define | GPIO_INTEN_PxIEN3_Pos (3UL)
#define | GPIO_INTEN_PxIEN3_Msk (0x8UL)
#define | GPIO_INTEN_PxIEN2_Pos (2UL)
#define | GPIO_INTEN_PxIEN2_Msk (0x4UL)
#define | GPIO_INTEN_PxIEN1_Pos (1UL)
#define | GPIO_INTEN_PxIEN1_Msk (0x2UL)
#define | GPIO_INTEN_PxIEN0_Pos (0UL)
#define | GPIO_INTEN_PxIEN0_Msk (0x1UL)
#define | GPIO_INTEN_PxIEN0 GPIO_INTEN_PxIEN0_Msk
#define | GPIO_RAWINTST_PxRIS7_Pos (7UL)
#define | GPIO_RAWINTST_PxRIS7_Msk (0x80UL)
#define | GPIO_RAWINTST_PxRIS6_Pos (6UL)
#define | GPIO_RAWINTST_PxRIS6_Msk (0x40UL)
#define | GPIO_RAWINTST_PxRIS5_Pos (5UL)
#define | GPIO_RAWINTST_PxRIS5_Msk (0x20UL)
#define | GPIO_RAWINTST_PxRIS4_Pos (4UL)
#define | GPIO_RAWINTST_PxRIS4_Msk (0x10UL)
#define | GPIO_RAWINTST_PxRIS3_Pos (3UL)
#define | GPIO_RAWINTST_PxRIS3_Msk (0x8UL)
#define | GPIO_RAWINTST_PxRIS2_Pos (2UL)
#define | GPIO_RAWINTST_PxRIS2_Msk (0x4UL)
#define | GPIO_RAWINTST_PxRIS1_Pos (1UL)
#define | GPIO_RAWINTST_PxRIS1_Msk (0x2UL)
#define | GPIO_RAWINTST_PxRIS0_Pos (0UL)
#define | GPIO_RAWINTST_PxRIS0_Msk (0x1UL)
#define | GPIO_MSKINTCR_PxMIS7_Pos (7UL)
#define | GPIO_MSKINTCR_PxMIS7_Msk (0x80UL)
#define | GPIO_MSKINTCR_PxMIS6_Pos (6UL)
#define | GPIO_MSKINTCR_PxMIS6_Msk (0x40UL)
#define | GPIO_MSKINTCR_PxMIS5_Pos (5UL)
#define | GPIO_MSKINTCR_PxMIS5_Msk (0x20UL)
#define | GPIO_MSKINTCR_PxMIS4_Pos (4UL)
#define | GPIO_MSKINTCR_PxMIS4_Msk (0x10UL)
#define | GPIO_MSKINTCR_PxMIS3_Pos (3UL)
#define | GPIO_MSKINTCR_PxMIS3_Msk (0x8UL)
#define | GPIO_MSKINTCR_PxMIS2_Pos (2UL)
#define | GPIO_MSKINTCR_PxMIS2_Msk (0x4UL)
#define | GPIO_MSKINTCR_PxMIS1_Pos (1UL)
#define | GPIO_MSKINTCR_PxMIS1_Msk (0x2UL)
#define | GPIO_MSKINTCR_PxMIS0_Pos (0UL)
#define | GPIO_MSKINTCR_PxMIS0_Msk (0x1UL)
#define | GPIO_INTCLR_PxICLR7_Pos (7UL)
#define | GPIO_INTCLR_PxICLR7_Msk (0x80UL)
#define | GPIO_INTCLR_PxICLR6_Pos (6UL)
#define | GPIO_INTCLR_PxICLR6_Msk (0x40UL)
#define | GPIO_INTCLR_PxICLR5_Pos (5UL)
#define | GPIO_INTCLR_PxICLR5_Msk (0x20UL)
#define | GPIO_INTCLR_PxICLR4_Pos (4UL)
#define | GPIO_INTCLR_PxICLR4_Msk (0x10UL)
#define | GPIO_INTCLR_PxICLR3_Pos (3UL)
#define | GPIO_INTCLR_PxICLR3_Msk (0x8UL)
#define | GPIO_INTCLR_PxICLR2_Pos (2UL)
#define | GPIO_INTCLR_PxICLR2_Msk (0x4UL)
#define | GPIO_INTCLR_PxICLR1_Pos (1UL)
#define | GPIO_INTCLR_PxICLR1_Msk (0x2UL)
#define | GPIO_INTCLR_PxICLR0_Pos (0UL)
#define | GPIO_INTCLR_PxICLR0_Msk (0x1UL)
#define | GPIO_INTTYPCR_PxITYPE7_Pos (7UL)
#define | GPIO_INTTYPCR_PxITYPE7_Msk (0x80UL)
#define | GPIO_INTTYPCR_PxITYPE6_Pos (6UL)
#define | GPIO_INTTYPCR_PxITYPE6_Msk (0x40UL)
#define | GPIO_INTTYPCR_PxITYPE5_Pos (5UL)
#define | GPIO_INTTYPCR_PxITYPE5_Msk (0x20UL)
#define | GPIO_INTTYPCR_PxITYPE4_Pos (4UL)
#define | GPIO_INTTYPCR_PxITYPE4_Msk (0x10UL)
#define | GPIO_INTTYPCR_PxITYPE3_Pos (3UL)
#define | GPIO_INTTYPCR_PxITYPE3_Msk (0x8UL)
#define | GPIO_INTTYPCR_PxITYPE2_Pos (2UL)
#define | GPIO_INTTYPCR_PxITYPE2_Msk (0x4UL)
#define | GPIO_INTTYPCR_PxITYPE1_Pos (1UL)
#define | GPIO_INTTYPCR_PxITYPE1_Msk (0x2UL)
#define | GPIO_INTTYPCR_PxITYPE0_Pos (0UL)
#define | GPIO_INTTYPCR_PxITYPE0_Msk (0x1UL)
#define | GPIO_INTTYPCR_PxITYPE0 GPIO_INTTYPCR_PxITYPE0_Msk
#define | GPIO_INTPOLCR_PxIVAL7_Pos (7UL)
#define | GPIO_INTPOLCR_PxIVAL7_Msk (0x80UL)
#define | GPIO_INTPOLCR_PxIVAL6_Pos (6UL)
#define | GPIO_INTPOLCR_PxIVAL6_Msk (0x40UL)
#define | GPIO_INTPOLCR_PxIVAL5_Pos (5UL)
#define | GPIO_INTPOLCR_PxIVAL5_Msk (0x20UL)
#define | GPIO_INTPOLCR_PxIVAL4_Pos (4UL)
#define | GPIO_INTPOLCR_PxIVAL4_Msk (0x10UL)
#define | GPIO_INTPOLCR_PxIVAL3_Pos (3UL)
#define | GPIO_INTPOLCR_PxIVAL3_Msk (0x8UL)
#define | GPIO_INTPOLCR_PxIVAL2_Pos (2UL)
#define | GPIO_INTPOLCR_PxIVAL2_Msk (0x4UL)
#define | GPIO_INTPOLCR_PxIVAL1_Pos (1UL)
#define | GPIO_INTPOLCR_PxIVAL1_Msk (0x2UL)
#define | GPIO_INTPOLCR_PxIVAL0_Pos (0UL)
#define | GPIO_INTPOLCR_PxIVAL0_Msk (0x1UL)
#define | GPIO_INTPOLCR_PxIVAL0 GPIO_INTPOLCR_PxIVAL0_Msk
#define | GPIO_INTANY_PxIANY7_Pos (7UL)
#define | GPIO_INTANY_PxIANY7_Msk (0x80UL)
#define | GPIO_INTANY_PxIANY6_Pos (6UL)
#define | GPIO_INTANY_PxIANY6_Msk (0x40UL)
#define | GPIO_INTANY_PxIANY5_Pos (5UL)
#define | GPIO_INTANY_PxIANY5_Msk (0x20UL)
#define | GPIO_INTANY_PxIANY4_Pos (4UL)
#define | GPIO_INTANY_PxIANY4_Msk (0x10UL)
#define | GPIO_INTANY_PxIANY3_Pos (3UL)
#define | GPIO_INTANY_PxIANY3_Msk (0x8UL)
#define | GPIO_INTANY_PxIANY2_Pos (2UL)
#define | GPIO_INTANY_PxIANY2_Msk (0x4UL)
#define | GPIO_INTANY_PxIANY1_Pos (1UL)
#define | GPIO_INTANY_PxIANY1_Msk (0x2UL)
#define | GPIO_INTANY_PxIANY0_Pos (0UL)
#define | GPIO_INTANY_PxIANY0_Msk (0x1UL)
#define | GPIO_INTANY_PxIANY0 GPIO_INTANY_PxIANY0_Msk
#define | GPIO_ODSET_PxODSET7_Pos (7UL)
#define | GPIO_ODSET_PxODSET7_Msk (0x80UL)
#define | GPIO_ODSET_PxODSET6_Pos (6UL)
#define | GPIO_ODSET_PxODSET6_Msk (0x40UL)
#define | GPIO_ODSET_PxODSET5_Pos (5UL)
#define | GPIO_ODSET_PxODSET5_Msk (0x20UL)
#define | GPIO_ODSET_PxODSET4_Pos (4UL)
#define | GPIO_ODSET_PxODSET4_Msk (0x10UL)
#define | GPIO_ODSET_PxODSET3_Pos (3UL)
#define | GPIO_ODSET_PxODSET3_Msk (0x8UL)
#define | GPIO_ODSET_PxODSET2_Pos (2UL)
#define | GPIO_ODSET_PxODSET2_Msk (0x4UL)
#define | GPIO_ODSET_PxODSET1_Pos (1UL)
#define | GPIO_ODSET_PxODSET1_Msk (0x2UL)
#define | GPIO_ODSET_PxODSET0_Pos (0UL)
#define | GPIO_ODSET_PxODSET0_Msk (0x1UL)
#define | GPIO_ODCLR_PxODCLR7_Pos (7UL)
#define | GPIO_ODCLR_PxODCLR7_Msk (0x80UL)
#define | GPIO_ODCLR_PxODCLR6_Pos (6UL)
#define | GPIO_ODCLR_PxODCLR6_Msk (0x40UL)
#define | GPIO_ODCLR_PxODCLR5_Pos (5UL)
#define | GPIO_ODCLR_PxODCLR5_Msk (0x20UL)
#define | GPIO_ODCLR_PxODCLR4_Pos (4UL)
#define | GPIO_ODCLR_PxODCLR4_Msk (0x10UL)
#define | GPIO_ODCLR_PxODCLR3_Pos (3UL)
#define | GPIO_ODCLR_PxODCLR3_Msk (0x8UL)
#define | GPIO_ODCLR_PxODCLR2_Pos (2UL)
#define | GPIO_ODCLR_PxODCLR2_Msk (0x4UL)
#define | GPIO_ODCLR_PxODCLR1_Pos (1UL)
#define | GPIO_ODCLR_PxODCLR1_Msk (0x2UL)
#define | GPIO_ODCLR_PxODCLR0_Pos (0UL)
#define | GPIO_ODCLR_PxODCLR0_Msk (0x1UL)
#define | GPIO_INDBEN_PxDIDB_Pos (0UL)
#define | GPIO_INDBEN_PxDIDB_Msk (0xFFUL)
#define | GPIO_INDBEN_PxDIDB GPIO_INDBEN_PxDIDB_Msk
#define | GPIO_INDBEN_SYNC_EN_Pos (8UL)
#define | GPIO_INDBEN_SYNC_EN_Msk (0x100UL)
#define | GPIO_INDBEN_SYNC_EN GPIO_INDBEN_SYNC_EN_Msk
#define | GPIO_DBCLKCR_DBCLK_DIV_Pos (0UL)
#define | GPIO_DBCLKCR_DBCLK_DIV_Msk (0xFUL)
#define | GPIO_DBCLKCR_DBCLK_DIV GPIO_DBCLKCR_DBCLK_DIV_Msk
#define | GPIO_DBCLKCR_DBCLKEN_Pos (4UL)
#define | GPIO_DBCLKCR_DBCLKEN_Msk (0x10UL)
#define | GPIO_DBCLKCR_DBCLKEN GPIO_DBCLKCR_DBCLKEN_Msk
#define | GPIO_PUPDR_PxPUPD7_Pos (14UL)
#define | GPIO_PUPDR_PxPUPD7_Msk (0xC000UL)
#define | GPIO_PUPDR_PxPUPD6_Pos (12UL)
#define | GPIO_PUPDR_PxPUPD6_Msk (0x3000UL)
#define | GPIO_PUPDR_PxPUPD5_Pos (10UL)
#define | GPIO_PUPDR_PxPUPD5_Msk (0xC00UL)
#define | GPIO_PUPDR_PxPUPD4_Pos (8UL)
#define | GPIO_PUPDR_PxPUPD4_Msk (0x300UL)
#define | GPIO_PUPDR_PxPUPD3_Pos (6UL)
#define | GPIO_PUPDR_PxPUPD3_Msk (0xC0UL)
#define | GPIO_PUPDR_PxPUPD2_Pos (4UL)
#define | GPIO_PUPDR_PxPUPD2_Msk (0x30UL)
#define | GPIO_PUPDR_PxPUPD1_Pos (2UL)
#define | GPIO_PUPDR_PxPUPD1_Msk (0xCUL)
#define | GPIO_PUPDR_PxPUPD0_Pos (0UL)
#define | GPIO_PUPDR_PxPUPD0_Msk (0x3UL)
#define | GPIO_PUPDR_PxPUPD0 GPIO_PUPDR_PxPUPD0_Msk
#define | GPIO_SLEWCR_PxSR7_Pos (7UL)
#define | GPIO_SLEWCR_PxSR7_Msk (0x80UL)
#define | GPIO_SLEWCR_PxSR6_Pos (6UL)
#define | GPIO_SLEWCR_PxSR6_Msk (0x40UL)
#define | GPIO_SLEWCR_PxSR5_Pos (5UL)
#define | GPIO_SLEWCR_PxSR5_Msk (0x20UL)
#define | GPIO_SLEWCR_PxSR4_Pos (4UL)
#define | GPIO_SLEWCR_PxSR4_Msk (0x10UL)
#define | GPIO_SLEWCR_PxSR3_Pos (3UL)
#define | GPIO_SLEWCR_PxSR3_Msk (0x8UL)
#define | GPIO_SLEWCR_PxSR2_Pos (2UL)
#define | GPIO_SLEWCR_PxSR2_Msk (0x4UL)
#define | GPIO_SLEWCR_PxSR1_Pos (1UL)
#define | GPIO_SLEWCR_PxSR1_Msk (0x2UL)
#define | GPIO_SLEWCR_PASR0_Pos (0UL)
#define | GPIO_SLEWCR_PASR0_Msk (0x1UL)
#define | GPIO_SLEWCR_PASR0 GPIO_SLEWCR_PASR0_Msk
#define | GPIO_DRVCR_PxDRV7_Pos (7UL)
#define | GPIO_DRVCR_PxDRV7_Msk (0x80UL)
#define | GPIO_DRVCR_PxDRV6_Pos (6UL)
#define | GPIO_DRVCR_PxDRV6_Msk (0x40UL)
#define | GPIO_DRVCR_PxDRV5_Pos (5UL)
#define | GPIO_DRVCR_PxDRV5_Msk (0x20UL)
#define | GPIO_DRVCR_PxDRV4_Pos (4UL)
#define | GPIO_DRVCR_PxDRV4_Msk (0x10UL)
#define | GPIO_DRVCR_PxDRV3_Pos (3UL)
#define | GPIO_DRVCR_PxDRV3_Msk (0x8UL)
#define | GPIO_DRVCR_PxDRV2_Pos (2UL)
#define | GPIO_DRVCR_PxDRV2_Msk (0x4UL)
#define | GPIO_DRVCR_PxDRV1_Pos (1UL)
#define | GPIO_DRVCR_PxDRV1_Msk (0x2UL)
#define | GPIO_DRVCR_PxDRV0_Pos (0UL)
#define | GPIO_DRVCR_PxDRV0_Msk (0x1UL)
#define | GPIO_DRVCR_PxDRV0 GPIO_DRVCR_PxDRV0_Msk
#define | GPIO_AFR_PxAFR7_Pos (28UL)
#define | GPIO_AFR_PxAFR7_Msk (0xF000000UL)
#define | GPIO_AFR_PxAFR6_Pos (24UL)
#define | GPIO_AFR_PxAFR6_Msk (0xF000000UL)
#define | GPIO_AFR_PxAFR5_Pos (20UL)
#define | GPIO_AFR_PxAFR5_Msk (0xF00000UL)
#define | GPIO_AFR_PxAFR4_Pos (16UL)
#define | GPIO_AFR_PxAFR4_Msk (0xF0000UL)
#define | GPIO_AFR_PxAFR3_Pos (12UL)
#define | GPIO_AFR_PxAFR3_Msk (0xF000UL)
#define | GPIO_AFR_PxAFR2_Pos (8UL)
#define | GPIO_AFR_PxAFR2_Msk (0xF00UL)
#define | GPIO_AFR_PxAFR1_Pos (4UL)
#define | GPIO_AFR_PxAFR1_Msk (0xF0UL)
#define | GPIO_AFR_PxAFR0_Pos (0UL)
#define | GPIO_AFR_PxAFR0_Msk (0x0FUL)
#define | GPIO_AFR_PxAFR0 GPIO_AFR_PxAFR0_Msk
#define | SYSCON_CFGR0_LOCKUPEN_Pos (0UL)
#define | SYSCON_CFGR0_LOCKUPEN_Msk (0x1UL)
#define | SYSCON_CFGR0_LOCKUPEN SYSCON_CFGR0_LOCKUPEN_Msk
#define | SYSCON_CFGR0_DBGDLSP_DIS_Pos (1UL)
#define | SYSCON_CFGR0_DBGDLSP_DIS_Msk (0x2UL)
#define | SYSCON_CFGR0_DBGDLSP_DIS SYSCON_CFGR0_DBGDLSP_DIS_Msk
#define | SYSCON_CFGR0_KEY_Pos (16UL)
#define | SYSCON_CFGR0_KEY_Msk (0xFFFF0000UL)
#define | SYSCON_CFGR0_KEY (0x5A69UL)
#define | SYSCON_PORTINTCR_PADINTSEL_Pos (0UL)
#define | SYSCON_PORTINTCR_PADINTSEL_Msk (0x1UL)
#define | SYSCON_PORTINTCR_PADINTSEL SYSCON_PORTINTCR_PADINTSEL_Msk
#define | SYSCON_PORTINTCR_PADDLSPCON_Pos (1UL)
#define | SYSCON_PORTINTCR_PADDLSPCON_Msk (0x2UL)
#define | SYSCON_PORTINTCR_PADDLSPCON SYSCON_PORTINTCR_PADDLSPCON_Msk
#define | SYSCON_PORTINTCR_KEY_Pos (16UL)
#define | SYSCON_PORTINTCR_KEY_Msk (0xFFFF0000UL)
#define | SYSCON_PORTINTCR_KEY SYSCON_PORTINTCR_KEY_Msk
#define | SYSCON_PORTCR_TIM10_GATE_SEL_Pos (4UL)
#define | SYSCON_PORTCR_TIM10_GATE_SEL_Msk (0x30UL)
#define | SYSCON_PORTCR_TIM10_GATE_SEL SYSCON_PORTCR_TIM10_GATE_SEL_Msk
#define | SYSCON_PORTCR_TIM11_GATE_SEL_Pos (6UL)
#define | SYSCON_PORTCR_TIM11_GATE_SEL_Msk (0xC0UL)
#define | SYSCON_PORTCR_TIM11_GATE_SEL SYSCON_PORTCR_TIM11_GATE_SEL_Msk
#define | SYSCON_PORTCR_LPTIM_GATE_SEL_Pos (8UL)
#define | SYSCON_PORTCR_LPTIM_GATE_SEL_Msk (0x300UL)
#define | SYSCON_PORTCR_LPTIM_GATE_SEL SYSCON_PORTCR_LPTIM_GATE_SEL_Msk
#define | SYSCON_PCACR_PCA_CAP0_SEL_Pos (0UL)
#define | SYSCON_PCACR_PCA_CAP0_SEL_Msk (0x3UL)
#define | SYSCON_PCACR_PCA_CAP0_SEL SYSCON_PCACR_PCA_CAP0_SEL_Msk
#define | SYSCON_PCACR_PCA_CAP1_SEL_Pos (2UL)
#define | SYSCON_PCACR_PCA_CAP1_SEL_Msk (0xCUL)
#define | SYSCON_PCACR_PCA_CAP1_SEL SYSCON_PCACR_PCA_CAP1_SEL_Msk
#define | SYSCON_PCACR_PCA_CAP2_SEL_Pos (4UL)
#define | SYSCON_PCACR_PCA_CAP2_SEL_Msk (0x30UL)
#define | SYSCON_PCACR_PCA_CAP2_SEL SYSCON_PCACR_PCA_CAP2_SEL_Msk
#define | SYSCON_PCACR_PCA_CAP3_SEL_Pos (6UL)
#define | SYSCON_PCACR_PCA_CAP3_SEL_Msk (0xC0UL)
#define | SYSCON_PCACR_PCA_CAP3_SEL SYSCON_PCACR_PCA_CAP3_SEL_Msk
#define | SYSCON_PCACR_PCA_CAP4_SEL_Pos (8UL)
#define | SYSCON_PCACR_PCA_CAP4_SEL_Msk (0x300UL)
#define | SYSCON_PCACR_PCA_CAP4_SEL SYSCON_PCACR_PCA_CAP4_SEL_Msk
#define | SYSCON_TIM1CR_TIM1CH1IN_SEL_Pos (0UL)
#define | SYSCON_TIM1CR_TIM1CH1IN_SEL_Msk (0x7UL)
#define | SYSCON_TIM1CR_TIM1CH1IN_SEL SYSCON_TIM1CR_TIM1CH1IN_SEL_Msk
#define | SYSCON_TIM1CR_TIM1CH2IN_SEL_Pos (4UL)
#define | SYSCON_TIM1CR_TIM1CH2IN_SEL_Msk (0x70UL)
#define | SYSCON_TIM1CR_TIM1CH2IN_SEL SYSCON_TIM1CR_TIM1CH2IN_SEL_Msk
#define | SYSCON_TIM1CR_TIM1CH3IN_SEL_Pos (8UL)
#define | SYSCON_TIM1CR_TIM1CH3IN_SEL_Msk (0x700UL)
#define | SYSCON_TIM1CR_TIM1CH3IN_SEL SYSCON_TIM1CR_TIM1CH3IN_SEL_Msk
#define | SYSCON_TIM1CR_TIM1CH4IN_SEL_Pos (12UL)
#define | SYSCON_TIM1CR_TIM1CH4IN_SEL_Msk (0x7000UL)
#define | SYSCON_TIM1CR_TIM1CH4IN_SEL SYSCON_TIM1CR_TIM1CH4IN_SEL_Msk
#define | SYSCON_TIM1CR_TIM1BRKOUTCFG_Pos (20UL)
#define | SYSCON_TIM1CR_TIM1BRKOUTCFG_Msk (0x100000UL)
#define | SYSCON_TIM1CR_TIM1BRKOUTCFG SYSCON_TIM1CR_TIM1BRKOUTCFG_Msk
#define | SYSCON_TIM1CR_DSLPBRKEN_Pos (21UL)
#define | SYSCON_TIM1CR_DSLPBRKEN_Msk (0x200000UL)
#define | SYSCON_TIM1CR_DSLPBRKEN SYSCON_TIM1CR_DSLPBRKEN_Msk
#define | SYSCON_TIM1CR_CLKFAILBRKEN_Pos (22UL)
#define | SYSCON_TIM1CR_CLKFAILBRKEN_Msk (0x400000UL)
#define | SYSCON_TIM1CR_CLKFAILBRKEN SYSCON_TIM1CR_CLKFAILBRKEN_Msk
#define | SYSCON_TIM2CR_TIM2CH1IN_SEL_Pos (0UL)
#define | SYSCON_TIM2CR_TIM2CH1IN_SEL_Msk (0x7UL)
#define | SYSCON_TIM2CR_TIM2CH1IN_SEL SYSCON_TIM2CR_TIM2CH1IN_SEL_Msk
#define | SYSCON_TIM2CR_TIM2CH2IN_SEL_Pos (4UL)
#define | SYSCON_TIM2CR_TIM2CH2IN_SEL_Msk (0x70UL)
#define | SYSCON_TIM2CR_TIM2CH2IN_SEL SYSCON_TIM2CR_TIM2CH2IN_SEL_Msk
#define | SYSCON_TIM2CR_TIM2CH3IN_SEL_Pos (8UL)
#define | SYSCON_TIM2CR_TIM2CH3IN_SEL_Msk (0x700UL)
#define | SYSCON_TIM2CR_TIM2CH3IN_SEL SYSCON_TIM2CR_TIM2CH3IN_SEL_Msk
#define | SYSCON_TIM2CR_TIM2CH4IN_SEL_Pos (12UL)
#define | SYSCON_TIM2CR_TIM2CH4IN_SEL_Msk (0x7000UL)
#define | SYSCON_TIM2CR_TIM2CH4IN_SEL SYSCON_TIM2CR_TIM2CH4IN_SEL_Msk
#define | SYSCON_UNLOCK_UNLOCK_Pos (0UL)
#define | SYSCON_UNLOCK_UNLOCK_Msk (0x1UL)
#define | SYSCON_UNLOCK_UNLOCK SYSCON_UNLOCK_UNLOCK_Msk
#define | SYSCON_UNLOCK_KEY_Pos (1UL)
#define | SYSCON_UNLOCK_KEY_Msk (0xFFFFFFFEUL)
#define | SYSCON_UNLOCK_KEY SYSCON_UNLOCK_KEY_Msk
#define | RCC_HCLKDIV_AHBCKDIV_Pos (0UL)
#define | RCC_HCLKDIV_AHBCKDIV_Msk (0xFFUL)
#define | RCC_HCLKDIV_AHBCKDIV RCC_HCLKDIV_AHBCKDIV_Msk
#define | RCC_HCLKDIV_AHBCKDIV_1 (0x00000000)
#define | RCC_PCLKDIV_APBCKDIV_Pos (0UL)
#define | RCC_PCLKDIV_APBCKDIV_Msk (0xFFUL)
#define | RCC_PCLKDIV_APBCKDIV RCC_PCLKDIV_APBCKDIV_Msk
#define | RCC_PCLKDIV_APBCKDIV_1 (0x00000000)
#define | RCC_HCLKEN_GPIOACKEN_Pos (0UL)
#define | RCC_HCLKEN_GPIOACKEN_Msk (0x1UL)
#define | RCC_HCLKEN_GPIOACKEN RCC_HCLKEN_GPIOACKEN_Msk
#define | RCC_HCLKEN_GPIOBCKEN_Pos (1UL)
#define | RCC_HCLKEN_GPIOBCKEN_Msk (0x2UL)
#define | RCC_HCLKEN_GPIOBCKEN RCC_HCLKEN_GPIOBCKEN_Msk
#define | RCC_HCLKEN_GPIOCCKEN_Pos (2UL)
#define | RCC_HCLKEN_GPIOCCKEN_Msk (0x4UL)
#define | RCC_HCLKEN_GPIOCCKEN RCC_HCLKEN_GPIOCCKEN_Msk
#define | RCC_HCLKEN_GPIODCKEN_Pos (3UL)
#define | RCC_HCLKEN_GPIODCKEN_Msk (0x8UL)
#define | RCC_HCLKEN_GPIODCKEN RCC_HCLKEN_GPIODCKEN_Msk
#define | RCC_HCLKEN_CRCCKEN_Pos (4UL)
#define | RCC_HCLKEN_CRCCKEN_Msk (0x10UL)
#define | RCC_HCLKEN_CRCCKEN RCC_HCLKEN_CRCCKEN_Msk
#define | RCC_HCLKEN_FLASHCKEN_Pos (8UL)
#define | RCC_HCLKEN_FLASHCKEN_Msk (0x100UL)
#define | RCC_HCLKEN_FLASHCKEN RCC_HCLKEN_FLASHCKEN_Msk
#define | RCC_PCLKEN_UART1CKEN_Pos (0UL)
#define | RCC_PCLKEN_UART1CKEN_Msk (0x1UL)
#define | RCC_PCLKEN_UART1CKEN RCC_PCLKEN_UART1CKEN_Msk
#define | RCC_PCLKEN_UART2CKEN_Pos (1UL)
#define | RCC_PCLKEN_UART2CKEN_Msk (0x2UL)
#define | RCC_PCLKEN_UART2CKEN RCC_PCLKEN_UART2CKEN_Msk
#define | RCC_PCLKEN_I2CCKEN_Pos (2UL)
#define | RCC_PCLKEN_I2CCKEN_Msk (0x4UL)
#define | RCC_PCLKEN_I2CCKEN RCC_PCLKEN_I2CCKEN_Msk
#define | RCC_PCLKEN_LPUARTCKEN_Pos (3UL)
#define | RCC_PCLKEN_LPUARTCKEN_Msk (0x8UL)
#define | RCC_PCLKEN_LPUARTCKEN RCC_PCLKEN_LPUARTCKEN_Msk
#define | RCC_PCLKEN_SPICKEN_Pos (4UL)
#define | RCC_PCLKEN_SPICKEN_Msk (0x10UL)
#define | RCC_PCLKEN_SPICKEN RCC_PCLKEN_SPICKEN_Msk
#define | RCC_PCLKEN_LPTIMCKEN_Pos (5UL)
#define | RCC_PCLKEN_LPTIMCKEN_Msk (0x20UL)
#define | RCC_PCLKEN_LPTIMCKEN RCC_PCLKEN_LPTIMCKEN_Msk
#define | RCC_PCLKEN_BASETIMCKEN_Pos (6UL)
#define | RCC_PCLKEN_BASETIMCKEN_Msk (0x40UL)
#define | RCC_PCLKEN_BASETIMCKEN RCC_PCLKEN_BASETIMCKEN_Msk
#define | RCC_PCLKEN_SYSCONCKEN_Pos (7UL)
#define | RCC_PCLKEN_SYSCONCKEN_Msk (0x80UL)
#define | RCC_PCLKEN_SYSCONCKEN RCC_PCLKEN_SYSCONCKEN_Msk
#define | RCC_PCLKEN_PCACKEN_Pos (8UL)
#define | RCC_PCLKEN_PCACKEN_Msk (0x100UL)
#define | RCC_PCLKEN_PCACKEN RCC_PCLKEN_PCACKEN_Msk
#define | RCC_PCLKEN_OWIRECKEN_Pos (9UL)
#define | RCC_PCLKEN_OWIRECKEN_Msk (0x200UL)
#define | RCC_PCLKEN_OWIRECKEN RCC_PCLKEN_OWIRECKEN_Msk
#define | RCC_PCLKEN_TIM1CKEN_Pos (10UL)
#define | RCC_PCLKEN_TIM1CKEN_Msk (0x400UL)
#define | RCC_PCLKEN_TIM1CKEN RCC_PCLKEN_TIM1CKEN_Msk
#define | RCC_PCLKEN_TIM2CKEN_Pos (11UL)
#define | RCC_PCLKEN_TIM2CKEN_Msk (0x800UL)
#define | RCC_PCLKEN_TIM2CKEN RCC_PCLKEN_TIM2CKEN_Msk
#define | RCC_PCLKEN_WWDGCKEN_Pos (12UL)
#define | RCC_PCLKEN_WWDGCKEN_Msk (0x1000UL)
#define | RCC_PCLKEN_WWDGCKEN RCC_PCLKEN_WWDGCKEN_Msk
#define | RCC_PCLKEN_ADCCKEN_Pos (13UL)
#define | RCC_PCLKEN_ADCCKEN_Msk (0x2000UL)
#define | RCC_PCLKEN_ADCCKEN RCC_PCLKEN_ADCCKEN_Msk
#define | RCC_PCLKEN_AWKCKEN_Pos (14UL)
#define | RCC_PCLKEN_AWKCKEN_Msk (0x4000UL)
#define | RCC_PCLKEN_AWKCKEN RCC_PCLKEN_AWKCKEN_Msk
#define | RCC_PCLKEN_RTCCKEN_Pos (15UL)
#define | RCC_PCLKEN_RTCCKEN_Msk (0x8000UL)
#define | RCC_PCLKEN_RTCCKEN RCC_PCLKEN_RTCCKEN_Msk
#define | RCC_PCLKEN_CLKCTRIMCKEN_Pos (16UL)
#define | RCC_PCLKEN_CLKCTRIMCKEN_Msk (0x10000UL)
#define | RCC_PCLKEN_CLKCTRIMCKEN RCC_PCLKEN_CLKCTRIMCKEN_Msk
#define | RCC_PCLKEN_IWDGCKEN_Pos (17UL)
#define | RCC_PCLKEN_IWDGCKEN_Msk (0x20000UL)
#define | RCC_PCLKEN_IWDGCKEN RCC_PCLKEN_IWDGCKEN_Msk
#define | RCC_PCLKEN_LVDVCCKEN_Pos (18UL)
#define | RCC_PCLKEN_LVDVCCKEN_Msk (0x40000UL)
#define | RCC_PCLKEN_LVDVCCKEN RCC_PCLKEN_LVDVCCKEN_Msk
#define | RCC_PCLKEN_BEEPCKEN_Pos (19UL)
#define | RCC_PCLKEN_BEEPCKEN_Msk (0x80000UL)
#define | RCC_PCLKEN_BEEPCKEN RCC_PCLKEN_BEEPCKEN_Msk
#define | RCC_PCLKEN_DBGCKEN_Pos (20UL)
#define | RCC_PCLKEN_DBGCKEN_Msk (0x100000UL)
#define | RCC_PCLKEN_DBGCKEN RCC_PCLKEN_DBGCKEN_Msk
#define | RCC_MCOCR_MCODIV_Pos (0UL)
#define | RCC_MCOCR_MCODIV_Msk (0xFFUL)
#define | RCC_MCOCR_MCODIV RCC_MCOCR_MCODIV_Msk
#define | RCC_MCOCR_MCOSEL_Pos (8UL)
#define | RCC_MCOCR_MCOSEL_Msk (0x700UL)
#define | RCC_MCOCR_MCOSEL RCC_MCOCR_MCOSEL_Msk
#define | RCC_MCOCR_MCOSEL_0 (0x1 << RCC_MCOCR_MCOSEL_Pos)
#define | RCC_MCOCR_MCOSEL_1 (0x2 << RCC_MCOCR_MCOSEL_Pos)
#define | RCC_MCOCR_MCOSEL_2 (0x4 << RCC_MCOCR_MCOSEL_Pos)
#define | RCC_MCOCR_MCOEN_Pos (12UL)
#define | RCC_MCOCR_MCOEN_Msk (0x1000UL)
#define | RCC_MCOCR_MCOEN RCC_MCOCR_MCOEN_Msk
#define | RCC_RSTCR_MCURST_Pos (0UL)
#define | RCC_RSTCR_MCURST_Msk (0x1UL)
#define | RCC_RSTCR_CPURST_Pos (1UL)
#define | RCC_RSTCR_CPURST_Msk (0x2UL)
#define | RCC_RSTCR_RSTKEY_Pos (2UL)
#define | RCC_RSTCR_RSTKEY_Msk (0xFFFFFFFCUL)
#define | RCC_RSTSR_MCURST_Pos (0UL)
#define | RCC_RSTSR_MCURST_Msk (0x1UL)
#define | RCC_RSTSR_MCURST RCC_RSTSR_MCURST_Msk
#define | RCC_RSTSR_CPURST_Pos (1UL)
#define | RCC_RSTSR_CPURST_Msk (0x2UL)
#define | RCC_RSTSR_CPURST RCC_RSTSR_CPURST_Msk
#define | RCC_RSTSR_WWDGRST_Pos (2UL)
#define | RCC_RSTSR_WWDGRST_Msk (0x4UL)
#define | RCC_RSTSR_WWDGRST RCC_RSTSR_WWDGRST_Msk
#define | RCC_RSTSR_IWDGRST_Pos (3UL)
#define | RCC_RSTSR_IWDGRST_Msk (0x8UL)
#define | RCC_RSTSR_IWDGRST RCC_RSTSR_IWDGRST_Msk
#define | RCC_RSTSR_LVDRST_Pos (4UL)
#define | RCC_RSTSR_LVDRST_Msk (0x10UL)
#define | RCC_RSTSR_LVDRST RCC_RSTSR_LVDRST_Msk
#define | RCC_RSTSR_PORRST_Pos (5UL)
#define | RCC_RSTSR_PORRST_Msk (0x20UL)
#define | RCC_RSTSR_PORRST RCC_RSTSR_PORRST_Msk
#define | RCC_RSTSR_LOCKUPRST_Pos (6UL)
#define | RCC_RSTSR_LOCKUPRST_Msk (0x40UL)
#define | RCC_RSTSR_LOCKUPRST RCC_RSTSR_LOCKUPRST_Msk
#define | RCC_RSTSR_PADRST_Pos (7UL)
#define | RCC_RSTSR_PADRST_Msk (0x80UL)
#define | RCC_RSTSR_PADRST RCC_RSTSR_PADRST_Msk
#define | RCC_RSTSR_SFTRST_Pos (8UL)
#define | RCC_RSTSR_SFTRST_Msk (0x100UL)
#define | RCC_RSTSR_SFTRST RCC_RSTSR_SFTRST_Msk
#define | RCC_SYSCLKCR_HSIEN_Pos (0UL)
#define | RCC_SYSCLKCR_HSIEN_Msk (0x1UL)
#define | RCC_SYSCLKCR_HSIEN RCC_SYSCLKCR_HSIEN_Msk
#define | RCC_SYSCLKCR_HSEEN_Pos (1UL)
#define | RCC_SYSCLKCR_HSEEN_Msk (0x2UL)
#define | RCC_SYSCLKCR_HSEEN RCC_SYSCLKCR_HSEEN_Msk
#define | RCC_SYSCLKCR_LSIEN_Pos (2UL)
#define | RCC_SYSCLKCR_LSIEN_Msk (0x4UL)
#define | RCC_SYSCLKCR_LSIEN RCC_SYSCLKCR_LSIEN_Msk
#define | RCC_SYSCLKCR_HSEBYP_Pos (5UL)
#define | RCC_SYSCLKCR_HSEBYP_Msk (0x20UL)
#define | RCC_SYSCLKCR_HSEBYP RCC_SYSCLKCR_HSEBYP_Msk
#define | RCC_SYSCLKCR_HSEPORT_Pos (6UL)
#define | RCC_SYSCLKCR_HSEPORT_Msk (0x40UL)
#define | RCC_SYSCLKCR_HSEPORT RCC_SYSCLKCR_HSEPORT_Msk
#define | RCC_SYSCLKCR_CLKFAILEN_Pos (8UL)
#define | RCC_SYSCLKCR_CLKFAILEN_Msk (0x100UL)
#define | RCC_SYSCLKCR_CLKFAILEN RCC_SYSCLKCR_CLKFAILEN_Msk
#define | RCC_SYSCLKCR_WKBYHSI_Pos (15UL)
#define | RCC_SYSCLKCR_WKBYHSI_Msk (0x8000UL)
#define | RCC_SYSCLKCR_WKBYHSI RCC_SYSCLKCR_WKBYHSI_Msk
#define | RCC_SYSCLKCR_KEY_Pos (16UL)
#define | RCC_SYSCLKCR_KEY_Msk (0xFFFF0000UL)
#define | RCC_SYSCLKCR_KEY RCC_SYSCLKCR_KEY_Msk
#define | RCC_SYSCLKSEL_CLKSW_Pos (0UL)
#define | RCC_SYSCLKSEL_CLKSW_Msk (0xFUL)
#define | RCC_SYSCLKSEL_CLKSW RCC_SYSCLKSEL_CLKSW_Msk
#define | RCC_SYSCLKSEL_CLKSW_0 (0x1U << RCC_SYSCLKSEL_CLKSW_Pos)
#define | RCC_SYSCLKSEL_CLKSW_1 (0x2U << RCC_SYSCLKSEL_CLKSW_Pos)
#define | RCC_SYSCLKSEL_CLKSW_2 (0x4U << RCC_SYSCLKSEL_CLKSW_Pos)
#define | RCC_SYSCLKSEL_CLKSW_3 (0x8U << RCC_SYSCLKSEL_CLKSW_Pos)
#define | RCC_SYSCLKSEL_KEY_Pos (16UL)
#define | RCC_SYSCLKSEL_KEY_Msk (0xFFFF0000UL)
#define | RCC_SYSCLKSEL_KEY RCC_SYSCLKSEL_KEY_Msk
#define | RCC_HSICR_HSITRIM_Pos (0UL)
#define | RCC_HSICR_HSITRIM_Msk (0xFFFUL)
#define | RCC_HSICR_HSITRIM RCC_HSICR_HSITRIM_Msk
#define | RCC_HSICR_HSITRIM_0_8_Mask (0x1FFUL)
#define | RCC_HSICR_HSITRIM_9 (0x200 << RCC_HSICR_HSITRIM_Pos)
#define | RCC_HSICR_HSITRIM_10 (0x400 << RCC_HSICR_HSITRIM_Pos)
#define | RCC_HSICR_HSITRIM_11 (0x800 << RCC_HSICR_HSITRIM_Pos)
#define | RCC_HSICR_HSITCTRIM_Pos (0UL)
#define | RCC_HSICR_HSITCTRIM_Msk (0xFFFUL)
#define | RCC_HSICR_HSITCTRIM_0_3_Mask (0xFUL)
#define | RCC_HSICR_HSITCTRIM_9_15 (0)
#define | RCC_HSICR_HSIRDY_Pos (12UL)
#define | RCC_HSICR_HSIRDY_Msk (0x1000UL)
#define | RCC_HSICR_HSIRDY RCC_HSICR_HSIRDY_Msk
#define | RCC_HSICR_KEY_Pos (16UL)
#define | RCC_HSICR_KEY_Msk (0xFFFF0000UL)
#define | RCC_HSICR_KEY RCC_HSICR_KEY_Msk
#define | RCC_HSECR_HSEDRV_Pos (0UL)
#define | RCC_HSECR_HSEDRV_Msk (0x7UL)
#define | RCC_HSECR_HSEDRV RCC_HSECR_HSEDRV_Msk
#define | RCC_HSECR_HSESTARTUP_Pos (4UL)
#define | RCC_HSECR_HSESTARTUP_Msk (0x30UL)
#define | RCC_HSECR_HSESTARTUP RCC_HSECR_HSESTARTUP_Msk
#define | RCC_HSECR_HSERDY_Pos (6UL)
#define | RCC_HSECR_HSERDY_Msk (0x40UL)
#define | RCC_HSECR_HSERDY RCC_HSECR_HSERDY_Msk
#define | RCC_LSICR_LSITRIM_Pos (0UL)
#define | RCC_LSICR_LSITRIM_Msk (0x1FFUL)
#define | RCC_LSICR_LSITRIM RCC_LSICR_LSITRIM_Msk
#define | RCC_LSICR_LSISTARTUP_Pos (10UL)
#define | RCC_LSICR_LSISTARTUP_Msk (0xC00UL)
#define | RCC_LSICR_LSISTARTUP RCC_LSICR_LSISTARTUP_Msk
#define | RCC_LSICR_LSISTARTUP_0 (0x01 << RCC_LSICR_LSISTARTUP_Pos)
#define | RCC_LSICR_LSISTARTUP_1 (0x02 << RCC_LSICR_LSISTARTUP_Pos)
#define | RCC_LSICR_LSIRDY_Pos (12UL)
#define | RCC_LSICR_LSIRDY_Msk (0x1000UL)
#define | RCC_LSICR_LSIRDY RCC_LSICR_LSIRDY_Msk
#define | RCC_LSICR_KEY_Pos (16UL)
#define | RCC_LSICR_KEY_Msk (0xFFFF0000UL)
#define | RCC_LSICR_KEY RCC_LSICR_KEY_Msk
#define | RCC_LSECR_LSEDRV_Pos (0UL)
#define | RCC_LSECR_LSEDRV_Msk (0xFUL)
#define | RCC_LSECR_LSEDRV RCC_LSECR_LSEDRV_Msk
#define | RCC_LSECR_LSESTARTUP_Pos (4UL)
#define | RCC_LSECR_LSESTARTUP_Msk (0x30UL)
#define | RCC_LSECR_LSESTARTUP RCC_LSECR_LSESTARTUP_Msk
#define | RCC_LSECR_LSERDY_Pos (6UL)
#define | RCC_LSECR_LSERDY_Msk (0x40UL)
#define | RCC_LSECR_LSERDY RCC_LSECR_LSERDY_Msk
#define | RCC_LSECR_LSEEN_Pos (8UL)
#define | RCC_LSECR_LSEEN_Msk (0x100UL)
#define | RCC_LSECR_LSEEN RCC_LSECR_LSEEN_Msk
#define | RCC_LSECR_LSEBYP_Pos (9UL)
#define | RCC_LSECR_LSEBYP_Msk (0x200UL)
#define | RCC_LSECR_LSEBYP RCC_LSECR_LSEBYP_Msk
#define | RCC_LSECR_LSEAON_Pos (10UL)
#define | RCC_LSECR_LSEAON_Msk (0x400UL)
#define | RCC_LSECR_LSEAON RCC_LSECR_LSEAON_Msk
#define | RCC_LSECR_LSEPORT_Pos (11UL)
#define | RCC_LSECR_LSEPORT_Msk (0x800UL)
#define | RCC_LSECR_LSEPORT RCC_LSECR_LSEPORT_Msk
#define | RCC_LSECR_KEY_Pos (16UL)
#define | RCC_LSECR_KEY_Msk (0xFFFF0000UL)
#define | RCC_LSECR_KEY RCC_LSECR_KEY_Msk
#define | RCC_IRQLATENCY_IRQLATENCY_Pos (0UL)
#define | RCC_IRQLATENCY_IRQLATENCY_Msk (0xFFUL)
#define | RCC_STICKCR_STCALIB_Pos (0UL)
#define | RCC_STICKCR_STCALIB_Msk (0xFFFFFFUL)
#define | RCC_STICKCR_SKEW_Pos (24UL)
#define | RCC_STICKCR_SKEW_Msk (0x1000000UL)
#define | RCC_STICKCR_NOREF_Pos (25UL)
#define | RCC_STICKCR_NOREF_Msk (0x2000000UL)
#define | RCC_SWDIOCR_SWDPORT_Pos (0UL)
#define | RCC_SWDIOCR_SWDPORT_Msk (0x1UL)
#define | RCC_SWDIOCR_KEY_Pos (16UL)
#define | RCC_SWDIOCR_KEY_Msk (0xFFFF0000UL)
#define | RCC_PERIRST_UART1RST_Pos (0UL)
#define | RCC_PERIRST_UART1RST_Msk (0x1UL)
#define | RCC_PERIRST_UART1RST RCC_PERIRST_UART1RST_Msk
#define | RCC_PERIRST_UART2RST_Pos (1UL)
#define | RCC_PERIRST_UART2RST_Msk (0x2UL)
#define | RCC_PERIRST_UART2RST RCC_PERIRST_UART2RST_Msk
#define | RCC_PERIRST_I2CRST_Pos (2UL)
#define | RCC_PERIRST_I2CRST_Msk (0x4UL)
#define | RCC_PERIRST_I2CRST RCC_PERIRST_I2CRST_Msk
#define | RCC_PERIRST_LPUARTRST_Pos (3UL)
#define | RCC_PERIRST_LPUARTRST_Msk (0x8UL)
#define | RCC_PERIRST_LPUARTRST RCC_PERIRST_LPUARTRST_Msk
#define | RCC_PERIRST_SPIRST_Pos (4UL)
#define | RCC_PERIRST_SPIRST_Msk (0x10UL)
#define | RCC_PERIRST_SPIRST RCC_PERIRST_SPIRST_Msk
#define | RCC_PERIRST_LPTIMRST_Pos (5UL)
#define | RCC_PERIRST_LPTIMRST_Msk (0x20UL)
#define | RCC_PERIRST_LPTIMRST RCC_PERIRST_LPTIMRST_Msk
#define | RCC_PERIRST_BASETIMRST_Pos (6UL)
#define | RCC_PERIRST_BASETIMRST_Msk (0x40UL)
#define | RCC_PERIRST_BASETIMRST RCC_PERIRST_BASETIMRST_Msk
#define | RCC_PERIRST_SYSCONRST_Pos (7UL)
#define | RCC_PERIRST_SYSCONRST_Msk (0x80UL)
#define | RCC_PERIRST_SYSCONRST RCC_PERIRST_SYSCONRST_Msk
#define | RCC_PERIRST_PCARST_Pos (8UL)
#define | RCC_PERIRST_PCARST_Msk (0x100UL)
#define | RCC_PERIRST_PCARST RCC_PERIRST_PCARST_Msk
#define | RCC_PERIRST_OWIRERST_Pos (9UL)
#define | RCC_PERIRST_OWIRERST_Msk (0x200UL)
#define | RCC_PERIRST_OWIRERST RCC_PERIRST_OWIRERST_Msk
#define | RCC_PERIRST_TIM1RST_Pos (10UL)
#define | RCC_PERIRST_TIM1RST_Msk (0x400UL)
#define | RCC_PERIRST_TIM1RST RCC_PERIRST_TIM1RST_Msk
#define | RCC_PERIRST_TIM2RST_Pos (11UL)
#define | RCC_PERIRST_TIM2RST_Msk (0x800UL)
#define | RCC_PERIRST_TIM2RST RCC_PERIRST_TIM2RST_Msk
#define | RCC_PERIRST_WWDGRST_Pos (12UL)
#define | RCC_PERIRST_WWDGRST_Msk (0x1000UL)
#define | RCC_PERIRST_WWDGRST RCC_PERIRST_WWDGRST_Msk
#define | RCC_PERIRST_ADCRST_Pos (13UL)
#define | RCC_PERIRST_ADCRST_Msk (0x2000UL)
#define | RCC_PERIRST_ADCRST RCC_PERIRST_ADCRST_Msk
#define | RCC_PERIRST_AWKRST_Pos (14UL)
#define | RCC_PERIRST_AWKRST_Msk (0x4000UL)
#define | RCC_PERIRST_AWKRST RCC_PERIRST_AWKRST_Msk
#define | RCC_PERIRST_CLKTRIMRST_Pos (16UL)
#define | RCC_PERIRST_CLKTRIMRST_Msk (0x10000UL)
#define | RCC_PERIRST_CLKTRIMRST RCC_PERIRST_CLKTRIMRST_Msk
#define | RCC_PERIRST_LVDVCRST_Pos (18UL)
#define | RCC_PERIRST_LVDVCRST_Msk (0x40000UL)
#define | RCC_PERIRST_LVDVCRST RCC_PERIRST_LVDVCRST_Msk
#define | RCC_PERIRST_BEEPRST_Pos (19UL)
#define | RCC_PERIRST_BEEPRST_Msk (0x80000UL)
#define | RCC_PERIRST_BEEPRST RCC_PERIRST_BEEPRST_Msk
#define | RCC_PERIRST_DBGRST_Pos (20UL)
#define | RCC_PERIRST_DBGRST_Msk (0x100000UL)
#define | RCC_PERIRST_DBGRST RCC_PERIRST_DBGRST_Msk
#define | RCC_PERIRST_GPIOARST_Pos (24UL)
#define | RCC_PERIRST_GPIOARST_Msk (0x1000000UL)
#define | RCC_PERIRST_GPIOARST RCC_PERIRST_GPIOARST_Msk
#define | RCC_PERIRST_GPIOBRST_Pos (25UL)
#define | RCC_PERIRST_GPIOBRST_Msk (0x2000000UL)
#define | RCC_PERIRST_GPIOBRST RCC_PERIRST_GPIOBRST_Msk
#define | RCC_PERIRST_GPIOCRST_Pos (26UL)
#define | RCC_PERIRST_GPIOCRST_Msk (0x4000000UL)
#define | RCC_PERIRST_GPIOCRST RCC_PERIRST_GPIOCRST_Msk
#define | RCC_PERIRST_GPIODRST_Pos (27UL)
#define | RCC_PERIRST_GPIODRST_Msk (0x8000000UL)
#define | RCC_PERIRST_GPIODRST RCC_PERIRST_GPIODRST_Msk
#define | RCC_PERIRST_CRCRST_Pos (28UL)
#define | RCC_PERIRST_CRCRST_Msk (0x10000000UL)
#define | RCC_PERIRST_CRCRST RCC_PERIRST_CRCRST_Msk
#define | RCC_RTCRST_RTCRST_Pos (0UL)
#define | RCC_RTCRST_RTCRST_Msk (0x1UL)
#define | RCC_RTCRST_RTCRST RCC_RTCRST_RTCRST_Msk
#define | RCC_RTCRST_KEY_Pos (16UL)
#define | RCC_RTCRST_KEY_Msk (0xFFFF0000UL)
#define | RCC_RTCRST_KEY RCC_RTCRST_KEY_Msk
#define | RCC_UNLOCK_UNLOCK_Pos (0UL)
#define | RCC_UNLOCK_UNLOCK_Msk (0x1UL)
#define | RCC_UNLOCK_UNLOCK RCC_UNLOCK_UNLOCK_Msk
#define | RCC_UNLOCK_KEY_Pos (1UL)
#define | RCC_UNLOCK_KEY_Msk (0xFFFFFFFEUL)
#define | RCC_UNLOCK_KEY RCC_UNLOCK_KEY_Msk
#define | M8(adr) (*((volatile uint8_t *) (adr)))
#define | M16(adr) (*((volatile uint16_t *) (adr)))
#define | M32(adr) (*((volatile uint32_t *) (adr)))

## 类型定义
typedef enum IRQn | IRQn_Type
typedef enum FlagStatus | ITStatus

## 枚举
enum | IRQn { NonMaskableInt_IRQn = -14, HardFault_IRQn = -13, SVCall_IRQn = -5, PendSV_IRQn = -2, SysTick_IRQn = -1, GPIOA_IRQn = 0, GPIOB_IRQn = 1, GPIOC_IRQn = 2, GPIOD_IRQn = 3, FLASH_IRQn = 4, UART1_IRQn = 6, UART2_IRQn = 7, LPUART_IRQn = 8, SPI_IRQn = 10, I2C_IRQn = 12, TIM10_IRQn = 14, TIM11_IRQn = 15, LPTIM_IRQn = 16, TIM1_IRQn = 18, TIM2_IRQn = 19, PCA_IRQn = 21, WWDG_IRQn = 22, IWDG_IRQn = 23, ADC_IRQn = 24, LVD_IRQn = 25, VCMP_IRQn = 26, AWK_IRQn = 28, OWIRE_IRQn = 29, RTC_IRQn = 30, CLKTRIM_IRQn = 31 }
enum | FlagStatus { RESET = 0, SET = !RESET }
enum | FunctionalState { DISABLE = 0, ENABLE = !DISABLE }
enum | SignalState { INACTIVE = 0, ACTIVE = !INACTIVE }
enum | ErrorStatus { ERROR = 0, SUCCESS = !ERROR }

## 详细描述

## 宏定义说明

## ◆ ADC_CR0_ADCEN_Msk

#define ADC_CR0_ADCEN_Msk (0x1UL)

ADC CR0: ADCEN (Bitfield-Mask: 0x01)

## ◆ ADC_CR0_ADCEN_Pos

#define ADC_CR0_ADCEN_Pos (0UL)

ADC CR0: ADCEN (Bit 0)

## ◆ ADC_CR0_CLKSEL_Msk

#define ADC_CR0_CLKSEL_Msk (0x70UL)

ADC CR0: CLKSEL (Bitfield-Mask: 0x07)

## ◆ ADC_CR0_CLKSEL_Pos

#define ADC_CR0_CLKSEL_Pos (4UL)

ADC CR0: CLKSEL (Bit 4)

## ◆ ADC_CR0_SAM_Msk

#define ADC_CR0_SAM_Msk (0x800UL)

ADC CR0: SAM (Bitfield-Mask: 0x01)

## ◆ ADC_CR0_SAM_Pos

#define ADC_CR0_SAM_Pos (11UL)

ADC CR0: SAM (Bit 11)

## ◆ ADC_CR0_SEL_Msk

#define ADC_CR0_SEL_Msk (0x700UL | 0x80UL)

ADC CR0: SEL (Bitfield-Mask: 0x07)

## ◆ ADC_CR0_SEL_Pos

#define ADC_CR0_SEL_Pos (8UL)

ADC CR0: SEL (Bit 8)

## ◆ ADC_CR0_START_Msk

#define ADC_CR0_START_Msk (0x2UL)

ADC CR0: START (Bitfield-Mask: 0x01)

## ◆ ADC_CR0_START_Pos

#define ADC_CR0_START_Pos (1UL)

ADC CR0: START (Bit 1)

## ◆ ADC_CR0_STATERST_Msk

#define ADC_CR0_STATERST_Msk (0x8000UL)

ADC CR0: STATERST (Bitfield-Mask: 0x01)

## ◆ ADC_CR0_STATERST_Pos

#define ADC_CR0_STATERST_Pos (15UL)

ADC CR0: STATERST (Bit 15)

## ◆ ADC_CR1_CT_Msk

#define ADC_CR1_CT_Msk (0x400UL)

ADC CR1: CT (Bitfield-Mask: 0x01)

## ◆ ADC_CR1_CT_Pos

#define ADC_CR1_CT_Pos (10UL)

ADC CR1: CT (Bit 10)

## ◆ ADC_CR1_HTCMP_Msk

#define ADC_CR1_HTCMP_Msk (0x2000UL)

ADC CR1: HTCMP (Bitfield-Mask: 0x01)

## ◆ ADC_CR1_HTCMP_Pos

#define ADC_CR1_HTCMP_Pos (13UL)

ADC CR1: HTCMP (Bit 13)

## ◆ ADC_CR1_LTCMP_Msk

#define ADC_CR1_LTCMP_Msk (0x1000UL)

ADC CR1: LTCMP (Bitfield-Mask: 0x01)

## ◆ ADC_CR1_LTCMP_Pos

#define ADC_CR1_LTCMP_Pos (12UL)

ADC CR1: LTCMP (Bit 12)

## ◆ ADC_CR1_RACC_CLR_Msk

#define ADC_CR1_RACC_CLR_Msk (0x8000UL)

ADC CR1: RACC_CLR (Bitfield-Mask: 0x01)

## ◆ ADC_CR1_RACC_CLR_Pos

#define ADC_CR1_RACC_CLR_Pos (15UL)

ADC CR1: RACC_CLR (Bit 15)

## ◆ ADC_CR1_RACC_EN_Msk

#define ADC_CR1_RACC_EN_Msk (0x800UL)

ADC CR1: RACC_EN (Bitfield-Mask: 0x01)

## ◆ ADC_CR1_RACC_EN_Pos

#define ADC_CR1_RACC_EN_Pos (11UL)

ADC CR1: RACC_EN (Bit 11)

## ◆ ADC_CR1_REGCMP_Msk

#define ADC_CR1_REGCMP_Msk (0x4000UL)

ADC CR1: REGCMP (Bitfield-Mask: 0x01)

## ◆ ADC_CR1_REGCMP_Pos

#define ADC_CR1_REGCMP_Pos (14UL)

ADC CR1: REGCMP (Bit 14)

## ◆ ADC_CR1_TRIGS0_Msk

#define ADC_CR1_TRIGS0_Msk (0x1001FUL)

ADC CR1: TRIGS0 (Bitfield-Mask: 0x1F)

## ◆ ADC_CR1_TRIGS0_Pos

#define ADC_CR1_TRIGS0_Pos (0UL)

ADC CR1: TRIGS0 (Bit 0)

## ◆ ADC_CR1_TRIGS1_Msk

#define ADC_CR1_TRIGS1_Msk (0x203E0UL)

ADC CR1: TRIGS1 (Bitfield-Mask: 0x1F)

## ◆ ADC_CR1_TRIGS1_Pos

#define ADC_CR1_TRIGS1_Pos (5UL)

ADC CR1: TRIGS1 (Bit 5)

## ◆ ADC_CR2_ADCCNT_Msk

#define ADC_CR2_ADCCNT_Msk (0xFF00UL)

ADC CR2: ADCCNT (Bitfield-Mask: 0xFF)

## ◆ ADC_CR2_ADCCNT_Pos

#define ADC_CR2_ADCCNT_Pos (8UL)

ADC CR2: ADCCNT (Bit 8)

## ◆ ADC_CR2_CHEN_Msk

#define ADC_CR2_CHEN_Msk (0xFFUL | (0xFF00000UL))

ADC CR2: CHEN (Bitfield-Mask: 0xFF)

## ◆ ADC_CR2_CHEN_Pos

#define ADC_CR2_CHEN_Pos (0UL)

ADC CR2: CHEN (Bit 0)

## ◆ ADC_CR2_CIRCLE_MODE_Msk

#define ADC_CR2_CIRCLE_MODE_Msk (0x10000UL)

ADC CR2: Circle_Mode (Bitfield-Mask: 0x01)

## ◆ ADC_CR2_CIRCLE_MODE_Pos

#define ADC_CR2_CIRCLE_MODE_Pos (16UL)

ADC CR2: Circle_Mode (Bit 16)

## ◆ ADC_HT_HT_Msk

#define ADC_HT_HT_Msk (0xFFFUL)

ADC HT: HT (Bitfield-Mask: 0xFFF)

## ◆ ADC_HT_HT_Pos

#define ADC_HT_HT_Pos (0UL)

ADC HT: HT (Bit 0)

## ◆ ADC_INTCLR_ADCICLR_Msk

#define ADC_INTCLR_ADCICLR_Msk (0xFFUL | 0xFF000UL)

ADC INTCLR: ADCICLR (Bitfield-Mask: 0xFF)

## ◆ ADC_INTCLR_ADCICLR_Pos

#define ADC_INTCLR_ADCICLR_Pos (0UL)

ADC INTCLR: ADCICLR (Bit 0)

## ◆ ADC_INTCLR_CONT_INTC_Msk

#define ADC_INTCLR_CONT_INTC_Msk (0x800UL)

ADC INTCLR: CONT_INTC (Bitfield-Mask: 0x01)

## ◆ ADC_INTCLR_CONT_INTC_Pos

#define ADC_INTCLR_CONT_INTC_Pos (11UL)

ADC INTCLR: CONT_INTC (Bit 11)

## ◆ ADC_INTCLR_HHT_INTC_Msk

#define ADC_INTCLR_HHT_INTC_Msk (0x200UL)

ADC INTCLR: HHT_INTC (Bitfield-Mask: 0x01)

## ◆ ADC_INTCLR_HHT_INTC_Pos

#define ADC_INTCLR_HHT_INTC_Pos (9UL)

ADC INTCLR: HHT_INTC (Bit 9)

## ◆ ADC_INTCLR_LLT_INTC_Msk

#define ADC_INTCLR_LLT_INTC_Msk (0x100UL)

ADC INTCLR: LLT_INTC (Bitfield-Mask: 0x01)

## ◆ ADC_INTCLR_LLT_INTC_Pos

#define ADC_INTCLR_LLT_INTC_Pos (8UL)

ADC INTCLR: LLT_INTC (Bit 8)

## ◆ ADC_INTCLR_REG_INTC_Msk

#define ADC_INTCLR_REG_INTC_Msk (0x400UL)

ADC INTCLR: REG_INTC (Bitfield-Mask: 0x01)

## ◆ ADC_INTCLR_REG_INTC_Pos

#define ADC_INTCLR_REG_INTC_Pos (10UL)

ADC INTCLR: REG_INTC (Bit 10)

## ◆ ADC_INTEN_ADCXIEN_Msk

#define ADC_INTEN_ADCXIEN_Msk (0xFFUL | 0xFF000UL)

ADC INTEN: ADCXIEN (Bitfield-Mask: 0xFF)

## ◆ ADC_INTEN_ADCXIEN_Pos

#define ADC_INTEN_ADCXIEN_Pos (0UL)

ADC INTEN: ADCXIEN (Bit 0)

## ◆ ADC_INTEN_CONT_IEN_Msk

#define ADC_INTEN_CONT_IEN_Msk (0x800UL)

ADC INTEN: CONT_IEN (Bitfield-Mask: 0x01)

## ◆ ADC_INTEN_CONT_IEN_Pos

#define ADC_INTEN_CONT_IEN_Pos (11UL)

ADC INTEN: CONT_IEN (Bit 11)

## ◆ ADC_INTEN_HHT_IEN_Msk

#define ADC_INTEN_HHT_IEN_Msk (0x200UL)

ADC INTEN: HHT_IEN (Bitfield-Mask: 0x01)

## ◆ ADC_INTEN_HHT_IEN_Pos

#define ADC_INTEN_HHT_IEN_Pos (9UL)

ADC INTEN: HHT_IEN (Bit 9)

## ◆ ADC_INTEN_LLT_IEN_Msk

#define ADC_INTEN_LLT_IEN_Msk (0x100UL)

ADC INTEN: LLT_IEN (Bitfield-Mask: 0x01)

## ◆ ADC_INTEN_LLT_IEN_Pos

#define ADC_INTEN_LLT_IEN_Pos (8UL)

ADC INTEN: LLT_IEN (Bit 8)

## ◆ ADC_INTEN_REG_IEN_Msk

#define ADC_INTEN_REG_IEN_Msk (0x400UL)

ADC INTEN: REG_IEN (Bitfield-Mask: 0x01)

## ◆ ADC_INTEN_REG_IEN_Pos

#define ADC_INTEN_REG_IEN_Pos (10UL)

ADC INTEN: REG_IEN (Bit 10)

## ◆ ADC_LT_LT_Msk

#define ADC_LT_LT_Msk (0xFFFUL)

ADC LT: LT (Bitfield-Mask: 0xFFF)

## ◆ ADC_LT_LT_Pos

#define ADC_LT_LT_Pos (0UL)

ADC LT: LT (Bit 0)

## ◆ ADC_MSKINTSR_ADCMIS_Msk

#define ADC_MSKINTSR_ADCMIS_Msk (0xFFUL | 0xFF000UL)

ADC MSKINTSR: ADCMIS (Bitfield-Mask: 0xFF)

## ◆ ADC_MSKINTSR_ADCMIS_Pos

#define ADC_MSKINTSR_ADCMIS_Pos (0UL)

ADC MSKINTSR: ADCMIS (Bit 0)

## ◆ ADC_MSKINTSR_CONT_MIF_Msk

#define ADC_MSKINTSR_CONT_MIF_Msk (0x800UL)

ADC MSKINTSR: CONT_MIF (Bitfield-Mask: 0x01)

## ◆ ADC_MSKINTSR_CONT_MIF_Pos

#define ADC_MSKINTSR_CONT_MIF_Pos (11UL)

ADC MSKINTSR: CONT_MIF (Bit 11)

## ◆ ADC_MSKINTSR_HHT_MIF_Msk

#define ADC_MSKINTSR_HHT_MIF_Msk (0x200UL)

ADC MSKINTSR: HHT_MIF (Bitfield-Mask: 0x01)

## ◆ ADC_MSKINTSR_HHT_MIF_Pos

#define ADC_MSKINTSR_HHT_MIF_Pos (9UL)

ADC MSKINTSR: HHT_MIF (Bit 9)

## ◆ ADC_MSKINTSR_LLT_MIF_Msk

#define ADC_MSKINTSR_LLT_MIF_Msk (0x100UL)

ADC MSKINTSR: LLT_MIF (Bitfield-Mask: 0x01)

## ◆ ADC_MSKINTSR_LLT_MIF_Pos

#define ADC_MSKINTSR_LLT_MIF_Pos (8UL)

ADC MSKINTSR: LLT_MIF (Bit 8)

## ◆ ADC_MSKINTSR_REG_MIF_Msk

#define ADC_MSKINTSR_REG_MIF_Msk (0x400UL)

ADC MSKINTSR: REG_MIF (Bitfield-Mask: 0x01)

## ◆ ADC_MSKINTSR_REG_MIF_Pos

#define ADC_MSKINTSR_REG_MIF_Pos (10UL)

ADC MSKINTSR: REG_MIF (Bit 10)

## ◆ ADC_RAWINTSR_ADCRIS_Msk

#define ADC_RAWINTSR_ADCRIS_Msk (0xFFUL | 0xFF000UL)

ADC RAWINTSR: ADCRIS (Bitfield-Mask: 0xFF)

## ◆ ADC_RAWINTSR_ADCRIS_Pos

#define ADC_RAWINTSR_ADCRIS_Pos (0UL)

ADC RAWINTSR: ADCRIS (Bit 0)

## ◆ ADC_RAWINTSR_CONT_INTF_Msk

#define ADC_RAWINTSR_CONT_INTF_Msk (0x800UL)

ADC RAWINTSR: CONT_INTF (Bitfield-Mask: 0x01)

## ◆ ADC_RAWINTSR_CONT_INTF_Pos

#define ADC_RAWINTSR_CONT_INTF_Pos (11UL)

ADC RAWINTSR: CONT_INTF (Bit 11)

## ◆ ADC_RAWINTSR_HHT_INTF_Msk

#define ADC_RAWINTSR_HHT_INTF_Msk (0x200UL)

ADC RAWINTSR: HHT_INTF (Bitfield-Mask: 0x01)

## ◆ ADC_RAWINTSR_HHT_INTF_Pos

#define ADC_RAWINTSR_HHT_INTF_Pos (9UL)

ADC RAWINTSR: HHT_INTF (Bit 9)

## ◆ ADC_RAWINTSR_LLT_INTF_Msk

#define ADC_RAWINTSR_LLT_INTF_Msk (0x100UL)

ADC RAWINTSR: LLT_INTF (Bitfield-Mask: 0x01)

## ◆ ADC_RAWINTSR_LLT_INTF_Pos

#define ADC_RAWINTSR_LLT_INTF_Pos (8UL)

ADC RAWINTSR: LLT_INTF (Bit 8)

## ◆ ADC_RAWINTSR_REG_INTF_Msk

#define ADC_RAWINTSR_REG_INTF_Msk (0x400UL)

ADC RAWINTSR: REG_INTF (Bitfield-Mask: 0x01)

## ◆ ADC_RAWINTSR_REG_INTF_Pos

#define ADC_RAWINTSR_REG_INTF_Pos (10UL)

ADC RAWINTSR: REG_INTF (Bit 10)

## ◆ ADC_RESULT0_Result0_Msk

#define ADC_RESULT0_Result0_Msk (0xFFFUL)

ADC RESULT0: Result0 (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT0_Result0_Pos

#define ADC_RESULT0_Result0_Pos (0UL)

ADC RESULT0: Result0 (Bit 0)

## ◆ ADC_RESULT10_Result10_Msk

#define ADC_RESULT10_Result10_Msk (0xFFFUL)

ADC RESULT10: Result10 (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT10_Result10_Pos

#define ADC_RESULT10_Result10_Pos (0UL)

ADC RESULT10: Result10 (Bit 0)

## ◆ ADC_RESULT11_Result11_Msk

#define ADC_RESULT11_Result11_Msk (0xFFFUL)

ADC RESULT11: Result11 (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT11_Result11_Pos

#define ADC_RESULT11_Result11_Pos (0UL)

ADC RESULT11: Result11 (Bit 0)

## ◆ ADC_RESULT12_Result12_Msk

#define ADC_RESULT12_Result12_Msk (0xFFFUL)

ADC RESULT12: Result12 (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT12_Result12_Pos

#define ADC_RESULT12_Result12_Pos (0UL)

ADC RESULT12: Result12 (Bit 0)

## ◆ ADC_RESULT13_Result13_Msk

#define ADC_RESULT13_Result13_Msk (0xFFFUL)

ADC RESULT13: Result13 (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT13_Result13_Pos

#define ADC_RESULT13_Result13_Pos (0UL)

ADC RESULT13: Result13 (Bit 0)

## ◆ ADC_RESULT14_Result14_Msk

#define ADC_RESULT14_Result14_Msk (0xFFFUL)

ADC RESULT14: Result14 (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT14_Result14_Pos

#define ADC_RESULT14_Result14_Pos (0UL)

ADC RESULT14: Result14 (Bit 0)

## ◆ ADC_RESULT15_Result15_Msk

#define ADC_RESULT15_Result15_Msk (0xFFFUL)

ADC RESULT15: Result15 (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT15_Result15_Pos

#define ADC_RESULT15_Result15_Pos (0UL)

ADC RESULT15: Result15 (Bit 0)

## ◆ ADC_RESULT1_Result1_Msk

#define ADC_RESULT1_Result1_Msk (0xFFFFFFUL)

ADC RESULT1: Result1 (Bitfield-Mask: 0xFFFFFF)

## ◆ ADC_RESULT1_Result1_Pos

#define ADC_RESULT1_Result1_Pos (0UL)

ADC RESULT1: Result1 (Bit 0)

## ◆ ADC_RESULT2_Result2_Msk

#define ADC_RESULT2_Result2_Msk (0xFFFUL)

ADC RESULT2: Result2 (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT2_Result2_Pos

#define ADC_RESULT2_Result2_Pos (0UL)

ADC RESULT2: Result2 (Bit 0)

## ◆ ADC_RESULT3_Result3_Msk

#define ADC_RESULT3_Result3_Msk (0xFFFUL)

ADC RESULT3: Result3 (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT3_Result3_Pos

#define ADC_RESULT3_Result3_Pos (0UL)

ADC RESULT3: Result3 (Bit 0)

## ◆ ADC_RESULT4_Result4_Msk

#define ADC_RESULT4_Result4_Msk (0xFFFUL)

ADC RESULT4: Result4 (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT4_Result4_Pos

#define ADC_RESULT4_Result4_Pos (0UL)

ADC RESULT4: Result4 (Bit 0)

## ◆ ADC_RESULT5_Result5_Msk

#define ADC_RESULT5_Result5_Msk (0xFFFUL)

ADC RESULT5: Result5 (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT5_Result5_Pos

#define ADC_RESULT5_Result5_Pos (0UL)

ADC RESULT5: Result5 (Bit 0)

## ◆ ADC_RESULT6_Result6_Msk

#define ADC_RESULT6_Result6_Msk (0xFFFUL)

ADC RESULT6: Result6 (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT6_Result6_Pos

#define ADC_RESULT6_Result6_Pos (0UL)

ADC RESULT6: Result6 (Bit 0)

## ◆ ADC_RESULT7_Result7_Msk

#define ADC_RESULT7_Result7_Msk (0xFFFUL)

ADC RESULT7: Result7 (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT7_Result7_Pos

#define ADC_RESULT7_Result7_Pos (0UL)

ADC RESULT7: Result7 (Bit 0)

## ◆ ADC_RESULT8_Result8_Msk

#define ADC_RESULT8_Result8_Msk (0xFFFUL)

ADC RESULT8: Result8 (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT8_Result8_Pos

#define ADC_RESULT8_Result8_Pos (0UL)

ADC RESULT8: Result8 (Bit 0)

## ◆ ADC_RESULT9_Result9_Msk

#define ADC_RESULT9_Result9_Msk (0xFFFUL)

ADC RESULT9: Result9 (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT9_Result9_Pos

#define ADC_RESULT9_Result9_Pos (0UL)

ADC RESULT9: Result9 (Bit 0)

## ◆ ADC_RESULT_ACC_HT_Msk

#define ADC_RESULT_ACC_HT_Msk (0xFFFUL)

ADC RESULT_ACC: HT (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT_ACC_HT_Pos

#define ADC_RESULT_ACC_HT_Pos (0UL)

ADC RESULT_ACC: HT (Bit 0)

## ◆ ADC_RESULT_RESULT_Msk

#define ADC_RESULT_RESULT_Msk (0xFFFUL)

ADC RESULT: RESULT (Bitfield-Mask: 0xFFF)

## ◆ ADC_RESULT_RESULT_Pos

#define ADC_RESULT_RESULT_Pos (0UL)

ADC RESULT: RESULT (Bit 0)

## ◆ AWK_CR_AWKEN_Msk

#define AWK_CR_AWKEN_Msk (0x10UL)

AWK CR: AWKEN (Bitfield-Mask: 0x01)

## ◆ AWK_CR_AWKEN_Pos

#define AWK_CR_AWKEN_Pos (4UL)

AWK CR: AWKEN (Bit 4)

## ◆ AWK_CR_DIVSEL_Msk

#define AWK_CR_DIVSEL_Msk (0xFUL)

AWK CR: DIVSEL (Bitfield-Mask: 0x0F)

## ◆ AWK_CR_DIVSEL_Pos

#define AWK_CR_DIVSEL_Pos (0UL)

AWK CR: DIVSEL (Bit 0)

## ◆ AWK_CR_HXPRSC_Msk

#define AWK_CR_HXPRSC_Msk (0x7FFF00UL)

AWK CR: HXPRSC (Bitfield-Mask: 0x7FFF)

## ◆ AWK_CR_HXPRSC_Pos

#define AWK_CR_HXPRSC_Pos (8UL)

AWK CR: HXPRSC (Bit 8)

## ◆ AWK_CR_TCLKSEL_Msk

#define AWK_CR_TCLKSEL_Msk (0x60UL)

AWK CR: TCLKSEL (Bitfield-Mask: 0x03)

## ◆ AWK_CR_TCLKSEL_Pos

#define AWK_CR_TCLKSEL_Pos (5UL)

AWK CR: TCLKSEL (Bit 5)

## ◆ AWK_INTCLR_INTCLR_Msk

#define AWK_INTCLR_INTCLR_Msk (0x1UL)

AWK INTCLR: INTCLR (Bitfield-Mask: 0x01)

## ◆ AWK_INTCLR_INTCLR_Pos

#define AWK_INTCLR_INTCLR_Pos (0UL)

AWK INTCLR: INTCLR (Bit 0)

## ◆ AWK_RLOAD_RLDVAL_Msk

#define AWK_RLOAD_RLDVAL_Msk (0xFFUL)

AWK RLOAD: RLDVAL (Bitfield-Mask: 0xFF)

## ◆ AWK_RLOAD_RLDVAL_Pos

#define AWK_RLOAD_RLDVAL_Pos (0UL)

AWK RLOAD: RLDVAL (Bit 0)

## ◆ AWK_SR_AWUF_Msk

#define AWK_SR_AWUF_Msk (0x1UL)

AWK SR: AWUF (Bitfield-Mask: 0x01)

## ◆ AWK_SR_AWUF_Pos

#define AWK_SR_AWUF_Pos (0UL)

AWK SR: AWUF (Bit 0)

## ◆ BASETIM_BGLOAD_BGLOAD_Msk

#define BASETIM_BGLOAD_BGLOAD_Msk (0xFFFFFFFFUL)

BASETIM BGLOAD: BGLOAD (Bitfield-Mask: 0xFFFFFFFF)

## ◆ BASETIM_BGLOAD_BGLOAD_Pos

#define BASETIM_BGLOAD_BGLOAD_Pos (0UL)

BASETIM BGLOAD: BGLOAD (Bit 0)

## ◆ BASETIM_CNT_CNT_Msk

#define BASETIM_CNT_CNT_Msk (0xFFFFFFFFUL)

BASETIM CNT: CNT (Bitfield-Mask: 0xFFFFFFFF)

## ◆ BASETIM_CNT_CNT_Pos

#define BASETIM_CNT_CNT_Pos (0UL)

BASETIM CNT: CNT (Bit 0)

## ◆ BASETIM_CR_ALL_Msk

#define BASETIM_CR_ALL_Msk (0xFFFUL)

BASETIM CR: All valid be mask (Bitfield-Mask: 0xFFF)

## ◆ BASETIM_CR_CT_SEL_Msk

#define BASETIM_CR_CT_SEL_Msk (0x100UL)

BASETIM CR: CT_SEL (Bitfield-Mask: 0x01)

## ◆ BASETIM_CR_CT_SEL_Pos

#define BASETIM_CR_CT_SEL_Pos (8UL)

BASETIM CR: CT_SEL (Bit 8)

## ◆ BASETIM_CR_GATE_EN_Msk

#define BASETIM_CR_GATE_EN_Msk (0x400UL)

BASETIM CR: GATE_EN (Bitfield-Mask: 0x01)

## ◆ BASETIM_CR_GATE_EN_Pos

#define BASETIM_CR_GATE_EN_Pos (10UL)

BASETIM CR: GATE_EN (Bit 10)

## ◆ BASETIM_CR_GATE_P_Msk

#define BASETIM_CR_GATE_P_Msk (0x800UL)

BASETIM CR: GATE_P (Bitfield-Mask: 0x01)

## ◆ BASETIM_CR_GATE_P_Pos

#define BASETIM_CR_GATE_P_Pos (11UL)

BASETIM CR: GATE_P (Bit 11)

## ◆ BASETIM_CR_INTEN_Msk

#define BASETIM_CR_INTEN_Msk (0x20UL)

BASETIM CR: INTEN (Bitfield-Mask: 0x01)

## ◆ BASETIM_CR_INTEN_Pos

#define BASETIM_CR_INTEN_Pos (5UL)

BASETIM CR: INTEN (Bit 5)

## ◆ BASETIM_CR_MODE_Msk

#define BASETIM_CR_MODE_Msk (0x40UL)

BASETIM CR: MODE (Bitfield-Mask: 0x01)

## ◆ BASETIM_CR_MODE_Pos

#define BASETIM_CR_MODE_Pos (6UL)

BASETIM CR: MODE (Bit 6)

## ◆ BASETIM_CR_ONESHOT_Msk

#define BASETIM_CR_ONESHOT_Msk (0x8UL)

BASETIM CR: ONESHOT (Bitfield-Mask: 0x01)

## ◆ BASETIM_CR_ONESHOT_Pos

#define BASETIM_CR_ONESHOT_Pos (3UL)

BASETIM CR: ONESHOT (Bit 3)

## ◆ BASETIM_CR_TMR_PRSC_Msk

#define BASETIM_CR_TMR_PRSC_Msk (0x7UL)

BASETIM CR: TMR_PRSC (Bitfield-Mask: 0x07)

## ◆ BASETIM_CR_TMR_PRSC_Pos

#define BASETIM_CR_TMR_PRSC_Pos (0UL)

BASETIM CR: TMR_PRSC (Bit 0)

## ◆ BASETIM_CR_TMR_SIZE_Msk

#define BASETIM_CR_TMR_SIZE_Msk (0x10UL)

BASETIM CR: TMR_SIZE (Bitfield-Mask: 0x01)

## ◆ BASETIM_CR_TMR_SIZE_Pos

#define BASETIM_CR_TMR_SIZE_Pos (4UL)

BASETIM CR: TMR_SIZE (Bit 4)

## ◆ BASETIM_CR_TOG_EN_Msk

#define BASETIM_CR_TOG_EN_Msk (0x200UL)

BASETIM CR: TOG_EN (Bitfield-Mask: 0x01)

## ◆ BASETIM_CR_TOG_EN_Pos

#define BASETIM_CR_TOG_EN_Pos (9UL)

BASETIM CR: TOG_EN (Bit 9)

## ◆ BASETIM_CR_TR_Msk

#define BASETIM_CR_TR_Msk (0x80UL)

BASETIM CR: TR (Bitfield-Mask: 0x01)

## ◆ BASETIM_CR_TR_Pos

#define BASETIM_CR_TR_Pos (7UL)

BASETIM CR: TR (Bit 7)

## ◆ BASETIM_INTCLR_INTCLR_Msk

#define BASETIM_INTCLR_INTCLR_Msk (0x1UL)

BASETIM INTCLR: INTCLR (Bitfield-Mask: 0x01)

## ◆ BASETIM_INTCLR_INTCLR_Pos

#define BASETIM_INTCLR_INTCLR_Pos (0UL)

BASETIM INTCLR: INTCLR (Bit 0)

## ◆ BASETIM_LOAD_LOAD_Msk

#define BASETIM_LOAD_LOAD_Msk (0xFFFFFFFFUL)

BASETIM LOAD: LOAD (Bitfield-Mask: 0xFFFFFFFF)

## ◆ BASETIM_LOAD_LOAD_Pos

#define BASETIM_LOAD_LOAD_Pos (0UL)

BASETIM LOAD: LOAD (Bit 0)

## ◆ BASETIM_MSKINTSR_TF_Msk

#define BASETIM_MSKINTSR_TF_Msk (0x1UL)

BASETIM MSKINTSR: TF (Bitfield-Mask: 0x01)

## ◆ BASETIM_MSKINTSR_TF_Pos

#define BASETIM_MSKINTSR_TF_Pos (0UL)

BASETIM MSKINTSR: TF (Bit 0)

## ◆ BASETIM_RAWINTSR_RIS_Msk

#define BASETIM_RAWINTSR_RIS_Msk (0x1UL)

BASETIM RAWINTSR: RIS (Bitfield-Mask: 0x01)

## ◆ BASETIM_RAWINTSR_RIS_Pos

#define BASETIM_RAWINTSR_RIS_Pos (0UL)

BASETIM RAWINTSR: RIS (Bit 0)

## ◆ BEEP_CSR_BEEPDIV_Msk

#define BEEP_CSR_BEEPDIV_Msk (0xFFFUL)

BEEP CSR: BEEPDIV (Bitfield-Mask: 0xFFF)

## ◆ BEEP_CSR_BEEPDIV_Pos

#define BEEP_CSR_BEEPDIV_Pos (0UL)

BEEP CSR: BEEPDIV (Bit 0)

## ◆ BEEP_CSR_BEEPEN_Msk

#define BEEP_CSR_BEEPEN_Msk (0x40000UL)

BEEP CSR: BEEPEN (Bitfield-Mask: 0x01)

## ◆ BEEP_CSR_BEEPEN_Pos

#define BEEP_CSR_BEEPEN_Pos (18UL)

BEEP CSR: BEEPEN (Bit 18)

## ◆ BEEP_CSR_BEEPSEL_Msk

#define BEEP_CSR_BEEPSEL_Msk (0x30000UL)

BEEP CSR: BEEPSEL (Bitfield-Mask: 0x03)

## ◆ BEEP_CSR_BEEPSEL_Pos

#define BEEP_CSR_BEEPSEL_Pos (16UL)

BEEP CSR: BEEPSEL (Bit 16)

## ◆ BEEP_CSR_CLKSEL_Msk

#define BEEP_CSR_CLKSEL_Msk (0x300000UL)

BEEP CSR: CLKSEL (Bitfield-Mask: 0x03)

## ◆ BEEP_CSR_CLKSEL_Pos

#define BEEP_CSR_CLKSEL_Pos (20UL)

BEEP CSR: CLKSEL (Bit 20)

## ◆ CLKTRIM_CALCNT_CALCNT_Msk

#define CLKTRIM_CALCNT_CALCNT_Msk (0xFFFFFFFFUL)

CLKTRIM CALCNT: CALCNT (Bitfield-Mask: 0xFFFFFFFF)

## ◆ CLKTRIM_CALCNT_CALCNT_Pos

#define CLKTRIM_CALCNT_CALCNT_Pos (0UL)

CLKTRIM CALCNT: CALCNT (Bit 0)

## ◆ CLKTRIM_CALCON_CALOVCNT_Msk

#define CLKTRIM_CALCON_CALOVCNT_Msk (0xFFFFUL)

CLKTRIM CALCON: CALOVCNT (Bitfield-Mask: 0xFFFF)

## ◆ CLKTRIM_CALCON_CALOVCNT_Pos

#define CLKTRIM_CALCON_CALOVCNT_Pos (0UL)

CLKTRIM CALCON: CALOVCNT (Bit 0)

## ◆ CLKTRIM_CR_CALCLK_SEL_Msk

#define CLKTRIM_CR_CALCLK_SEL_Msk (0x30UL)

CLKTRIM CR: CALCLK_SEL (Bitfield-Mask: 0x03)

## ◆ CLKTRIM_CR_CALCLK_SEL_Pos

#define CLKTRIM_CR_CALCLK_SEL_Pos (4UL)

CLKTRIM CR: CALCLK_SEL (Bit 4)

## ◆ CLKTRIM_CR_CLKEN_Msk

#define CLKTRIM_CR_CLKEN_Msk (0x100UL)

CLKTRIM CR: CLKEN (Bitfield-Mask: 0x01)

## ◆ CLKTRIM_CR_CLKEN_Pos

#define CLKTRIM_CR_CLKEN_Pos (8UL)

CLKTRIM CR: CLKEN (Bit 8)

## ◆ CLKTRIM_CR_IE_Msk

#define CLKTRIM_CR_IE_Msk (0x80UL)

CLKTRIM CR: IE (Bitfield-Mask: 0x01)

## ◆ CLKTRIM_CR_IE_Pos

#define CLKTRIM_CR_IE_Pos (7UL)

CLKTRIM CR: IE (Bit 7)

## ◆ CLKTRIM_CR_MON_EN_Msk

#define CLKTRIM_CR_MON_EN_Msk (0x40UL)

CLKTRIM CR: MON_EN (Bitfield-Mask: 0x01)

## ◆ CLKTRIM_CR_MON_EN_Pos

#define CLKTRIM_CR_MON_EN_Pos (6UL)

CLKTRIM CR: MON_EN (Bit 6)

## ◆ CLKTRIM_CR_REFCLK_SEL_Msk

#define CLKTRIM_CR_REFCLK_SEL_Msk (0xEUL)

CLKTRIM CR: REFCLK_SEL (Bitfield-Mask: 0x07)

## ◆ CLKTRIM_CR_REFCLK_SEL_Pos

#define CLKTRIM_CR_REFCLK_SEL_Pos (1UL)

CLKTRIM CR: REFCLK_SEL (Bit 1)

## ◆ CLKTRIM_CR_TRIM_START_Msk

#define CLKTRIM_CR_TRIM_START_Msk (0x1UL)

CLKTRIM CR: TRIM_START (Bitfield-Mask: 0x01)

## ◆ CLKTRIM_CR_TRIM_START_Pos

#define CLKTRIM_CR_TRIM_START_Pos (0UL)

CLKTRIM CR: TRIM_START (Bit 0)

## ◆ CLKTRIM_ICLR_HSE_FAULT_CLR_Msk

#define CLKTRIM_ICLR_HSE_FAULT_CLR_Msk (0x8UL)

CLKTRIM ICLR: HSE_FAULT_CLR (Bitfield-Mask: 0x01)

## ◆ CLKTRIM_ICLR_HSE_FAULT_CLR_Pos

#define CLKTRIM_ICLR_HSE_FAULT_CLR_Pos (3UL)

CLKTRIM ICLR: HSE_FAULT_CLR (Bit 3)

## ◆ CLKTRIM_ICLR_LSE_FAULT_CLR_Msk

#define CLKTRIM_ICLR_LSE_FAULT_CLR_Msk (0x4UL)

CLKTRIM ICLR: LSE_FAULT_CLR (Bitfield-Mask: 0x01)

## ◆ CLKTRIM_ICLR_LSE_FAULT_CLR_Pos

#define CLKTRIM_ICLR_LSE_FAULT_CLR_Pos (2UL)

CLKTRIM ICLR: LSE_FAULT_CLR (Bit 2)

## ◆ CLKTRIM_IFR_CALCNT_OVF_Msk

#define CLKTRIM_IFR_CALCNT_OVF_Msk (0x2UL)

CLKTRIM IFR: CALCNT_OVF (Bitfield-Mask: 0x01)

## ◆ CLKTRIM_IFR_CALCNT_OVF_Pos

#define CLKTRIM_IFR_CALCNT_OVF_Pos (1UL)

CLKTRIM IFR: CALCNT_OVF (Bit 1)

## ◆ CLKTRIM_IFR_HSE_FAULT_Msk

#define CLKTRIM_IFR_HSE_FAULT_Msk (0x8UL)

CLKTRIM IFR: HSE_FAULT (Bitfield-Mask: 0x01)

## ◆ CLKTRIM_IFR_HSE_FAULT_Pos

#define CLKTRIM_IFR_HSE_FAULT_Pos (3UL)

CLKTRIM IFR: HSE_FAULT (Bit 3)

## ◆ CLKTRIM_IFR_LSE_FAULT_Msk

#define CLKTRIM_IFR_LSE_FAULT_Msk (0x4UL)

CLKTRIM IFR: LSE_FAULT (Bitfield-Mask: 0x01)

## ◆ CLKTRIM_IFR_LSE_FAULT_Pos

#define CLKTRIM_IFR_LSE_FAULT_Pos (2UL)

CLKTRIM IFR: LSE_FAULT (Bit 2)

## ◆ CLKTRIM_IFR_STOP_Msk

#define CLKTRIM_IFR_STOP_Msk (0x1UL)

CLKTRIM IFR: STOP (Bitfield-Mask: 0x01)

## ◆ CLKTRIM_IFR_STOP_Pos

#define CLKTRIM_IFR_STOP_Pos (0UL)

CLKTRIM IFR: STOP (Bit 0)

## ◆ CLKTRIM_REFCNT_REFCNT_Msk

#define CLKTRIM_REFCNT_REFCNT_Msk (0xFFFFFFFFUL)

CLKTRIM REFCNT: REFCNT (Bitfield-Mask: 0xFFFFFFFF)

## ◆ CLKTRIM_REFCNT_REFCNT_Pos

#define CLKTRIM_REFCNT_REFCNT_Pos (0UL)

CLKTRIM REFCNT: REFCNT (Bit 0)

## ◆ CLKTRIM_REFCON_RCNTVAL_Msk

#define CLKTRIM_REFCON_RCNTVAL_Msk (0xFFFFFFFFUL)

CLKTRIM REFCON: RCNTVAL (Bitfield-Mask: 0xFFFFFFFF)

## ◆ CLKTRIM_REFCON_RCNTVAL_Pos

#define CLKTRIM_REFCON_RCNTVAL_Pos (0UL)

CLKTRIM REFCON: RCNTVAL (Bit 0)

## ◆ CRC_RESULT_FLAG_Msk

#define CRC_RESULT_FLAG_Msk (0x10000UL)

CRC RESULT: FLAG (Bitfield-Mask: 0x01)

## ◆ CRC_RESULT_FLAG_Pos

#define CRC_RESULT_FLAG_Pos (16UL)

CRC RESULT: FLAG (Bit 16)

## ◆ CRC_RESULT_RESULT_Msk

#define CRC_RESULT_RESULT_Msk (0xFFFFUL)

CRC RESULT: RESULT (Bitfield-Mask: 0xFFFF)

## ◆ CRC_RESULT_RESULT_Pos

#define CRC_RESULT_RESULT_Pos (0UL)

CRC RESULT: RESULT (Bit 0)

## ◆ DBG_APBFZ_BEEPDBGSTOP_Msk

#define DBG_APBFZ_BEEPDBGSTOP_Msk (0x1UL)

DBG APBFZ: BEEPDBGSTOP (Bitfield-Mask: 0x01)

## ◆ DBG_APBFZ_BEEPDBGSTOP_Pos

#define DBG_APBFZ_BEEPDBGSTOP_Pos (8UL)

DBG APBFZ: BEEPDBGSTOP (Bit 8)

## ◆ DBG_APBFZ_IWDGDBGSTOP_Msk

#define DBG_APBFZ_IWDGDBGSTOP_Msk (0x1UL)

DBG APBFZ: IWDGDBGSTOP (Bitfield-Mask: 0x01)

## ◆ DBG_APBFZ_IWDGDBGSTOP_Pos

#define DBG_APBFZ_IWDGDBGSTOP_Pos (9UL)

DBG APBFZ: IWDGDBGSTOP (Bit 9)

## ◆ DBG_APBFZ_KEY_Msk

#define DBG_APBFZ_KEY_Msk (0xFFUL)

DBG APBFZ: KEY (Bitfield-Mask: 0xFF)

## ◆ DBG_APBFZ_KEY_Pos

#define DBG_APBFZ_KEY_Pos (16UL)

DBG APBFZ: KEY (Bit 16)

## ◆ DBG_APBFZ_LPTIMDBGSTOP_Msk

#define DBG_APBFZ_LPTIMDBGSTOP_Msk (0x1UL)

DBG APBFZ: LPTIMDBGSTOP (Bitfield-Mask: 0x01)

## ◆ DBG_APBFZ_LPTIMDBGSTOP_Pos

#define DBG_APBFZ_LPTIMDBGSTOP_Pos (2UL)

DBG APBFZ: LPTIMDBGSTOP (Bit 2)

## ◆ DBG_APBFZ_PCADBGSTOP_Msk

#define DBG_APBFZ_PCADBGSTOP_Msk (0x1UL)

DBG APBFZ: PCADBGSTOP (Bitfield-Mask: 0x01)

## ◆ DBG_APBFZ_PCADBGSTOP_Pos

#define DBG_APBFZ_PCADBGSTOP_Pos (4UL)

DBG APBFZ: PCADBGSTOP (Bit 4)

## ◆ DBG_APBFZ_RTCDBGSTOP_Msk

#define DBG_APBFZ_RTCDBGSTOP_Msk (0x1UL)

DBG APBFZ: RTCDBGSTOP (Bitfield-Mask: 0x01)

## ◆ DBG_APBFZ_RTCDBGSTOP_Pos

#define DBG_APBFZ_RTCDBGSTOP_Pos (6UL)

DBG APBFZ: RTCDBGSTOP (Bit 6)

## ◆ DBG_APBFZ_TIM10DBGSTOP_Msk

#define DBG_APBFZ_TIM10DBGSTOP_Msk (0x1UL)

DBG APBFZ: TIM10DBGSTOP (Bitfield-Mask: 0x01)

## ◆ DBG_APBFZ_TIM10DBGSTOP_Pos

#define DBG_APBFZ_TIM10DBGSTOP_Pos (0UL)

DBG APBFZ: TIM10DBGSTOP (Bit 0)

## ◆ DBG_APBFZ_TIM11DBGSTOP_Msk

#define DBG_APBFZ_TIM11DBGSTOP_Msk (0x1UL)

DBG APBFZ: TIM11DBGSTOP (Bitfield-Mask: 0x01)

## ◆ DBG_APBFZ_TIM11DBGSTOP_Pos

#define DBG_APBFZ_TIM11DBGSTOP_Pos (1UL)

DBG APBFZ: TIM11DBGSTOP (Bit 1)

## ◆ DBG_APBFZ_TIM1DBGSTOP_Msk

#define DBG_APBFZ_TIM1DBGSTOP_Msk (0x1UL)

DBG APBFZ: TIM1DBGSTOP (Bitfield-Mask: 0x01)

## ◆ DBG_APBFZ_TIM1DBGSTOP_Pos

#define DBG_APBFZ_TIM1DBGSTOP_Pos (5UL)

DBG APBFZ: TIM1DBGSTOP (Bit 5)

## ◆ DBG_APBFZ_TIM2DBGSTOP_Msk

#define DBG_APBFZ_TIM2DBGSTOP_Msk (0x1UL)

DBG APBFZ: TIM2DBGSTOP (Bitfield-Mask: 0x01)

## ◆ DBG_APBFZ_TIM2DBGSTOP_Pos

#define DBG_APBFZ_TIM2DBGSTOP_Pos (11UL)

DBG APBFZ: TIM2DBGSTOP (Bit 11)

## ◆ DBG_APBFZ_WWDGDBGSTOP_Msk

#define DBG_APBFZ_WWDGDBGSTOP_Msk (0x1UL)

DBG APBFZ: WWDGDBGSTOP (Bitfield-Mask: 0x01)

## ◆ DBG_APBFZ_WWDGDBGSTOP_Pos

#define DBG_APBFZ_WWDGDBGSTOP_Pos (10UL)

DBG APBFZ: WWDGDBGSTOP (Bit 10)

## ◆ FLASH_BYPASS_BYPASSSEQ_Msk

#define FLASH_BYPASS_BYPASSSEQ_Msk (0xFFFFUL)

FLASH BYPASS: BYPASSSEQ (Bitfield-Mask: 0xFFFF)

## ◆ FLASH_BYPASS_BYPASSSEQ_Pos

#define FLASH_BYPASS_BYPASSSEQ_Pos (0UL)

FLASH BYPASS: BYPASSSEQ (Bit 0)

## ◆ FLASH_CR_BUSY_Msk

#define FLASH_CR_BUSY_Msk (0x4UL)

FLASH CR: BUSY (Bitfield-Mask: 0x01)

## ◆ FLASH_CR_BUSY_Pos

#define FLASH_CR_BUSY_Pos (2UL)

FLASH CR: BUSY (Bit 2)

## ◆ FLASH_CR_IE_Msk

#define FLASH_CR_IE_Msk (0x18UL)

FLASH CR: IE (Bitfield-Mask: 0x03)

## ◆ FLASH_CR_IE_Pos

#define FLASH_CR_IE_Pos (3UL)

FLASH CR: IE (Bit 3)

## ◆ FLASH_CR_OP_Msk

#define FLASH_CR_OP_Msk (0x3UL)

FLASH CR: OP (Bitfield-Mask: 0x03)

## ◆ FLASH_CR_OP_Pos

#define FLASH_CR_OP_Pos (0UL)

FLASH CR: OP (Bit 0)

## ◆ FLASH_ICLR_ICLR0_Msk

#define FLASH_ICLR_ICLR0_Msk (0x1UL)

FLASH ICLR: ICLR0 (Bitfield-Mask: 0x01)

## ◆ FLASH_ICLR_ICLR0_Pos

#define FLASH_ICLR_ICLR0_Pos (0UL)

FLASH ICLR: ICLR0 (Bit 0)

## ◆ FLASH_ICLR_ICLR1_Msk

#define FLASH_ICLR_ICLR1_Msk (0x2UL)

FLASH ICLR: ICLR1 (Bitfield-Mask: 0x01)

## ◆ FLASH_ICLR_ICLR1_Pos

#define FLASH_ICLR_ICLR1_Pos (1UL)

FLASH ICLR: ICLR1 (Bit 1)

## ◆ FLASH_IFR_IF0_Msk

#define FLASH_IFR_IF0_Msk (0x1UL)

FLASH IFR: IF0 (Bitfield-Mask: 0x01)

## ◆ FLASH_IFR_IF0_Pos

#define FLASH_IFR_IF0_Pos (0UL)

FLASH IFR: IF0 (Bit 0)

## ◆ FLASH_IFR_IF1_Msk

#define FLASH_IFR_IF1_Msk (0x2UL)

FLASH IFR: IF1 (Bitfield-Mask: 0x01)

## ◆ FLASH_IFR_IF1_Pos

#define FLASH_IFR_IF1_Pos (1UL)

FLASH IFR: IF1 (Bit 1)

## ◆ FLASH_ISPCON_ISP_CON_Msk

#define FLASH_ISPCON_ISP_CON_Msk (0x1UL)

FLASH ISPCON: ISP_CON (Bitfield-Mask: 0x01)

## ◆ FLASH_ISPCON_ISP_CON_Pos

#define FLASH_ISPCON_ISP_CON_Pos (0UL)

FLASH ISPCON: ISP_CON (Bit 0)

## ◆ FLASH_MEMORY_BASE

#define FLASH_MEMORY_BASE ((uint32_t)0x00000000UL)

FLASH base address in the alias region

## ◆ FLASH_SLOCK0_SLOCK0_0_Msk

#define FLASH_SLOCK0_SLOCK0_0_Msk (0x1UL)

FLASH SLOCK0: SLOCK0_0 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_0_Pos

#define FLASH_SLOCK0_SLOCK0_0_Pos (0UL)

FLASH SLOCK0: SLOCK0_0 (Bit 0)

## ◆ FLASH_SLOCK0_SLOCK0_10_Msk

#define FLASH_SLOCK0_SLOCK0_10_Msk (0x400UL)

FLASH SLOCK0: SLOCK0_10 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_10_Pos

#define FLASH_SLOCK0_SLOCK0_10_Pos (10UL)

FLASH SLOCK0: SLOCK0_10 (Bit 10)

## ◆ FLASH_SLOCK0_SLOCK0_11_Msk

#define FLASH_SLOCK0_SLOCK0_11_Msk (0x800UL)

FLASH SLOCK0: SLOCK0_11 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_11_Pos

#define FLASH_SLOCK0_SLOCK0_11_Pos (11UL)

FLASH SLOCK0: SLOCK0_11 (Bit 11)

## ◆ FLASH_SLOCK0_SLOCK0_12_Msk

#define FLASH_SLOCK0_SLOCK0_12_Msk (0x1000UL)

FLASH SLOCK0: SLOCK0_12 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_12_Pos

#define FLASH_SLOCK0_SLOCK0_12_Pos (12UL)

FLASH SLOCK0: SLOCK0_12 (Bit 12)

## ◆ FLASH_SLOCK0_SLOCK0_13_Msk

#define FLASH_SLOCK0_SLOCK0_13_Msk (0x2000UL)

FLASH SLOCK0: SLOCK0_13 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_13_Pos

#define FLASH_SLOCK0_SLOCK0_13_Pos (13UL)

FLASH SLOCK0: SLOCK0_13 (Bit 13)

## ◆ FLASH_SLOCK0_SLOCK0_14_Msk

#define FLASH_SLOCK0_SLOCK0_14_Msk (0x4000UL)

FLASH SLOCK0: SLOCK0_14 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_14_Pos

#define FLASH_SLOCK0_SLOCK0_14_Pos (14UL)

FLASH SLOCK0: SLOCK0_14 (Bit 14)

## ◆ FLASH_SLOCK0_SLOCK0_15_Msk

#define FLASH_SLOCK0_SLOCK0_15_Msk (0x8000UL)

FLASH SLOCK0: SLOCK0_15 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_15_Pos

#define FLASH_SLOCK0_SLOCK0_15_Pos (15UL)

FLASH SLOCK0: SLOCK0_15 (Bit 15)

## ◆ FLASH_SLOCK0_SLOCK0_16_Msk

#define FLASH_SLOCK0_SLOCK0_16_Msk (0x10000UL)

FLASH SLOCK0: SLOCK0_16 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_16_Pos

#define FLASH_SLOCK0_SLOCK0_16_Pos (16UL)

FLASH SLOCK0: SLOCK0_16 (Bit 16)

## ◆ FLASH_SLOCK0_SLOCK0_17_Msk

#define FLASH_SLOCK0_SLOCK0_17_Msk (0x20000UL)

FLASH SLOCK0: SLOCK0_17 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_17_Pos

#define FLASH_SLOCK0_SLOCK0_17_Pos (17UL)

FLASH SLOCK0: SLOCK0_17 (Bit 17)

## ◆ FLASH_SLOCK0_SLOCK0_18_Msk

#define FLASH_SLOCK0_SLOCK0_18_Msk (0x40000UL)

FLASH SLOCK0: SLOCK0_18 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_18_Pos

#define FLASH_SLOCK0_SLOCK0_18_Pos (18UL)

FLASH SLOCK0: SLOCK0_18 (Bit 18)

## ◆ FLASH_SLOCK0_SLOCK0_19_Msk

#define FLASH_SLOCK0_SLOCK0_19_Msk (0x80000UL)

FLASH SLOCK0: SLOCK0_19 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_19_Pos

#define FLASH_SLOCK0_SLOCK0_19_Pos (19UL)

FLASH SLOCK0: SLOCK0_19 (Bit 19)

## ◆ FLASH_SLOCK0_SLOCK0_1_Msk

#define FLASH_SLOCK0_SLOCK0_1_Msk (0x2UL)

FLASH SLOCK0: SLOCK0_1 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_1_Pos

#define FLASH_SLOCK0_SLOCK0_1_Pos (1UL)

FLASH SLOCK0: SLOCK0_1 (Bit 1)

## ◆ FLASH_SLOCK0_SLOCK0_20_Msk

#define FLASH_SLOCK0_SLOCK0_20_Msk (0x100000UL)

FLASH SLOCK0: SLOCK0_20 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_20_Pos

#define FLASH_SLOCK0_SLOCK0_20_Pos (20UL)

FLASH SLOCK0: SLOCK0_20 (Bit 20)

## ◆ FLASH_SLOCK0_SLOCK0_21_Msk

#define FLASH_SLOCK0_SLOCK0_21_Msk (0x200000UL)

FLASH SLOCK0: SLOCK0_21 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_21_Pos

#define FLASH_SLOCK0_SLOCK0_21_Pos (21UL)

FLASH SLOCK0: SLOCK0_21 (Bit 21)

## ◆ FLASH_SLOCK0_SLOCK0_22_Msk

#define FLASH_SLOCK0_SLOCK0_22_Msk (0x400000UL)

FLASH SLOCK0: SLOCK0_22 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_22_Pos

#define FLASH_SLOCK0_SLOCK0_22_Pos (22UL)

FLASH SLOCK0: SLOCK0_22 (Bit 22)

## ◆ FLASH_SLOCK0_SLOCK0_23_Msk

#define FLASH_SLOCK0_SLOCK0_23_Msk (0x800000UL)

FLASH SLOCK0: SLOCK0_23 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_23_Pos

#define FLASH_SLOCK0_SLOCK0_23_Pos (23UL)

FLASH SLOCK0: SLOCK0_23 (Bit 23)

## ◆ FLASH_SLOCK0_SLOCK0_24_Msk

#define FLASH_SLOCK0_SLOCK0_24_Msk (0x1000000UL)

FLASH SLOCK0: SLOCK0_24 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_24_Pos

#define FLASH_SLOCK0_SLOCK0_24_Pos (24UL)

FLASH SLOCK0: SLOCK0_24 (Bit 24)

## ◆ FLASH_SLOCK0_SLOCK0_25_Msk

#define FLASH_SLOCK0_SLOCK0_25_Msk (0x2000000UL)

FLASH SLOCK0: SLOCK0_25 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_25_Pos

#define FLASH_SLOCK0_SLOCK0_25_Pos (25UL)

FLASH SLOCK0: SLOCK0_25 (Bit 25)

## ◆ FLASH_SLOCK0_SLOCK0_26_Msk

#define FLASH_SLOCK0_SLOCK0_26_Msk (0x4000000UL)

FLASH SLOCK0: SLOCK0_26 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_26_Pos

#define FLASH_SLOCK0_SLOCK0_26_Pos (26UL)

FLASH SLOCK0: SLOCK0_26 (Bit 26)

## ◆ FLASH_SLOCK0_SLOCK0_27_Msk

#define FLASH_SLOCK0_SLOCK0_27_Msk (0x8000000UL)

FLASH SLOCK0: SLOCK0_27 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_27_Pos

#define FLASH_SLOCK0_SLOCK0_27_Pos (27UL)

FLASH SLOCK0: SLOCK0_27 (Bit 27)

## ◆ FLASH_SLOCK0_SLOCK0_28_Msk

#define FLASH_SLOCK0_SLOCK0_28_Msk (0x10000000UL)

FLASH SLOCK0: SLOCK0_28 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_28_Pos

#define FLASH_SLOCK0_SLOCK0_28_Pos (28UL)

FLASH SLOCK0: SLOCK0_28 (Bit 28)

## ◆ FLASH_SLOCK0_SLOCK0_29_Msk

#define FLASH_SLOCK0_SLOCK0_29_Msk (0x20000000UL)

FLASH SLOCK0: SLOCK0_29 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_29_Pos

#define FLASH_SLOCK0_SLOCK0_29_Pos (29UL)

FLASH SLOCK0: SLOCK0_29 (Bit 29)

## ◆ FLASH_SLOCK0_SLOCK0_2_Msk

#define FLASH_SLOCK0_SLOCK0_2_Msk (0x4UL)

FLASH SLOCK0: SLOCK0_2 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_2_Pos

#define FLASH_SLOCK0_SLOCK0_2_Pos (2UL)

FLASH SLOCK0: SLOCK0_2 (Bit 2)

## ◆ FLASH_SLOCK0_SLOCK0_30_Msk

#define FLASH_SLOCK0_SLOCK0_30_Msk (0x40000000UL)

FLASH SLOCK0: SLOCK0_30 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_30_Pos

#define FLASH_SLOCK0_SLOCK0_30_Pos (30UL)

FLASH SLOCK0: SLOCK0_30 (Bit 30)

## ◆ FLASH_SLOCK0_SLOCK0_31_Msk

#define FLASH_SLOCK0_SLOCK0_31_Msk (0x80000000UL)

FLASH SLOCK0: SLOCK0_31 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_31_Pos

#define FLASH_SLOCK0_SLOCK0_31_Pos (31UL)

FLASH SLOCK0: SLOCK0_31 (Bit 31)

## ◆ FLASH_SLOCK0_SLOCK0_3_Msk

#define FLASH_SLOCK0_SLOCK0_3_Msk (0x8UL)

FLASH SLOCK0: SLOCK0_3 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_3_Pos

#define FLASH_SLOCK0_SLOCK0_3_Pos (3UL)

FLASH SLOCK0: SLOCK0_3 (Bit 3)

## ◆ FLASH_SLOCK0_SLOCK0_4_Msk

#define FLASH_SLOCK0_SLOCK0_4_Msk (0x10UL)

FLASH SLOCK0: SLOCK0_4 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_4_Pos

#define FLASH_SLOCK0_SLOCK0_4_Pos (4UL)

FLASH SLOCK0: SLOCK0_4 (Bit 4)

## ◆ FLASH_SLOCK0_SLOCK0_5_Msk

#define FLASH_SLOCK0_SLOCK0_5_Msk (0x20UL)

FLASH SLOCK0: SLOCK0_5 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_5_Pos

#define FLASH_SLOCK0_SLOCK0_5_Pos (5UL)

FLASH SLOCK0: SLOCK0_5 (Bit 5)

## ◆ FLASH_SLOCK0_SLOCK0_6_Msk

#define FLASH_SLOCK0_SLOCK0_6_Msk (0x40UL)

FLASH SLOCK0: SLOCK0_6 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_6_Pos

#define FLASH_SLOCK0_SLOCK0_6_Pos (6UL)

FLASH SLOCK0: SLOCK0_6 (Bit 6)

## ◆ FLASH_SLOCK0_SLOCK0_7_Msk

#define FLASH_SLOCK0_SLOCK0_7_Msk (0x80UL)

FLASH SLOCK0: SLOCK0_7 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_7_Pos

#define FLASH_SLOCK0_SLOCK0_7_Pos (7UL)

FLASH SLOCK0: SLOCK0_7 (Bit 7)

## ◆ FLASH_SLOCK0_SLOCK0_8_Msk

#define FLASH_SLOCK0_SLOCK0_8_Msk (0x100UL)

FLASH SLOCK0: SLOCK0_8 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_8_Pos

#define FLASH_SLOCK0_SLOCK0_8_Pos (8UL)

FLASH SLOCK0: SLOCK0_8 (Bit 8)

## ◆ FLASH_SLOCK0_SLOCK0_9_Msk

#define FLASH_SLOCK0_SLOCK0_9_Msk (0x200UL)

FLASH SLOCK0: SLOCK0_9 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK0_SLOCK0_9_Pos

#define FLASH_SLOCK0_SLOCK0_9_Pos (9UL)

FLASH SLOCK0: SLOCK0_9 (Bit 9)

## ◆ FLASH_SLOCK1_SLOCK1_0_Msk

#define FLASH_SLOCK1_SLOCK1_0_Msk (0x1UL)

FLASH SLOCK1: SLOCK1_0 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_0_Pos

#define FLASH_SLOCK1_SLOCK1_0_Pos (0UL)

FLASH SLOCK1: SLOCK1_0 (Bit 0)

## ◆ FLASH_SLOCK1_SLOCK1_10_Msk

#define FLASH_SLOCK1_SLOCK1_10_Msk (0x400UL)

FLASH SLOCK1: SLOCK1_10 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_10_Pos

#define FLASH_SLOCK1_SLOCK1_10_Pos (10UL)

FLASH SLOCK1: SLOCK1_10 (Bit 10)

## ◆ FLASH_SLOCK1_SLOCK1_11_Msk

#define FLASH_SLOCK1_SLOCK1_11_Msk (0x800UL)

FLASH SLOCK1: SLOCK1_11 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_11_Pos

#define FLASH_SLOCK1_SLOCK1_11_Pos (11UL)

FLASH SLOCK1: SLOCK1_11 (Bit 11)

## ◆ FLASH_SLOCK1_SLOCK1_12_Msk

#define FLASH_SLOCK1_SLOCK1_12_Msk (0x1000UL)

FLASH SLOCK1: SLOCK1_12 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_12_Pos

#define FLASH_SLOCK1_SLOCK1_12_Pos (12UL)

FLASH SLOCK1: SLOCK1_12 (Bit 12)

## ◆ FLASH_SLOCK1_SLOCK1_13_Msk

#define FLASH_SLOCK1_SLOCK1_13_Msk (0x2000UL)

FLASH SLOCK1: SLOCK1_13 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_13_Pos

#define FLASH_SLOCK1_SLOCK1_13_Pos (13UL)

FLASH SLOCK1: SLOCK1_13 (Bit 13)

## ◆ FLASH_SLOCK1_SLOCK1_14_Msk

#define FLASH_SLOCK1_SLOCK1_14_Msk (0x4000UL)

FLASH SLOCK1: SLOCK1_14 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_14_Pos

#define FLASH_SLOCK1_SLOCK1_14_Pos (14UL)

FLASH SLOCK1: SLOCK1_14 (Bit 14)

## ◆ FLASH_SLOCK1_SLOCK1_15_Msk

#define FLASH_SLOCK1_SLOCK1_15_Msk (0x8000UL)

FLASH SLOCK1: SLOCK1_15 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_15_Pos

#define FLASH_SLOCK1_SLOCK1_15_Pos (15UL)

FLASH SLOCK1: SLOCK1_15 (Bit 15)

## ◆ FLASH_SLOCK1_SLOCK1_16_Msk

#define FLASH_SLOCK1_SLOCK1_16_Msk (0x10000UL)

FLASH SLOCK1: SLOCK1_16 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_16_Pos

#define FLASH_SLOCK1_SLOCK1_16_Pos (16UL)

FLASH SLOCK1: SLOCK1_16 (Bit 16)

## ◆ FLASH_SLOCK1_SLOCK1_17_Msk

#define FLASH_SLOCK1_SLOCK1_17_Msk (0x20000UL)

FLASH SLOCK1: SLOCK1_17 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_17_Pos

#define FLASH_SLOCK1_SLOCK1_17_Pos (17UL)

FLASH SLOCK1: SLOCK1_17 (Bit 17)

## ◆ FLASH_SLOCK1_SLOCK1_18_Msk

#define FLASH_SLOCK1_SLOCK1_18_Msk (0x40000UL)

FLASH SLOCK1: SLOCK1_18 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_18_Pos

#define FLASH_SLOCK1_SLOCK1_18_Pos (18UL)

FLASH SLOCK1: SLOCK1_18 (Bit 18)

## ◆ FLASH_SLOCK1_SLOCK1_19_Msk

#define FLASH_SLOCK1_SLOCK1_19_Msk (0x80000UL)

FLASH SLOCK1: SLOCK1_19 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_19_Pos

#define FLASH_SLOCK1_SLOCK1_19_Pos (19UL)

FLASH SLOCK1: SLOCK1_19 (Bit 19)

## ◆ FLASH_SLOCK1_SLOCK1_1_Msk

#define FLASH_SLOCK1_SLOCK1_1_Msk (0x2UL)

FLASH SLOCK1: SLOCK1_1 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_1_Pos

#define FLASH_SLOCK1_SLOCK1_1_Pos (1UL)

FLASH SLOCK1: SLOCK1_1 (Bit 1)

## ◆ FLASH_SLOCK1_SLOCK1_20_Msk

#define FLASH_SLOCK1_SLOCK1_20_Msk (0x100000UL)

FLASH SLOCK1: SLOCK1_20 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_20_Pos

#define FLASH_SLOCK1_SLOCK1_20_Pos (20UL)

FLASH SLOCK1: SLOCK1_20 (Bit 20)

## ◆ FLASH_SLOCK1_SLOCK1_21_Msk

#define FLASH_SLOCK1_SLOCK1_21_Msk (0x200000UL)

FLASH SLOCK1: SLOCK1_21 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_21_Pos

#define FLASH_SLOCK1_SLOCK1_21_Pos (21UL)

FLASH SLOCK1: SLOCK1_21 (Bit 21)

## ◆ FLASH_SLOCK1_SLOCK1_22_Msk

#define FLASH_SLOCK1_SLOCK1_22_Msk (0x400000UL)

FLASH SLOCK1: SLOCK1_22 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_22_Pos

#define FLASH_SLOCK1_SLOCK1_22_Pos (22UL)

FLASH SLOCK1: SLOCK1_22 (Bit 22)

## ◆ FLASH_SLOCK1_SLOCK1_23_Msk

#define FLASH_SLOCK1_SLOCK1_23_Msk (0x800000UL)

FLASH SLOCK1: SLOCK1_23 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_23_Pos

#define FLASH_SLOCK1_SLOCK1_23_Pos (23UL)

FLASH SLOCK1: SLOCK1_23 (Bit 23)

## ◆ FLASH_SLOCK1_SLOCK1_24_Msk

#define FLASH_SLOCK1_SLOCK1_24_Msk (0x1000000UL)

FLASH SLOCK1: SLOCK1_24 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_24_Pos

#define FLASH_SLOCK1_SLOCK1_24_Pos (24UL)

FLASH SLOCK1: SLOCK1_24 (Bit 24)

## ◆ FLASH_SLOCK1_SLOCK1_25_Msk

#define FLASH_SLOCK1_SLOCK1_25_Msk (0x2000000UL)

FLASH SLOCK1: SLOCK1_25 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_25_Pos

#define FLASH_SLOCK1_SLOCK1_25_Pos (25UL)

FLASH SLOCK1: SLOCK1_25 (Bit 25)

## ◆ FLASH_SLOCK1_SLOCK1_26_Msk

#define FLASH_SLOCK1_SLOCK1_26_Msk (0x4000000UL)

FLASH SLOCK1: SLOCK1_26 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_26_Pos

#define FLASH_SLOCK1_SLOCK1_26_Pos (26UL)

FLASH SLOCK1: SLOCK1_26 (Bit 26)

## ◆ FLASH_SLOCK1_SLOCK1_27_Msk

#define FLASH_SLOCK1_SLOCK1_27_Msk (0x8000000UL)

FLASH SLOCK1: SLOCK1_27 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_27_Pos

#define FLASH_SLOCK1_SLOCK1_27_Pos (27UL)

FLASH SLOCK1: SLOCK1_27 (Bit 27)

## ◆ FLASH_SLOCK1_SLOCK1_28_Msk

#define FLASH_SLOCK1_SLOCK1_28_Msk (0x10000000UL)

FLASH SLOCK1: SLOCK1_28 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_28_Pos

#define FLASH_SLOCK1_SLOCK1_28_Pos (28UL)

FLASH SLOCK1: SLOCK1_28 (Bit 28)

## ◆ FLASH_SLOCK1_SLOCK1_29_Msk

#define FLASH_SLOCK1_SLOCK1_29_Msk (0x20000000UL)

FLASH SLOCK1: SLOCK1_29 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_29_Pos

#define FLASH_SLOCK1_SLOCK1_29_Pos (29UL)

FLASH SLOCK1: SLOCK1_29 (Bit 29)

## ◆ FLASH_SLOCK1_SLOCK1_2_Msk

#define FLASH_SLOCK1_SLOCK1_2_Msk (0x4UL)

FLASH SLOCK1: SLOCK1_2 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_2_Pos

#define FLASH_SLOCK1_SLOCK1_2_Pos (2UL)

FLASH SLOCK1: SLOCK1_2 (Bit 2)

## ◆ FLASH_SLOCK1_SLOCK1_30_Msk

#define FLASH_SLOCK1_SLOCK1_30_Msk (0x40000000UL)

FLASH SLOCK1: SLOCK1_30 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_30_Pos

#define FLASH_SLOCK1_SLOCK1_30_Pos (30UL)

FLASH SLOCK1: SLOCK1_30 (Bit 30)

## ◆ FLASH_SLOCK1_SLOCK1_31_Msk

#define FLASH_SLOCK1_SLOCK1_31_Msk (0x80000000UL)

FLASH SLOCK1: SLOCK1_31 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_31_Pos

#define FLASH_SLOCK1_SLOCK1_31_Pos (31UL)

FLASH SLOCK1: SLOCK1_31 (Bit 31)

## ◆ FLASH_SLOCK1_SLOCK1_3_Msk

#define FLASH_SLOCK1_SLOCK1_3_Msk (0x8UL)

FLASH SLOCK1: SLOCK1_3 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_3_Pos

#define FLASH_SLOCK1_SLOCK1_3_Pos (3UL)

FLASH SLOCK1: SLOCK1_3 (Bit 3)

## ◆ FLASH_SLOCK1_SLOCK1_4_Msk

#define FLASH_SLOCK1_SLOCK1_4_Msk (0x10UL)

FLASH SLOCK1: SLOCK1_4 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_4_Pos

#define FLASH_SLOCK1_SLOCK1_4_Pos (4UL)

FLASH SLOCK1: SLOCK1_4 (Bit 4)

## ◆ FLASH_SLOCK1_SLOCK1_5_Msk

#define FLASH_SLOCK1_SLOCK1_5_Msk (0x20UL)

FLASH SLOCK1: SLOCK1_5 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_5_Pos

#define FLASH_SLOCK1_SLOCK1_5_Pos (5UL)

FLASH SLOCK1: SLOCK1_5 (Bit 5)

## ◆ FLASH_SLOCK1_SLOCK1_6_Msk

#define FLASH_SLOCK1_SLOCK1_6_Msk (0x40UL)

FLASH SLOCK1: SLOCK1_6 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_6_Pos

#define FLASH_SLOCK1_SLOCK1_6_Pos (6UL)

FLASH SLOCK1: SLOCK1_6 (Bit 6)

## ◆ FLASH_SLOCK1_SLOCK1_7_Msk

#define FLASH_SLOCK1_SLOCK1_7_Msk (0x80UL)

FLASH SLOCK1: SLOCK1_7 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_7_Pos

#define FLASH_SLOCK1_SLOCK1_7_Pos (7UL)

FLASH SLOCK1: SLOCK1_7 (Bit 7)

## ◆ FLASH_SLOCK1_SLOCK1_8_Msk

#define FLASH_SLOCK1_SLOCK1_8_Msk (0x100UL)

FLASH SLOCK1: SLOCK1_8 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_8_Pos

#define FLASH_SLOCK1_SLOCK1_8_Pos (8UL)

FLASH SLOCK1: SLOCK1_8 (Bit 8)

## ◆ FLASH_SLOCK1_SLOCK1_9_Msk

#define FLASH_SLOCK1_SLOCK1_9_Msk (0x200UL)

FLASH SLOCK1: SLOCK1_9 (Bitfield-Mask: 0x01)

## ◆ FLASH_SLOCK1_SLOCK1_9_Pos

#define FLASH_SLOCK1_SLOCK1_9_Pos (9UL)

FLASH SLOCK1: SLOCK1_9 (Bit 9)

## ◆ GPIO_AFR_PxAFR0_Msk

#define GPIO_AFR_PxAFR0_Msk (0x0FUL)

GPIO AFR: PxAFR0 (Bitfield-Mask: 0x0F)

## ◆ GPIO_AFR_PxAFR0_Pos

#define GPIO_AFR_PxAFR0_Pos (0UL)

GPIO AFR: PxAFR0 (Bit 0)

## ◆ GPIO_AFR_PxAFR1_Msk

#define GPIO_AFR_PxAFR1_Msk (0xF0UL)

GPIO AFR: PxAFR1 (Bitfield-Mask: 0x0F)

## ◆ GPIO_AFR_PxAFR1_Pos

#define GPIO_AFR_PxAFR1_Pos (4UL)

GPIO AFR: PxAFR1 (Bit 4)

## ◆ GPIO_AFR_PxAFR2_Msk

#define GPIO_AFR_PxAFR2_Msk (0xF00UL)

GPIO AFR: PxAFR2 (Bitfield-Mask: 0x0F)

## ◆ GPIO_AFR_PxAFR2_Pos

#define GPIO_AFR_PxAFR2_Pos (8UL)

GPIO AFR: PxAFR2 (Bit 8)

## ◆ GPIO_AFR_PxAFR3_Msk

#define GPIO_AFR_PxAFR3_Msk (0xF000UL)

GPIO AFR: PxAFR3 (Bitfield-Mask: 0x0F)

## ◆ GPIO_AFR_PxAFR3_Pos

#define GPIO_AFR_PxAFR3_Pos (12UL)

GPIO AFR: PxAFR3 (Bit 12)

## ◆ GPIO_AFR_PxAFR4_Msk

#define GPIO_AFR_PxAFR4_Msk (0xF0000UL)

GPIO AFR: PxAFR4 (Bitfield-Mask: 0x0F)

## ◆ GPIO_AFR_PxAFR4_Pos

#define GPIO_AFR_PxAFR4_Pos (16UL)

GPIO AFR: PxAFR4 (Bit 16)

## ◆ GPIO_AFR_PxAFR5_Msk

#define GPIO_AFR_PxAFR5_Msk (0xF00000UL)

GPIO AFR: PxAFR5 (Bitfield-Mask: 0x0F)

## ◆ GPIO_AFR_PxAFR5_Pos

#define GPIO_AFR_PxAFR5_Pos (20UL)

GPIO AFR: PxAFR5 (Bit 20)

## ◆ GPIO_AFR_PxAFR6_Msk

#define GPIO_AFR_PxAFR6_Msk (0xF000000UL)

GPIO AFR: PxAFR6 (Bitfield-Mask: 0x0F)

## ◆ GPIO_AFR_PxAFR6_Pos

#define GPIO_AFR_PxAFR6_Pos (24UL)

GPIO AFR: PxAFR6 (Bit 24)

## ◆ GPIO_AFR_PxAFR7_Msk

#define GPIO_AFR_PxAFR7_Msk (0xF000000UL)

GPIO AFR: PxAFR7 (Bitfield-Mask: 0x0F)

## ◆ GPIO_AFR_PxAFR7_Pos

#define GPIO_AFR_PxAFR7_Pos (28UL)

GPIO AFR: PxAFR7 (Bit 28)

## ◆ GPIO_DBCLKCR_DBCLK_DIV_Msk

#define GPIO_DBCLKCR_DBCLK_DIV_Msk (0xFUL)

GPIO DBCLKCR: DBCLK_DIV (Bitfield-Mask: 0x0F)

## ◆ GPIO_DBCLKCR_DBCLK_DIV_Pos

#define GPIO_DBCLKCR_DBCLK_DIV_Pos (0UL)

GPIO DBCLKCR: DBCLK_DIV (Bit 0)

## ◆ GPIO_DBCLKCR_DBCLKEN_Msk

#define GPIO_DBCLKCR_DBCLKEN_Msk (0x10UL)

GPIO DBCLKCR: DBCLKEN (Bitfield-Mask: 0x01)

## ◆ GPIO_DBCLKCR_DBCLKEN_Pos

#define GPIO_DBCLKCR_DBCLKEN_Pos (4UL)

GPIO DBCLKCR: DBCLKEN (Bit 4)

## ◆ GPIO_DIRCR_PxDIR0_Msk

#define GPIO_DIRCR_PxDIR0_Msk (0x1UL)

GPIO DIRCR: PxDIR0 (Bitfield-Mask: 0x01)

## ◆ GPIO_DIRCR_PxDIR0_Pos

#define GPIO_DIRCR_PxDIR0_Pos (0UL)

GPIO DIRCR: PxDIR0 (Bit 0)

## ◆ GPIO_DIRCR_PxDIR1_Msk

#define GPIO_DIRCR_PxDIR1_Msk (0x2UL)

GPIO DIRCR: PxDIR1 (Bitfield-Mask: 0x01)

## ◆ GPIO_DIRCR_PxDIR1_Pos

#define GPIO_DIRCR_PxDIR1_Pos (1UL)

GPIO DIRCR: PxDIR1 (Bit 1)

## ◆ GPIO_DIRCR_PxDIR2_Msk

#define GPIO_DIRCR_PxDIR2_Msk (0x4UL)

GPIO DIRCR: PxDIR2 (Bitfield-Mask: 0x01)

## ◆ GPIO_DIRCR_PxDIR2_Pos

#define GPIO_DIRCR_PxDIR2_Pos (2UL)

GPIO DIRCR: PxDIR2 (Bit 2)

## ◆ GPIO_DIRCR_PxDIR3_Msk

#define GPIO_DIRCR_PxDIR3_Msk (0x8UL)

GPIO DIRCR: PxDIR3 (Bitfield-Mask: 0x01)

## ◆ GPIO_DIRCR_PxDIR3_Pos

#define GPIO_DIRCR_PxDIR3_Pos (3UL)

GPIO DIRCR: PxDIR3 (Bit 3)

## ◆ GPIO_DIRCR_PxDIR4_Msk

#define GPIO_DIRCR_PxDIR4_Msk (0x10UL)

GPIO DIRCR: PxDIR4 (Bitfield-Mask: 0x01)

## ◆ GPIO_DIRCR_PxDIR4_Pos

#define GPIO_DIRCR_PxDIR4_Pos (4UL)

GPIO DIRCR: PxDIR4 (Bit 4)

## ◆ GPIO_DIRCR_PxDIR5_Msk

#define GPIO_DIRCR_PxDIR5_Msk (0x20UL)

GPIO DIRCR: PxDIR5 (Bitfield-Mask: 0x01)

## ◆ GPIO_DIRCR_PxDIR5_Pos

#define GPIO_DIRCR_PxDIR5_Pos (5UL)

GPIO DIRCR: PxDIR5 (Bit 5)

## ◆ GPIO_DIRCR_PxDIR6_Msk

#define GPIO_DIRCR_PxDIR6_Msk (0x40UL)

GPIO DIRCR: PxDIR6 (Bitfield-Mask: 0x01)

## ◆ GPIO_DIRCR_PxDIR6_Pos

#define GPIO_DIRCR_PxDIR6_Pos (6UL)

GPIO DIRCR: PxDIR6 (Bit 6)

## ◆ GPIO_DIRCR_PxDIR7_Msk

#define GPIO_DIRCR_PxDIR7_Msk (0x80UL)

GPIO DIRCR: PxDIR7 (Bitfield-Mask: 0x01)

## ◆ GPIO_DIRCR_PxDIR7_Pos

#define GPIO_DIRCR_PxDIR7_Pos (7UL)

GPIO DIRCR: PxDIR7 (Bit 7)

## ◆ GPIO_DRVCR_PxDRV0_Msk

#define GPIO_DRVCR_PxDRV0_Msk (0x1UL)

GPIO DRVCR: PxDRV0 (Bitfield-Mask: 0x01)

## ◆ GPIO_DRVCR_PxDRV0_Pos

#define GPIO_DRVCR_PxDRV0_Pos (0UL)

GPIO DRVCR: PxDRV0 (Bit 0)

## ◆ GPIO_DRVCR_PxDRV1_Msk

#define GPIO_DRVCR_PxDRV1_Msk (0x2UL)

GPIO DRVCR: PxDRV1 (Bitfield-Mask: 0x01)

## ◆ GPIO_DRVCR_PxDRV1_Pos

#define GPIO_DRVCR_PxDRV1_Pos (1UL)

GPIO DRVCR: PxDRV1 (Bit 1)

## ◆ GPIO_DRVCR_PxDRV2_Msk

#define GPIO_DRVCR_PxDRV2_Msk (0x4UL)

GPIO DRVCR: PxDRV2 (Bitfield-Mask: 0x01)

## ◆ GPIO_DRVCR_PxDRV2_Pos

#define GPIO_DRVCR_PxDRV2_Pos (2UL)

GPIO DRVCR: PxDRV2 (Bit 2)

## ◆ GPIO_DRVCR_PxDRV3_Msk

#define GPIO_DRVCR_PxDRV3_Msk (0x8UL)

GPIO DRVCR: PxDRV3 (Bitfield-Mask: 0x01)

## ◆ GPIO_DRVCR_PxDRV3_Pos

#define GPIO_DRVCR_PxDRV3_Pos (3UL)

GPIO DRVCR: PxDRV3 (Bit 3)

## ◆ GPIO_DRVCR_PxDRV4_Msk

#define GPIO_DRVCR_PxDRV4_Msk (0x10UL)

GPIO DRVCR: PxDRV4 (Bitfield-Mask: 0x01)

## ◆ GPIO_DRVCR_PxDRV4_Pos

#define GPIO_DRVCR_PxDRV4_Pos (4UL)

GPIO DRVCR: PxDRV4 (Bit 4)

## ◆ GPIO_DRVCR_PxDRV5_Msk

#define GPIO_DRVCR_PxDRV5_Msk (0x20UL)

GPIO DRVCR: PxDRV5 (Bitfield-Mask: 0x01)

## ◆ GPIO_DRVCR_PxDRV5_Pos

#define GPIO_DRVCR_PxDRV5_Pos (5UL)

GPIO DRVCR: PxDRV5 (Bit 5)

## ◆ GPIO_DRVCR_PxDRV6_Msk

#define GPIO_DRVCR_PxDRV6_Msk (0x40UL)

GPIO DRVCR: PxDRV6 (Bitfield-Mask: 0x01)

## ◆ GPIO_DRVCR_PxDRV6_Pos

#define GPIO_DRVCR_PxDRV6_Pos (6UL)

GPIO DRVCR: PxDRV6 (Bit 6)

## ◆ GPIO_DRVCR_PxDRV7_Msk

#define GPIO_DRVCR_PxDRV7_Msk (0x80UL)

GPIO DRVCR: PxDRV7 (Bitfield-Mask: 0x01)

## ◆ GPIO_DRVCR_PxDRV7_Pos

#define GPIO_DRVCR_PxDRV7_Pos (7UL)

GPIO DRVCR: PxDRV7 (Bit 7)

## ◆ GPIO_IDR_PxID0_Msk

#define GPIO_IDR_PxID0_Msk (0x1UL)

GPIO IDR: PxID0 (Bitfield-Mask: 0x01)

## ◆ GPIO_IDR_PxID0_Pos

#define GPIO_IDR_PxID0_Pos (0UL)

GPIO IDR: PxID0 (Bit 0)

## ◆ GPIO_IDR_PxID1_Msk

#define GPIO_IDR_PxID1_Msk (0x2UL)

GPIO IDR: PxID1 (Bitfield-Mask: 0x01)

## ◆ GPIO_IDR_PxID1_Pos

#define GPIO_IDR_PxID1_Pos (1UL)

GPIO IDR: PxID1 (Bit 1)

## ◆ GPIO_IDR_PxID2_Msk

#define GPIO_IDR_PxID2_Msk (0x4UL)

GPIO IDR: PxID2 (Bitfield-Mask: 0x01)

## ◆ GPIO_IDR_PxID2_Pos

#define GPIO_IDR_PxID2_Pos (2UL)

GPIO IDR: PxID2 (Bit 2)

## ◆ GPIO_IDR_PxID3_Msk

#define GPIO_IDR_PxID3_Msk (0x8UL)

GPIO IDR: PxID3 (Bitfield-Mask: 0x01)

## ◆ GPIO_IDR_PxID3_Pos

#define GPIO_IDR_PxID3_Pos (3UL)

GPIO IDR: PxID3 (Bit 3)

## ◆ GPIO_IDR_PxID4_Msk

#define GPIO_IDR_PxID4_Msk (0x10UL)

GPIO IDR: PxID4 (Bitfield-Mask: 0x01)

## ◆ GPIO_IDR_PxID4_Pos

#define GPIO_IDR_PxID4_Pos (4UL)

GPIO IDR: PxID4 (Bit 4)

## ◆ GPIO_IDR_PxID5_Msk

#define GPIO_IDR_PxID5_Msk (0x20UL)

GPIO IDR: PxID5 (Bitfield-Mask: 0x01)

## ◆ GPIO_IDR_PxID5_Pos

#define GPIO_IDR_PxID5_Pos (5UL)

GPIO IDR: PxID5 (Bit 5)

## ◆ GPIO_IDR_PxID6_Msk

#define GPIO_IDR_PxID6_Msk (0x40UL)

GPIO IDR: PxID6 (Bitfield-Mask: 0x01)

## ◆ GPIO_IDR_PxID6_Pos

#define GPIO_IDR_PxID6_Pos (6UL)

GPIO IDR: PxID6 (Bit 6)

## ◆ GPIO_IDR_PxID7_Msk

#define GPIO_IDR_PxID7_Msk (0x80UL)

GPIO IDR: PxID7 (Bitfield-Mask: 0x01)

## ◆ GPIO_IDR_PxID7_Pos

#define GPIO_IDR_PxID7_Pos (7UL)

GPIO IDR: PxID7 (Bit 7)

## ◆ GPIO_INDBEN_PxDIDB_Msk

#define GPIO_INDBEN_PxDIDB_Msk (0xFFUL)

GPIO INDBEN: PxDIDB (Bitfield-Mask: 0xFF)

## ◆ GPIO_INDBEN_PxDIDB_Pos

#define GPIO_INDBEN_PxDIDB_Pos (0UL)

GPIO INDBEN: PxDIDB (Bit 0)

## ◆ GPIO_INDBEN_SYNC_EN_Msk

#define GPIO_INDBEN_SYNC_EN_Msk (0x100UL)

GPIO INDBEN: SYNC_EN (Bitfield-Mask: 0x01)

## ◆ GPIO_INDBEN_SYNC_EN_Pos

#define GPIO_INDBEN_SYNC_EN_Pos (8UL)

GPIO INDBEN: SYNC_EN (Bit 8)

## ◆ GPIO_INTANY_PxIANY0_Msk

#define GPIO_INTANY_PxIANY0_Msk (0x1UL)

GPIO INTANY: PxIANY0 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTANY_PxIANY0_Pos

#define GPIO_INTANY_PxIANY0_Pos (0UL)

GPIO INTANY: PxIANY0 (Bit 0)

## ◆ GPIO_INTANY_PxIANY1_Msk

#define GPIO_INTANY_PxIANY1_Msk (0x2UL)

GPIO INTANY: PxIANY1 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTANY_PxIANY1_Pos

#define GPIO_INTANY_PxIANY1_Pos (1UL)

GPIO INTANY: PxIANY1 (Bit 1)

## ◆ GPIO_INTANY_PxIANY2_Msk

#define GPIO_INTANY_PxIANY2_Msk (0x4UL)

GPIO INTANY: PxIANY2 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTANY_PxIANY2_Pos

#define GPIO_INTANY_PxIANY2_Pos (2UL)

GPIO INTANY: PxIANY2 (Bit 2)

## ◆ GPIO_INTANY_PxIANY3_Msk

#define GPIO_INTANY_PxIANY3_Msk (0x8UL)

GPIO INTANY: PxIANY3 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTANY_PxIANY3_Pos

#define GPIO_INTANY_PxIANY3_Pos (3UL)

GPIO INTANY: PxIANY3 (Bit 3)

## ◆ GPIO_INTANY_PxIANY4_Msk

#define GPIO_INTANY_PxIANY4_Msk (0x10UL)

GPIO INTANY: PxIANY4 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTANY_PxIANY4_Pos

#define GPIO_INTANY_PxIANY4_Pos (4UL)

GPIO INTANY: PxIANY4 (Bit 4)

## ◆ GPIO_INTANY_PxIANY5_Msk

#define GPIO_INTANY_PxIANY5_Msk (0x20UL)

GPIO INTANY: PxIANY5 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTANY_PxIANY5_Pos

#define GPIO_INTANY_PxIANY5_Pos (5UL)

GPIO INTANY: PxIANY5 (Bit 5)

## ◆ GPIO_INTANY_PxIANY6_Msk

#define GPIO_INTANY_PxIANY6_Msk (0x40UL)

GPIO INTANY: PxIANY6 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTANY_PxIANY6_Pos

#define GPIO_INTANY_PxIANY6_Pos (6UL)

GPIO INTANY: PxIANY6 (Bit 6)

## ◆ GPIO_INTANY_PxIANY7_Msk

#define GPIO_INTANY_PxIANY7_Msk (0x80UL)

GPIO INTANY: PxIANY7 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTANY_PxIANY7_Pos

#define GPIO_INTANY_PxIANY7_Pos (7UL)

GPIO INTANY: PxIANY7 (Bit 7)

## ◆ GPIO_INTCLR_PxICLR0_Msk

#define GPIO_INTCLR_PxICLR0_Msk (0x1UL)

GPIO INTCLR: PxICLR0 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTCLR_PxICLR0_Pos

#define GPIO_INTCLR_PxICLR0_Pos (0UL)

GPIO INTCLR: PxICLR0 (Bit 0)

## ◆ GPIO_INTCLR_PxICLR1_Msk

#define GPIO_INTCLR_PxICLR1_Msk (0x2UL)

GPIO INTCLR: PxICLR1 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTCLR_PxICLR1_Pos

#define GPIO_INTCLR_PxICLR1_Pos (1UL)

GPIO INTCLR: PxICLR1 (Bit 1)

## ◆ GPIO_INTCLR_PxICLR2_Msk

#define GPIO_INTCLR_PxICLR2_Msk (0x4UL)

GPIO INTCLR: PxICLR2 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTCLR_PxICLR2_Pos

#define GPIO_INTCLR_PxICLR2_Pos (2UL)

GPIO INTCLR: PxICLR2 (Bit 2)

## ◆ GPIO_INTCLR_PxICLR3_Msk

#define GPIO_INTCLR_PxICLR3_Msk (0x8UL)

GPIO INTCLR: PxICLR3 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTCLR_PxICLR3_Pos

#define GPIO_INTCLR_PxICLR3_Pos (3UL)

GPIO INTCLR: PxICLR3 (Bit 3)

## ◆ GPIO_INTCLR_PxICLR4_Msk

#define GPIO_INTCLR_PxICLR4_Msk (0x10UL)

GPIO INTCLR: PxICLR4 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTCLR_PxICLR4_Pos

#define GPIO_INTCLR_PxICLR4_Pos (4UL)

GPIO INTCLR: PxICLR4 (Bit 4)

## ◆ GPIO_INTCLR_PxICLR5_Msk

#define GPIO_INTCLR_PxICLR5_Msk (0x20UL)

GPIO INTCLR: PxICLR5 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTCLR_PxICLR5_Pos

#define GPIO_INTCLR_PxICLR5_Pos (5UL)

GPIO INTCLR: PxICLR5 (Bit 5)

## ◆ GPIO_INTCLR_PxICLR6_Msk

#define GPIO_INTCLR_PxICLR6_Msk (0x40UL)

GPIO INTCLR: PxICLR6 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTCLR_PxICLR6_Pos

#define GPIO_INTCLR_PxICLR6_Pos (6UL)

GPIO INTCLR: PxICLR6 (Bit 6)

## ◆ GPIO_INTCLR_PxICLR7_Msk

#define GPIO_INTCLR_PxICLR7_Msk (0x80UL)

GPIO INTCLR: PxICLR7 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTCLR_PxICLR7_Pos

#define GPIO_INTCLR_PxICLR7_Pos (7UL)

GPIO INTCLR: PxICLR7 (Bit 7)

## ◆ GPIO_INTEN_PxIEN0_Msk

#define GPIO_INTEN_PxIEN0_Msk (0x1UL)

GPIO INTEN: PxIEN0 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTEN_PxIEN0_Pos

#define GPIO_INTEN_PxIEN0_Pos (0UL)

GPIO INTEN: PxIEN0 (Bit 0)

## ◆ GPIO_INTEN_PxIEN1_Msk

#define GPIO_INTEN_PxIEN1_Msk (0x2UL)

GPIO INTEN: PxIEN1 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTEN_PxIEN1_Pos

#define GPIO_INTEN_PxIEN1_Pos (1UL)

GPIO INTEN: PxIEN1 (Bit 1)

## ◆ GPIO_INTEN_PxIEN2_Msk

#define GPIO_INTEN_PxIEN2_Msk (0x4UL)

GPIO INTEN: PxIEN2 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTEN_PxIEN2_Pos

#define GPIO_INTEN_PxIEN2_Pos (2UL)

GPIO INTEN: PxIEN2 (Bit 2)

## ◆ GPIO_INTEN_PxIEN3_Msk

#define GPIO_INTEN_PxIEN3_Msk (0x8UL)

GPIO INTEN: PxIEN3 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTEN_PxIEN3_Pos

#define GPIO_INTEN_PxIEN3_Pos (3UL)

GPIO INTEN: PxIEN3 (Bit 3)

## ◆ GPIO_INTEN_PxIEN4_Msk

#define GPIO_INTEN_PxIEN4_Msk (0x10UL)

GPIO INTEN: PxIEN4 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTEN_PxIEN4_Pos

#define GPIO_INTEN_PxIEN4_Pos (4UL)

GPIO INTEN: PxIEN4 (Bit 4)

## ◆ GPIO_INTEN_PxIEN5_Msk

#define GPIO_INTEN_PxIEN5_Msk (0x20UL)

GPIO INTEN: PxIEN5 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTEN_PxIEN5_Pos

#define GPIO_INTEN_PxIEN5_Pos (5UL)

GPIO INTEN: PxIEN5 (Bit 5)

## ◆ GPIO_INTEN_PxIEN6_Msk

#define GPIO_INTEN_PxIEN6_Msk (0x40UL)

GPIO INTEN: PxIEN6 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTEN_PxIEN6_Pos

#define GPIO_INTEN_PxIEN6_Pos (6UL)

GPIO INTEN: PxIEN6 (Bit 6)

## ◆ GPIO_INTEN_PxIEN7_Msk

#define GPIO_INTEN_PxIEN7_Msk (0x80UL)

GPIO INTEN: PxIEN7 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTEN_PxIEN7_Pos

#define GPIO_INTEN_PxIEN7_Pos (7UL)

GPIO INTEN: PxIEN7 (Bit 7)

## ◆ GPIO_INTPOLCR_PxIVAL0_Msk

#define GPIO_INTPOLCR_PxIVAL0_Msk (0x1UL)

GPIO INTPOLCR: PxIVAL0 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTPOLCR_PxIVAL0_Pos

#define GPIO_INTPOLCR_PxIVAL0_Pos (0UL)

GPIO INTPOLCR: PxIVAL0 (Bit 0)

## ◆ GPIO_INTPOLCR_PxIVAL1_Msk

#define GPIO_INTPOLCR_PxIVAL1_Msk (0x2UL)

GPIO INTPOLCR: PxIVAL1 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTPOLCR_PxIVAL1_Pos

#define GPIO_INTPOLCR_PxIVAL1_Pos (1UL)

GPIO INTPOLCR: PxIVAL1 (Bit 1)

## ◆ GPIO_INTPOLCR_PxIVAL2_Msk

#define GPIO_INTPOLCR_PxIVAL2_Msk (0x4UL)

GPIO INTPOLCR: PxIVAL2 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTPOLCR_PxIVAL2_Pos

#define GPIO_INTPOLCR_PxIVAL2_Pos (2UL)

GPIO INTPOLCR: PxIVAL2 (Bit 2)

## ◆ GPIO_INTPOLCR_PxIVAL3_Msk

#define GPIO_INTPOLCR_PxIVAL3_Msk (0x8UL)

GPIO INTPOLCR: PxIVAL3 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTPOLCR_PxIVAL3_Pos

#define GPIO_INTPOLCR_PxIVAL3_Pos (3UL)

GPIO INTPOLCR: PxIVAL3 (Bit 3)

## ◆ GPIO_INTPOLCR_PxIVAL4_Msk

#define GPIO_INTPOLCR_PxIVAL4_Msk (0x10UL)

GPIO INTPOLCR: PxIVAL4 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTPOLCR_PxIVAL4_Pos

#define GPIO_INTPOLCR_PxIVAL4_Pos (4UL)

GPIO INTPOLCR: PxIVAL4 (Bit 4)

## ◆ GPIO_INTPOLCR_PxIVAL5_Msk

#define GPIO_INTPOLCR_PxIVAL5_Msk (0x20UL)

GPIO INTPOLCR: PxIVAL5 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTPOLCR_PxIVAL5_Pos

#define GPIO_INTPOLCR_PxIVAL5_Pos (5UL)

GPIO INTPOLCR: PxIVAL5 (Bit 5)

## ◆ GPIO_INTPOLCR_PxIVAL6_Msk

#define GPIO_INTPOLCR_PxIVAL6_Msk (0x40UL)

GPIO INTPOLCR: PxIVAL6 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTPOLCR_PxIVAL6_Pos

#define GPIO_INTPOLCR_PxIVAL6_Pos (6UL)

GPIO INTPOLCR: PxIVAL6 (Bit 6)

## ◆ GPIO_INTPOLCR_PxIVAL7_Msk

#define GPIO_INTPOLCR_PxIVAL7_Msk (0x80UL)

GPIO INTPOLCR: PxIVAL7 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTPOLCR_PxIVAL7_Pos

#define GPIO_INTPOLCR_PxIVAL7_Pos (7UL)

GPIO INTPOLCR: PxIVAL7 (Bit 7)

## ◆ GPIO_INTTYPCR_PxITYPE0_Msk

#define GPIO_INTTYPCR_PxITYPE0_Msk (0x1UL)

GPIO INTTYPCR: PxITYPE0 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTTYPCR_PxITYPE0_Pos

#define GPIO_INTTYPCR_PxITYPE0_Pos (0UL)

GPIO INTTYPCR: PxITYPE0 (Bit 0)

## ◆ GPIO_INTTYPCR_PxITYPE1_Msk

#define GPIO_INTTYPCR_PxITYPE1_Msk (0x2UL)

GPIO INTTYPCR: PxITYPE1 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTTYPCR_PxITYPE1_Pos

#define GPIO_INTTYPCR_PxITYPE1_Pos (1UL)

GPIO INTTYPCR: PxITYPE1 (Bit 1)

## ◆ GPIO_INTTYPCR_PxITYPE2_Msk

#define GPIO_INTTYPCR_PxITYPE2_Msk (0x4UL)

GPIO INTTYPCR: PxITYPE2 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTTYPCR_PxITYPE2_Pos

#define GPIO_INTTYPCR_PxITYPE2_Pos (2UL)

GPIO INTTYPCR: PxITYPE2 (Bit 2)

## ◆ GPIO_INTTYPCR_PxITYPE3_Msk

#define GPIO_INTTYPCR_PxITYPE3_Msk (0x8UL)

GPIO INTTYPCR: PxITYPE3 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTTYPCR_PxITYPE3_Pos

#define GPIO_INTTYPCR_PxITYPE3_Pos (3UL)

GPIO INTTYPCR: PxITYPE3 (Bit 3)

## ◆ GPIO_INTTYPCR_PxITYPE4_Msk

#define GPIO_INTTYPCR_PxITYPE4_Msk (0x10UL)

GPIO INTTYPCR: PxITYPE4 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTTYPCR_PxITYPE4_Pos

#define GPIO_INTTYPCR_PxITYPE4_Pos (4UL)

GPIO INTTYPCR: PxITYPE4 (Bit 4)

## ◆ GPIO_INTTYPCR_PxITYPE5_Msk

#define GPIO_INTTYPCR_PxITYPE5_Msk (0x20UL)

GPIO INTTYPCR: PxITYPE5 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTTYPCR_PxITYPE5_Pos

#define GPIO_INTTYPCR_PxITYPE5_Pos (5UL)

GPIO INTTYPCR: PxITYPE5 (Bit 5)

## ◆ GPIO_INTTYPCR_PxITYPE6_Msk

#define GPIO_INTTYPCR_PxITYPE6_Msk (0x40UL)

GPIO INTTYPCR: PxITYPE6 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTTYPCR_PxITYPE6_Pos

#define GPIO_INTTYPCR_PxITYPE6_Pos (6UL)

GPIO INTTYPCR: PxITYPE6 (Bit 6)

## ◆ GPIO_INTTYPCR_PxITYPE7_Msk

#define GPIO_INTTYPCR_PxITYPE7_Msk (0x80UL)

GPIO INTTYPCR: PxITYPE7 (Bitfield-Mask: 0x01)

## ◆ GPIO_INTTYPCR_PxITYPE7_Pos

#define GPIO_INTTYPCR_PxITYPE7_Pos (7UL)

GPIO INTTYPCR: PxITYPE7 (Bit 7)

## ◆ GPIO_MSKINTCR_PxMIS0_Msk

#define GPIO_MSKINTCR_PxMIS0_Msk (0x1UL)

GPIO MSKINTCR: PxMIS0 (Bitfield-Mask: 0x01)

## ◆ GPIO_MSKINTCR_PxMIS0_Pos

#define GPIO_MSKINTCR_PxMIS0_Pos (0UL)

GPIO MSKINTCR: PxMIS0 (Bit 0)

## ◆ GPIO_MSKINTCR_PxMIS1_Msk

#define GPIO_MSKINTCR_PxMIS1_Msk (0x2UL)

GPIO MSKINTCR: PxMIS1 (Bitfield-Mask: 0x01)

## ◆ GPIO_MSKINTCR_PxMIS1_Pos

#define GPIO_MSKINTCR_PxMIS1_Pos (1UL)

GPIO MSKINTCR: PxMIS1 (Bit 1)

## ◆ GPIO_MSKINTCR_PxMIS2_Msk

#define GPIO_MSKINTCR_PxMIS2_Msk (0x4UL)

GPIO MSKINTCR: PxMIS2 (Bitfield-Mask: 0x01)

## ◆ GPIO_MSKINTCR_PxMIS2_Pos

#define GPIO_MSKINTCR_PxMIS2_Pos (2UL)

GPIO MSKINTCR: PxMIS2 (Bit 2)

## ◆ GPIO_MSKINTCR_PxMIS3_Msk

#define GPIO_MSKINTCR_PxMIS3_Msk (0x8UL)

GPIO MSKINTCR: PxMIS3 (Bitfield-Mask: 0x01)

## ◆ GPIO_MSKINTCR_PxMIS3_Pos

#define GPIO_MSKINTCR_PxMIS3_Pos (3UL)

GPIO MSKINTCR: PxMIS3 (Bit 3)

## ◆ GPIO_MSKINTCR_PxMIS4_Msk

#define GPIO_MSKINTCR_PxMIS4_Msk (0x10UL)

GPIO MSKINTCR: PxMIS4 (Bitfield-Mask: 0x01)

## ◆ GPIO_MSKINTCR_PxMIS4_Pos

#define GPIO_MSKINTCR_PxMIS4_Pos (4UL)

GPIO MSKINTCR: PxMIS4 (Bit 4)

## ◆ GPIO_MSKINTCR_PxMIS5_Msk

#define GPIO_MSKINTCR_PxMIS5_Msk (0x20UL)

GPIO MSKINTCR: PxMIS5 (Bitfield-Mask: 0x01)

## ◆ GPIO_MSKINTCR_PxMIS5_Pos

#define GPIO_MSKINTCR_PxMIS5_Pos (5UL)

GPIO MSKINTCR: PxMIS5 (Bit 5)

## ◆ GPIO_MSKINTCR_PxMIS6_Msk

#define GPIO_MSKINTCR_PxMIS6_Msk (0x40UL)

GPIO MSKINTCR: PxMIS6 (Bitfield-Mask: 0x01)

## ◆ GPIO_MSKINTCR_PxMIS6_Pos

#define GPIO_MSKINTCR_PxMIS6_Pos (6UL)

GPIO MSKINTCR: PxMIS6 (Bit 6)

## ◆ GPIO_MSKINTCR_PxMIS7_Msk

#define GPIO_MSKINTCR_PxMIS7_Msk (0x80UL)

GPIO MSKINTCR: PxMIS7 (Bitfield-Mask: 0x01)

## ◆ GPIO_MSKINTCR_PxMIS7_Pos

#define GPIO_MSKINTCR_PxMIS7_Pos (7UL)

GPIO MSKINTCR: PxMIS7 (Bit 7)

## ◆ GPIO_ODCLR_PxODCLR0_Msk

#define GPIO_ODCLR_PxODCLR0_Msk (0x1UL)

GPIO ODCLR: PxODCLR0 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODCLR_PxODCLR0_Pos

#define GPIO_ODCLR_PxODCLR0_Pos (0UL)

GPIO ODCLR: PxODCLR0 (Bit 0)

## ◆ GPIO_ODCLR_PxODCLR1_Msk

#define GPIO_ODCLR_PxODCLR1_Msk (0x2UL)

GPIO ODCLR: PxODCLR1 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODCLR_PxODCLR1_Pos

#define GPIO_ODCLR_PxODCLR1_Pos (1UL)

GPIO ODCLR: PxODCLR1 (Bit 1)

## ◆ GPIO_ODCLR_PxODCLR2_Msk

#define GPIO_ODCLR_PxODCLR2_Msk (0x4UL)

GPIO ODCLR: PxODCLR2 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODCLR_PxODCLR2_Pos

#define GPIO_ODCLR_PxODCLR2_Pos (2UL)

GPIO ODCLR: PxODCLR2 (Bit 2)

## ◆ GPIO_ODCLR_PxODCLR3_Msk

#define GPIO_ODCLR_PxODCLR3_Msk (0x8UL)

GPIO ODCLR: PxODCLR3 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODCLR_PxODCLR3_Pos

#define GPIO_ODCLR_PxODCLR3_Pos (3UL)

GPIO ODCLR: PxODCLR3 (Bit 3)

## ◆ GPIO_ODCLR_PxODCLR4_Msk

#define GPIO_ODCLR_PxODCLR4_Msk (0x10UL)

GPIO ODCLR: PxODCLR4 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODCLR_PxODCLR4_Pos

#define GPIO_ODCLR_PxODCLR4_Pos (4UL)

GPIO ODCLR: PxODCLR4 (Bit 4)

## ◆ GPIO_ODCLR_PxODCLR5_Msk

#define GPIO_ODCLR_PxODCLR5_Msk (0x20UL)

GPIO ODCLR: PxODCLR5 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODCLR_PxODCLR5_Pos

#define GPIO_ODCLR_PxODCLR5_Pos (5UL)

GPIO ODCLR: PxODCLR5 (Bit 5)

## ◆ GPIO_ODCLR_PxODCLR6_Msk

#define GPIO_ODCLR_PxODCLR6_Msk (0x40UL)

GPIO ODCLR: PxODCLR6 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODCLR_PxODCLR6_Pos

#define GPIO_ODCLR_PxODCLR6_Pos (6UL)

GPIO ODCLR: PxODCLR6 (Bit 6)

## ◆ GPIO_ODCLR_PxODCLR7_Msk

#define GPIO_ODCLR_PxODCLR7_Msk (0x80UL)

GPIO ODCLR: PxODCLR7 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODCLR_PxODCLR7_Pos

#define GPIO_ODCLR_PxODCLR7_Pos (7UL)

GPIO ODCLR: PxODCLR7 (Bit 7)

## ◆ GPIO_ODR_PxOD0_Msk

#define GPIO_ODR_PxOD0_Msk (0x1UL)

GPIO ODR: PxOD0 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODR_PxOD0_Pos

#define GPIO_ODR_PxOD0_Pos (0UL)

GPIO ODR: PxOD0 (Bit 0)

## ◆ GPIO_ODR_PxOD1_Msk

#define GPIO_ODR_PxOD1_Msk (0x2UL)

GPIO ODR: PxOD1 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODR_PxOD1_Pos

#define GPIO_ODR_PxOD1_Pos (1UL)

GPIO ODR: PxOD1 (Bit 1)

## ◆ GPIO_ODR_PxOD2_Msk

#define GPIO_ODR_PxOD2_Msk (0x4UL)

GPIO ODR: PxOD2 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODR_PxOD2_Pos

#define GPIO_ODR_PxOD2_Pos (2UL)

GPIO ODR: PxOD2 (Bit 2)

## ◆ GPIO_ODR_PxOD3_Msk

#define GPIO_ODR_PxOD3_Msk (0x8UL)

GPIO ODR: PxOD3 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODR_PxOD3_Pos

#define GPIO_ODR_PxOD3_Pos (3UL)

GPIO ODR: PxOD3 (Bit 3)

## ◆ GPIO_ODR_PxOD4_Msk

#define GPIO_ODR_PxOD4_Msk (0x10UL)

GPIO ODR: PxOD4 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODR_PxOD4_Pos

#define GPIO_ODR_PxOD4_Pos (4UL)

GPIO ODR: PxOD4 (Bit 4)

## ◆ GPIO_ODR_PxOD5_Msk

#define GPIO_ODR_PxOD5_Msk (0x20UL)

GPIO ODR: PxOD5 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODR_PxOD5_Pos

#define GPIO_ODR_PxOD5_Pos (5UL)

GPIO ODR: PxOD5 (Bit 5)

## ◆ GPIO_ODR_PxOD6_Msk

#define GPIO_ODR_PxOD6_Msk (0x40UL)

GPIO ODR: PxOD6 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODR_PxOD6_Pos

#define GPIO_ODR_PxOD6_Pos (6UL)

GPIO ODR: PxOD6 (Bit 6)

## ◆ GPIO_ODR_PxOD7_Msk

#define GPIO_ODR_PxOD7_Msk (0x80UL)

GPIO ODR: PxOD7 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODR_PxOD7_Pos

#define GPIO_ODR_PxOD7_Pos (7UL)

GPIO ODR: PxOD7 (Bit 7)

## ◆ GPIO_ODSET_PxODSET0_Msk

#define GPIO_ODSET_PxODSET0_Msk (0x1UL)

GPIO ODSET: PxODSET0 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODSET_PxODSET0_Pos

#define GPIO_ODSET_PxODSET0_Pos (0UL)

GPIO ODSET: PxODSET0 (Bit 0)

## ◆ GPIO_ODSET_PxODSET1_Msk

#define GPIO_ODSET_PxODSET1_Msk (0x2UL)

GPIO ODSET: PxODSET1 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODSET_PxODSET1_Pos

#define GPIO_ODSET_PxODSET1_Pos (1UL)

GPIO ODSET: PxODSET1 (Bit 1)

## ◆ GPIO_ODSET_PxODSET2_Msk

#define GPIO_ODSET_PxODSET2_Msk (0x4UL)

GPIO ODSET: PxODSET2 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODSET_PxODSET2_Pos

#define GPIO_ODSET_PxODSET2_Pos (2UL)

GPIO ODSET: PxODSET2 (Bit 2)

## ◆ GPIO_ODSET_PxODSET3_Msk

#define GPIO_ODSET_PxODSET3_Msk (0x8UL)

GPIO ODSET: PxODSET3 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODSET_PxODSET3_Pos

#define GPIO_ODSET_PxODSET3_Pos (3UL)

GPIO ODSET: PxODSET3 (Bit 3)

## ◆ GPIO_ODSET_PxODSET4_Msk

#define GPIO_ODSET_PxODSET4_Msk (0x10UL)

GPIO ODSET: PxODSET4 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODSET_PxODSET4_Pos

#define GPIO_ODSET_PxODSET4_Pos (4UL)

GPIO ODSET: PxODSET4 (Bit 4)

## ◆ GPIO_ODSET_PxODSET5_Msk

#define GPIO_ODSET_PxODSET5_Msk (0x20UL)

GPIO ODSET: PxODSET5 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODSET_PxODSET5_Pos

#define GPIO_ODSET_PxODSET5_Pos (5UL)

GPIO ODSET: PxODSET5 (Bit 5)

## ◆ GPIO_ODSET_PxODSET6_Msk

#define GPIO_ODSET_PxODSET6_Msk (0x40UL)

GPIO ODSET: PxODSET6 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODSET_PxODSET6_Pos

#define GPIO_ODSET_PxODSET6_Pos (6UL)

GPIO ODSET: PxODSET6 (Bit 6)

## ◆ GPIO_ODSET_PxODSET7_Msk

#define GPIO_ODSET_PxODSET7_Msk (0x80UL)

GPIO ODSET: PxODSET7 (Bitfield-Mask: 0x01)

## ◆ GPIO_ODSET_PxODSET7_Pos

#define GPIO_ODSET_PxODSET7_Pos (7UL)

GPIO ODSET: PxODSET7 (Bit 7)

## ◆ GPIO_OTYPER_PxOTYP0_Msk

#define GPIO_OTYPER_PxOTYP0_Msk (0x1UL)

GPIO OTYPER: PxOTYP0 (Bitfield-Mask: 0x01)

## ◆ GPIO_OTYPER_PxOTYP0_Pos

#define GPIO_OTYPER_PxOTYP0_Pos (0UL)

GPIO OTYPER: PxOTYP0 (Bit 0)

## ◆ GPIO_OTYPER_PxOTYP1_Msk

#define GPIO_OTYPER_PxOTYP1_Msk (0x2UL)

GPIO OTYPER: PxOTYP1 (Bitfield-Mask: 0x01)

## ◆ GPIO_OTYPER_PxOTYP1_Pos

#define GPIO_OTYPER_PxOTYP1_Pos (1UL)

GPIO OTYPER: PxOTYP1 (Bit 1)

## ◆ GPIO_OTYPER_PxOTYP2_Msk

#define GPIO_OTYPER_PxOTYP2_Msk (0x4UL)

GPIO OTYPER: PxOTYP2 (Bitfield-Mask: 0x01)

## ◆ GPIO_OTYPER_PxOTYP2_Pos

#define GPIO_OTYPER_PxOTYP2_Pos (2UL)

GPIO OTYPER: PxOTYP2 (Bit 2)

## ◆ GPIO_OTYPER_PxOTYP3_Msk

#define GPIO_OTYPER_PxOTYP3_Msk (0x8UL)

GPIO OTYPER: PxOTYP3 (Bitfield-Mask: 0x01)

## ◆ GPIO_OTYPER_PxOTYP3_Pos

#define GPIO_OTYPER_PxOTYP3_Pos (3UL)

GPIO OTYPER: PxOTYP3 (Bit 3)

## ◆ GPIO_OTYPER_PxOTYP4_Msk

#define GPIO_OTYPER_PxOTYP4_Msk (0x10UL)

GPIO OTYPER: PxOTYP4 (Bitfield-Mask: 0x01)

## ◆ GPIO_OTYPER_PxOTYP4_Pos

#define GPIO_OTYPER_PxOTYP4_Pos (4UL)

GPIO OTYPER: PxOTYP4 (Bit 4)

## ◆ GPIO_OTYPER_PxOTYP5_Msk

#define GPIO_OTYPER_PxOTYP5_Msk (0x20UL)

GPIO OTYPER: PxOTYP5 (Bitfield-Mask: 0x01)

## ◆ GPIO_OTYPER_PxOTYP5_Pos

#define GPIO_OTYPER_PxOTYP5_Pos (5UL)

GPIO OTYPER: PxOTYP5 (Bit 5)

## ◆ GPIO_OTYPER_PxOTYP6_Msk

#define GPIO_OTYPER_PxOTYP6_Msk (0x40UL)

GPIO OTYPER: PxOTYP6 (Bitfield-Mask: 0x01)

## ◆ GPIO_OTYPER_PxOTYP6_Pos

#define GPIO_OTYPER_PxOTYP6_Pos (6UL)

GPIO OTYPER: PxOTYP6 (Bit 6)

## ◆ GPIO_OTYPER_PxOTYP7_Msk

#define GPIO_OTYPER_PxOTYP7_Msk (0x80UL)

GPIO OTYPER: PxOTYP7 (Bitfield-Mask: 0x01)

## ◆ GPIO_OTYPER_PxOTYP7_Pos

#define GPIO_OTYPER_PxOTYP7_Pos (7UL)

GPIO OTYPER: PxOTYP7 (Bit 7)

## ◆ GPIO_PUPDR_PxPUPD0_Msk

#define GPIO_PUPDR_PxPUPD0_Msk (0x3UL)

GPIO PUPDR: PxPUPD0 (Bitfield-Mask: 0x03)

## ◆ GPIO_PUPDR_PxPUPD0_Pos

#define GPIO_PUPDR_PxPUPD0_Pos (0UL)

GPIO PUPDR: PxPUPD0 (Bit 0)

## ◆ GPIO_PUPDR_PxPUPD1_Msk

#define GPIO_PUPDR_PxPUPD1_Msk (0xCUL)

GPIO PUPDR: PxPUPD1 (Bitfield-Mask: 0x03)

## ◆ GPIO_PUPDR_PxPUPD1_Pos

#define GPIO_PUPDR_PxPUPD1_Pos (2UL)

GPIO PUPDR: PxPUPD1 (Bit 2)

## ◆ GPIO_PUPDR_PxPUPD2_Msk

#define GPIO_PUPDR_PxPUPD2_Msk (0x30UL)

GPIO PUPDR: PxPUPD2 (Bitfield-Mask: 0x03)

## ◆ GPIO_PUPDR_PxPUPD2_Pos

#define GPIO_PUPDR_PxPUPD2_Pos (4UL)

GPIO PUPDR: PxPUPD2 (Bit 4)

## ◆ GPIO_PUPDR_PxPUPD3_Msk

#define GPIO_PUPDR_PxPUPD3_Msk (0xC0UL)

GPIO PUPDR: PxPUPD3 (Bitfield-Mask: 0x03)

## ◆ GPIO_PUPDR_PxPUPD3_Pos

#define GPIO_PUPDR_PxPUPD3_Pos (6UL)

GPIO PUPDR: PxPUPD3 (Bit 6)

## ◆ GPIO_PUPDR_PxPUPD4_Msk

#define GPIO_PUPDR_PxPUPD4_Msk (0x300UL)

GPIO PUPDR: PxPUPD4 (Bitfield-Mask: 0x03)

## ◆ GPIO_PUPDR_PxPUPD4_Pos

#define GPIO_PUPDR_PxPUPD4_Pos (8UL)

GPIO PUPDR: PxPUPD4 (Bit 8)

## ◆ GPIO_PUPDR_PxPUPD5_Msk

#define GPIO_PUPDR_PxPUPD5_Msk (0xC00UL)

GPIO PUPDR: PxPUPD5 (Bitfield-Mask: 0x03)

## ◆ GPIO_PUPDR_PxPUPD5_Pos

#define GPIO_PUPDR_PxPUPD5_Pos (10UL)

GPIO PUPDR: PxPUPD5 (Bit 10)

## ◆ GPIO_PUPDR_PxPUPD6_Msk

#define GPIO_PUPDR_PxPUPD6_Msk (0x3000UL)

GPIO PUPDR: PxPUPD6 (Bitfield-Mask: 0x03)

## ◆ GPIO_PUPDR_PxPUPD6_Pos

#define GPIO_PUPDR_PxPUPD6_Pos (12UL)

GPIO PUPDR: PxPUPD6 (Bit 12)

## ◆ GPIO_PUPDR_PxPUPD7_Msk

#define GPIO_PUPDR_PxPUPD7_Msk (0xC000UL)

GPIO PUPDR: PxPUPD7 (Bitfield-Mask: 0x03)

## ◆ GPIO_PUPDR_PxPUPD7_Pos

#define GPIO_PUPDR_PxPUPD7_Pos (14UL)

GPIO PUPDR: PxPUPD7 (Bit 14)

## ◆ GPIO_RAWINTST_PxRIS0_Msk

#define GPIO_RAWINTST_PxRIS0_Msk (0x1UL)

GPIO RAWINTST: PxRIS0 (Bitfield-Mask: 0x01)

## ◆ GPIO_RAWINTST_PxRIS0_Pos

#define GPIO_RAWINTST_PxRIS0_Pos (0UL)

GPIO RAWINTST: PxRIS0 (Bit 0)

## ◆ GPIO_RAWINTST_PxRIS1_Msk

#define GPIO_RAWINTST_PxRIS1_Msk (0x2UL)

GPIO RAWINTST: PxRIS1 (Bitfield-Mask: 0x01)

## ◆ GPIO_RAWINTST_PxRIS1_Pos

#define GPIO_RAWINTST_PxRIS1_Pos (1UL)

GPIO RAWINTST: PxRIS1 (Bit 1)

## ◆ GPIO_RAWINTST_PxRIS2_Msk

#define GPIO_RAWINTST_PxRIS2_Msk (0x4UL)

GPIO RAWINTST: PxRIS2 (Bitfield-Mask: 0x01)

## ◆ GPIO_RAWINTST_PxRIS2_Pos

#define GPIO_RAWINTST_PxRIS2_Pos (2UL)

GPIO RAWINTST: PxRIS2 (Bit 2)

## ◆ GPIO_RAWINTST_PxRIS3_Msk

#define GPIO_RAWINTST_PxRIS3_Msk (0x8UL)

GPIO RAWINTST: PxRIS3 (Bitfield-Mask: 0x01)

## ◆ GPIO_RAWINTST_PxRIS3_Pos

#define GPIO_RAWINTST_PxRIS3_Pos (3UL)

GPIO RAWINTST: PxRIS3 (Bit 3)

## ◆ GPIO_RAWINTST_PxRIS4_Msk

#define GPIO_RAWINTST_PxRIS4_Msk (0x10UL)

GPIO RAWINTST: PxRIS4 (Bitfield-Mask: 0x01)

## ◆ GPIO_RAWINTST_PxRIS4_Pos

#define GPIO_RAWINTST_PxRIS4_Pos (4UL)

GPIO RAWINTST: PxRIS4 (Bit 4)

## ◆ GPIO_RAWINTST_PxRIS5_Msk

#define GPIO_RAWINTST_PxRIS5_Msk (0x20UL)

GPIO RAWINTST: PxRIS5 (Bitfield-Mask: 0x01)

## ◆ GPIO_RAWINTST_PxRIS5_Pos

#define GPIO_RAWINTST_PxRIS5_Pos (5UL)

GPIO RAWINTST: PxRIS5 (Bit 5)

## ◆ GPIO_RAWINTST_PxRIS6_Msk

#define GPIO_RAWINTST_PxRIS6_Msk (0x40UL)

GPIO RAWINTST: PxRIS6 (Bitfield-Mask: 0x01)

## ◆ GPIO_RAWINTST_PxRIS6_Pos

#define GPIO_RAWINTST_PxRIS6_Pos (6UL)

GPIO RAWINTST: PxRIS6 (Bit 6)

## ◆ GPIO_RAWINTST_PxRIS7_Msk

#define GPIO_RAWINTST_PxRIS7_Msk (0x80UL)

GPIO RAWINTST: PxRIS7 (Bitfield-Mask: 0x01)

## ◆ GPIO_RAWINTST_PxRIS7_Pos

#define GPIO_RAWINTST_PxRIS7_Pos (7UL)

GPIO RAWINTST: PxRIS7 (Bit 7)

## ◆ GPIO_SLEWCR_PASR0_Msk

#define GPIO_SLEWCR_PASR0_Msk (0x1UL)

GPIO SLEWCR: PASR0 (Bitfield-Mask: 0x01)

## ◆ GPIO_SLEWCR_PASR0_Pos

#define GPIO_SLEWCR_PASR0_Pos (0UL)

GPIO SLEWCR: PASR0 (Bit 0)

## ◆ GPIO_SLEWCR_PxSR1_Msk

#define GPIO_SLEWCR_PxSR1_Msk (0x2UL)

GPIO SLEWCR: PxSR1 (Bitfield-Mask: 0x01)

## ◆ GPIO_SLEWCR_PxSR1_Pos

#define GPIO_SLEWCR_PxSR1_Pos (1UL)

GPIO SLEWCR: PxSR1 (Bit 1)

## ◆ GPIO_SLEWCR_PxSR2_Msk

#define GPIO_SLEWCR_PxSR2_Msk (0x4UL)

GPIO SLEWCR: PxSR2 (Bitfield-Mask: 0x01)

## ◆ GPIO_SLEWCR_PxSR2_Pos

#define GPIO_SLEWCR_PxSR2_Pos (2UL)

GPIO SLEWCR: PxSR2 (Bit 2)

## ◆ GPIO_SLEWCR_PxSR3_Msk

#define GPIO_SLEWCR_PxSR3_Msk (0x8UL)

GPIO SLEWCR: PxSR3 (Bitfield-Mask: 0x01)

## ◆ GPIO_SLEWCR_PxSR3_Pos

#define GPIO_SLEWCR_PxSR3_Pos (3UL)

GPIO SLEWCR: PxSR3 (Bit 3)

## ◆ GPIO_SLEWCR_PxSR4_Msk

#define GPIO_SLEWCR_PxSR4_Msk (0x10UL)

GPIO SLEWCR: PxSR4 (Bitfield-Mask: 0x01)

## ◆ GPIO_SLEWCR_PxSR4_Pos

#define GPIO_SLEWCR_PxSR4_Pos (4UL)

GPIO SLEWCR: PxSR4 (Bit 4)

## ◆ GPIO_SLEWCR_PxSR5_Msk

#define GPIO_SLEWCR_PxSR5_Msk (0x20UL)

GPIO SLEWCR: PxSR5 (Bitfield-Mask: 0x01)

## ◆ GPIO_SLEWCR_PxSR5_Pos

#define GPIO_SLEWCR_PxSR5_Pos (5UL)

GPIO SLEWCR: PxSR5 (Bit 5)

## ◆ GPIO_SLEWCR_PxSR6_Msk

#define GPIO_SLEWCR_PxSR6_Msk (0x40UL)

GPIO SLEWCR: PxSR6 (Bitfield-Mask: 0x01)

## ◆ GPIO_SLEWCR_PxSR6_Pos

#define GPIO_SLEWCR_PxSR6_Pos (6UL)

GPIO SLEWCR: PxSR6 (Bit 6)

## ◆ GPIO_SLEWCR_PxSR7_Msk

#define GPIO_SLEWCR_PxSR7_Msk (0x80UL)

GPIO SLEWCR: PxSR7 (Bitfield-Mask: 0x01)

## ◆ GPIO_SLEWCR_PxSR7_Pos

#define GPIO_SLEWCR_PxSR7_Pos (7UL)

GPIO SLEWCR: PxSR7 (Bit 7)

## ◆ HSE_VALUE

#define HSE_VALUE (24000000)

In the following line adjust the value of External High Speed oscillator (HSE) used in your application.

Tip: To avoid modifying this file each time you need to use different HSE, you can define the HSE value in your toolchain compiler preprocessor.Value of the External oscillator in Hz

## ◆ HSI_VALUE

#define HSI_VALUE (24000000)

In the following line adjust the value of External High Speed oscillator (HSI) used in your application.

Tip: To avoid modifying this file each time you need to use different HSI, you can define the HSI value in your toolchain compiler preprocessor.Value of the External oscillator in Hz

## ◆ I2C_ADDR_GC_Msk

#define I2C_ADDR_GC_Msk (0x1UL)

I2C ADDR: GC (Bitfield-Mask: 0x01)

## ◆ I2C_ADDR_GC_Pos

#define I2C_ADDR_GC_Pos (0UL)

I2C ADDR: GC (Bit 0)

## ◆ I2C_ADDR_I2CADR_Msk

#define I2C_ADDR_I2CADR_Msk (0xFEUL)

I2C ADDR: I2CADR (Bitfield-Mask: 0x7F)

## ◆ I2C_ADDR_I2CADR_Pos

#define I2C_ADDR_I2CADR_Pos (1UL)

I2C ADDR: I2CADR (Bit 1)

## ◆ I2C_BAUDCR_TM_Msk

#define I2C_BAUDCR_TM_Msk (0xFFUL)

I2C BAUDCR: TM (Bitfield-Mask: 0xFF)

## ◆ I2C_BAUDCR_TM_Pos

#define I2C_BAUDCR_TM_Pos (0UL)

I2C BAUDCR: TM (Bit 0)

## ◆ I2C_CR_AA_Msk

#define I2C_CR_AA_Msk (0x4UL)

I2C CR: AA (Bitfield-Mask: 0x01)

## ◆ I2C_CR_AA_Pos

#define I2C_CR_AA_Pos (2UL)

I2C CR: AA (Bit 2)

## ◆ I2C_CR_ENS_Msk

#define I2C_CR_ENS_Msk (0x40UL)

I2C CR: ENS (Bitfield-Mask: 0x01)

## ◆ I2C_CR_ENS_Pos

#define I2C_CR_ENS_Pos (6UL)

I2C CR: ENS (Bit 6)

## ◆ I2C_CR_H1M_Msk

#define I2C_CR_H1M_Msk (0x1UL)

I2C CR: H1M (Bitfield-Mask: 0x01)

## ◆ I2C_CR_H1M_Pos

#define I2C_CR_H1M_Pos (0UL)

I2C CR: H1M (Bit 0)

## ◆ I2C_CR_SI_Msk

#define I2C_CR_SI_Msk (0x8UL)

I2C CR: SI (Bitfield-Mask: 0x01)

## ◆ I2C_CR_SI_Pos

#define I2C_CR_SI_Pos (3UL)

I2C CR: SI (Bit 3)

## ◆ I2C_CR_STA_Msk

#define I2C_CR_STA_Msk (0x20UL)

I2C CR: STA (Bitfield-Mask: 0x01)

## ◆ I2C_CR_STA_Pos

#define I2C_CR_STA_Pos (5UL)

I2C CR: STA (Bit 5)

## ◆ I2C_CR_STO_Msk

#define I2C_CR_STO_Msk (0x10UL)

I2C CR: STO (Bitfield-Mask: 0x01)

## ◆ I2C_CR_STO_Pos

#define I2C_CR_STO_Pos (4UL)

I2C CR: STO (Bit 4)

## ◆ I2C_DATA_DAT_Msk

#define I2C_DATA_DAT_Msk (0xFFUL)

I2C DATA: DAT (Bitfield-Mask: 0xFF)

## ◆ I2C_DATA_DAT_Pos

#define I2C_DATA_DAT_Pos (0UL)

I2C DATA: DAT (Bit 0)

## ◆ I2C_SR_I2CSTA_Msk

#define I2C_SR_I2CSTA_Msk (0xFFUL)

I2C SR: I2CSTA (Bitfield-Mask: 0xFF)

## ◆ I2C_SR_I2CSTA_Pos

#define I2C_SR_I2CSTA_Pos (0UL)

I2C SR: I2CSTA (Bit 0)

## ◆ I2C_TIMRUN_TME_Msk

#define I2C_TIMRUN_TME_Msk (0x1UL)

I2C TIMRUN: TME (Bitfield-Mask: 0x01)

## ◆ I2C_TIMRUN_TME_Pos

#define I2C_TIMRUN_TME_Pos (0UL)

I2C TIMRUN: TME (Bit 0)

## ◆ IWDG_CFGR_IWDGINTMSK_Msk

#define IWDG_CFGR_IWDGINTMSK_Msk (0x2UL)

IWDG CFGR: IWDGINTMSK (Bitfield-Mask: 0x01)

## ◆ IWDG_CFGR_IWDGINTMSK_Pos

#define IWDG_CFGR_IWDGINTMSK_Pos (1UL)

IWDG CFGR: IWDGINTMSK (Bit 1)

## ◆ IWDG_CFGR_IWDGMODE_Msk

#define IWDG_CFGR_IWDGMODE_Msk (0x1UL)

IWDG CFGR: IWDGMODE (Bitfield-Mask: 0x01)

## ◆ IWDG_CFGR_IWDGMODE_Pos

#define IWDG_CFGR_IWDGMODE_Pos (0UL)

IWDG CFGR: IWDGMODE (Bit 0)

## ◆ IWDG_CFGR_IWDGRUNF_Msk

#define IWDG_CFGR_IWDGRUNF_Msk (0x4UL)

IWDG CFGR: IWDGRUNF (Bitfield-Mask: 0x01)

## ◆ IWDG_CFGR_IWDGRUNF_Pos

#define IWDG_CFGR_IWDGRUNF_Pos (2UL)

IWDG CFGR: IWDGRUNF (Bit 2)

## ◆ IWDG_CMDCR_CMD_Msk

#define IWDG_CMDCR_CMD_Msk (0xFFUL)

IWDG CMDCR: CMD (Bitfield-Mask: 0xFF)

## ◆ IWDG_CMDCR_CMD_Pos

#define IWDG_CMDCR_CMD_Pos (0UL)

IWDG CMDCR: CMD (Bit 0)

## ◆ IWDG_CNTVAL_IWDGCNT_Msk

#define IWDG_CNTVAL_IWDGCNT_Msk (0xFFFFFUL)

IWDG CNTVAL: IWDGCNT (Bitfield-Mask: 0xFFFFF)

## ◆ IWDG_CNTVAL_IWDGCNT_Pos

#define IWDG_CNTVAL_IWDGCNT_Pos (0UL)

IWDG CNTVAL: IWDGCNT (Bit 0)

## ◆ IWDG_INTCLR_IWDGINTCLR_Msk

#define IWDG_INTCLR_IWDGINTCLR_Msk (0x1UL)

IWDG INTCLR: IWDGINTCLR (Bitfield-Mask: 0x01)

## ◆ IWDG_INTCLR_IWDGINTCLR_Pos

#define IWDG_INTCLR_IWDGINTCLR_Pos (0UL)

IWDG INTCLR: IWDGINTCLR (Bit 0)

## ◆ IWDG_RLOAD_IWDGRLOAD_Msk

#define IWDG_RLOAD_IWDGRLOAD_Msk (0xFFFFFUL)

IWDG RLOAD: IWDGRLOAD (Bitfield-Mask: 0xFFFFF)

## ◆ IWDG_RLOAD_IWDGRLOAD_Pos

#define IWDG_RLOAD_IWDGRLOAD_Pos (0UL)

IWDG RLOAD: IWDGRLOAD (Bit 0)

## ◆ IWDG_SR_IWDGOVF_Msk

#define IWDG_SR_IWDGOVF_Msk (0x1UL)

IWDG SR: IWDGOVF (Bitfield-Mask: 0x01)

## ◆ IWDG_SR_IWDGOVF_Pos

#define IWDG_SR_IWDGOVF_Pos (0UL)

IWDG SR: IWDGOVF (Bit 0)

## ◆ IWDG_UNLOCK_IWDGREN_Msk

#define IWDG_UNLOCK_IWDGREN_Msk (0x1UL)

IWDG UNLOCK: IWDGREN (Bitfield-Mask: 0x01)

## ◆ IWDG_UNLOCK_IWDGREN_Pos

#define IWDG_UNLOCK_IWDGREN_Pos (0UL)

IWDG UNLOCK: IWDGREN (Bit 0)

## ◆ LPTIM_BGLOAD_BGLOAD_Msk

#define LPTIM_BGLOAD_BGLOAD_Msk (0xFFFFUL)

LPTIM BGLOAD: BGLOAD (Bitfield-Mask: 0xFFFF)

## ◆ LPTIM_BGLOAD_BGLOAD_Pos

#define LPTIM_BGLOAD_BGLOAD_Pos (0UL)

LPTIM BGLOAD: BGLOAD (Bit 0)

## ◆ LPTIM_CNTVAL_LPT_CNT_Msk

#define LPTIM_CNTVAL_LPT_CNT_Msk (0x1UL)

LPTIM CNTVAL: LPT_CNT (Bitfield-Mask: 0x01)

## ◆ LPTIM_CNTVAL_LPT_CNT_Pos

#define LPTIM_CNTVAL_LPT_CNT_Pos (0UL)

LPTIM CNTVAL: LPT_CNT (Bit 0)

## ◆ LPTIM_CR_ALL_Msk

#define LPTIM_CR_ALL_Msk (0x3FFUL)

LPTIM CR: ALL (Bitfield-Mask: 0x3FF)

## ◆ LPTIM_CR_CT_SEL_Msk

#define LPTIM_CR_CT_SEL_Msk (0x4UL)

LPTIM CR: CT_SEL (Bitfield-Mask: 0x01)

## ◆ LPTIM_CR_CT_SEL_Pos

#define LPTIM_CR_CT_SEL_Pos (2UL)

LPTIM CR: CT_SEL (Bit 2)

## ◆ LPTIM_CR_GATE_EN_Msk

#define LPTIM_CR_GATE_EN_Msk (0x40UL)

LPTIM CR: GATE_EN (Bitfield-Mask: 0x01)

## ◆ LPTIM_CR_GATE_EN_Pos

#define LPTIM_CR_GATE_EN_Pos (6UL)

LPTIM CR: GATE_EN (Bit 6)

## ◆ LPTIM_CR_GATE_P_Msk

#define LPTIM_CR_GATE_P_Msk (0x80UL)

LPTIM CR: GATE_P (Bitfield-Mask: 0x01)

## ◆ LPTIM_CR_GATE_P_Pos

#define LPTIM_CR_GATE_P_Pos (7UL)

LPTIM CR: GATE_P (Bit 7)

## ◆ LPTIM_CR_INT_EN_Msk

#define LPTIM_CR_INT_EN_Msk (0x100UL)

LPTIM CR: INT_EN (Bitfield-Mask: 0x01)

## ◆ LPTIM_CR_INT_EN_Pos

#define LPTIM_CR_INT_EN_Pos (8UL)

LPTIM CR: INT_EN (Bit 8)

## ◆ LPTIM_CR_MODE_Msk

#define LPTIM_CR_MODE_Msk (0x2UL)

LPTIM CR: MODE (Bitfield-Mask: 0x01)

## ◆ LPTIM_CR_MODE_Pos

#define LPTIM_CR_MODE_Pos (1UL)

LPTIM CR: MODE (Bit 1)

## ◆ LPTIM_CR_TCK_EN_Msk

#define LPTIM_CR_TCK_EN_Msk (0x200UL)

LPTIM CR: TCK_EN (Bitfield-Mask: 0x01)

## ◆ LPTIM_CR_TCK_EN_Pos

#define LPTIM_CR_TCK_EN_Pos (9UL)

LPTIM CR: TCK_EN (Bit 9)

## ◆ LPTIM_CR_TCK_SEL_Msk

#define LPTIM_CR_TCK_SEL_Msk (0x30UL)

LPTIM CR: TCK_SEL (Bitfield-Mask: 0x03)

## ◆ LPTIM_CR_TCK_SEL_Pos

#define LPTIM_CR_TCK_SEL_Pos (4UL)

LPTIM CR: TCK_SEL (Bit 4)

## ◆ LPTIM_CR_TIM_RUN_Msk

#define LPTIM_CR_TIM_RUN_Msk (0x1UL)

LPTIM CR: TIM_RUN (Bitfield-Mask: 0x01)

## ◆ LPTIM_CR_TIM_RUN_Pos

#define LPTIM_CR_TIM_RUN_Pos (0UL)

LPTIM CR: TIM_RUN (Bit 0)

## ◆ LPTIM_CR_TOG_EN_Msk

#define LPTIM_CR_TOG_EN_Msk (0x8UL)

LPTIM CR: TOG_EN (Bitfield-Mask: 0x01)

## ◆ LPTIM_CR_TOG_EN_Pos

#define LPTIM_CR_TOG_EN_Pos (3UL)

LPTIM CR: TOG_EN (Bit 3)

## ◆ LPTIM_CR_WT_FLAG_Msk

#define LPTIM_CR_WT_FLAG_Msk (0x10000UL)

LPTIM CR: WT_FLAG (Bitfield-Mask: 0x01)

## ◆ LPTIM_CR_WT_FLAG_Pos

#define LPTIM_CR_WT_FLAG_Pos (16UL)

LPTIM CR: WT_FLAG (Bit 16)

## ◆ LPTIM_INTCLR_ICLR_Msk

#define LPTIM_INTCLR_ICLR_Msk (0x1UL)

LPTIM INTCLR: ICLR (Bitfield-Mask: 0x01)

## ◆ LPTIM_INTCLR_ICLR_Pos

#define LPTIM_INTCLR_ICLR_Pos (0UL)

LPTIM INTCLR: ICLR (Bit 0)

## ◆ LPTIM_INTSR_INTF_Msk

#define LPTIM_INTSR_INTF_Msk (0x01UL)

LPTIM INTSR: INTF (Bitfield-Mask: 0x01)

## ◆ LPTIM_INTSR_INTF_Pos

#define LPTIM_INTSR_INTF_Pos (0UL)

LPTIM INTSR: INTF (Bit 0)

## ◆ LPTIM_LOAD_LOAD_Msk

#define LPTIM_LOAD_LOAD_Msk (0xFFFFUL)

LPTIM LOAD: LOAD (Bitfield-Mask: 0xFFFF)

## ◆ LPTIM_LOAD_LOAD_Pos

#define LPTIM_LOAD_LOAD_Pos (0UL)

LPTIM LOAD: LOAD (Bit 0)

## ◆ LPUART_BAUDCR_BRG_Msk

#define LPUART_BAUDCR_BRG_Msk (0xFFFFUL)

LPUART BAUDCR: BRG (Bitfield-Mask: 0xFFFF)

## ◆ LPUART_BAUDCR_BRG_Pos

#define LPUART_BAUDCR_BRG_Pos (0UL)

LPUART BAUDCR: BRG (Bit 0)

## ◆ LPUART_BAUDCR_SELF_BRG_Msk

#define LPUART_BAUDCR_SELF_BRG_Msk (0x10000UL)

LPUART BAUDCR: SELF_BRG (Bitfield-Mask: 0x01)

## ◆ LPUART_BAUDCR_SELF_BRG_Pos

#define LPUART_BAUDCR_SELF_BRG_Pos (16UL)

LPUART BAUDCR: SELF_BRG (Bit 16)

## ◆ LPUART_INTCLR_FECLR_Msk

#define LPUART_INTCLR_FECLR_Msk (0x4UL)

LPUART INTCLR: FECLR (Bitfield-Mask: 0x01)

## ◆ LPUART_INTCLR_FECLR_Pos

#define LPUART_INTCLR_FECLR_Pos (2UL)

LPUART INTCLR: FECLR (Bit 2)

## ◆ LPUART_INTCLR_RICLR_Msk

#define LPUART_INTCLR_RICLR_Msk (0x1UL)

LPUART INTCLR: RICLR (Bitfield-Mask: 0x01)

## ◆ LPUART_INTCLR_RICLR_Pos

#define LPUART_INTCLR_RICLR_Pos (0UL)

LPUART INTCLR: RICLR (Bit 0)

## ◆ LPUART_INTCLR_TICLR_Msk

#define LPUART_INTCLR_TICLR_Msk (0x2UL)

LPUART INTCLR: TICLR (Bitfield-Mask: 0x01)

## ◆ LPUART_INTCLR_TICLR_Pos

#define LPUART_INTCLR_TICLR_Pos (1UL)

LPUART INTCLR: TICLR (Bit 1)

## ◆ LPUART_INTSR_FE_Msk

#define LPUART_INTSR_FE_Msk (0x4UL)

LPUART INTSR: FE (Bitfield-Mask: 0x01)

## ◆ LPUART_INTSR_FE_Pos

#define LPUART_INTSR_FE_Pos (2UL)

LPUART INTSR: FE (Bit 2)

## ◆ LPUART_INTSR_RI_Msk

#define LPUART_INTSR_RI_Msk (0x1UL)

LPUART INTSR: RI (Bitfield-Mask: 0x01)

## ◆ LPUART_INTSR_RI_Pos

#define LPUART_INTSR_RI_Pos (0UL)

LPUART INTSR: RI (Bit 0)

## ◆ LPUART_INTSR_TI_Msk

#define LPUART_INTSR_TI_Msk (0x2UL)

LPUART INTSR: TI (Bitfield-Mask: 0x01)

## ◆ LPUART_INTSR_TI_Pos

#define LPUART_INTSR_TI_Pos (1UL)

LPUART INTSR: TI (Bit 1)

## ◆ LPUART_SADDR_SADDR_Msk

#define LPUART_SADDR_SADDR_Msk (0xFFUL)

LPUART SADDR: SADDR (Bitfield-Mask: 0xFF)

## ◆ LPUART_SADDR_SADDR_Pos

#define LPUART_SADDR_SADDR_Pos (0UL)

LPUART SADDR: SADDR (Bit 0)

## ◆ LPUART_SADEN_SADEN_Msk

#define LPUART_SADEN_SADEN_Msk (0xFFUL)

LPUART SADEN: SADEN (Bitfield-Mask: 0xFF)

## ◆ LPUART_SADEN_SADEN_Pos

#define LPUART_SADEN_SADEN_Pos (0UL)

LPUART SADEN: SADEN (Bit 0)

## ◆ LPUART_SBUF_SBUF_Msk

#define LPUART_SBUF_SBUF_Msk (0xFFUL)

LPUART SBUF: SBUF (Bitfield-Mask: 0xFF)

## ◆ LPUART_SBUF_SBUF_Pos

#define LPUART_SBUF_SBUF_Pos (0UL)

LPUART SBUF: SBUF (Bit 0)

## ◆ LPUART_SCON_DBAUD_Msk

#define LPUART_SCON_DBAUD_Msk (0x200UL)

LPUART SCON: DBAUD (Bitfield-Mask: 0x01)

## ◆ LPUART_SCON_DBAUD_Pos

#define LPUART_SCON_DBAUD_Pos (9UL)

LPUART SCON: DBAUD (Bit 9)

## ◆ LPUART_SCON_EN_Msk

#define LPUART_SCON_EN_Msk (0x10000UL)

LPUART SCON: EN (Bitfield-Mask: 0x01)

## ◆ LPUART_SCON_EN_Pos

#define LPUART_SCON_EN_Pos (16UL)

LPUART SCON: EN (Bit 16)

## ◆ LPUART_SCON_LPMODE_Msk

#define LPUART_SCON_LPMODE_Msk (0x400UL)

LPUART SCON: LPMODE (Bitfield-Mask: 0x01)

## ◆ LPUART_SCON_LPMODE_Pos

#define LPUART_SCON_LPMODE_Pos (10UL)

LPUART SCON: LPMODE (Bit 10)

## ◆ LPUART_SCON_PRSC_Msk

#define LPUART_SCON_PRSC_Msk (0xE000UL)

LPUART SCON: PRSC (Bitfield-Mask: 0x07)

## ◆ LPUART_SCON_PRSC_Pos

#define LPUART_SCON_PRSC_Pos (13UL)

LPUART SCON: PRSC (Bit 13)

## ◆ LPUART_SCON_RB8_Msk

#define LPUART_SCON_RB8_Msk (0x4UL)

LPUART SCON: RB8 (Bitfield-Mask: 0x01)

## ◆ LPUART_SCON_RB8_Pos

#define LPUART_SCON_RB8_Pos (2UL)

LPUART SCON: RB8 (Bit 2)

## ◆ LPUART_SCON_REN_Msk

#define LPUART_SCON_REN_Msk (0x10UL)

LPUART SCON: REN (Bitfield-Mask: 0x01)

## ◆ LPUART_SCON_REN_Pos

#define LPUART_SCON_REN_Pos (4UL)

LPUART SCON: REN (Bit 4)

## ◆ LPUART_SCON_RIEN_Msk

#define LPUART_SCON_RIEN_Msk (0x1UL)

LPUART SCON: RIEN (Bitfield-Mask: 0x01)

## ◆ LPUART_SCON_RIEN_Pos

#define LPUART_SCON_RIEN_Pos (0UL)

LPUART SCON: RIEN (Bit 0)

## ◆ LPUART_SCON_SCLKSEL_Msk

#define LPUART_SCON_SCLKSEL_Msk (0x1800UL)

LPUART SCON: SCLKSEL (Bitfield-Mask: 0x03)

## ◆ LPUART_SCON_SCLKSEL_Pos

#define LPUART_SCON_SCLKSEL_Pos (11UL)

LPUART SCON: SCLKSEL (Bit 11)

## ◆ LPUART_SCON_SM0_SM1_Msk

#define LPUART_SCON_SM0_SM1_Msk (0x40UL)

LPUART SCON: SM0_SM1 (Bitfield-Mask: 0x01)

## ◆ LPUART_SCON_SM0_SM1_Pos

#define LPUART_SCON_SM0_SM1_Pos (6UL)

LPUART SCON: SM0_SM1 (Bit 6)

## ◆ LPUART_SCON_SM2_Msk

#define LPUART_SCON_SM2_Msk (0x20UL)

LPUART SCON: SM2 (Bitfield-Mask: 0x01)

## ◆ LPUART_SCON_SM2_Pos

#define LPUART_SCON_SM2_Pos (5UL)

LPUART SCON: SM2 (Bit 5)

## ◆ LPUART_SCON_TB8_Msk

#define LPUART_SCON_TB8_Msk (0x8UL)

LPUART SCON: TB8 (Bitfield-Mask: 0x01)

## ◆ LPUART_SCON_TB8_Pos

#define LPUART_SCON_TB8_Pos (3UL)

LPUART SCON: TB8 (Bit 3)

## ◆ LPUART_SCON_TEEN_Msk

#define LPUART_SCON_TEEN_Msk (0x100UL)

LPUART SCON: TEEN (Bitfield-Mask: 0x01)

## ◆ LPUART_SCON_TEEN_Pos

#define LPUART_SCON_TEEN_Pos (8UL)

LPUART SCON: TEEN (Bit 8)

## ◆ LPUART_SCON_TIEN_Msk

#define LPUART_SCON_TIEN_Msk (0x2UL)

LPUART SCON: TIEN (Bitfield-Mask: 0x01)

## ◆ LPUART_SCON_TIEN_Pos

#define LPUART_SCON_TIEN_Pos (1UL)

LPUART SCON: TIEN (Bit 1)

## ◆ LSE_VALUE

#define LSE_VALUE (32768)

In the following line adjust the value of External High Speed oscillator (LSE) used in your application.

Tip: To avoid modifying this file each time you need to use different LSE, you can define the LSE value in your toolchain compiler preprocessor.Value of the External oscillator in Hz

## ◆ LSI_VALUE

#define LSI_VALUE (32768)

In the following line adjust the value of External High Speed oscillator (LSI) used in your application.

Tip: To avoid modifying this file each time you need to use different LSI, you can define the LSI value in your toolchain compiler preprocessor.Value of the External oscillator in Hz

## ◆ LVD_CR_ACT_Msk

#define LVD_CR_ACT_Msk (0x40UL)

LVD CR: ACT (Bitfield-Mask: 0x01)

## ◆ LVD_CR_ACT_Pos

#define LVD_CR_ACT_Pos (6UL)

LVD CR: ACT (Bit 6)

## ◆ LVD_CR_DIV_SEL_Msk

#define LVD_CR_DIV_SEL_Msk (0xFUL)

LVD CR: DIV_SEL (Bitfield-Mask: 0x0F)

## ◆ LVD_CR_DIV_SEL_Pos

#define LVD_CR_DIV_SEL_Pos (0UL)

LVD CR: DIV_SEL (Bit 0)

## ◆ LVD_CR_FALLINTEN_Msk

#define LVD_CR_FALLINTEN_Msk (0x1000UL)

LVD CR: FALLINTEN (Bitfield-Mask: 0x01)

## ◆ LVD_CR_FALLINTEN_Pos

#define LVD_CR_FALLINTEN_Pos (12UL)

LVD CR: FALLINTEN (Bit 12)

## ◆ LVD_CR_FLT_NUM_Msk

#define LVD_CR_FLT_NUM_Msk (0xFFFF0000UL)

LVD CR: FLT_NUM (Bitfield-Mask: 0xFFFF)

## ◆ LVD_CR_FLT_NUM_Pos

#define LVD_CR_FLT_NUM_Pos (16UL)

LVD CR: FLT_NUM (Bit 16)

## ◆ LVD_CR_FLTCLK_SEL_Msk

#define LVD_CR_FLTCLK_SEL_Msk (0x300UL)

LVD CR: FLTCLK_SEL (Bitfield-Mask: 0x03)

## ◆ LVD_CR_FLTCLK_SEL_Pos

#define LVD_CR_FLTCLK_SEL_Pos (8UL)

LVD CR: FLTCLK_SEL (Bit 8)

## ◆ LVD_CR_FLTEN_Msk

#define LVD_CR_FLTEN_Msk (0x80UL)

LVD CR: FLTEN (Bitfield-Mask: 0x01)

## ◆ LVD_CR_FLTEN_Pos

#define LVD_CR_FLTEN_Pos (7UL)

LVD CR: FLTEN (Bit 7)

## ◆ LVD_CR_HIGHINTEN_Msk

#define LVD_CR_HIGHINTEN_Msk (0x4000UL)

LVD CR: HIGHINTEN (Bitfield-Mask: 0x01)

## ◆ LVD_CR_HIGHINTEN_Pos

#define LVD_CR_HIGHINTEN_Pos (14UL)

LVD CR: HIGHINTEN (Bit 14)

## ◆ LVD_CR_INT_EN_Msk

#define LVD_CR_INT_EN_Msk (0x8000UL)

LVD CR: INT_EN (Bitfield-Mask: 0x01)

## ◆ LVD_CR_INT_EN_Pos

#define LVD_CR_INT_EN_Pos (15UL)

LVD CR: INT_EN (Bit 15)

## ◆ LVD_CR_LVDEN_Msk

#define LVD_CR_LVDEN_Msk (0x20UL)

LVD CR: LVDEN (Bitfield-Mask: 0x01)

## ◆ LVD_CR_LVDEN_Pos

#define LVD_CR_LVDEN_Pos (5UL)

LVD CR: LVDEN (Bit 5)

## ◆ LVD_CR_RISEINTEN_Msk

#define LVD_CR_RISEINTEN_Msk (0x2000UL)

LVD CR: RISEINTEN (Bitfield-Mask: 0x01)

## ◆ LVD_CR_RISEINTEN_Pos

#define LVD_CR_RISEINTEN_Pos (13UL)

LVD CR: RISEINTEN (Bit 13)

## ◆ LVD_SR_INTF_Msk

#define LVD_SR_INTF_Msk (0x1UL)

LVD SR: INTF (Bitfield-Mask: 0x01)

## ◆ LVD_SR_INTF_Pos

#define LVD_SR_INTF_Pos (0UL)

LVD SR: INTF (Bit 0)

## ◆ OWIRE_BITRATECNT_BITRATECNT_Msk

#define OWIRE_BITRATECNT_BITRATECNT_Msk (0xFFFUL)

OWIRE BITRATECNT: BITRATECNT (Bitfield-Mask: 0xFFF)

## ◆ OWIRE_BITRATECNT_BITRATECNT_Pos

#define OWIRE_BITRATECNT_BITRATECNT_Pos (0UL)

OWIRE BITRATECNT: BITRATECNT (Bit 0)

## ◆ OWIRE_CMD_CMD_Msk

#define OWIRE_CMD_CMD_Msk (0x3UL)

OWIRE CMD: CMD (Bitfield-Mask: 0x03)

## ◆ OWIRE_CMD_CMD_Pos

#define OWIRE_CMD_CMD_Pos (0UL)

OWIRE CMD: CMD (Bit 0)

## ◆ OWIRE_CR_CLKDIV_Msk

#define OWIRE_CR_CLKDIV_Msk (0x3UL)

OWIRE CR: CLKDIV (Bitfield-Mask: 0x03)

## ◆ OWIRE_CR_CLKDIV_Pos

#define OWIRE_CR_CLKDIV_Pos (0UL)

OWIRE CR: CLKDIV (Bit 0)

## ◆ OWIRE_CR_EN_Msk

#define OWIRE_CR_EN_Msk (0x20UL)

OWIRE CR: EN (Bitfield-Mask: 0x01)

## ◆ OWIRE_CR_EN_Pos

#define OWIRE_CR_EN_Pos (5UL)

OWIRE CR: EN (Bit 5)

## ◆ OWIRE_CR_MSBFIRST_Msk

#define OWIRE_CR_MSBFIRST_Msk (0x40UL)

OWIRE CR: MSBRIRST (Bitfield-Mask: 0x01)

## ◆ OWIRE_CR_MSBFIRST_Pos

#define OWIRE_CR_MSBFIRST_Pos (6UL)

OWIRE CR: MSBRIRST (Bit 6)

## ◆ OWIRE_CR_RDMODE_Msk

#define OWIRE_CR_RDMODE_Msk (0x80UL)

OWIRE CR: RDMODE (Bitfield-Mask: 0x01)

## ◆ OWIRE_CR_RDMODE_Pos

#define OWIRE_CR_RDMODE_Pos (7UL)

OWIRE CR: RDMODE (Bit 7)

## ◆ OWIRE_CR_SIZE_Msk

#define OWIRE_CR_SIZE_Msk (0x10UL)

OWIRE CR: SIZE (Bitfield-Mask: 0x01)

## ◆ OWIRE_CR_SIZE_Pos

#define OWIRE_CR_SIZE_Pos (4UL)

OWIRE CR: SIZE (Bit 4)

## ◆ OWIRE_DATA_DRVCNT_Msk

#define OWIRE_DATA_DRVCNT_Msk (0xFFUL)

OWIRE DATA: DRVCNT (Bitfield-Mask: 0xFF)

## ◆ OWIRE_DATA_DRVCNT_Pos

#define OWIRE_DATA_DRVCNT_Pos (0UL)

OWIRE DATA: DRVCNT (Bit 0)

## ◆ OWIRE_DRVCNT_DRVCNT_Msk

#define OWIRE_DRVCNT_DRVCNT_Msk (0x1FFUL)

OWIRE DRVCNT: DRVCNT (Bitfield-Mask: 0x1FF)

## ◆ OWIRE_DRVCNT_DRVCNT_Pos

#define OWIRE_DRVCNT_DRVCNT_Pos (0UL)

OWIRE DRVCNT: DRVCNT (Bit 0)

## ◆ OWIRE_INTCLR_ACKERRCLR_Msk

#define OWIRE_INTCLR_ACKERRCLR_Msk (0x1UL)

OWIRE INTCLR: ACKERRCLR (Bitfield-Mask: 0x01)

## ◆ OWIRE_INTCLR_ACKERRCLR_Pos

#define OWIRE_INTCLR_ACKERRCLR_Pos (0UL)

OWIRE INTCLR: ACKERRCLR (Bit 0)

## ◆ OWIRE_INTCLR_INTDONCECLR_Msk

#define OWIRE_INTCLR_INTDONCECLR_Msk (0x2UL)

OWIRE INTCLR: INTDONCECLR (Bitfield-Mask: 0x01)

## ◆ OWIRE_INTCLR_INTDONCECLR_Pos

#define OWIRE_INTCLR_INTDONCECLR_Pos (1UL)

OWIRE INTCLR: INTDONCECLR (Bit 1)

## ◆ OWIRE_INTCLR_RXDONECLR_Msk

#define OWIRE_INTCLR_RXDONECLR_Msk (0x8UL)

OWIRE INTCLR: RXDONECLR (Bitfield-Mask: 0x01)

## ◆ OWIRE_INTCLR_RXDONECLR_Pos

#define OWIRE_INTCLR_RXDONECLR_Pos (3UL)

OWIRE INTCLR: RXDONECLR (Bit 3)

## ◆ OWIRE_INTCLR_TXDONECLR_Msk

#define OWIRE_INTCLR_TXDONECLR_Msk (0x4UL)

OWIRE INTCLR: TXDONECLR (Bitfield-Mask: 0x01)

## ◆ OWIRE_INTCLR_TXDONECLR_Pos

#define OWIRE_INTCLR_TXDONECLR_Pos (2UL)

OWIRE INTCLR: TXDONECLR (Bit 2)

## ◆ OWIRE_INTEN_ACKERREN_Msk

#define OWIRE_INTEN_ACKERREN_Msk (0x1UL)

OWIRE INTEN: ACKERREN (Bitfield-Mask: 0x01)

## ◆ OWIRE_INTEN_ACKERREN_Pos

#define OWIRE_INTEN_ACKERREN_Pos (0UL)

OWIRE INTEN: ACKERREN (Bit 0)

## ◆ OWIRE_INTEN_INITEN_Msk

#define OWIRE_INTEN_INITEN_Msk (0x2UL)

OWIRE INTEN: INITEN (Bitfield-Mask: 0x01)

## ◆ OWIRE_INTEN_INITEN_Pos

#define OWIRE_INTEN_INITEN_Pos (1UL)

OWIRE INTEN: INITEN (Bit 1)

## ◆ OWIRE_INTEN_RXDONEEN_Msk

#define OWIRE_INTEN_RXDONEEN_Msk (0x8UL)

OWIRE INTEN: RXDONEEN (Bitfield-Mask: 0x01)

## ◆ OWIRE_INTEN_RXDONEEN_Pos

#define OWIRE_INTEN_RXDONEEN_Pos (3UL)

OWIRE INTEN: RXDONEEN (Bit 3)

## ◆ OWIRE_INTEN_TXDONEEN_Msk

#define OWIRE_INTEN_TXDONEEN_Msk (0x4UL)

OWIRE INTEN: TXDONEEN (Bitfield-Mask: 0x01)

## ◆ OWIRE_INTEN_TXDONEEN_Pos

#define OWIRE_INTEN_TXDONEEN_Pos (2UL)

OWIRE INTEN: TXDONEEN (Bit 2)

## ◆ OWIRE_NFCR_NFDIV_Msk

#define OWIRE_NFCR_NFDIV_Msk (0x3UL)

OWIRE NFCR: NFDIV (Bitfield-Mask: 0x03)

## ◆ OWIRE_NFCR_NFDIV_Pos

#define OWIRE_NFCR_NFDIV_Pos (0UL)

OWIRE NFCR: NFDIV (Bit 0)

## ◆ OWIRE_NFCR_NFEN_Msk

#define OWIRE_NFCR_NFEN_Msk (0x10UL)

OWIRE NFCR: NFEN (Bitfield-Mask: 0x01)

## ◆ OWIRE_NFCR_NFEN_Pos

#define OWIRE_NFCR_NFEN_Pos (4UL)

OWIRE NFCR: NFEN (Bit 4)

## ◆ OWIRE_PRESCNT_PRESCNT_Msk

#define OWIRE_PRESCNT_PRESCNT_Msk (0x1FFFUL)

OWIRE PRESCNT: PRESCNT (Bitfield-Mask: 0x1FFF)

## ◆ OWIRE_PRESCNT_PRESCNT_Pos

#define OWIRE_PRESCNT_PRESCNT_Pos (0UL)

OWIRE PRESCNT: PRESCNT (Bit 0)

## ◆ OWIRE_RDSMPCNT_RDSMPCNT_Msk

#define OWIRE_RDSMPCNT_RDSMPCNT_Msk (0x1FFUL)

OWIRE RDSMPCNT: RDSMPCNT (Bitfield-Mask: 0x1FF)

## ◆ OWIRE_RDSMPCNT_RDSMPCNT_Pos

#define OWIRE_RDSMPCNT_RDSMPCNT_Pos (0UL)

OWIRE RDSMPCNT: RDSMPCNT (Bit 0)

## ◆ OWIRE_RECCNT_RECCNT_Msk

#define OWIRE_RECCNT_RECCNT_Msk (0x7FFUL)

OWIRE RECCNT: RECCNT (Bitfield-Mask: 0x7FF)

## ◆ OWIRE_RECCNT_RECCNT_Pos

#define OWIRE_RECCNT_RECCNT_Pos (0UL)

OWIRE RECCNT: RECCNT (Bit 0)

## ◆ OWIRE_RSTCNT_RSTCNT_Msk

#define OWIRE_RSTCNT_RSTCNT_Msk (0xFFFFUL)

OWIRE RSTCNT: RSTCNT (Bitfield-Mask: 0xFFFF)

## ◆ OWIRE_RSTCNT_RSTCNT_Pos

#define OWIRE_RSTCNT_RSTCNT_Pos (0UL)

OWIRE RSTCNT: RSTCNT (Bit 0)

## ◆ OWIRE_SR_ACKERR_Msk

#define OWIRE_SR_ACKERR_Msk (0x1UL)

OWIRE SR: ACKERR (Bitfield-Mask: 0x01)

## ◆ OWIRE_SR_ACKERR_Pos

#define OWIRE_SR_ACKERR_Pos (0UL)

OWIRE SR: ACKERR (Bit 0)

## ◆ OWIRE_SR_INITDONE_Msk

#define OWIRE_SR_INITDONE_Msk (0x2UL)

OWIRE SR: INITDONE (Bitfield-Mask: 0x01)

## ◆ OWIRE_SR_INITDONE_Pos

#define OWIRE_SR_INITDONE_Pos (1UL)

OWIRE SR: INITDONE (Bit 1)

## ◆ OWIRE_SR_RXDONE_Msk

#define OWIRE_SR_RXDONE_Msk (0x8UL)

OWIRE SR: RXDONE (Bitfield-Mask: 0x01)

## ◆ OWIRE_SR_RXDONE_Pos

#define OWIRE_SR_RXDONE_Pos (3UL)

OWIRE SR: RXDONE (Bit 3)

## ◆ OWIRE_SR_TXDONE_Msk

#define OWIRE_SR_TXDONE_Msk (0x4UL)

OWIRE SR: TXDONE (Bitfield-Mask: 0x01)

## ◆ OWIRE_SR_TXDONE_Pos

#define OWIRE_SR_TXDONE_Pos (2UL)

OWIRE SR: TXDONE (Bit 2)

## ◆ PCA_CCAP0_CCAP0_Msk

#define PCA_CCAP0_CCAP0_Msk (0xFFFFUL)

PCA CCAP0: CCAP0 (Bitfield-Mask: 0xFFFF)

## ◆ PCA_CCAP0_CCAP0_Pos

#define PCA_CCAP0_CCAP0_Pos (0UL)

PCA CCAP0: CCAP0 (Bit 0)

## ◆ PCA_CCAP0H_CCAP0_Msk

#define PCA_CCAP0H_CCAP0_Msk (0xFF00UL)

PCA CCAP0H: CCAP0 (Bitfield-Mask: 0xFF)

## ◆ PCA_CCAP0H_CCAP0_Pos

#define PCA_CCAP0H_CCAP0_Pos (8UL)

PCA CCAP0H: CCAP0 (Bit 8)

## ◆ PCA_CCAP0L_CCAP0_Msk

#define PCA_CCAP0L_CCAP0_Msk (0xFFUL)

PCA CCAP0L: CCAP0 (Bitfield-Mask: 0xFF)

## ◆ PCA_CCAP0L_CCAP0_Pos

#define PCA_CCAP0L_CCAP0_Pos (0UL)

PCA CCAP0L: CCAP0 (Bit 0)

## ◆ PCA_CCAP1_CCAP1_Msk

#define PCA_CCAP1_CCAP1_Msk (0xFFFFUL)

PCA CCAP1: CCAP1 (Bitfield-Mask: 0xFFFF)

## ◆ PCA_CCAP1_CCAP1_Pos

#define PCA_CCAP1_CCAP1_Pos (0UL)

PCA CCAP1: CCAP1 (Bit 0)

## ◆ PCA_CCAP1H_CCAP1_Msk

#define PCA_CCAP1H_CCAP1_Msk (0xFF00UL)

PCA CCAP1H: CCAP1 (Bitfield-Mask: 0xFF)

## ◆ PCA_CCAP1H_CCAP1_Pos

#define PCA_CCAP1H_CCAP1_Pos (8UL)

PCA CCAP1H: CCAP1 (Bit 8)

## ◆ PCA_CCAP1L_CCAP1_Msk

#define PCA_CCAP1L_CCAP1_Msk (0xFFUL)

PCA CCAP1L: CCAP1 (Bitfield-Mask: 0xFF)

## ◆ PCA_CCAP1L_CCAP1_Pos

#define PCA_CCAP1L_CCAP1_Pos (0UL)

PCA CCAP1L: CCAP1 (Bit 0)

## ◆ PCA_CCAP2_CCAP2_Msk

#define PCA_CCAP2_CCAP2_Msk (0xFFFFUL)

PCA CCAP2: CCAP2 (Bitfield-Mask: 0xFFFF)

## ◆ PCA_CCAP2_CCAP2_Pos

#define PCA_CCAP2_CCAP2_Pos (0UL)

PCA CCAP2: CCAP2 (Bit 0)

## ◆ PCA_CCAP2H_CCAP2_Msk

#define PCA_CCAP2H_CCAP2_Msk (0xFFUL)

PCA CCAP2H: CCAP2 (Bitfield-Mask: 0xFF)

## ◆ PCA_CCAP2H_CCAP2_Pos

#define PCA_CCAP2H_CCAP2_Pos (0UL)

PCA CCAP2H: CCAP2 (Bit 0)

## ◆ PCA_CCAP2L_CCAP2_Msk

#define PCA_CCAP2L_CCAP2_Msk (0xFFUL)

PCA CCAP2L: CCAP2 (Bitfield-Mask: 0xFF)

## ◆ PCA_CCAP2L_CCAP2_Pos

#define PCA_CCAP2L_CCAP2_Pos (0UL)

PCA CCAP2L: CCAP2 (Bit 0)

## ◆ PCA_CCAP3_CCAP3_Msk

#define PCA_CCAP3_CCAP3_Msk (0x7FFFUL)

PCA CCAP3: CCAP3 (Bitfield-Mask: 0x7FFF)

## ◆ PCA_CCAP3_CCAP3_Pos

#define PCA_CCAP3_CCAP3_Pos (0UL)

PCA CCAP3: CCAP3 (Bit 0)

## ◆ PCA_CCAP3H_CCAP3_Msk

#define PCA_CCAP3H_CCAP3_Msk (0xFF00UL)

PCA CCAP3H: CCAP3 (Bitfield-Mask: 0xFF)

## ◆ PCA_CCAP3H_CCAP3_Pos

#define PCA_CCAP3H_CCAP3_Pos (8UL)

PCA CCAP3H: CCAP3 (Bit 8)

## ◆ PCA_CCAP3L_CCAP3_Msk

#define PCA_CCAP3L_CCAP3_Msk (0xFFUL)

PCA CCAP3L: CCAP3 (Bitfield-Mask: 0xFF)

## ◆ PCA_CCAP3L_CCAP3_Pos

#define PCA_CCAP3L_CCAP3_Pos (0UL)

PCA CCAP3L: CCAP3 (Bit 0)

## ◆ PCA_CCAP4_CCAP4_Msk

#define PCA_CCAP4_CCAP4_Msk (0xFFFFUL)

PCA CCAP4: CCAP4 (Bitfield-Mask: 0xFFFF)

## ◆ PCA_CCAP4_CCAP4_Pos

#define PCA_CCAP4_CCAP4_Pos (0UL)

PCA CCAP4: CCAP4 (Bit 0)

## ◆ PCA_CCAP4H_CCAP4_Msk

#define PCA_CCAP4H_CCAP4_Msk (0xFF00UL)

PCA CCAP4H: CCAP4 (Bitfield-Mask: 0xFF)

## ◆ PCA_CCAP4H_CCAP4_Pos

#define PCA_CCAP4H_CCAP4_Pos (8UL)

PCA CCAP4H: CCAP4 (Bit 8)

## ◆ PCA_CCAP4L_CCAP4_Msk

#define PCA_CCAP4L_CCAP4_Msk (0xFFUL)

PCA CCAP4L: CCAP4 (Bitfield-Mask: 0xFF)

## ◆ PCA_CCAP4L_CCAP4_Pos

#define PCA_CCAP4L_CCAP4_Pos (0UL)

PCA CCAP4L: CCAP4 (Bit 0)

## ◆ PCA_CCAPM0_CAPN_Msk

#define PCA_CCAPM0_CAPN_Msk (0x10UL)

PCA CCAPM0: CAPN (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM0_CAPN_Pos

#define PCA_CCAPM0_CAPN_Pos (4UL)

PCA CCAPM0: CAPN (Bit 4)

## ◆ PCA_CCAPM0_CAPP_Msk

#define PCA_CCAPM0_CAPP_Msk (0x20UL)

PCA CCAPM0: CAPP (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM0_CAPP_Pos

#define PCA_CCAPM0_CAPP_Pos (5UL)

PCA CCAPM0: CAPP (Bit 5)

## ◆ PCA_CCAPM0_CCIE_Msk

#define PCA_CCAPM0_CCIE_Msk (0x1UL)

PCA CCAPM0: CCIE (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM0_CCIE_Pos

#define PCA_CCAPM0_CCIE_Pos (0UL)

PCA CCAPM0: CCIE (Bit 0)

## ◆ PCA_CCAPM0_ECOM_Msk

#define PCA_CCAPM0_ECOM_Msk (0x40UL)

PCA CCAPM0: ECOM (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM0_ECOM_Pos

#define PCA_CCAPM0_ECOM_Pos (6UL)

PCA CCAPM0: ECOM (Bit 6)

## ◆ PCA_CCAPM0_MAT_Msk

#define PCA_CCAPM0_MAT_Msk (0x8UL)

PCA CCAPM0: MAT (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM0_MAT_Pos

#define PCA_CCAPM0_MAT_Pos (3UL)

PCA CCAPM0: MAT (Bit 3)

## ◆ PCA_CCAPM0_PWM_Msk

#define PCA_CCAPM0_PWM_Msk (0x2UL)

PCA CCAPM0: PWM (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM0_PWM_Pos

#define PCA_CCAPM0_PWM_Pos (1UL)

PCA CCAPM0: PWM (Bit 1)

## ◆ PCA_CCAPM0_TOG_Msk

#define PCA_CCAPM0_TOG_Msk (0x4UL)

PCA CCAPM0: TOG (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM0_TOG_Pos

#define PCA_CCAPM0_TOG_Pos (2UL)

PCA CCAPM0: TOG (Bit 2)

## ◆ PCA_CCAPM1_CAPN_Msk

#define PCA_CCAPM1_CAPN_Msk (0x10UL)

PCA CCAPM1: CAPN (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM1_CAPN_Pos

#define PCA_CCAPM1_CAPN_Pos (4UL)

PCA CCAPM1: CAPN (Bit 4)

## ◆ PCA_CCAPM1_CAPP_Msk

#define PCA_CCAPM1_CAPP_Msk (0x20UL)

PCA CCAPM1: CAPP (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM1_CAPP_Pos

#define PCA_CCAPM1_CAPP_Pos (5UL)

PCA CCAPM1: CAPP (Bit 5)

## ◆ PCA_CCAPM1_CCIE_Msk

#define PCA_CCAPM1_CCIE_Msk (0x1UL)

PCA CCAPM1: CCIE (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM1_CCIE_Pos

#define PCA_CCAPM1_CCIE_Pos (0UL)

PCA CCAPM1: CCIE (Bit 0)

## ◆ PCA_CCAPM1_ECOM_Msk

#define PCA_CCAPM1_ECOM_Msk (0x40UL)

PCA CCAPM1: ECOM (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM1_ECOM_Pos

#define PCA_CCAPM1_ECOM_Pos (6UL)

PCA CCAPM1: ECOM (Bit 6)

## ◆ PCA_CCAPM1_MAT_Msk

#define PCA_CCAPM1_MAT_Msk (0x8UL)

PCA CCAPM1: MAT (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM1_MAT_Pos

#define PCA_CCAPM1_MAT_Pos (3UL)

PCA CCAPM1: MAT (Bit 3)

## ◆ PCA_CCAPM1_PWM_Msk

#define PCA_CCAPM1_PWM_Msk (0x2UL)

PCA CCAPM1: PWM (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM1_PWM_Pos

#define PCA_CCAPM1_PWM_Pos (1UL)

PCA CCAPM1: PWM (Bit 1)

## ◆ PCA_CCAPM1_TOG_Msk

#define PCA_CCAPM1_TOG_Msk (0x4UL)

PCA CCAPM1: TOG (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM1_TOG_Pos

#define PCA_CCAPM1_TOG_Pos (2UL)

PCA CCAPM1: TOG (Bit 2)

## ◆ PCA_CCAPM2_CAPN_Msk

#define PCA_CCAPM2_CAPN_Msk (0x10UL)

PCA CCAPM2: CAPN (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM2_CAPN_Pos

#define PCA_CCAPM2_CAPN_Pos (4UL)

PCA CCAPM2: CAPN (Bit 4)

## ◆ PCA_CCAPM2_CAPP_Msk

#define PCA_CCAPM2_CAPP_Msk (0x20UL)

PCA CCAPM2: CAPP (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM2_CAPP_Pos

#define PCA_CCAPM2_CAPP_Pos (5UL)

PCA CCAPM2: CAPP (Bit 5)

## ◆ PCA_CCAPM2_CCIE_Msk

#define PCA_CCAPM2_CCIE_Msk (0x1UL)

PCA CCAPM2: CCIE (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM2_CCIE_Pos

#define PCA_CCAPM2_CCIE_Pos (0UL)

PCA CCAPM2: CCIE (Bit 0)

## ◆ PCA_CCAPM2_ECOM_Msk

#define PCA_CCAPM2_ECOM_Msk (0x40UL)

PCA CCAPM2: ECOM (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM2_ECOM_Pos

#define PCA_CCAPM2_ECOM_Pos (6UL)

PCA CCAPM2: ECOM (Bit 6)

## ◆ PCA_CCAPM2_MAT_Msk

#define PCA_CCAPM2_MAT_Msk (0x8UL)

PCA CCAPM2: MAT (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM2_MAT_Pos

#define PCA_CCAPM2_MAT_Pos (3UL)

PCA CCAPM2: MAT (Bit 3)

## ◆ PCA_CCAPM2_PWM_Msk

#define PCA_CCAPM2_PWM_Msk (0x2UL)

PCA CCAPM2: PWM (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM2_PWM_Pos

#define PCA_CCAPM2_PWM_Pos (1UL)

PCA CCAPM2: PWM (Bit 1)

## ◆ PCA_CCAPM2_TOG_Msk

#define PCA_CCAPM2_TOG_Msk (0x4UL)

PCA CCAPM2: TOG (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM2_TOG_Pos

#define PCA_CCAPM2_TOG_Pos (2UL)

PCA CCAPM2: TOG (Bit 2)

## ◆ PCA_CCAPM3_CAPN_Msk

#define PCA_CCAPM3_CAPN_Msk (0x10UL)

PCA CCAPM3: CAPN (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM3_CAPN_Pos

#define PCA_CCAPM3_CAPN_Pos (4UL)

PCA CCAPM3: CAPN (Bit 4)

## ◆ PCA_CCAPM3_CAPP_Msk

#define PCA_CCAPM3_CAPP_Msk (0x20UL)

PCA CCAPM3: CAPP (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM3_CAPP_Pos

#define PCA_CCAPM3_CAPP_Pos (5UL)

PCA CCAPM3: CAPP (Bit 5)

## ◆ PCA_CCAPM3_CCIE_Msk

#define PCA_CCAPM3_CCIE_Msk (0x1UL)

PCA CCAPM3: CCIE (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM3_CCIE_Pos

#define PCA_CCAPM3_CCIE_Pos (0UL)

PCA CCAPM3: CCIE (Bit 0)

## ◆ PCA_CCAPM3_ECOM_Msk

#define PCA_CCAPM3_ECOM_Msk (0x40UL)

PCA CCAPM3: ECOM (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM3_ECOM_Pos

#define PCA_CCAPM3_ECOM_Pos (6UL)

PCA CCAPM3: ECOM (Bit 6)

## ◆ PCA_CCAPM3_MAT_Msk

#define PCA_CCAPM3_MAT_Msk (0x8UL)

PCA CCAPM3: MAT (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM3_MAT_Pos

#define PCA_CCAPM3_MAT_Pos (3UL)

PCA CCAPM3: MAT (Bit 3)

## ◆ PCA_CCAPM3_PWM_Msk

#define PCA_CCAPM3_PWM_Msk (0x2UL)

PCA CCAPM3: PWM (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM3_PWM_Pos

#define PCA_CCAPM3_PWM_Pos (1UL)

PCA CCAPM3: PWM (Bit 1)

## ◆ PCA_CCAPM3_TOG_Msk

#define PCA_CCAPM3_TOG_Msk (0x4UL)

PCA CCAPM3: TOG (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM3_TOG_Pos

#define PCA_CCAPM3_TOG_Pos (2UL)

PCA CCAPM3: TOG (Bit 2)

## ◆ PCA_CCAPM4_CAPN_Msk

#define PCA_CCAPM4_CAPN_Msk (0x10UL)

PCA CCAPM4: CAPN (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM4_CAPN_Pos

#define PCA_CCAPM4_CAPN_Pos (4UL)

PCA CCAPM4: CAPN (Bit 4)

## ◆ PCA_CCAPM4_CAPP_Msk

#define PCA_CCAPM4_CAPP_Msk (0x20UL)

PCA CCAPM4: CAPP (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM4_CAPP_Pos

#define PCA_CCAPM4_CAPP_Pos (5UL)

PCA CCAPM4: CAPP (Bit 5)

## ◆ PCA_CCAPM4_CCIE_Msk

#define PCA_CCAPM4_CCIE_Msk (0x1UL)

PCA CCAPM4: CCIE (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM4_CCIE_Pos

#define PCA_CCAPM4_CCIE_Pos (0UL)

PCA CCAPM4: CCIE (Bit 0)

## ◆ PCA_CCAPM4_ECOM_Msk

#define PCA_CCAPM4_ECOM_Msk (0x40UL)

PCA CCAPM4: ECOM (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM4_ECOM_Pos

#define PCA_CCAPM4_ECOM_Pos (6UL)

PCA CCAPM4: ECOM (Bit 6)

## ◆ PCA_CCAPM4_MAT_Msk

#define PCA_CCAPM4_MAT_Msk (0x8UL)

PCA CCAPM4: MAT (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM4_MAT_Pos

#define PCA_CCAPM4_MAT_Pos (3UL)

PCA CCAPM4: MAT (Bit 3)

## ◆ PCA_CCAPM4_PWM_Msk

#define PCA_CCAPM4_PWM_Msk (0x2UL)

PCA CCAPM4: PWM (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM4_PWM_Pos

#define PCA_CCAPM4_PWM_Pos (1UL)

PCA CCAPM4: PWM (Bit 1)

## ◆ PCA_CCAPM4_TOG_Msk

#define PCA_CCAPM4_TOG_Msk (0x4UL)

PCA CCAPM4: TOG (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPM4_TOG_Pos

#define PCA_CCAPM4_TOG_Pos (2UL)

PCA CCAPM4: TOG (Bit 2)

## ◆ PCA_CCAPO_CCAPO0_Msk

#define PCA_CCAPO_CCAPO0_Msk (0x1UL)

PCA CCAPO: CCAPO0 (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPO_CCAPO0_Pos

#define PCA_CCAPO_CCAPO0_Pos (0UL)

PCA CCAPO: CCAPO0 (Bit 0)

## ◆ PCA_CCAPO_CCAPO1_Msk

#define PCA_CCAPO_CCAPO1_Msk (0x2UL)

PCA CCAPO: CCAPO1 (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPO_CCAPO1_Pos

#define PCA_CCAPO_CCAPO1_Pos (1UL)

PCA CCAPO: CCAPO1 (Bit 1)

## ◆ PCA_CCAPO_CCAPO2_Msk

#define PCA_CCAPO_CCAPO2_Msk (0x4UL)

PCA CCAPO: CCAPO2 (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPO_CCAPO2_Pos

#define PCA_CCAPO_CCAPO2_Pos (2UL)

PCA CCAPO: CCAPO2 (Bit 2)

## ◆ PCA_CCAPO_CCAPO3_Msk

#define PCA_CCAPO_CCAPO3_Msk (0x8UL)

PCA CCAPO: CCAPO3 (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPO_CCAPO3_Pos

#define PCA_CCAPO_CCAPO3_Pos (3UL)

PCA CCAPO: CCAPO3 (Bit 3)

## ◆ PCA_CCAPO_CCAPO4_Msk

#define PCA_CCAPO_CCAPO4_Msk (0x10UL)

PCA CCAPO: CCAPO4 (Bitfield-Mask: 0x01)

## ◆ PCA_CCAPO_CCAPO4_Pos

#define PCA_CCAPO_CCAPO4_Pos (4UL)

PCA CCAPO: CCAPO4 (Bit 4)

## ◆ PCA_CNT_CNT_Msk

#define PCA_CNT_CNT_Msk (0xFFUL)

PCA CNT: CNT (Bitfield-Mask: 0xFF)

## ◆ PCA_CNT_CNT_Pos

#define PCA_CNT_CNT_Pos (0UL)

PCA CNT: CNT (Bit 0)

## ◆ PCA_CR_CCF0_Msk

#define PCA_CR_CCF0_Msk (0x1UL)

PCA CR: CCF0 (Bitfield-Mask: 0x01)

## ◆ PCA_CR_CCF0_Pos

#define PCA_CR_CCF0_Pos (0UL)

PCA CR: CCF0 (Bit 0)

## ◆ PCA_CR_CCF1_Msk

#define PCA_CR_CCF1_Msk (0x2UL)

PCA CR: CCF1 (Bitfield-Mask: 0x01)

## ◆ PCA_CR_CCF1_Pos

#define PCA_CR_CCF1_Pos (1UL)

PCA CR: CCF1 (Bit 1)

## ◆ PCA_CR_CCF2_Msk

#define PCA_CR_CCF2_Msk (0x4UL)

PCA CR: CCF2 (Bitfield-Mask: 0x01)

## ◆ PCA_CR_CCF2_Pos

#define PCA_CR_CCF2_Pos (2UL)

PCA CR: CCF2 (Bit 2)

## ◆ PCA_CR_CCF3_Msk

#define PCA_CR_CCF3_Msk (0x8UL)

PCA CR: CCF3 (Bitfield-Mask: 0x01)

## ◆ PCA_CR_CCF3_Pos

#define PCA_CR_CCF3_Pos (3UL)

PCA CR: CCF3 (Bit 3)

## ◆ PCA_CR_CCF4_Msk

#define PCA_CR_CCF4_Msk (0x10UL)

PCA CR: CCF4 (Bitfield-Mask: 0x01)

## ◆ PCA_CR_CCF4_Pos

#define PCA_CR_CCF4_Pos (4UL)

PCA CR: CCF4 (Bit 4)

## ◆ PCA_CR_CF_Msk

#define PCA_CR_CF_Msk (0x80UL)

PCA CR: CF (Bitfield-Mask: 0x01)

## ◆ PCA_CR_CF_Pos

#define PCA_CR_CF_Pos (7UL)

PCA CR: CF (Bit 7)

## ◆ PCA_CR_CR_Msk

#define PCA_CR_CR_Msk (0x40UL)

PCA CR: CR (Bitfield-Mask: 0x01)

## ◆ PCA_CR_CR_Pos

#define PCA_CR_CR_Pos (6UL)

PCA CR: CR (Bit 6)

## ◆ PCA_INTCLR_CCF0_Msk

#define PCA_INTCLR_CCF0_Msk (0x1UL)

PCA INTCLR: CCF0 (Bitfield-Mask: 0x01)

## ◆ PCA_INTCLR_CCF0_Pos

#define PCA_INTCLR_CCF0_Pos (0UL)

PCA INTCLR: CCF0 (Bit 0)

## ◆ PCA_INTCLR_CCF1_Msk

#define PCA_INTCLR_CCF1_Msk (0x2UL)

PCA INTCLR: CCF1 (Bitfield-Mask: 0x01)

## ◆ PCA_INTCLR_CCF1_Pos

#define PCA_INTCLR_CCF1_Pos (1UL)

PCA INTCLR: CCF1 (Bit 1)

## ◆ PCA_INTCLR_CCF2_Msk

#define PCA_INTCLR_CCF2_Msk (0x4UL)

PCA INTCLR: CCF2 (Bitfield-Mask: 0x01)

## ◆ PCA_INTCLR_CCF2_Pos

#define PCA_INTCLR_CCF2_Pos (2UL)

PCA INTCLR: CCF2 (Bit 2)

## ◆ PCA_INTCLR_CCF3_Msk

#define PCA_INTCLR_CCF3_Msk (0x8UL)

PCA INTCLR: CCF3 (Bitfield-Mask: 0x01)

## ◆ PCA_INTCLR_CCF3_Pos

#define PCA_INTCLR_CCF3_Pos (3UL)

PCA INTCLR: CCF3 (Bit 3)

## ◆ PCA_INTCLR_CCF4_Msk

#define PCA_INTCLR_CCF4_Msk (0x10UL)

PCA INTCLR: CCF4 (Bitfield-Mask: 0x01)

## ◆ PCA_INTCLR_CCF4_Pos

#define PCA_INTCLR_CCF4_Pos (4UL)

PCA INTCLR: CCF4 (Bit 4)

## ◆ PCA_INTCLR_CF_Msk

#define PCA_INTCLR_CF_Msk (0x80UL)

PCA INTCLR: CF (Bitfield-Mask: 0x01)

## ◆ PCA_INTCLR_CF_Pos

#define PCA_INTCLR_CF_Pos (7UL)

PCA INTCLR: CF (Bit 7)

## ◆ PCA_MOD_CFIE_Msk

#define PCA_MOD_CFIE_Msk (0x1UL)

PCA MOD: CFIE (Bitfield-Mask: 0x01)

## ◆ PCA_MOD_CFIE_Pos

#define PCA_MOD_CFIE_Pos (0UL)

PCA MOD: CFIE (Bit 0)

## ◆ PCA_MOD_CIDL_Msk

#define PCA_MOD_CIDL_Msk (0x80UL)

PCA MOD: CIDL (Bitfield-Mask: 0x01)

## ◆ PCA_MOD_CIDL_Pos

#define PCA_MOD_CIDL_Pos (7UL)

PCA MOD: CIDL (Bit 7)

## ◆ PCA_MOD_CPS_Msk

#define PCA_MOD_CPS_Msk (0xEUL)

PCA MOD: CPS (Bitfield-Mask: 0x07)

## ◆ PCA_MOD_CPS_Pos

#define PCA_MOD_CPS_Pos (1UL)

PCA MOD: CPS (Bit 1)

## ◆ PCA_POCR_POE0_Msk

#define PCA_POCR_POE0_Msk (0x1UL)

PCA POCR: POE0 (Bitfield-Mask: 0x01)

## ◆ PCA_POCR_POE0_Pos

#define PCA_POCR_POE0_Pos (0UL)

PCA POCR: POE0 (Bit 0)

## ◆ PCA_POCR_POE1_Msk

#define PCA_POCR_POE1_Msk (0x2UL)

PCA POCR: POE1 (Bitfield-Mask: 0x01)

## ◆ PCA_POCR_POE1_Pos

#define PCA_POCR_POE1_Pos (1UL)

PCA POCR: POE1 (Bit 1)

## ◆ PCA_POCR_POE2_Msk

#define PCA_POCR_POE2_Msk (0x4UL)

PCA POCR: POE2 (Bitfield-Mask: 0x01)

## ◆ PCA_POCR_POE2_Pos

#define PCA_POCR_POE2_Pos (2UL)

PCA POCR: POE2 (Bit 2)

## ◆ PCA_POCR_POE3_Msk

#define PCA_POCR_POE3_Msk (0x8UL)

PCA POCR: POE3 (Bitfield-Mask: 0x01)

## ◆ PCA_POCR_POE3_Pos

#define PCA_POCR_POE3_Pos (3UL)

PCA POCR: POE3 (Bit 3)

## ◆ PCA_POCR_POE4_Msk

#define PCA_POCR_POE4_Msk (0x10UL)

PCA POCR: POE4 (Bitfield-Mask: 0x01)

## ◆ PCA_POCR_POE4_Pos

#define PCA_POCR_POE4_Pos (4UL)

PCA POCR: POE4 (Bit 4)

## ◆ PCA_POCR_POINV0_Msk

#define PCA_POCR_POINV0_Msk (0x100UL)

PCA POCR: POINV0 (Bitfield-Mask: 0x01)

## ◆ PCA_POCR_POINV0_Pos

#define PCA_POCR_POINV0_Pos (8UL)

PCA POCR: POINV0 (Bit 8)

## ◆ PCA_POCR_POINV1_Msk

#define PCA_POCR_POINV1_Msk (0x200UL)

PCA POCR: POINV1 (Bitfield-Mask: 0x01)

## ◆ PCA_POCR_POINV1_Pos

#define PCA_POCR_POINV1_Pos (9UL)

PCA POCR: POINV1 (Bit 9)

## ◆ PCA_POCR_POINV2_Msk

#define PCA_POCR_POINV2_Msk (0x400UL)

PCA POCR: POINV2 (Bitfield-Mask: 0x01)

## ◆ PCA_POCR_POINV2_Pos

#define PCA_POCR_POINV2_Pos (10UL)

PCA POCR: POINV2 (Bit 10)

## ◆ PCA_POCR_POINV3_Msk

#define PCA_POCR_POINV3_Msk (0x800UL)

PCA POCR: POINV3 (Bitfield-Mask: 0x01)

## ◆ PCA_POCR_POINV3_Pos

#define PCA_POCR_POINV3_Pos (11UL)

PCA POCR: POINV3 (Bit 11)

## ◆ PCA_POCR_POINV4_Msk

#define PCA_POCR_POINV4_Msk (0x1000UL)

PCA POCR: POINV4 (Bitfield-Mask: 0x01)

## ◆ PCA_POCR_POINV4_Pos

#define PCA_POCR_POINV4_Pos (12UL)

PCA POCR: POINV4 (Bit 12)

## ◆ PERIPH_BASE

#define PERIPH_BASE ((uint32_t)0x40000000UL)

Peripheral base address in the alias region

## ◆ RCC_HCLKDIV_AHBCKDIV_Msk

#define RCC_HCLKDIV_AHBCKDIV_Msk (0xFFUL)

RCC HCLKDIV: AHBCKDIV (Bitfield-Mask: 0xFF)

## ◆ RCC_HCLKDIV_AHBCKDIV_Pos

#define RCC_HCLKDIV_AHBCKDIV_Pos (0UL)

RCC HCLKDIV: AHBCKDIV (Bit 0)

## ◆ RCC_HCLKEN_CRCCKEN_Msk

#define RCC_HCLKEN_CRCCKEN_Msk (0x10UL)

RCC HCLKEN: CRCCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_HCLKEN_CRCCKEN_Pos

#define RCC_HCLKEN_CRCCKEN_Pos (4UL)

RCC HCLKEN: CRCCKEN (Bit 4)

## ◆ RCC_HCLKEN_FLASHCKEN_Msk

#define RCC_HCLKEN_FLASHCKEN_Msk (0x100UL)

RCC HCLKEN: FLASHCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_HCLKEN_FLASHCKEN_Pos

#define RCC_HCLKEN_FLASHCKEN_Pos (8UL)

RCC HCLKEN: FLASHCKEN (Bit 8)

## ◆ RCC_HCLKEN_GPIOACKEN_Msk

#define RCC_HCLKEN_GPIOACKEN_Msk (0x1UL)

RCC HCLKEN: GPIOACKEN (Bitfield-Mask: 0x01)

## ◆ RCC_HCLKEN_GPIOACKEN_Pos

#define RCC_HCLKEN_GPIOACKEN_Pos (0UL)

RCC HCLKEN: GPIOACKEN (Bit 0)

## ◆ RCC_HCLKEN_GPIOBCKEN_Msk

#define RCC_HCLKEN_GPIOBCKEN_Msk (0x2UL)

RCC HCLKEN: GPIOBCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_HCLKEN_GPIOBCKEN_Pos

#define RCC_HCLKEN_GPIOBCKEN_Pos (1UL)

RCC HCLKEN: GPIOBCKEN (Bit 1)

## ◆ RCC_HCLKEN_GPIOCCKEN_Msk

#define RCC_HCLKEN_GPIOCCKEN_Msk (0x4UL)

RCC HCLKEN: GPIOCCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_HCLKEN_GPIOCCKEN_Pos

#define RCC_HCLKEN_GPIOCCKEN_Pos (2UL)

RCC HCLKEN: GPIOCCKEN (Bit 2)

## ◆ RCC_HCLKEN_GPIODCKEN_Msk

#define RCC_HCLKEN_GPIODCKEN_Msk (0x8UL)

RCC HCLKEN: GPIODCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_HCLKEN_GPIODCKEN_Pos

#define RCC_HCLKEN_GPIODCKEN_Pos (3UL)

RCC HCLKEN: GPIODCKEN (Bit 3)

## ◆ RCC_HSECR_HSEDRV_Msk

#define RCC_HSECR_HSEDRV_Msk (0x7UL)

RCC HSECR: HSEDRV (Bitfield-Mask: 0x07)

## ◆ RCC_HSECR_HSEDRV_Pos

#define RCC_HSECR_HSEDRV_Pos (0UL)

RCC HSECR: HSEDRV (Bit 0)

## ◆ RCC_HSECR_HSERDY_Msk

#define RCC_HSECR_HSERDY_Msk (0x40UL)

RCC HSECR: HSERDY (Bitfield-Mask: 0x01)

## ◆ RCC_HSECR_HSERDY_Pos

#define RCC_HSECR_HSERDY_Pos (6UL)

RCC HSECR: HSERDY (Bit 6)

## ◆ RCC_HSECR_HSESTARTUP_Msk

#define RCC_HSECR_HSESTARTUP_Msk (0x30UL)

RCC HSECR: HSESTARTUP (Bitfield-Mask: 0x03)

## ◆ RCC_HSECR_HSESTARTUP_Pos

#define RCC_HSECR_HSESTARTUP_Pos (4UL)

RCC HSECR: HSESTARTUP (Bit 4)

## ◆ RCC_HSICR_HSIRDY_Msk

#define RCC_HSICR_HSIRDY_Msk (0x1000UL)

RCC HSICR: HSIRDY (Bitfield-Mask: 0x01)

## ◆ RCC_HSICR_HSIRDY_Pos

#define RCC_HSICR_HSIRDY_Pos (12UL)

RCC HSICR: HSIRDY (Bit 12)

## ◆ RCC_HSICR_HSITCTRIM_Msk

#define RCC_HSICR_HSITCTRIM_Msk (0xFFFUL)

RCC HSITCCR: HSITCTRIM (Bitfield-Mask: 0xFFF)

## ◆ RCC_HSICR_HSITCTRIM_Pos

#define RCC_HSICR_HSITCTRIM_Pos (0UL)

RCC HSITCCR: HSITCTRIM (Bit 0)

## ◆ RCC_HSICR_HSITRIM_Msk

#define RCC_HSICR_HSITRIM_Msk (0xFFFUL)

RCC HSICR: HSITRIM (Bitfield-Mask: 0xFFF)

## ◆ RCC_HSICR_HSITRIM_Pos

#define RCC_HSICR_HSITRIM_Pos (0UL)

RCC HSICR: HSITRIM (Bit 0)

## ◆ RCC_HSICR_KEY_Msk

#define RCC_HSICR_KEY_Msk (0xFFFF0000UL)

RCC HSICR: KEY (Bitfield-Mask: 0xFFFF)

## ◆ RCC_HSICR_KEY_Pos

#define RCC_HSICR_KEY_Pos (16UL)

RCC HSICR: KEY (Bit 16)

## ◆ RCC_IRQLATENCY_IRQLATENCY_Msk

#define RCC_IRQLATENCY_IRQLATENCY_Msk (0xFFUL)

RCC IRQLATENCY: IRQLATENCY (Bitfield-Mask: 0xFF)

## ◆ RCC_IRQLATENCY_IRQLATENCY_Pos

#define RCC_IRQLATENCY_IRQLATENCY_Pos (0UL)

RCC IRQLATENCY: IRQLATENCY (Bit 0)

## ◆ RCC_LSECR_KEY_Msk

#define RCC_LSECR_KEY_Msk (0xFFFF0000UL)

RCC LSECR: KEY (Bitfield-Mask: 0xFFFF)

## ◆ RCC_LSECR_KEY_Pos

#define RCC_LSECR_KEY_Pos (16UL)

RCC LSECR: KEY (Bit 16)

## ◆ RCC_LSECR_LSEAON_Msk

#define RCC_LSECR_LSEAON_Msk (0x400UL)

RCC LSECR: LSEAON (Bitfield-Mask: 0x01)

## ◆ RCC_LSECR_LSEAON_Pos

#define RCC_LSECR_LSEAON_Pos (10UL)

RCC LSECR: LSEAON (Bit 10)

## ◆ RCC_LSECR_LSEBYP_Msk

#define RCC_LSECR_LSEBYP_Msk (0x200UL)

RCC LSECR: LSEBYP (Bitfield-Mask: 0x01)

## ◆ RCC_LSECR_LSEBYP_Pos

#define RCC_LSECR_LSEBYP_Pos (9UL)

RCC LSECR: LSEBYP (Bit 9)

## ◆ RCC_LSECR_LSEDRV_Msk

#define RCC_LSECR_LSEDRV_Msk (0xFUL)

RCC LSECR: LSEDRV (Bitfield-Mask: 0x0F)

## ◆ RCC_LSECR_LSEDRV_Pos

#define RCC_LSECR_LSEDRV_Pos (0UL)

RCC LSECR: LSEDRV (Bit 0)

## ◆ RCC_LSECR_LSEEN_Msk

#define RCC_LSECR_LSEEN_Msk (0x100UL)

RCC LSECR: LSEEN (Bitfield-Mask: 0x01)

## ◆ RCC_LSECR_LSEEN_Pos

#define RCC_LSECR_LSEEN_Pos (8UL)

RCC LSECR: LSEEN (Bit 8)

## ◆ RCC_LSECR_LSEPORT_Msk

#define RCC_LSECR_LSEPORT_Msk (0x800UL)

RCC LSECR: LSEPORT (Bitfield-Mask: 0x01)

## ◆ RCC_LSECR_LSEPORT_Pos

#define RCC_LSECR_LSEPORT_Pos (11UL)

RCC LSECR: LSEPORT (Bit 11)

## ◆ RCC_LSECR_LSERDY_Msk

#define RCC_LSECR_LSERDY_Msk (0x40UL)

RCC LSECR: LSERDY (Bitfield-Mask: 0x01)

## ◆ RCC_LSECR_LSERDY_Pos

#define RCC_LSECR_LSERDY_Pos (6UL)

RCC LSECR: LSERDY (Bit 6)

## ◆ RCC_LSECR_LSESTARTUP_Msk

#define RCC_LSECR_LSESTARTUP_Msk (0x30UL)

RCC LSECR: LSESTARTUP (Bitfield-Mask: 0x03)

## ◆ RCC_LSECR_LSESTARTUP_Pos

#define RCC_LSECR_LSESTARTUP_Pos (4UL)

RCC LSECR: LSESTARTUP (Bit 4)

## ◆ RCC_LSICR_KEY_Msk

#define RCC_LSICR_KEY_Msk (0xFFFF0000UL)

RCC LSICR: KEY (Bitfield-Mask: 0xFFFF)

## ◆ RCC_LSICR_KEY_Pos

#define RCC_LSICR_KEY_Pos (16UL)

RCC LSICR: KEY (Bit 16)

## ◆ RCC_LSICR_LSIRDY_Msk

#define RCC_LSICR_LSIRDY_Msk (0x1000UL)

RCC LSICR: LSIRDY (Bitfield-Mask: 0x01)

## ◆ RCC_LSICR_LSIRDY_Pos

#define RCC_LSICR_LSIRDY_Pos (12UL)

RCC LSICR: LSIRDY (Bit 12)

## ◆ RCC_LSICR_LSISTARTUP_Msk

#define RCC_LSICR_LSISTARTUP_Msk (0xC00UL)

RCC LSICR: LSISTARTUP (Bitfield-Mask: 0x03)

## ◆ RCC_LSICR_LSISTARTUP_Pos

#define RCC_LSICR_LSISTARTUP_Pos (10UL)

RCC LSICR: LSISTARTUP (Bit 10)

## ◆ RCC_LSICR_LSITRIM_Msk

#define RCC_LSICR_LSITRIM_Msk (0x1FFUL)

RCC LSICR: LSITRIM (Bitfield-Mask: 0x1FF)

## ◆ RCC_LSICR_LSITRIM_Pos

#define RCC_LSICR_LSITRIM_Pos (0UL)

RCC LSICR: LSITRIM (Bit 0)

## ◆ RCC_MCOCR_MCODIV_Msk

#define RCC_MCOCR_MCODIV_Msk (0xFFUL)

RCC MCOCR: MCODIV (Bitfield-Mask: 0xFF)

## ◆ RCC_MCOCR_MCODIV_Pos

#define RCC_MCOCR_MCODIV_Pos (0UL)

RCC MCOCR: MCODIV (Bit 0)

## ◆ RCC_MCOCR_MCOEN_Msk

#define RCC_MCOCR_MCOEN_Msk (0x1000UL)

RCC MCOCR: MCOEN (Bitfield-Mask: 0x01)

## ◆ RCC_MCOCR_MCOEN_Pos

#define RCC_MCOCR_MCOEN_Pos (12UL)

RCC MCOCR: MCOEN (Bit 12)

## ◆ RCC_MCOCR_MCOSEL_Msk

#define RCC_MCOCR_MCOSEL_Msk (0x700UL)

RCC MCOCR: MCOSEL (Bitfield-Mask: 0x07)

## ◆ RCC_MCOCR_MCOSEL_Pos

#define RCC_MCOCR_MCOSEL_Pos (8UL)

RCC MCOCR: MCOSEL (Bit 8)

## ◆ RCC_PCLKDIV_APBCKDIV_Msk

#define RCC_PCLKDIV_APBCKDIV_Msk (0xFFUL)

RCC PCLKDIV: APBCKDIV (Bitfield-Mask: 0xFF)

## ◆ RCC_PCLKDIV_APBCKDIV_Pos

#define RCC_PCLKDIV_APBCKDIV_Pos (0UL)

RCC PCLKDIV: APBCKDIV (Bit 0)

## ◆ RCC_PCLKEN_ADCCKEN_Msk

#define RCC_PCLKEN_ADCCKEN_Msk (0x2000UL)

RCC PCLKEN: ADCCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_ADCCKEN_Pos

#define RCC_PCLKEN_ADCCKEN_Pos (13UL)

RCC PCLKEN: ADCCKEN (Bit 13)

## ◆ RCC_PCLKEN_AWKCKEN_Msk

#define RCC_PCLKEN_AWKCKEN_Msk (0x4000UL)

RCC PCLKEN: AWKCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_AWKCKEN_Pos

#define RCC_PCLKEN_AWKCKEN_Pos (14UL)

RCC PCLKEN: AWKCKEN (Bit 14)

## ◆ RCC_PCLKEN_BASETIMCKEN_Msk

#define RCC_PCLKEN_BASETIMCKEN_Msk (0x40UL)

RCC PCLKEN: BASETIMCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_BASETIMCKEN_Pos

#define RCC_PCLKEN_BASETIMCKEN_Pos (6UL)

RCC PCLKEN: BASETIMCKEN (Bit 6)

## ◆ RCC_PCLKEN_BEEPCKEN_Msk

#define RCC_PCLKEN_BEEPCKEN_Msk (0x80000UL)

RCC PCLKEN: BEEPCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_BEEPCKEN_Pos

#define RCC_PCLKEN_BEEPCKEN_Pos (19UL)

RCC PCLKEN: BEEPCKEN (Bit 19)

## ◆ RCC_PCLKEN_CLKCTRIMCKEN_Msk

#define RCC_PCLKEN_CLKCTRIMCKEN_Msk (0x10000UL)

RCC PCLKEN: CLKCTRIMCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_CLKCTRIMCKEN_Pos

#define RCC_PCLKEN_CLKCTRIMCKEN_Pos (16UL)

RCC PCLKEN: CLKCTRIMCKEN (Bit 16)

## ◆ RCC_PCLKEN_DBGCKEN_Msk

#define RCC_PCLKEN_DBGCKEN_Msk (0x100000UL)

RCC PCLKEN: DBGCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_DBGCKEN_Pos

#define RCC_PCLKEN_DBGCKEN_Pos (20UL)

RCC PCLKEN: DBGCKEN (Bit 20)

## ◆ RCC_PCLKEN_I2CCKEN_Msk

#define RCC_PCLKEN_I2CCKEN_Msk (0x4UL)

RCC PCLKEN: I2CCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_I2CCKEN_Pos

#define RCC_PCLKEN_I2CCKEN_Pos (2UL)

RCC PCLKEN: I2CCKEN (Bit 2)

## ◆ RCC_PCLKEN_IWDGCKEN_Msk

#define RCC_PCLKEN_IWDGCKEN_Msk (0x20000UL)

RCC PCLKEN: IWDGCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_IWDGCKEN_Pos

#define RCC_PCLKEN_IWDGCKEN_Pos (17UL)

RCC PCLKEN: IWDGCKEN (Bit 17)

## ◆ RCC_PCLKEN_LPTIMCKEN_Msk

#define RCC_PCLKEN_LPTIMCKEN_Msk (0x20UL)

RCC PCLKEN: LPTIMCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_LPTIMCKEN_Pos

#define RCC_PCLKEN_LPTIMCKEN_Pos (5UL)

RCC PCLKEN: LPTIMCKEN (Bit 5)

## ◆ RCC_PCLKEN_LPUARTCKEN_Msk

#define RCC_PCLKEN_LPUARTCKEN_Msk (0x8UL)

RCC PCLKEN: LPUARTCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_LPUARTCKEN_Pos

#define RCC_PCLKEN_LPUARTCKEN_Pos (3UL)

RCC PCLKEN: LPUARTCKEN (Bit 3)

## ◆ RCC_PCLKEN_LVDVCCKEN_Msk

#define RCC_PCLKEN_LVDVCCKEN_Msk (0x40000UL)

RCC PCLKEN: LVDVCCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_LVDVCCKEN_Pos

#define RCC_PCLKEN_LVDVCCKEN_Pos (18UL)

RCC PCLKEN: LVDVCCKEN (Bit 18)

## ◆ RCC_PCLKEN_OWIRECKEN_Msk

#define RCC_PCLKEN_OWIRECKEN_Msk (0x200UL)

RCC PCLKEN: OWIRECKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_OWIRECKEN_Pos

#define RCC_PCLKEN_OWIRECKEN_Pos (9UL)

RCC PCLKEN: OWIRECKEN (Bit 9)

## ◆ RCC_PCLKEN_PCACKEN_Msk

#define RCC_PCLKEN_PCACKEN_Msk (0x100UL)

RCC PCLKEN: PCACKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_PCACKEN_Pos

#define RCC_PCLKEN_PCACKEN_Pos (8UL)

RCC PCLKEN: PCACKEN (Bit 8)

## ◆ RCC_PCLKEN_RTCCKEN_Msk

#define RCC_PCLKEN_RTCCKEN_Msk (0x8000UL)

RCC PCLKEN: RTCCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_RTCCKEN_Pos

#define RCC_PCLKEN_RTCCKEN_Pos (15UL)

RCC PCLKEN: RTCCKEN (Bit 15)

## ◆ RCC_PCLKEN_SPICKEN_Msk

#define RCC_PCLKEN_SPICKEN_Msk (0x10UL)

RCC PCLKEN: SPICKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_SPICKEN_Pos

#define RCC_PCLKEN_SPICKEN_Pos (4UL)

RCC PCLKEN: SPICKEN (Bit 4)

## ◆ RCC_PCLKEN_SYSCONCKEN_Msk

#define RCC_PCLKEN_SYSCONCKEN_Msk (0x80UL)

RCC PCLKEN: SYSCONCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_SYSCONCKEN_Pos

#define RCC_PCLKEN_SYSCONCKEN_Pos (7UL)

RCC PCLKEN: SYSCONCKEN (Bit 7)

## ◆ RCC_PCLKEN_TIM1CKEN_Msk

#define RCC_PCLKEN_TIM1CKEN_Msk (0x400UL)

RCC PCLKEN: TIM1CKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_TIM1CKEN_Pos

#define RCC_PCLKEN_TIM1CKEN_Pos (10UL)

RCC PCLKEN: TIM1CKEN (Bit 10)

## ◆ RCC_PCLKEN_TIM2CKEN_Msk

#define RCC_PCLKEN_TIM2CKEN_Msk (0x800UL)

RCC PCLKEN: TIM2CKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_TIM2CKEN_Pos

#define RCC_PCLKEN_TIM2CKEN_Pos (11UL)

RCC PCLKEN: TIM2CKEN (Bit 11)

## ◆ RCC_PCLKEN_UART1CKEN_Msk

#define RCC_PCLKEN_UART1CKEN_Msk (0x1UL)

RCC PCLKEN: UART1CKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_UART1CKEN_Pos

#define RCC_PCLKEN_UART1CKEN_Pos (0UL)

RCC PCLKEN: UART1CKEN (Bit 0)

## ◆ RCC_PCLKEN_UART2CKEN_Msk

#define RCC_PCLKEN_UART2CKEN_Msk (0x2UL)

RCC PCLKEN: UART2CKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_UART2CKEN_Pos

#define RCC_PCLKEN_UART2CKEN_Pos (1UL)

RCC PCLKEN: UART2CKEN (Bit 1)

## ◆ RCC_PCLKEN_WWDGCKEN_Msk

#define RCC_PCLKEN_WWDGCKEN_Msk (0x1000UL)

RCC PCLKEN: WWDGCKEN (Bitfield-Mask: 0x01)

## ◆ RCC_PCLKEN_WWDGCKEN_Pos

#define RCC_PCLKEN_WWDGCKEN_Pos (12UL)

RCC PCLKEN: WWDGCKEN (Bit 12)

## ◆ RCC_PERIRST_ADCRST_Msk

#define RCC_PERIRST_ADCRST_Msk (0x2000UL)

RCC PERIRST: ADCRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_ADCRST_Pos

#define RCC_PERIRST_ADCRST_Pos (13UL)

RCC PERIRST: ADCRST (Bit 13)

## ◆ RCC_PERIRST_AWKRST_Msk

#define RCC_PERIRST_AWKRST_Msk (0x4000UL)

RCC PERIRST: AWKRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_AWKRST_Pos

#define RCC_PERIRST_AWKRST_Pos (14UL)

RCC PERIRST: AWKRST (Bit 14)

## ◆ RCC_PERIRST_BASETIMRST_Msk

#define RCC_PERIRST_BASETIMRST_Msk (0x40UL)

RCC PERIRST: BASETIMRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_BASETIMRST_Pos

#define RCC_PERIRST_BASETIMRST_Pos (6UL)

RCC PERIRST: BASETIMRST (Bit 6)

## ◆ RCC_PERIRST_BEEPRST_Msk

#define RCC_PERIRST_BEEPRST_Msk (0x80000UL)

RCC PERIRST: BEEPRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_BEEPRST_Pos

#define RCC_PERIRST_BEEPRST_Pos (19UL)

RCC PERIRST: BEEPRST (Bit 19)

## ◆ RCC_PERIRST_CLKTRIMRST_Msk

#define RCC_PERIRST_CLKTRIMRST_Msk (0x10000UL)

RCC PERIRST: CLKTRIMRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_CLKTRIMRST_Pos

#define RCC_PERIRST_CLKTRIMRST_Pos (16UL)

RCC PERIRST: CLKTRIMRST (Bit 16)

## ◆ RCC_PERIRST_CRCRST_Msk

#define RCC_PERIRST_CRCRST_Msk (0x10000000UL)

RCC PERIRST: CRCRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_CRCRST_Pos

#define RCC_PERIRST_CRCRST_Pos (28UL)

RCC PERIRST: CRCRST (Bit 28)

## ◆ RCC_PERIRST_DBGRST_Msk

#define RCC_PERIRST_DBGRST_Msk (0x100000UL)

RCC PERIRST: DBGRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_DBGRST_Pos

#define RCC_PERIRST_DBGRST_Pos (20UL)

RCC PERIRST: DBGRST (Bit 20)

## ◆ RCC_PERIRST_GPIOARST_Msk

#define RCC_PERIRST_GPIOARST_Msk (0x1000000UL)

RCC PERIRST: GPIOARST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_GPIOARST_Pos

#define RCC_PERIRST_GPIOARST_Pos (24UL)

RCC PERIRST: GPIOARST (Bit 24)

## ◆ RCC_PERIRST_GPIOBRST_Msk

#define RCC_PERIRST_GPIOBRST_Msk (0x2000000UL)

RCC PERIRST: GPIOBRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_GPIOBRST_Pos

#define RCC_PERIRST_GPIOBRST_Pos (25UL)

RCC PERIRST: GPIOBRST (Bit 25)

## ◆ RCC_PERIRST_GPIOCRST_Msk

#define RCC_PERIRST_GPIOCRST_Msk (0x4000000UL)

RCC PERIRST: GPIOCRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_GPIOCRST_Pos

#define RCC_PERIRST_GPIOCRST_Pos (26UL)

RCC PERIRST: GPIOCRST (Bit 26)

## ◆ RCC_PERIRST_GPIODRST_Msk

#define RCC_PERIRST_GPIODRST_Msk (0x8000000UL)

RCC PERIRST: GPIODRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_GPIODRST_Pos

#define RCC_PERIRST_GPIODRST_Pos (27UL)

RCC PERIRST: GPIODRST (Bit 27)

## ◆ RCC_PERIRST_I2CRST_Msk

#define RCC_PERIRST_I2CRST_Msk (0x4UL)

RCC PERIRST: I2CRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_I2CRST_Pos

#define RCC_PERIRST_I2CRST_Pos (2UL)

RCC PERIRST: I2CRST (Bit 2)

## ◆ RCC_PERIRST_LPTIMRST_Msk

#define RCC_PERIRST_LPTIMRST_Msk (0x20UL)

RCC PERIRST: LPTIMRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_LPTIMRST_Pos

#define RCC_PERIRST_LPTIMRST_Pos (5UL)

RCC PERIRST: LPTIMRST (Bit 5)

## ◆ RCC_PERIRST_LPUARTRST_Msk

#define RCC_PERIRST_LPUARTRST_Msk (0x8UL)

RCC PERIRST: LPUARTRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_LPUARTRST_Pos

#define RCC_PERIRST_LPUARTRST_Pos (3UL)

RCC PERIRST: LPUARTRST (Bit 3)

## ◆ RCC_PERIRST_LVDVCRST_Msk

#define RCC_PERIRST_LVDVCRST_Msk (0x40000UL)

RCC PERIRST: LVDVCRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_LVDVCRST_Pos

#define RCC_PERIRST_LVDVCRST_Pos (18UL)

RCC PERIRST: LVDVCRST (Bit 18)

## ◆ RCC_PERIRST_OWIRERST_Msk

#define RCC_PERIRST_OWIRERST_Msk (0x200UL)

RCC PERIRST: OWIRERST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_OWIRERST_Pos

#define RCC_PERIRST_OWIRERST_Pos (9UL)

RCC PERIRST: OWIRERST (Bit 9)

## ◆ RCC_PERIRST_PCARST_Msk

#define RCC_PERIRST_PCARST_Msk (0x100UL)

RCC PERIRST: PCARST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_PCARST_Pos

#define RCC_PERIRST_PCARST_Pos (8UL)

RCC PERIRST: PCARST (Bit 8)

## ◆ RCC_PERIRST_SPIRST_Msk

#define RCC_PERIRST_SPIRST_Msk (0x10UL)

RCC PERIRST: SPIRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_SPIRST_Pos

#define RCC_PERIRST_SPIRST_Pos (4UL)

RCC PERIRST: SPIRST (Bit 4)

## ◆ RCC_PERIRST_SYSCONRST_Msk

#define RCC_PERIRST_SYSCONRST_Msk (0x80UL)

RCC PERIRST: SYSCONRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_SYSCONRST_Pos

#define RCC_PERIRST_SYSCONRST_Pos (7UL)

RCC PERIRST: SYSCONRST (Bit 7)

## ◆ RCC_PERIRST_TIM1RST_Msk

#define RCC_PERIRST_TIM1RST_Msk (0x400UL)

RCC PERIRST: TIM1RST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_TIM1RST_Pos

#define RCC_PERIRST_TIM1RST_Pos (10UL)

RCC PERIRST: TIM1RST (Bit 10)

## ◆ RCC_PERIRST_TIM2RST_Msk

#define RCC_PERIRST_TIM2RST_Msk (0x800UL)

RCC PERIRST: TIM2RST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_TIM2RST_Pos

#define RCC_PERIRST_TIM2RST_Pos (11UL)

RCC PERIRST: TIM2RST (Bit 11)

## ◆ RCC_PERIRST_UART1RST_Msk

#define RCC_PERIRST_UART1RST_Msk (0x1UL)

RCC PERIRST: UART1RST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_UART1RST_Pos

#define RCC_PERIRST_UART1RST_Pos (0UL)

RCC PERIRST: UART1RST (Bit 0)

## ◆ RCC_PERIRST_UART2RST_Msk

#define RCC_PERIRST_UART2RST_Msk (0x2UL)

RCC PERIRST: UART2RST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_UART2RST_Pos

#define RCC_PERIRST_UART2RST_Pos (1UL)

RCC PERIRST: UART2RST (Bit 1)

## ◆ RCC_PERIRST_WWDGRST_Msk

#define RCC_PERIRST_WWDGRST_Msk (0x1000UL)

RCC PERIRST: WWDGRST (Bitfield-Mask: 0x01)

## ◆ RCC_PERIRST_WWDGRST_Pos

#define RCC_PERIRST_WWDGRST_Pos (12UL)

RCC PERIRST: WWDGRST (Bit 12)

## ◆ RCC_RSTCR_CPURST_Msk

#define RCC_RSTCR_CPURST_Msk (0x2UL)

RCC RSTCR: CPURST (Bitfield-Mask: 0x01)

## ◆ RCC_RSTCR_CPURST_Pos

#define RCC_RSTCR_CPURST_Pos (1UL)

RCC RSTCR: CPURST (Bit 1)

## ◆ RCC_RSTCR_MCURST_Msk

#define RCC_RSTCR_MCURST_Msk (0x1UL)

RCC RSTCR: MCURST (Bitfield-Mask: 0x01)

## ◆ RCC_RSTCR_MCURST_Pos

#define RCC_RSTCR_MCURST_Pos (0UL)

RCC RSTCR: MCURST (Bit 0)

## ◆ RCC_RSTCR_RSTKEY_Msk

#define RCC_RSTCR_RSTKEY_Msk (0xFFFFFFFCUL)

RCC RSTCR: RSTKEY (Bitfield-Mask: 0x3FFFFFFF)

## ◆ RCC_RSTCR_RSTKEY_Pos

#define RCC_RSTCR_RSTKEY_Pos (2UL)

RCC RSTCR: RSTKEY (Bit 2)

## ◆ RCC_RSTSR_CPURST_Msk

#define RCC_RSTSR_CPURST_Msk (0x2UL)

RCC RSTSR: CPURST (Bitfield-Mask: 0x01)

## ◆ RCC_RSTSR_CPURST_Pos

#define RCC_RSTSR_CPURST_Pos (1UL)

RCC RSTSR: CPURST (Bit 1)

## ◆ RCC_RSTSR_IWDGRST_Msk

#define RCC_RSTSR_IWDGRST_Msk (0x8UL)

RCC RSTSR: IWDGRST (Bitfield-Mask: 0x01)

## ◆ RCC_RSTSR_IWDGRST_Pos

#define RCC_RSTSR_IWDGRST_Pos (3UL)

RCC RSTSR: IWDGRST (Bit 3)

## ◆ RCC_RSTSR_LOCKUPRST_Msk

#define RCC_RSTSR_LOCKUPRST_Msk (0x40UL)

RCC RSTSR: LOCKUPRST (Bitfield-Mask: 0x01)

## ◆ RCC_RSTSR_LOCKUPRST_Pos

#define RCC_RSTSR_LOCKUPRST_Pos (6UL)

RCC RSTSR: LOCKUPRST (Bit 6)

## ◆ RCC_RSTSR_LVDRST_Msk

#define RCC_RSTSR_LVDRST_Msk (0x10UL)

RCC RSTSR: LVDRST (Bitfield-Mask: 0x01)

## ◆ RCC_RSTSR_LVDRST_Pos

#define RCC_RSTSR_LVDRST_Pos (4UL)

RCC RSTSR: LVDRST (Bit 4)

## ◆ RCC_RSTSR_MCURST_Msk

#define RCC_RSTSR_MCURST_Msk (0x1UL)

RCC RSTSR: MCURST (Bitfield-Mask: 0x01)

## ◆ RCC_RSTSR_MCURST_Pos

#define RCC_RSTSR_MCURST_Pos (0UL)

RCC RSTSR: MCURST (Bit 0)

## ◆ RCC_RSTSR_PADRST_Msk

#define RCC_RSTSR_PADRST_Msk (0x80UL)

RCC RSTSR: PADRST (Bitfield-Mask: 0x01)

## ◆ RCC_RSTSR_PADRST_Pos

#define RCC_RSTSR_PADRST_Pos (7UL)

RCC RSTSR: PADRST (Bit 7)

## ◆ RCC_RSTSR_PORRST_Msk

#define RCC_RSTSR_PORRST_Msk (0x20UL)

RCC RSTSR: PORRST (Bitfield-Mask: 0x01)

## ◆ RCC_RSTSR_PORRST_Pos

#define RCC_RSTSR_PORRST_Pos (5UL)

RCC RSTSR: PORRST (Bit 5)

## ◆ RCC_RSTSR_SFTRST_Msk

#define RCC_RSTSR_SFTRST_Msk (0x100UL)

RCC RSTSR: SFTRST (Bitfield-Mask: 0x01)

## ◆ RCC_RSTSR_SFTRST_Pos

#define RCC_RSTSR_SFTRST_Pos (8UL)

RCC RSTSR: SFTRST (Bit 8)

## ◆ RCC_RSTSR_WWDGRST_Msk

#define RCC_RSTSR_WWDGRST_Msk (0x4UL)

RCC RSTSR: WWDGRST (Bitfield-Mask: 0x01)

## ◆ RCC_RSTSR_WWDGRST_Pos

#define RCC_RSTSR_WWDGRST_Pos (2UL)

RCC RSTSR: WWDGRST (Bit 2)

## ◆ RCC_RTCRST_KEY_Msk

#define RCC_RTCRST_KEY_Msk (0xFFFF0000UL)

RCC RTCRST: KEY (Bitfield-Mask: 0xFFFF)

## ◆ RCC_RTCRST_KEY_Pos

#define RCC_RTCRST_KEY_Pos (16UL)

RCC RTCRST: KEY (Bit 16)

## ◆ RCC_RTCRST_RTCRST_Msk

#define RCC_RTCRST_RTCRST_Msk (0x1UL)

RCC RTCRST: RTCRST (Bitfield-Mask: 0x01)

## ◆ RCC_RTCRST_RTCRST_Pos

#define RCC_RTCRST_RTCRST_Pos (0UL)

RCC RTCRST: RTCRST (Bit 0)

## ◆ RCC_STICKCR_NOREF_Msk

#define RCC_STICKCR_NOREF_Msk (0x2000000UL)

RCC STICKCR: NOREF (Bitfield-Mask: 0x01)

## ◆ RCC_STICKCR_NOREF_Pos

#define RCC_STICKCR_NOREF_Pos (25UL)

RCC STICKCR: NOREF (Bit 25)

## ◆ RCC_STICKCR_SKEW_Msk

#define RCC_STICKCR_SKEW_Msk (0x1000000UL)

RCC STICKCR: SKEW (Bitfield-Mask: 0x01)

## ◆ RCC_STICKCR_SKEW_Pos

#define RCC_STICKCR_SKEW_Pos (24UL)

RCC STICKCR: SKEW (Bit 24)

## ◆ RCC_STICKCR_STCALIB_Msk

#define RCC_STICKCR_STCALIB_Msk (0xFFFFFFUL)

RCC STICKCR: STCALIB (Bitfield-Mask: 0xFFFFFF)

## ◆ RCC_STICKCR_STCALIB_Pos

#define RCC_STICKCR_STCALIB_Pos (0UL)

RCC STICKCR: STCALIB (Bit 0)

## ◆ RCC_SWDIOCR_KEY_Msk

#define RCC_SWDIOCR_KEY_Msk (0xFFFF0000UL)

RCC SWDIOCR: KEY (Bitfield-Mask: 0xFFFF)

## ◆ RCC_SWDIOCR_KEY_Pos

#define RCC_SWDIOCR_KEY_Pos (16UL)

RCC SWDIOCR: KEY (Bit 16)

## ◆ RCC_SWDIOCR_SWDPORT_Msk

#define RCC_SWDIOCR_SWDPORT_Msk (0x1UL)

RCC SWDIOCR: SWDPORT (Bitfield-Mask: 0x01)

## ◆ RCC_SWDIOCR_SWDPORT_Pos

#define RCC_SWDIOCR_SWDPORT_Pos (0UL)

RCC SWDIOCR: SWDPORT (Bit 0)

## ◆ RCC_SYSCLKCR_CLKFAILEN_Msk

#define RCC_SYSCLKCR_CLKFAILEN_Msk (0x100UL)

RCC SYSCLKCR: CLKFAILEN (Bitfield-Mask: 0x01)

## ◆ RCC_SYSCLKCR_CLKFAILEN_Pos

#define RCC_SYSCLKCR_CLKFAILEN_Pos (8UL)

RCC SYSCLKCR: CLKFAILEN (Bit 8)

## ◆ RCC_SYSCLKCR_HSEBYP_Msk

#define RCC_SYSCLKCR_HSEBYP_Msk (0x20UL)

RCC SYSCLKCR: HSEBYP (Bitfield-Mask: 0x01)

## ◆ RCC_SYSCLKCR_HSEBYP_Pos

#define RCC_SYSCLKCR_HSEBYP_Pos (5UL)

RCC SYSCLKCR: HSEBYP (Bit 5)

## ◆ RCC_SYSCLKCR_HSEEN_Msk

#define RCC_SYSCLKCR_HSEEN_Msk (0x2UL)

RCC SYSCLKCR: HSEEN (Bitfield-Mask: 0x01)

## ◆ RCC_SYSCLKCR_HSEEN_Pos

#define RCC_SYSCLKCR_HSEEN_Pos (1UL)

RCC SYSCLKCR: HSEEN (Bit 1)

## ◆ RCC_SYSCLKCR_HSEPORT_Msk

#define RCC_SYSCLKCR_HSEPORT_Msk (0x40UL)

RCC SYSCLKCR: HSEPORT (Bitfield-Mask: 0x01)

## ◆ RCC_SYSCLKCR_HSEPORT_Pos

#define RCC_SYSCLKCR_HSEPORT_Pos (6UL)

RCC SYSCLKCR: HSEPORT (Bit 6)

## ◆ RCC_SYSCLKCR_HSIEN_Msk

#define RCC_SYSCLKCR_HSIEN_Msk (0x1UL)

RCC SYSCLKCR: HSIEN (Bitfield-Mask: 0x01)

## ◆ RCC_SYSCLKCR_HSIEN_Pos

#define RCC_SYSCLKCR_HSIEN_Pos (0UL)

RCC SYSCLKCR: HSIEN (Bit 0)

## ◆ RCC_SYSCLKCR_KEY_Msk

#define RCC_SYSCLKCR_KEY_Msk (0xFFFF0000UL)

RCC SYSCLKCR: KEY (Bitfield-Mask: 0xFFFF)

## ◆ RCC_SYSCLKCR_KEY_Pos

#define RCC_SYSCLKCR_KEY_Pos (16UL)

RCC SYSCLKCR: KEY (Bit 16)

## ◆ RCC_SYSCLKCR_LSIEN_Msk

#define RCC_SYSCLKCR_LSIEN_Msk (0x4UL)

RCC SYSCLKCR: LSIEN (Bitfield-Mask: 0x01)

## ◆ RCC_SYSCLKCR_LSIEN_Pos

#define RCC_SYSCLKCR_LSIEN_Pos (2UL)

RCC SYSCLKCR: LSIEN (Bit 2)

## ◆ RCC_SYSCLKCR_WKBYHSI_Msk

#define RCC_SYSCLKCR_WKBYHSI_Msk (0x8000UL)

RCC SYSCLKCR: WKBYHSI (Bitfield-Mask: 0x01)

## ◆ RCC_SYSCLKCR_WKBYHSI_Pos

#define RCC_SYSCLKCR_WKBYHSI_Pos (15UL)

RCC SYSCLKCR: WKBYHSI (Bit 15)

## ◆ RCC_SYSCLKSEL_CLKSW_Msk

#define RCC_SYSCLKSEL_CLKSW_Msk (0xFUL)

RCC SYSCLKSEL: CLKSW (Bitfield-Mask: 0x0F)

## ◆ RCC_SYSCLKSEL_CLKSW_Pos

#define RCC_SYSCLKSEL_CLKSW_Pos (0UL)

RCC SYSCLKSEL: CLKSW (Bit 0)

## ◆ RCC_SYSCLKSEL_KEY_Msk

#define RCC_SYSCLKSEL_KEY_Msk (0xFFFF0000UL)

RCC SYSCLKSEL: KEY (Bitfield-Mask: 0xFFFF)

## ◆ RCC_SYSCLKSEL_KEY_Pos

#define RCC_SYSCLKSEL_KEY_Pos (16UL)

RCC SYSCLKSEL: KEY (Bit 16)

## ◆ RCC_UNLOCK_KEY_Msk

#define RCC_UNLOCK_KEY_Msk (0xFFFFFFFEUL)

RCC UNLOCK: KEY (Bitfield-Mask: 0x7FFFFFFF)

## ◆ RCC_UNLOCK_KEY_Pos

#define RCC_UNLOCK_KEY_Pos (1UL)

RCC UNLOCK: KEY (Bit 1)

## ◆ RCC_UNLOCK_UNLOCK_Msk

#define RCC_UNLOCK_UNLOCK_Msk (0x1UL)

RCC UNLOCK: UNLOCK (Bitfield-Mask: 0x01)

## ◆ RCC_UNLOCK_UNLOCK_Pos

#define RCC_UNLOCK_UNLOCK_Pos (0UL)

RCC UNLOCK: UNLOCK (Bit 0)

## ◆ RTC_ALM1DATE_ALCEN_Msk

#define RTC_ALM1DATE_ALCEN_Msk (0x8000UL)

RTC ALM1DATE: ALCEN (Bitfield-Mask: 0x01)

## ◆ RTC_ALM1DATE_ALCEN_Pos

#define RTC_ALM1DATE_ALCEN_Pos (15UL)

RTC ALM1DATE: ALCEN (Bit 15)

## ◆ RTC_ALM1DATE_ALDAY_Msk

#define RTC_ALM1DATE_ALDAY_Msk (0x3FUL)

RTC ALM1DATE: ALDAY (Bitfield-Mask: 0x3F)

## ◆ RTC_ALM1DATE_ALDAY_Pos

#define RTC_ALM1DATE_ALDAY_Pos (0UL)

RTC ALM1DATE: ALDAY (Bit 0)

## ◆ RTC_ALM1DATE_ALMDAYEN_Msk

#define RTC_ALM1DATE_ALMDAYEN_Msk (0x10000000UL)

RTC ALM1DATE: ALMDAYEN (Bitfield-Mask: 0x01)

## ◆ RTC_ALM1DATE_ALMDAYEN_Pos

#define RTC_ALM1DATE_ALMDAYEN_Pos (28UL)

RTC ALM1DATE: ALMDAYEN (Bit 28)

## ◆ RTC_ALM1DATE_ALMHOUREN_Msk

#define RTC_ALM1DATE_ALMHOUREN_Msk (0x4000000UL)

RTC ALM1DATE: ALMHOUREN (Bitfield-Mask: 0x01)

## ◆ RTC_ALM1DATE_ALMHOUREN_Pos

#define RTC_ALM1DATE_ALMHOUREN_Pos (26UL)

RTC ALM1DATE: ALMHOUREN (Bit 26)

## ◆ RTC_ALM1DATE_ALMMINEN_Msk

#define RTC_ALM1DATE_ALMMINEN_Msk (0x2000000UL)

RTC ALM1DATE: ALMMINEN (Bitfield-Mask: 0x01)

## ◆ RTC_ALM1DATE_ALMMINEN_Pos

#define RTC_ALM1DATE_ALMMINEN_Pos (25UL)

RTC ALM1DATE: ALMMINEN (Bit 25)

## ◆ RTC_ALM1DATE_ALMMONEN_Msk

#define RTC_ALM1DATE_ALMMONEN_Msk (0x20000000UL)

RTC ALM1DATE: ALMMONEN (Bitfield-Mask: 0x01)

## ◆ RTC_ALM1DATE_ALMMONEN_Pos

#define RTC_ALM1DATE_ALMMONEN_Pos (29UL)

RTC ALM1DATE: ALMMONEN (Bit 29)

## ◆ RTC_ALM1DATE_ALMONTH_Msk

#define RTC_ALM1DATE_ALMONTH_Msk (0x1F00UL)

RTC ALM1DATE: ALMONTH (Bitfield-Mask: 0x1F)

## ◆ RTC_ALM1DATE_ALMONTH_Pos

#define RTC_ALM1DATE_ALMONTH_Pos (8UL)

RTC ALM1DATE: ALMONTH (Bit 8)

## ◆ RTC_ALM1DATE_ALMSECEN_Msk

#define RTC_ALM1DATE_ALMSECEN_Msk (0x1000000UL)

RTC ALM1DATE: ALMSECEN (Bitfield-Mask: 0x01)

## ◆ RTC_ALM1DATE_ALMSECEN_Pos

#define RTC_ALM1DATE_ALMSECEN_Pos (24UL)

RTC ALM1DATE: ALMSECEN (Bit 24)

## ◆ RTC_ALM1DATE_ALMWEEKEN_Msk

#define RTC_ALM1DATE_ALMWEEKEN_Msk (0x8000000UL)

RTC ALM1DATE: ALMWEEKEN (Bitfield-Mask: 0x01)

## ◆ RTC_ALM1DATE_ALMWEEKEN_Pos

#define RTC_ALM1DATE_ALMWEEKEN_Pos (27UL)

RTC ALM1DATE: ALMWEEKEN (Bit 27)

## ◆ RTC_ALM1DATE_ALMYEAREN_Msk

#define RTC_ALM1DATE_ALMYEAREN_Msk (0x40000000UL)

RTC ALM1DATE: ALMYEAREN (Bitfield-Mask: 0x01)

## ◆ RTC_ALM1DATE_ALMYEAREN_Pos

#define RTC_ALM1DATE_ALMYEAREN_Pos (30UL)

RTC ALM1DATE: ALMYEAREN (Bit 30)

## ◆ RTC_ALM1DATE_ALYEAR_Msk

#define RTC_ALM1DATE_ALYEAR_Msk (0xFF0000UL)

RTC ALM1DATE: ALYEAR (Bitfield-Mask: 0xFF)

## ◆ RTC_ALM1DATE_ALYEAR_Pos

#define RTC_ALM1DATE_ALYEAR_Pos (16UL)

RTC ALM1DATE: ALYEAR (Bit 16)

## ◆ RTC_ALM1TIME_ALH20_PA_Msk

#define RTC_ALM1TIME_ALH20_PA_Msk (0x200000UL)

RTC ALM1TIME: ALH20_PA (Bitfield-Mask: 0x01)

## ◆ RTC_ALM1TIME_ALH20_PA_Pos

#define RTC_ALM1TIME_ALH20_PA_Pos (21UL)

RTC ALM1TIME: ALH20_PA (Bit 21)

## ◆ RTC_ALM1TIME_ALHOUR19_Msk

#define RTC_ALM1TIME_ALHOUR19_Msk (0x1F0000UL)

RTC ALM1TIME: ALHOUR19 (Bitfield-Mask: 0x1F)

## ◆ RTC_ALM1TIME_ALHOUR19_Pos

#define RTC_ALM1TIME_ALHOUR19_Pos (16UL)

RTC ALM1TIME: ALHOUR19 (Bit 16)

## ◆ RTC_ALM1TIME_ALMIN_Msk

#define RTC_ALM1TIME_ALMIN_Msk (0x7F00UL)

RTC ALM1TIME: ALMIN (Bitfield-Mask: 0x7F)

## ◆ RTC_ALM1TIME_ALMIN_Pos

#define RTC_ALM1TIME_ALMIN_Pos (8UL)

RTC ALM1TIME: ALMIN (Bit 8)

## ◆ RTC_ALM1TIME_ALSEC_Msk

#define RTC_ALM1TIME_ALSEC_Msk (0x7FUL)

RTC ALM1TIME: ALSEC (Bitfield-Mask: 0x7F)

## ◆ RTC_ALM1TIME_ALSEC_Pos

#define RTC_ALM1TIME_ALSEC_Pos (0UL)

RTC ALM1TIME: ALSEC (Bit 0)

## ◆ RTC_ALM1TIME_ALWEEK_Msk

#define RTC_ALM1TIME_ALWEEK_Msk (0x7000000UL)

RTC ALM1TIME: ALWEEK (Bitfield-Mask: 0x07)

## ◆ RTC_ALM1TIME_ALWEEK_Pos

#define RTC_ALM1TIME_ALWEEK_Pos (24UL)

RTC ALM1TIME: ALWEEK (Bit 24)

## ◆ RTC_ALM2PRD_ALM2PR_CNT_Msk

#define RTC_ALM2PRD_ALM2PR_CNT_Msk (0xFUL)

RTC ALM2PRD: ALM2PR_CNT (Bitfield-Mask: 0x0F)

## ◆ RTC_ALM2PRD_ALM2PR_CNT_Pos

#define RTC_ALM2PRD_ALM2PR_CNT_Pos (0UL)

RTC ALM2PRD: ALM2PR_CNT (Bit 0)

## ◆ RTC_CLKCR_HSEDIV_Msk

#define RTC_CLKCR_HSEDIV_Msk (0x3FFUL)

RTC CLKCR: HSEDIV (Bitfield-Mask: 0x3FF)

## ◆ RTC_CLKCR_HSEDIV_Pos

#define RTC_CLKCR_HSEDIV_Pos (0UL)

RTC CLKCR: HSEDIV (Bit 0)

## ◆ RTC_CLKCR_RTCCKEN_Msk

#define RTC_CLKCR_RTCCKEN_Msk (0x100000UL)

RTC CLKCR: RTCCKEN (Bitfield-Mask: 0x01)

## ◆ RTC_CLKCR_RTCCKEN_Pos

#define RTC_CLKCR_RTCCKEN_Pos (20UL)

RTC CLKCR: RTCCKEN (Bit 20)

## ◆ RTC_CLKCR_RTCCKSEL_Msk

#define RTC_CLKCR_RTCCKSEL_Msk (0x30000UL)

RTC CLKCR: RTCCKSEL (Bitfield-Mask: 0x03)

## ◆ RTC_CLKCR_RTCCKSEL_Pos

#define RTC_CLKCR_RTCCKSEL_Pos (16UL)

RTC CLKCR: RTCCKSEL (Bit 16)

## ◆ RTC_CLKTRIM_MODE_1_0_Msk

#define RTC_CLKTRIM_MODE_1_0_Msk (0x100UL)

RTC CLKTRIM: MODE_1_0 (Bitfield-Mask: 0x01)

## ◆ RTC_CLKTRIM_MODE_1_0_Pos

#define RTC_CLKTRIM_MODE_1_0_Pos (8UL)

RTC CLKTRIM: MODE_1_0 (Bit 8)

## ◆ RTC_CLKTRIM_TRIM_Msk

#define RTC_CLKTRIM_TRIM_Msk (0xFFUL)

RTC CLKTRIM: TRIM (Bitfield-Mask: 0xFF)

## ◆ RTC_CLKTRIM_TRIM_Pos

#define RTC_CLKTRIM_TRIM_Pos (0UL)

RTC CLKTRIM: TRIM (Bit 0)

## ◆ RTC_CR_ALM1_INTEN_Msk

#define RTC_CR_ALM1_INTEN_Msk (0x10UL)

RTC CR: ALM1_INTEN (Bitfield-Mask: 0x01)

## ◆ RTC_CR_ALM1_INTEN_Pos

#define RTC_CR_ALM1_INTEN_Pos (4UL)

RTC CR: ALM1_INTEN (Bit 4)

## ◆ RTC_CR_ALM1EN_Msk

#define RTC_CR_ALM1EN_Msk (0x40UL)

RTC CR: ALM1EN (Bitfield-Mask: 0x01)

## ◆ RTC_CR_ALM1EN_Pos

#define RTC_CR_ALM1EN_Pos (6UL)

RTC CR: ALM1EN (Bit 6)

## ◆ RTC_CR_ALM2_INTEN_Msk

#define RTC_CR_ALM2_INTEN_Msk (0x20UL)

RTC CR: ALM2_INTEN (Bitfield-Mask: 0x01)

## ◆ RTC_CR_ALM2_INTEN_Pos

#define RTC_CR_ALM2_INTEN_Pos (5UL)

RTC CR: ALM2_INTEN (Bit 5)

## ◆ RTC_CR_BYPSHAD_Msk

#define RTC_CR_BYPSHAD_Msk (0x1UL)

RTC CR: BYPSHAD (Bitfield-Mask: 0x01)

## ◆ RTC_CR_BYPSHAD_Pos

#define RTC_CR_BYPSHAD_Pos (0UL)

RTC CR: BYPSHAD (Bit 0)

## ◆ RTC_CR_FMT_Msk

#define RTC_CR_FMT_Msk (0x4UL)

RTC CR: FMT (Bitfield-Mask: 0x01)

## ◆ RTC_CR_FMT_Pos

#define RTC_CR_FMT_Pos (2UL)

RTC CR: FMT (Bit 2)

## ◆ RTC_CR_RTC1HZOE_Msk

#define RTC_CR_RTC1HZOE_Msk (0x2UL)

RTC CR: RTC1HZOE (Bitfield-Mask: 0x01)

## ◆ RTC_CR_RTC1HZOE_Pos

#define RTC_CR_RTC1HZOE_Pos (1UL)

RTC CR: RTC1HZOE (Bit 1)

## ◆ RTC_CR_START_Msk

#define RTC_CR_START_Msk (0x100UL)

RTC CR: START (Bitfield-Mask: 0x01)

## ◆ RTC_CR_START_Pos

#define RTC_CR_START_Pos (8UL)

RTC CR: START (Bit 8)

## ◆ RTC_DATE_CEN_Msk

#define RTC_DATE_CEN_Msk (0x8000UL)

RTC DATE: CEN (Bitfield-Mask: 0x01)

## ◆ RTC_DATE_CEN_Pos

#define RTC_DATE_CEN_Pos (15UL)

RTC DATE: CEN (Bit 15)

## ◆ RTC_DATE_DAY_Msk

#define RTC_DATE_DAY_Msk (0x3FUL)

RTC DATE: DAY (Bitfield-Mask: 0x3F)

## ◆ RTC_DATE_DAY_Pos

#define RTC_DATE_DAY_Pos (0UL)

RTC DATE: DAY (Bit 0)

## ◆ RTC_DATE_MONTH_Msk

#define RTC_DATE_MONTH_Msk (0x1F00UL)

RTC DATE: MONTH (Bitfield-Mask: 0x1F)

## ◆ RTC_DATE_MONTH_Pos

#define RTC_DATE_MONTH_Pos (8UL)

RTC DATE: MONTH (Bit 8)

## ◆ RTC_DATE_YEAR_Msk

#define RTC_DATE_YEAR_Msk (0xFF0000UL)

RTC DATE: YEAR (Bitfield-Mask: 0xFF)

## ◆ RTC_DATE_YEAR_Pos

#define RTC_DATE_YEAR_Pos (16UL)

RTC DATE: YEAR (Bit 16)

## ◆ RTC_INTCLR_ALM1_CLR_Msk

#define RTC_INTCLR_ALM1_CLR_Msk (0x10UL)

RTC INTCLR: ALM1_CLR (Bitfield-Mask: 0x01)

## ◆ RTC_INTCLR_ALM1_CLR_Pos

#define RTC_INTCLR_ALM1_CLR_Pos (4UL)

RTC INTCLR: ALM1_CLR (Bit 4)

## ◆ RTC_INTCLR_ALM2_CLR_Msk

#define RTC_INTCLR_ALM2_CLR_Msk (0x20UL)

RTC INTCLR: ALM2_CLR (Bitfield-Mask: 0x01)

## ◆ RTC_INTCLR_ALM2_CLR_Pos

#define RTC_INTCLR_ALM2_CLR_Pos (5UL)

RTC INTCLR: ALM2_CLR (Bit 5)

## ◆ RTC_ISR_ALM1_F_Msk

#define RTC_ISR_ALM1_F_Msk (0x10UL)

RTC ISR: ALM1_F (Bitfield-Mask: 0x01)

## ◆ RTC_ISR_ALM1_F_Pos

#define RTC_ISR_ALM1_F_Pos (4UL)

RTC ISR: ALM1_F (Bit 4)

## ◆ RTC_ISR_ALM2_F_Msk

#define RTC_ISR_ALM2_F_Msk (0x20UL)

RTC ISR: ALM2_F (Bitfield-Mask: 0x01)

## ◆ RTC_ISR_ALM2_F_Pos

#define RTC_ISR_ALM2_F_Pos (5UL)

RTC ISR: ALM2_F (Bit 5)

## ◆ RTC_ISR_RSF_Msk

#define RTC_ISR_RSF_Msk (0x4UL)

RTC ISR: RSF (Bitfield-Mask: 0x01)

## ◆ RTC_ISR_RSF_Pos

#define RTC_ISR_RSF_Pos (2UL)

RTC ISR: RSF (Bit 2)

## ◆ RTC_ISR_WAIT_Msk

#define RTC_ISR_WAIT_Msk (0x1UL)

RTC ISR: WAIT (Bitfield-Mask: 0x01)

## ◆ RTC_ISR_WAIT_Pos

#define RTC_ISR_WAIT_Pos (0UL)

RTC ISR: WAIT (Bit 0)

## ◆ RTC_ISR_WAITF_Msk

#define RTC_ISR_WAITF_Msk (0x2UL)

RTC ISR: WAITF (Bitfield-Mask: 0x01)

## ◆ RTC_ISR_WAITF_Pos

#define RTC_ISR_WAITF_Pos (1UL)

RTC ISR: WAITF (Bit 1)

## ◆ RTC_TIME_H20_PA_Msk

#define RTC_TIME_H20_PA_Msk (0x200000UL)

RTC TIME: H20_PA (Bitfield-Mask: 0x01)

## ◆ RTC_TIME_H20_PA_Pos

#define RTC_TIME_H20_PA_Pos (21UL)

RTC TIME: H20_PA (Bit 21)

## ◆ RTC_TIME_HOUR19_Msk

#define RTC_TIME_HOUR19_Msk (0x1F0000UL)

RTC TIME: HOUR19 (Bitfield-Mask: 0x1F)

## ◆ RTC_TIME_HOUR19_Pos

#define RTC_TIME_HOUR19_Pos (16UL)

RTC TIME: HOUR19 (Bit 16)

## ◆ RTC_TIME_MIN_Msk

#define RTC_TIME_MIN_Msk (0x7F00UL)

RTC TIME: MIN (Bitfield-Mask: 0x7F)

## ◆ RTC_TIME_MIN_Pos

#define RTC_TIME_MIN_Pos (8UL)

RTC TIME: MIN (Bit 8)

## ◆ RTC_TIME_SEC_Msk

#define RTC_TIME_SEC_Msk (0x7FUL)

RTC TIME: SEC (Bitfield-Mask: 0x3F)

## ◆ RTC_TIME_SEC_Pos

#define RTC_TIME_SEC_Pos (0UL)

RTC TIME: SEC (Bit 0)

## ◆ RTC_TIME_WEEK_Msk

#define RTC_TIME_WEEK_Msk (0x7000000UL)

RTC TIME: WEEK (Bitfield-Mask: 0x07)

## ◆ RTC_TIME_WEEK_Pos

#define RTC_TIME_WEEK_Pos (24UL)

RTC TIME: WEEK (Bit 24)

## ◆ RTC_WPR_WPR_Msk

#define RTC_WPR_WPR_Msk (0xFFUL)

RTC WPR: WPR (Bitfield-Mask: 0xFF)

## ◆ RTC_WPR_WPR_Pos

#define RTC_WPR_WPR_Pos (0UL)

RTC WPR: WPR (Bit 0)

## ◆ SPI_CR_CPHA_Msk

#define SPI_CR_CPHA_Msk (0x4UL)

SPI CR: CPHA (Bitfield-Mask: 0x01)

## ◆ SPI_CR_CPHA_Pos

#define SPI_CR_CPHA_Pos (2UL)

SPI CR: CPHA (Bit 2)

## ◆ SPI_CR_CPOL_Msk

#define SPI_CR_CPOL_Msk (0x8UL)

SPI CR: CPOL (Bitfield-Mask: 0x01)

## ◆ SPI_CR_CPOL_Pos

#define SPI_CR_CPOL_Pos (3UL)

SPI CR: CPOL (Bit 3)

## ◆ SPI_CR_MSTR_Msk

#define SPI_CR_MSTR_Msk (0x10UL)

SPI CR: MSTR (Bitfield-Mask: 0x01)

## ◆ SPI_CR_MSTR_Pos

#define SPI_CR_MSTR_Pos (4UL)

SPI CR: MSTR (Bit 4)

## ◆ SPI_CR_SPEN_Msk

#define SPI_CR_SPEN_Msk (0x40UL)

SPI CR: SPEN (Bitfield-Mask: 0x01)

## ◆ SPI_CR_SPEN_Pos

#define SPI_CR_SPEN_Pos (6UL)

SPI CR: SPEN (Bit 6)

## ◆ SPI_CR_SPR0_Msk

#define SPI_CR_SPR0_Msk (0x1UL)

SPI CR: SPR0 (Bitfield-Mask: 0x01)

## ◆ SPI_CR_SPR0_Pos

#define SPI_CR_SPR0_Pos (0UL)

SPI CR: SPR0 (Bit 0)

## ◆ SPI_CR_SPR1_Msk

#define SPI_CR_SPR1_Msk (0x2UL)

SPI CR: SPR1 (Bitfield-Mask: 0x01)

## ◆ SPI_CR_SPR1_Pos

#define SPI_CR_SPR1_Pos (1UL)

SPI CR: SPR1 (Bit 1)

## ◆ SPI_CR_SPR2_Msk

#define SPI_CR_SPR2_Msk (0x80UL)

SPI CR: SPR2 (Bitfield-Mask: 0x01)

## ◆ SPI_CR_SPR2_Pos

#define SPI_CR_SPR2_Pos (7UL)

SPI CR: SPR2 (Bit 7)

## ◆ SPI_DATA_SPDATA_Msk

#define SPI_DATA_SPDATA_Msk (0xFFUL)

SPI DATA: SPDATA (Bitfield-Mask: 0xFF)

## ◆ SPI_DATA_SPDATA_Pos

#define SPI_DATA_SPDATA_Pos (0UL)

SPI DATA: SPDATA (Bit 0)

## ◆ SPI_SR_MDF_Msk

#define SPI_SR_MDF_Msk (0x10UL)

SPI SR: MDF (Bitfield-Mask: 0x01)

## ◆ SPI_SR_MDF_Pos

#define SPI_SR_MDF_Pos (4UL)

SPI SR: MDF (Bit 4)

## ◆ SPI_SR_SPIF_Msk

#define SPI_SR_SPIF_Msk (0x80UL)

SPI SR: SPIF (Bitfield-Mask: 0x01)

## ◆ SPI_SR_SPIF_Pos

#define SPI_SR_SPIF_Pos (7UL)

SPI SR: SPIF (Bit 7)

## ◆ SPI_SR_SSERR_Msk

#define SPI_SR_SSERR_Msk (0x20UL)

SPI SR: SSERR (Bitfield-Mask: 0x01)

## ◆ SPI_SR_SSERR_Pos

#define SPI_SR_SSERR_Pos (5UL)

SPI SR: SSERR (Bit 5)

## ◆ SPI_SR_WCOL_Msk

#define SPI_SR_WCOL_Msk (0x40UL)

SPI SR: WCOL (Bitfield-Mask: 0x01)

## ◆ SPI_SR_WCOL_Pos

#define SPI_SR_WCOL_Pos (6UL)

SPI SR: WCOL (Bit 6)

## ◆ SPI_SSN_SSN_Msk

#define SPI_SSN_SSN_Msk (0x1UL)

SPI SSN: SSN (Bitfield-Mask: 0x01)

## ◆ SPI_SSN_SSN_Pos

#define SPI_SSN_SSN_Pos (0UL)

SPI SSN: SSN (Bit 0)

## ◆ SRAM_MEMORY_BASE

#define SRAM_MEMORY_BASE ((uint32_t)0x20000000UL)

SRAM base address in the alias region

## ◆ SYSCON_CFGR0_DBGDLSP_DIS_Msk

#define SYSCON_CFGR0_DBGDLSP_DIS_Msk (0x2UL)

SYSCON CFGR0: DBGDLSP_DIS (Bitfield-Mask: 0x01)

## ◆ SYSCON_CFGR0_DBGDLSP_DIS_Pos

#define SYSCON_CFGR0_DBGDLSP_DIS_Pos (1UL)

SYSCON CFGR0: DBGDLSP_DIS (Bit 1)

## ◆ SYSCON_CFGR0_KEY_Msk

#define SYSCON_CFGR0_KEY_Msk (0xFFFF0000UL)

SYSCON CFGR0: KEY (Bitfield-Mask: 0xFFFF)

## ◆ SYSCON_CFGR0_KEY_Pos

#define SYSCON_CFGR0_KEY_Pos (16UL)

SYSCON CFGR0: KEY (Bit 16)

## ◆ SYSCON_CFGR0_LOCKUPEN_Msk

#define SYSCON_CFGR0_LOCKUPEN_Msk (0x1UL)

SYSCON CFGR0: LOCKUPEN (Bitfield-Mask: 0x01)

## ◆ SYSCON_CFGR0_LOCKUPEN_Pos

#define SYSCON_CFGR0_LOCKUPEN_Pos (0UL)

SYSCON CFGR0: LOCKUPEN (Bit 0)

## ◆ SYSCON_PCACR_PCA_CAP0_SEL_Msk

#define SYSCON_PCACR_PCA_CAP0_SEL_Msk (0x3UL)

SYSCON PCACR: PCA_CAP0_SEL (Bitfield-Mask: 0x03)

## ◆ SYSCON_PCACR_PCA_CAP0_SEL_Pos

#define SYSCON_PCACR_PCA_CAP0_SEL_Pos (0UL)

SYSCON PCACR: PCA_CAP0_SEL (Bit 0)

## ◆ SYSCON_PCACR_PCA_CAP1_SEL_Msk

#define SYSCON_PCACR_PCA_CAP1_SEL_Msk (0xCUL)

SYSCON PCACR: PCA_CAP1_SEL (Bitfield-Mask: 0x03)

## ◆ SYSCON_PCACR_PCA_CAP1_SEL_Pos

#define SYSCON_PCACR_PCA_CAP1_SEL_Pos (2UL)

SYSCON PCACR: PCA_CAP1_SEL (Bit 2)

## ◆ SYSCON_PCACR_PCA_CAP2_SEL_Msk

#define SYSCON_PCACR_PCA_CAP2_SEL_Msk (0x30UL)

SYSCON PCACR: PCA_CAP2_SEL (Bitfield-Mask: 0x03)

## ◆ SYSCON_PCACR_PCA_CAP2_SEL_Pos

#define SYSCON_PCACR_PCA_CAP2_SEL_Pos (4UL)

SYSCON PCACR: PCA_CAP2_SEL (Bit 4)

## ◆ SYSCON_PCACR_PCA_CAP3_SEL_Msk

#define SYSCON_PCACR_PCA_CAP3_SEL_Msk (0xC0UL)

SYSCON PCACR: PCA_CAP3_SEL (Bitfield-Mask: 0x03)

## ◆ SYSCON_PCACR_PCA_CAP3_SEL_Pos

#define SYSCON_PCACR_PCA_CAP3_SEL_Pos (6UL)

SYSCON PCACR: PCA_CAP3_SEL (Bit 6)

## ◆ SYSCON_PCACR_PCA_CAP4_SEL_Msk

#define SYSCON_PCACR_PCA_CAP4_SEL_Msk (0x300UL)

SYSCON PCACR: PCA_CAP4_SEL (Bitfield-Mask: 0x03)

## ◆ SYSCON_PCACR_PCA_CAP4_SEL_Pos

#define SYSCON_PCACR_PCA_CAP4_SEL_Pos (8UL)

SYSCON PCACR: PCA_CAP4_SEL (Bit 8)

## ◆ SYSCON_PORTCR_LPTIM_GATE_SEL_Msk

#define SYSCON_PORTCR_LPTIM_GATE_SEL_Msk (0x300UL)

SYSCON PORTCR: LPTIM_GATE_SEL (Bitfield-Mask: 0x03)

## ◆ SYSCON_PORTCR_LPTIM_GATE_SEL_Pos

#define SYSCON_PORTCR_LPTIM_GATE_SEL_Pos (8UL)

SYSCON PORTCR: LPTIM GATE_SEL (Bit 8)

## ◆ SYSCON_PORTCR_TIM10_GATE_SEL_Msk

#define SYSCON_PORTCR_TIM10_GATE_SEL_Msk (0x30UL)

SYSCON PORTCR: TIM10_GATE_SEL (Bitfield-Mask: 0x03)

## ◆ SYSCON_PORTCR_TIM10_GATE_SEL_Pos

#define SYSCON_PORTCR_TIM10_GATE_SEL_Pos (4UL)

SYSCON PORTCR: TIM10_GATE_SEL (Bit 4)

## ◆ SYSCON_PORTCR_TIM11_GATE_SEL_Msk

#define SYSCON_PORTCR_TIM11_GATE_SEL_Msk (0xC0UL)

SYSCON PORTCR: TIM11_GATE_SEL (Bitfield-Mask: 0x03)

## ◆ SYSCON_PORTCR_TIM11_GATE_SEL_Pos

#define SYSCON_PORTCR_TIM11_GATE_SEL_Pos (6UL)

SYSCON PORTCR: TIM11_GATE_SEL (Bit 6)

## ◆ SYSCON_PORTINTCR_KEY_Msk

#define SYSCON_PORTINTCR_KEY_Msk (0xFFFF0000UL)

SYSCON PORTINTCR: KEY (Bitfield-Mask: 0xFFFF)

## ◆ SYSCON_PORTINTCR_KEY_Pos

#define SYSCON_PORTINTCR_KEY_Pos (16UL)

SYSCON PORTINTCR: KEY (Bit 16)

## ◆ SYSCON_PORTINTCR_PADDLSPCON_Msk

#define SYSCON_PORTINTCR_PADDLSPCON_Msk (0x2UL)

SYSCON PORTINTCR: PADDLSPCON (Bitfield-Mask: 0x01)

## ◆ SYSCON_PORTINTCR_PADDLSPCON_Pos

#define SYSCON_PORTINTCR_PADDLSPCON_Pos (1UL)

SYSCON PORTINTCR: PADDLSPCON (Bit 1)

## ◆ SYSCON_PORTINTCR_PADINTSEL_Msk

#define SYSCON_PORTINTCR_PADINTSEL_Msk (0x1UL)

SYSCON PORTINTCR: PADINTSEL (Bitfield-Mask: 0x01)

## ◆ SYSCON_PORTINTCR_PADINTSEL_Pos

#define SYSCON_PORTINTCR_PADINTSEL_Pos (0UL)

SYSCON PORTINTCR: PADINTSEL (Bit 0)

## ◆ SYSCON_TIM1CR_CLKFAILBRKEN_Msk

#define SYSCON_TIM1CR_CLKFAILBRKEN_Msk (0x400000UL)

SYSCON TIM1CR: CLKFAILBRKEN (Bitfield-Mask: 0x01)

## ◆ SYSCON_TIM1CR_CLKFAILBRKEN_Pos

#define SYSCON_TIM1CR_CLKFAILBRKEN_Pos (22UL)

SYSCON TIM1CR: CLKFAILBRKEN (Bit 22)

## ◆ SYSCON_TIM1CR_DSLPBRKEN_Msk

#define SYSCON_TIM1CR_DSLPBRKEN_Msk (0x200000UL)

SYSCON TIM1CR: DSLPBRKEN (Bitfield-Mask: 0x01)

## ◆ SYSCON_TIM1CR_DSLPBRKEN_Pos

#define SYSCON_TIM1CR_DSLPBRKEN_Pos (21UL)

SYSCON TIM1CR: DSLPBRKEN (Bit 21)

## ◆ SYSCON_TIM1CR_TIM1BRKOUTCFG_Msk

#define SYSCON_TIM1CR_TIM1BRKOUTCFG_Msk (0x100000UL)

SYSCON TIM1CR: TIM1BRKOUTCFG (Bitfield-Mask: 0x01)

## ◆ SYSCON_TIM1CR_TIM1BRKOUTCFG_Pos

#define SYSCON_TIM1CR_TIM1BRKOUTCFG_Pos (20UL)

SYSCON TIM1CR: TIM1BRKOUTCFG (Bit 20)

## ◆ SYSCON_TIM1CR_TIM1CH1IN_SEL_Msk

#define SYSCON_TIM1CR_TIM1CH1IN_SEL_Msk (0x7UL)

SYSCON TIM1CR: TIM1CH1IN_SEL (Bitfield-Mask: 0x07)

## ◆ SYSCON_TIM1CR_TIM1CH1IN_SEL_Pos

#define SYSCON_TIM1CR_TIM1CH1IN_SEL_Pos (0UL)

SYSCON TIM1CR: TIM1CH1IN_SEL (Bit 0)

## ◆ SYSCON_TIM1CR_TIM1CH2IN_SEL_Msk

#define SYSCON_TIM1CR_TIM1CH2IN_SEL_Msk (0x70UL)

SYSCON TIM1CR: TIM1CH2IN_SEL (Bitfield-Mask: 0x07)

## ◆ SYSCON_TIM1CR_TIM1CH2IN_SEL_Pos

#define SYSCON_TIM1CR_TIM1CH2IN_SEL_Pos (4UL)

SYSCON TIM1CR: TIM1CH2IN_SEL (Bit 4)

## ◆ SYSCON_TIM1CR_TIM1CH3IN_SEL_Msk

#define SYSCON_TIM1CR_TIM1CH3IN_SEL_Msk (0x700UL)

SYSCON TIM1CR: TIM1CH3IN_SEL (Bitfield-Mask: 0x07)

## ◆ SYSCON_TIM1CR_TIM1CH3IN_SEL_Pos

#define SYSCON_TIM1CR_TIM1CH3IN_SEL_Pos (8UL)

SYSCON TIM1CR: TIM1CH3IN_SEL (Bit 8)

## ◆ SYSCON_TIM1CR_TIM1CH4IN_SEL_Msk

#define SYSCON_TIM1CR_TIM1CH4IN_SEL_Msk (0x7000UL)

SYSCON TIM1CR: TIM1CH4IN_SEL (Bitfield-Mask: 0x07)

## ◆ SYSCON_TIM1CR_TIM1CH4IN_SEL_Pos

#define SYSCON_TIM1CR_TIM1CH4IN_SEL_Pos (12UL)

SYSCON TIM1CR: TIM1CH4IN_SEL (Bit 12)

## ◆ SYSCON_TIM2CR_TIM2CH1IN_SEL_Msk

#define SYSCON_TIM2CR_TIM2CH1IN_SEL_Msk (0x7UL)

SYSCON TIM2CR: TIM2CH1IN_SEL (Bitfield-Mask: 0x07)

## ◆ SYSCON_TIM2CR_TIM2CH1IN_SEL_Pos

#define SYSCON_TIM2CR_TIM2CH1IN_SEL_Pos (0UL)

SYSCON TIM2CR: TIM2CH1IN_SEL (Bit 0)

## ◆ SYSCON_TIM2CR_TIM2CH2IN_SEL_Msk

#define SYSCON_TIM2CR_TIM2CH2IN_SEL_Msk (0x70UL)

SYSCON TIM2CR: TIM2CH2IN_SEL (Bitfield-Mask: 0x07)

## ◆ SYSCON_TIM2CR_TIM2CH2IN_SEL_Pos

#define SYSCON_TIM2CR_TIM2CH2IN_SEL_Pos (4UL)

SYSCON TIM2CR: TIM2CH2IN_SEL (Bit 4)

## ◆ SYSCON_TIM2CR_TIM2CH3IN_SEL_Msk

#define SYSCON_TIM2CR_TIM2CH3IN_SEL_Msk (0x700UL)

SYSCON TIM2CR: TIM2CH3IN_SEL (Bitfield-Mask: 0x07)

## ◆ SYSCON_TIM2CR_TIM2CH3IN_SEL_Pos

#define SYSCON_TIM2CR_TIM2CH3IN_SEL_Pos (8UL)

SYSCON TIM2CR: TIM2CH3IN_SEL (Bit 8)

## ◆ SYSCON_TIM2CR_TIM2CH4IN_SEL_Msk

#define SYSCON_TIM2CR_TIM2CH4IN_SEL_Msk (0x7000UL)

SYSCON TIM2CR: TIM2CH4IN_SEL (Bitfield-Mask: 0x07)

## ◆ SYSCON_TIM2CR_TIM2CH4IN_SEL_Pos

#define SYSCON_TIM2CR_TIM2CH4IN_SEL_Pos (12UL)

SYSCON TIM2CR: TIM2CH4IN_SEL (Bit 12)

## ◆ SYSCON_UNLOCK_KEY_Msk

#define SYSCON_UNLOCK_KEY_Msk (0xFFFFFFFEUL)

SYSCON UNLOCK: KEY (Bitfield-Mask: 0x7FFFFFFF)

## ◆ SYSCON_UNLOCK_KEY_Pos

#define SYSCON_UNLOCK_KEY_Pos (1UL)

SYSCON UNLOCK: KEY (Bit 1)

## ◆ SYSCON_UNLOCK_UNLOCK_Msk

#define SYSCON_UNLOCK_UNLOCK_Msk (0x1UL)

SYSCON UNLOCK: UNLOCK (Bitfield-Mask: 0x01)

## ◆ SYSCON_UNLOCK_UNLOCK_Pos

#define SYSCON_UNLOCK_UNLOCK_Pos (0UL)

SYSCON UNLOCK: UNLOCK (Bit 0)

## ◆ TIM_ARR_ARR_Msk

#define TIM_ARR_ARR_Msk (0xFFFFUL)

TIM ARR: ARR (Bitfield-Mask: 0xFFFF)

## ◆ TIM_ARR_ARR_Pos

#define TIM_ARR_ARR_Pos (0UL)

TIM ARR: ARR (Bit 0)

## ◆ TIM_BDTR_AOE_Msk

#define TIM_BDTR_AOE_Msk (0x4000UL)

TIM BDTR: AOE (Bitfield-Mask: 0x01)

## ◆ TIM_BDTR_AOE_Pos

#define TIM_BDTR_AOE_Pos (14UL)

TIM BDTR: AOE (Bit 14)

## ◆ TIM_BDTR_BKE_Msk

#define TIM_BDTR_BKE_Msk (0x1000UL)

TIM BDTR: BKE (Bitfield-Mask: 0x01)

## ◆ TIM_BDTR_BKE_Pos

#define TIM_BDTR_BKE_Pos (12UL)

TIM BDTR: BKE (Bit 12)

## ◆ TIM_BDTR_BKP_Msk

#define TIM_BDTR_BKP_Msk (0x2000UL)

TIM BDTR: BKP (Bitfield-Mask: 0x01)

## ◆ TIM_BDTR_BKP_Pos

#define TIM_BDTR_BKP_Pos (13UL)

TIM BDTR: BKP (Bit 13)

## ◆ TIM_BDTR_DTG_Msk

#define TIM_BDTR_DTG_Msk (0xFFUL)

TIM BDTR: UTG (Bitfield-Mask: 0xFF)

## ◆ TIM_BDTR_DTG_Pos

#define TIM_BDTR_DTG_Pos (0UL)

TIM BDTR: UTG (Bit 0)

## ◆ TIM_BDTR_LOCK_Msk

#define TIM_BDTR_LOCK_Msk (0x300UL)

TIM BDTR: LOCK (Bitfield-Mask: 0x03)

## ◆ TIM_BDTR_LOCK_Pos

#define TIM_BDTR_LOCK_Pos (8UL)

TIM BDTR: LOCK (Bit 8)

## ◆ TIM_BDTR_MOE_Msk

#define TIM_BDTR_MOE_Msk (0x8000UL)

TIM BDTR: MOE (Bitfield-Mask: 0x01)

## ◆ TIM_BDTR_MOE_Pos

#define TIM_BDTR_MOE_Pos (15UL)

TIM BDTR: MOE (Bit 15)

## ◆ TIM_BDTR_OSSI_Msk

#define TIM_BDTR_OSSI_Msk (0x400UL)

TIM BDTR: OSSI (Bitfield-Mask: 0x01)

## ◆ TIM_BDTR_OSSI_Pos

#define TIM_BDTR_OSSI_Pos (10UL)

TIM BDTR: OSSI (Bit 10)

## ◆ TIM_BDTR_OSSR_Msk

#define TIM_BDTR_OSSR_Msk (0x800UL)

TIM BDTR: OSSR (Bitfield-Mask: 0x01)

## ◆ TIM_BDTR_OSSR_Pos

#define TIM_BDTR_OSSR_Pos (11UL)

TIM BDTR: OSSR (Bit 11)

## ◆ TIM_CCER_CC1E_Msk

#define TIM_CCER_CC1E_Msk (0x1UL)

TIM CCER: CC1E (Bitfield-Mask: 0x01)

## ◆ TIM_CCER_CC1E_Pos

#define TIM_CCER_CC1E_Pos (0UL)

TIM CCER: CC1E (Bit 0)

## ◆ TIM_CCER_CC1NE_Msk

#define TIM_CCER_CC1NE_Msk (0x4UL)

TIM CCER: CC1NE (Bitfield-Mask: 0x01)

## ◆ TIM_CCER_CC1NE_Pos

#define TIM_CCER_CC1NE_Pos (2UL)

TIM CCER: CC1NE (Bit 2)

## ◆ TIM_CCER_CC1NP_Msk

#define TIM_CCER_CC1NP_Msk (0x8UL)

TIM CCER: CC1NP (Bitfield-Mask: 0x01)

## ◆ TIM_CCER_CC1NP_Pos

#define TIM_CCER_CC1NP_Pos (3UL)

TIM CCER: CC1NP (Bit 3)

## ◆ TIM_CCER_CC1P_Msk

#define TIM_CCER_CC1P_Msk (0x2UL)

TIM CCER: CC1P (Bitfield-Mask: 0x01)

## ◆ TIM_CCER_CC1P_Pos

#define TIM_CCER_CC1P_Pos (1UL)

TIM CCER: CC1P (Bit 1)

## ◆ TIM_CCER_CC2E_Msk

#define TIM_CCER_CC2E_Msk (0x10UL)

TIM CCER: CC2E (Bitfield-Mask: 0x01)

## ◆ TIM_CCER_CC2E_Pos

#define TIM_CCER_CC2E_Pos (4UL)

TIM CCER: CC2E (Bit 4)

## ◆ TIM_CCER_CC2NE_Msk

#define TIM_CCER_CC2NE_Msk (0x40UL)

TIM CCER: CC2NE (Bitfield-Mask: 0x01)

## ◆ TIM_CCER_CC2NE_Pos

#define TIM_CCER_CC2NE_Pos (6UL)

TIM CCER: CC2NE (Bit 6)

## ◆ TIM_CCER_CC2NP_Msk

#define TIM_CCER_CC2NP_Msk (0x80UL)

TIM CCER: CC2NP (Bitfield-Mask: 0x01)

## ◆ TIM_CCER_CC2NP_Pos

#define TIM_CCER_CC2NP_Pos (7UL)

TIM CCER: CC2NP (Bit 7)

## ◆ TIM_CCER_CC2P_Msk

#define TIM_CCER_CC2P_Msk (0x20UL)

TIM CCER: CC2P (Bitfield-Mask: 0x01)

## ◆ TIM_CCER_CC2P_Pos

#define TIM_CCER_CC2P_Pos (5UL)

TIM CCER: CC2P (Bit 5)

## ◆ TIM_CCER_CC3E_Msk

#define TIM_CCER_CC3E_Msk (0x100UL)

TIM CCER: CC3E (Bitfield-Mask: 0x01)

## ◆ TIM_CCER_CC3E_Pos

#define TIM_CCER_CC3E_Pos (8UL)

TIM CCER: CC3E (Bit 8)

## ◆ TIM_CCER_CC3NE_Msk

#define TIM_CCER_CC3NE_Msk (0x400UL)

TIM CCER: CC3NE (Bitfield-Mask: 0x01)

## ◆ TIM_CCER_CC3NE_Pos

#define TIM_CCER_CC3NE_Pos (10UL)

TIM CCER: CC3NE (Bit 10)

## ◆ TIM_CCER_CC3NP_Msk

#define TIM_CCER_CC3NP_Msk (0x800UL)

TIM CCER: CC3NP (Bitfield-Mask: 0x01)

## ◆ TIM_CCER_CC3NP_Pos

#define TIM_CCER_CC3NP_Pos (11UL)

TIM CCER: CC3NP (Bit 11)

## ◆ TIM_CCER_CC3P_Msk

#define TIM_CCER_CC3P_Msk (0x200UL)

TIM CCER: CC3P (Bitfield-Mask: 0x01)

## ◆ TIM_CCER_CC3P_Pos

#define TIM_CCER_CC3P_Pos (9UL)

TIM CCER: CC3P (Bit 9)

## ◆ TIM_CCER_CC4E_Msk

#define TIM_CCER_CC4E_Msk (0x1000UL)

TIM CCER: CC4E (Bitfield-Mask: 0x01)

## ◆ TIM_CCER_CC4E_Pos

#define TIM_CCER_CC4E_Pos (12UL)

TIM CCER: CC4E (Bit 12)

## ◆ TIM_CCER_CC4P_Msk

#define TIM_CCER_CC4P_Msk (0x2000UL)

TIM CCER: CC4P (Bitfield-Mask: 0x01)

## ◆ TIM_CCER_CC4P_Pos

#define TIM_CCER_CC4P_Pos (13UL)

TIM CCER: CC4P (Bit 13)

## ◆ TIM_CCMR1_CC1S_Msk

#define TIM_CCMR1_CC1S_Msk (0x3UL)

TIM CCMR1: CC1S (Bitfield-Mask: 0x03)

## ◆ TIM_CCMR1_CC1S_Pos

#define TIM_CCMR1_CC1S_Pos (0UL)

TIM CCMR1: CC1S (Bit 0)

## ◆ TIM_CCMR1_CC2S_Msk

#define TIM_CCMR1_CC2S_Msk (0x300UL)

TIM CCMR1: CC2S (Bitfield-Mask: 0x03)

## ◆ TIM_CCMR1_CC2S_Pos

#define TIM_CCMR1_CC2S_Pos (8UL)

TIM CCMR1: CC2S (Bit 8)

## ◆ TIM_CCMR1_IC1F_Msk

#define TIM_CCMR1_IC1F_Msk (0x000000F0UL)

TIM CCMR1: IC1F (Bitfield-Mask: 0x0F)

## ◆ TIM_CCMR1_IC1F_Pos

#define TIM_CCMR1_IC1F_Pos (4UL)

TIM CCMR1: IC1F (Bit 4)

## ◆ TIM_CCMR1_IC1PSC_Msk

#define TIM_CCMR1_IC1PSC_Msk (0x0000000CUL)

TIM CCMR1: IC1PSC (Bitfield-Mask: 0x03)

## ◆ TIM_CCMR1_IC1PSC_Pos

#define TIM_CCMR1_IC1PSC_Pos (2UL)

TIM CCMR1: IC1PSC (Bit 2)

## ◆ TIM_CCMR1_IC2F_Msk

#define TIM_CCMR1_IC2F_Msk (0x0000F000UL)

TIM CCMR1: (Bitfield-Mask: 0x0F)

## ◆ TIM_CCMR1_IC2F_Pos

#define TIM_CCMR1_IC2F_Pos (12U)

TIM CCMR1: IC2F (Bit 12)

## ◆ TIM_CCMR1_IC2PSC_Msk

#define TIM_CCMR1_IC2PSC_Msk (0x00000C00UL)

TIM CCMR1: (Bitfield-Mask: 0x03)

## ◆ TIM_CCMR1_IC2PSC_Pos

#define TIM_CCMR1_IC2PSC_Pos (10UL)

TIM CCMR1: IC2PSC (Bit 10)

## ◆ TIM_CCMR1_OC1CE_Msk

#define TIM_CCMR1_OC1CE_Msk (0x80UL)

TIM CCMR1: OC1CE (Bitfield-Mask: 0x01)

## ◆ TIM_CCMR1_OC1CE_Pos

#define TIM_CCMR1_OC1CE_Pos (7UL)

TIM CCMR1: OC1CE (Bit 7)

## ◆ TIM_CCMR1_OC1FE_Msk

#define TIM_CCMR1_OC1FE_Msk (0x4UL)

TIM CCMR1: OC1FE (Bitfield-Mask: 0x01)

## ◆ TIM_CCMR1_OC1FE_Pos

#define TIM_CCMR1_OC1FE_Pos (2UL)

TIM CCMR1: OC1FE (Bit 2)

## ◆ TIM_CCMR1_OC1M_Msk

#define TIM_CCMR1_OC1M_Msk (0x70UL)

TIM CCMR1: OC1M (Bitfield-Mask: 0x07)

## ◆ TIM_CCMR1_OC1M_Pos

#define TIM_CCMR1_OC1M_Pos (4UL)

TIM CCMR1: OC1M (Bit 4)

## ◆ TIM_CCMR1_OC1PE_Msk

#define TIM_CCMR1_OC1PE_Msk (0x8UL)

TIM CCMR1: OC1PE (Bitfield-Mask: 0x01)

## ◆ TIM_CCMR1_OC1PE_Pos

#define TIM_CCMR1_OC1PE_Pos (3UL)

TIM CCMR1: OC1PE (Bit 3)

## ◆ TIM_CCMR1_OC2CE_Msk

#define TIM_CCMR1_OC2CE_Msk (0x8000UL)

TIM CCMR1: OC2CE (Bitfield-Mask: 0x01)

## ◆ TIM_CCMR1_OC2CE_Pos

#define TIM_CCMR1_OC2CE_Pos (15UL)

TIM CCMR1: OC2CE (Bit 15)

## ◆ TIM_CCMR1_OC2FE_Msk

#define TIM_CCMR1_OC2FE_Msk (0x400UL)

TIM CCMR1: OC2FE (Bitfield-Mask: 0x01)

## ◆ TIM_CCMR1_OC2FE_Pos

#define TIM_CCMR1_OC2FE_Pos (10UL)

TIM CCMR1: OC2FE (Bit 10)

## ◆ TIM_CCMR1_OC2M_Msk

#define TIM_CCMR1_OC2M_Msk (0x7000UL)

TIM CCMR1: OC2M (Bitfield-Mask: 0x07)

## ◆ TIM_CCMR1_OC2M_Pos

#define TIM_CCMR1_OC2M_Pos (12UL)

TIM CCMR1: OC2M (Bit 12)

## ◆ TIM_CCMR1_OC2PE_Msk

#define TIM_CCMR1_OC2PE_Msk (0x800UL)

TIM CCMR1: OC2PE (Bitfield-Mask: 0x01)

## ◆ TIM_CCMR1_OC2PE_Pos

#define TIM_CCMR1_OC2PE_Pos (11UL)

TIM CCMR1: OC2PE (Bit 11)

## ◆ TIM_CCMR2_CC3S_Msk

#define TIM_CCMR2_CC3S_Msk (0x3UL)

TIM CCMR2: CC3S (Bitfield-Mask: 0x03)

## ◆ TIM_CCMR2_CC3S_Pos

#define TIM_CCMR2_CC3S_Pos (0UL)

TIM CCMR2: CC3S (Bit 0)

## ◆ TIM_CCMR2_CC4S_Msk

#define TIM_CCMR2_CC4S_Msk (0x300UL)

TIM CCMR2: CC4S (Bitfield-Mask: 0x03)

## ◆ TIM_CCMR2_CC4S_Pos

#define TIM_CCMR2_CC4S_Pos (8UL)

TIM CCMR2: CC4S (Bit 8)

## ◆ TIM_CCMR2_OC3CE_Msk

#define TIM_CCMR2_OC3CE_Msk (0x80UL)

TIM CCMR2: OC3CE (Bitfield-Mask: 0x01)

## ◆ TIM_CCMR2_OC3CE_Pos

#define TIM_CCMR2_OC3CE_Pos (7UL)

TIM CCMR2: OC3CE (Bit 7)

## ◆ TIM_CCMR2_OC3FE_Msk

#define TIM_CCMR2_OC3FE_Msk (0x4UL)

TIM CCMR2: OC3FE (Bitfield-Mask: 0x01)

## ◆ TIM_CCMR2_OC3FE_Pos

#define TIM_CCMR2_OC3FE_Pos (2UL)

TIM CCMR2: OC3FE (Bit 2)

## ◆ TIM_CCMR2_OC3M_Msk

#define TIM_CCMR2_OC3M_Msk (0x70UL)

TIM CCMR2: OC3M (Bitfield-Mask: 0x07)

## ◆ TIM_CCMR2_OC3M_Pos

#define TIM_CCMR2_OC3M_Pos (4UL)

TIM CCMR2: OC3M (Bit 4)

## ◆ TIM_CCMR2_OC3PE_Msk

#define TIM_CCMR2_OC3PE_Msk (0x8UL)

TIM CCMR2: OC3PE (Bitfield-Mask: 0x01)

## ◆ TIM_CCMR2_OC3PE_Pos

#define TIM_CCMR2_OC3PE_Pos (3UL)

TIM CCMR2: OC3PE (Bit 3)

## ◆ TIM_CCMR2_OC4CE_Msk

#define TIM_CCMR2_OC4CE_Msk (0x8000UL)

TIM CCMR2: OC4CE (Bitfield-Mask: 0x01)

## ◆ TIM_CCMR2_OC4CE_Pos

#define TIM_CCMR2_OC4CE_Pos (15UL)

TIM CCMR2: OC4CE (Bit 15)

## ◆ TIM_CCMR2_OC4FE_Msk

#define TIM_CCMR2_OC4FE_Msk (0x400UL)

TIM CCMR2: OC4FE (Bitfield-Mask: 0x01)

## ◆ TIM_CCMR2_OC4FE_Pos

#define TIM_CCMR2_OC4FE_Pos (10UL)

TIM CCMR2: OC4FE (Bit 10)

## ◆ TIM_CCMR2_OC4M_Msk

#define TIM_CCMR2_OC4M_Msk (0x7000UL)

TIM CCMR2: OC4M (Bitfield-Mask: 0x07)

## ◆ TIM_CCMR2_OC4M_Pos

#define TIM_CCMR2_OC4M_Pos (12UL)

TIM CCMR2: OC4M (Bit 12)

## ◆ TIM_CCMR2_OC4PE_Msk

#define TIM_CCMR2_OC4PE_Msk (0x800UL)

TIM CCMR2: OC4PE (Bitfield-Mask: 0x01)

## ◆ TIM_CCMR2_OC4PE_Pos

#define TIM_CCMR2_OC4PE_Pos (11UL)

TIM CCMR2: OC4PE (Bit 11)

## ◆ TIM_CCR1_CCR1_Msk

#define TIM_CCR1_CCR1_Msk (0xFFFFUL)

TIM CCR1: CCR1 (Bitfield-Mask: 0xFFFF)

## ◆ TIM_CCR1_CCR1_Pos

#define TIM_CCR1_CCR1_Pos (0UL)

TIM CCR1: CCR1 (Bit 0)

## ◆ TIM_CCR2_CCR2_Msk

#define TIM_CCR2_CCR2_Msk (0xFFFFUL)

TIM CCR2: CCR2 (Bitfield-Mask: 0xFFFF)

## ◆ TIM_CCR2_CCR2_Pos

#define TIM_CCR2_CCR2_Pos (0UL)

TIM CCR2: CCR2 (Bit 0)

## ◆ TIM_CCR3_CCR3_Msk

#define TIM_CCR3_CCR3_Msk (0xFFFFUL)

TIM CCR3: CCR3 (Bitfield-Mask: 0xFFFF)

## ◆ TIM_CCR3_CCR3_Pos

#define TIM_CCR3_CCR3_Pos (0UL)

TIM CCR3: CCR3 (Bit 0)

## ◆ TIM_CCR4_CCR4_Msk

#define TIM_CCR4_CCR4_Msk (0xFFFFUL)

TIM CCR4: CCR4 (Bitfield-Mask: 0xFFFF)

## ◆ TIM_CCR4_CCR4_Pos

#define TIM_CCR4_CCR4_Pos (0UL)

TIM CCR4: CCR4 (Bit 0)

## ◆ TIM_CNT_CNT_Msk

#define TIM_CNT_CNT_Msk (0xFFFFUL)

TIM CNT: CNT (Bitfield-Mask: 0xFFFF)

## ◆ TIM_CNT_CNT_Pos

#define TIM_CNT_CNT_Pos (0UL)

TIM CNT: CNT (Bit 0)

## ◆ TIM_CR1_ARPE_Msk

#define TIM_CR1_ARPE_Msk (0x80UL)

TIM CR1: ARPE (Bitfield-Mask: 0x01)

## ◆ TIM_CR1_ARPE_Pos

#define TIM_CR1_ARPE_Pos (7UL)

TIM CR1: ARPE (Bit 7)

## ◆ TIM_CR1_CEN_Msk

#define TIM_CR1_CEN_Msk (0x1UL)

TIM CR1: CEN (Bitfield-Mask: 0x01)

## ◆ TIM_CR1_CEN_Pos

#define TIM_CR1_CEN_Pos (0UL)

TIM CR1: CEN (Bit 0)

## ◆ TIM_CR1_CKD_Msk

#define TIM_CR1_CKD_Msk (0x300UL)

TIM CR1: CKD (Bitfield-Mask: 0x03)

## ◆ TIM_CR1_CKD_Pos

#define TIM_CR1_CKD_Pos (8UL)

TIM CR1: CKD (Bit 8)

## ◆ TIM_CR1_CMS_Msk

#define TIM_CR1_CMS_Msk (0x60UL)

TIM CR1: CMS (Bitfield-Mask: 0x03)

## ◆ TIM_CR1_CMS_Pos

#define TIM_CR1_CMS_Pos (5UL)

TIM CR1: CMS (Bit 5)

## ◆ TIM_CR1_DIR_Msk

#define TIM_CR1_DIR_Msk (0x10UL)

TIM CR1: DIR (Bitfield-Mask: 0x01)

## ◆ TIM_CR1_DIR_Pos

#define TIM_CR1_DIR_Pos (4UL)

TIM CR1: DIR (Bit 4)

## ◆ TIM_CR1_OPM_Msk

#define TIM_CR1_OPM_Msk (0x8UL)

TIM CR1: OPM (Bitfield-Mask: 0x01)

## ◆ TIM_CR1_OPM_Pos

#define TIM_CR1_OPM_Pos (3UL)

TIM CR1: OPM (Bit 3)

## ◆ TIM_CR1_UDIS_Msk

#define TIM_CR1_UDIS_Msk (0x2UL)

TIM CR1: UDIS (Bitfield-Mask: 0x01)

## ◆ TIM_CR1_UDIS_Pos

#define TIM_CR1_UDIS_Pos (1UL)

TIM CR1: UDIS (Bit 1)

## ◆ TIM_CR1_URS_Msk

#define TIM_CR1_URS_Msk (0x4UL)

TIM CR1: URS (Bitfield-Mask: 0x01)

## ◆ TIM_CR1_URS_Pos

#define TIM_CR1_URS_Pos (2UL)

TIM CR1: URS (Bit 2)

## ◆ TIM_CR2_CCPC_Msk

#define TIM_CR2_CCPC_Msk (0x1UL)

TIM CR2: CCPC (Bitfield-Mask: 0x01)

## ◆ TIM_CR2_CCPC_Pos

#define TIM_CR2_CCPC_Pos (0UL)

TIM CR2: CCPC (Bit 0)

## ◆ TIM_CR2_CCUS_Msk

#define TIM_CR2_CCUS_Msk (0x4UL)

TIM CR2: CCUS (Bitfield-Mask: 0x01)

## ◆ TIM_CR2_CCUS_Pos

#define TIM_CR2_CCUS_Pos (2UL)

TIM CR2: CCUS (Bit 2)

## ◆ TIM_CR2_MMS_Msk

#define TIM_CR2_MMS_Msk (0x70UL)

TIM CR2: MMS (Bitfield-Mask: 0x07)

## ◆ TIM_CR2_MMS_Pos

#define TIM_CR2_MMS_Pos (4UL)

TIM CR2: MMS (Bit 4)

## ◆ TIM_CR2_OIS1_Msk

#define TIM_CR2_OIS1_Msk (0x100UL)

TIM CR2: OIS1 (Bitfield-Mask: 0x01)

## ◆ TIM_CR2_OIS1_Pos

#define TIM_CR2_OIS1_Pos (8UL)

TIM CR2: OIS1 (Bit 8)

## ◆ TIM_CR2_OIS1N_Msk

#define TIM_CR2_OIS1N_Msk (0x200UL)

TIM CR2: OIS1N (Bitfield-Mask: 0x01)

## ◆ TIM_CR2_OIS1N_Pos

#define TIM_CR2_OIS1N_Pos (9UL)

TIM CR2: OIS1N (Bit 9)

## ◆ TIM_CR2_OIS2_Msk

#define TIM_CR2_OIS2_Msk (0x400UL)

TIM CR2: OIS2 (Bitfield-Mask: 0x01)

## ◆ TIM_CR2_OIS2_Pos

#define TIM_CR2_OIS2_Pos (10UL)

TIM CR2: OIS2 (Bit 10)

## ◆ TIM_CR2_OIS2N_Msk

#define TIM_CR2_OIS2N_Msk (0x800UL)

TIM CR2: OIS2N (Bitfield-Mask: 0x01)

## ◆ TIM_CR2_OIS2N_Pos

#define TIM_CR2_OIS2N_Pos (11UL)

TIM CR2: OIS2N (Bit 11)

## ◆ TIM_CR2_OIS3_Msk

#define TIM_CR2_OIS3_Msk (0x1000UL)

TIM CR2: OIS3 (Bitfield-Mask: 0x01)

## ◆ TIM_CR2_OIS3_Pos

#define TIM_CR2_OIS3_Pos (12UL)

TIM CR2: OIS3 (Bit 12)

## ◆ TIM_CR2_OIS3N_Msk

#define TIM_CR2_OIS3N_Msk (0x2000UL)

TIM CR2: OIS3N (Bitfield-Mask: 0x01)

## ◆ TIM_CR2_OIS3N_Pos

#define TIM_CR2_OIS3N_Pos (13UL)

TIM CR2: OIS3N (Bit 13)

## ◆ TIM_CR2_OIS4_Msk

#define TIM_CR2_OIS4_Msk (0x4000UL)

TIM CR2: OIS4 (Bitfield-Mask: 0x01)

## ◆ TIM_CR2_OIS4_Pos

#define TIM_CR2_OIS4_Pos (14UL)

TIM CR2: OIS4 (Bit 14)

## ◆ TIM_CR2_TI1S_Msk

#define TIM_CR2_TI1S_Msk (0x80UL)

TIM CR2: TI1S (Bitfield-Mask: 0x01)

## ◆ TIM_CR2_TI1S_Pos

#define TIM_CR2_TI1S_Pos (7UL)

TIM CR2: TI1S (Bit 7)

## ◆ TIM_DIER_BIE_Msk

#define TIM_DIER_BIE_Msk (0x80UL)

TIM DIER: BIE (Bitfield-Mask: 0x01)

## ◆ TIM_DIER_BIE_Pos

#define TIM_DIER_BIE_Pos (7UL)

TIM DIER: BIE (Bit 7)

## ◆ TIM_DIER_CC1IE_Msk

#define TIM_DIER_CC1IE_Msk (0x2UL)

TIM DIER: CC1IE (Bitfield-Mask: 0x01)

## ◆ TIM_DIER_CC1IE_Pos

#define TIM_DIER_CC1IE_Pos (1UL)

TIM DIER: CC1IE (Bit 1)

## ◆ TIM_DIER_CC2IE_Msk

#define TIM_DIER_CC2IE_Msk (0x4UL)

TIM DIER: CC2IE (Bitfield-Mask: 0x01)

## ◆ TIM_DIER_CC2IE_Pos

#define TIM_DIER_CC2IE_Pos (2UL)

TIM DIER: CC2IE (Bit 2)

## ◆ TIM_DIER_CC3IE_Msk

#define TIM_DIER_CC3IE_Msk (0x8UL)

TIM DIER: CC3IE (Bitfield-Mask: 0x01)

## ◆ TIM_DIER_CC3IE_Pos

#define TIM_DIER_CC3IE_Pos (3UL)

TIM DIER: CC3IE (Bit 3)

## ◆ TIM_DIER_CC4IE_Msk

#define TIM_DIER_CC4IE_Msk (0x10UL)

TIM DIER: CC4IE (Bitfield-Mask: 0x01)

## ◆ TIM_DIER_CC4IE_Pos

#define TIM_DIER_CC4IE_Pos (4UL)

TIM DIER: CC4IE (Bit 4)

## ◆ TIM_DIER_COMIE_Msk

#define TIM_DIER_COMIE_Msk (0x20UL)

TIM DIER: COMIE (Bitfield-Mask: 0x01)

## ◆ TIM_DIER_COMIE_Pos

#define TIM_DIER_COMIE_Pos (5UL)

TIM DIER: COMIE (Bit 5)

## ◆ TIM_DIER_TIE_Msk

#define TIM_DIER_TIE_Msk (0x40UL)

TIM DIER: TIE (Bitfield-Mask: 0x01)

## ◆ TIM_DIER_TIE_Pos

#define TIM_DIER_TIE_Pos (6UL)

TIM DIER: TIE (Bit 6)

## ◆ TIM_DIER_UIE_Msk

#define TIM_DIER_UIE_Msk (0x1UL)

TIM DIER: UIE (Bitfield-Mask: 0x01)

## ◆ TIM_DIER_UIE_Pos

#define TIM_DIER_UIE_Pos (0UL)

TIM DIER: UIE (Bit 0)

## ◆ TIM_EGR_BG_Msk

#define TIM_EGR_BG_Msk (0x80UL)

TIM EGR: BG (Bitfield-Mask: 0x01)

## ◆ TIM_EGR_BG_Pos

#define TIM_EGR_BG_Pos (7UL)

TIM EGR: BG (Bit 7)

## ◆ TIM_EGR_CC1G_Msk

#define TIM_EGR_CC1G_Msk (0x2UL)

TIM EGR: CC1G (Bitfield-Mask: 0x01)

## ◆ TIM_EGR_CC1G_Pos

#define TIM_EGR_CC1G_Pos (1UL)

TIM EGR: CC1G (Bit 1)

## ◆ TIM_EGR_CC2G_Msk

#define TIM_EGR_CC2G_Msk (0x4UL)

TIM EGR: CC2G (Bitfield-Mask: 0x01)

## ◆ TIM_EGR_CC2G_Pos

#define TIM_EGR_CC2G_Pos (2UL)

TIM EGR: CC2G (Bit 2)

## ◆ TIM_EGR_CC3G_Msk

#define TIM_EGR_CC3G_Msk (0x8UL)

TIM EGR: CC3G (Bitfield-Mask: 0x01)

## ◆ TIM_EGR_CC3G_Pos

#define TIM_EGR_CC3G_Pos (3UL)

TIM EGR: CC3G (Bit 3)

## ◆ TIM_EGR_CC4G_Msk

#define TIM_EGR_CC4G_Msk (0x10UL)

TIM EGR: CC4G (Bitfield-Mask: 0x01)

## ◆ TIM_EGR_CC4G_Pos

#define TIM_EGR_CC4G_Pos (4UL)

TIM EGR: CC4G (Bit 4)

## ◆ TIM_EGR_COMG_Msk

#define TIM_EGR_COMG_Msk (0x20UL)

TIM EGR: COMG (Bitfield-Mask: 0x01)

## ◆ TIM_EGR_COMG_Pos

#define TIM_EGR_COMG_Pos (5UL)

TIM EGR: COMG (Bit 5)

## ◆ TIM_EGR_TG_Msk

#define TIM_EGR_TG_Msk (0x40UL)

TIM EGR: TG (Bitfield-Mask: 0x01)

## ◆ TIM_EGR_TG_Pos

#define TIM_EGR_TG_Pos (6UL)

TIM EGR: TG (Bit 6)

## ◆ TIM_EGR_UG_Msk

#define TIM_EGR_UG_Msk (0x1UL)

TIM EGR: UG (Bitfield-Mask: 0x01)

## ◆ TIM_EGR_UG_Pos

#define TIM_EGR_UG_Pos (0UL)

TIM EGR: UG (Bit 0)

## ◆ TIM_PSC_PSC_Msk

#define TIM_PSC_PSC_Msk (0xFFFFUL)

TIM PSC: PSC (Bitfield-Mask: 0xFFFF)

## ◆ TIM_PSC_PSC_Pos

#define TIM_PSC_PSC_Pos (0UL)

TIM PSC: PSC (Bit 0)

## ◆ TIM_RCR_REP_Msk

#define TIM_RCR_REP_Msk (0xFFUL)

TIM RCR: REP (Bitfield-Mask: 0xFF)

## ◆ TIM_RCR_REP_Pos

#define TIM_RCR_REP_Pos (0UL)

TIM RCR: REP (Bit 0)

## ◆ TIM_SMCR_ECE_Msk

#define TIM_SMCR_ECE_Msk (0x4000UL)

TIM SMCR: ECE (Bitfield-Mask: 0x01)

## ◆ TIM_SMCR_ECE_Pos

#define TIM_SMCR_ECE_Pos (14UL)

TIM SMCR: ECE (Bit 14)

## ◆ TIM_SMCR_ETF_Msk

#define TIM_SMCR_ETF_Msk (0xF00UL)

TIM SMCR: ETF (Bitfield-Mask: 0x0F)

## ◆ TIM_SMCR_ETF_Pos

#define TIM_SMCR_ETF_Pos (8UL)

TIM SMCR: ETF (Bit 8)

## ◆ TIM_SMCR_ETP_Msk

#define TIM_SMCR_ETP_Msk (0x8000UL)

TIM SMCR: ETP (Bitfield-Mask: 0x01)

## ◆ TIM_SMCR_ETP_Pos

#define TIM_SMCR_ETP_Pos (15UL)

TIM SMCR: ETP (Bit 15)

## ◆ TIM_SMCR_ETPS_Msk

#define TIM_SMCR_ETPS_Msk (0x3000UL)

TIM SMCR: ETPS (Bitfield-Mask: 0x03)

## ◆ TIM_SMCR_ETPS_Pos

#define TIM_SMCR_ETPS_Pos (12UL)

TIM SMCR: ETPS (Bit 12)

## ◆ TIM_SMCR_MSM_Msk

#define TIM_SMCR_MSM_Msk (0x80UL)

TIM SMCR: MSM (Bitfield-Mask: 0x01)

## ◆ TIM_SMCR_MSM_Pos

#define TIM_SMCR_MSM_Pos (7UL)

TIM SMCR: MSM (Bit 7)

## ◆ TIM_SMCR_SMS_Msk

#define TIM_SMCR_SMS_Msk (0x7UL)

TIM SMCR: SMS (Bitfield-Mask: 0x07)

## ◆ TIM_SMCR_SMS_Pos

#define TIM_SMCR_SMS_Pos (0UL)

TIM SMCR: SMS (Bit 0)

## ◆ TIM_SMCR_TS_Msk

#define TIM_SMCR_TS_Msk (0x70UL)

TIM SMCR: TS (Bitfield-Mask: 0x07)

## ◆ TIM_SMCR_TS_Pos

#define TIM_SMCR_TS_Pos (4UL)

TIM SMCR: TS (Bit 4)

## ◆ TIM_SR_BIF_Msk

#define TIM_SR_BIF_Msk (0x80UL)

TIM SR: BIF (Bitfield-Mask: 0x01)

## ◆ TIM_SR_BIF_Pos

#define TIM_SR_BIF_Pos (7UL)

TIM SR: BIF (Bit 7)

## ◆ TIM_SR_CC1IF_Msk

#define TIM_SR_CC1IF_Msk (0x2UL)

TIM SR: CC1IF (Bitfield-Mask: 0x01)

## ◆ TIM_SR_CC1IF_Pos

#define TIM_SR_CC1IF_Pos (1UL)

TIM SR: CC1IF (Bit 1)

## ◆ TIM_SR_CC1OF_Msk

#define TIM_SR_CC1OF_Msk (0x200UL)

TIM SR: CC1OF (Bitfield-Mask: 0x01)

## ◆ TIM_SR_CC1OF_Pos

#define TIM_SR_CC1OF_Pos (9UL)

TIM SR: CC1OF (Bit 9)

## ◆ TIM_SR_CC2IF_Msk

#define TIM_SR_CC2IF_Msk (0x4UL)

TIM SR: CC2IF (Bitfield-Mask: 0x01)

## ◆ TIM_SR_CC2IF_Pos

#define TIM_SR_CC2IF_Pos (2UL)

TIM SR: CC2IF (Bit 2)

## ◆ TIM_SR_CC2OF_Msk

#define TIM_SR_CC2OF_Msk (0x400UL)

TIM SR: CC2OF (Bitfield-Mask: 0x01)

## ◆ TIM_SR_CC2OF_Pos

#define TIM_SR_CC2OF_Pos (10UL)

TIM SR: CC2OF (Bit 10)

## ◆ TIM_SR_CC3IF_Msk

#define TIM_SR_CC3IF_Msk (0x8UL)

TIM SR: CC3IF (Bitfield-Mask: 0x01)

## ◆ TIM_SR_CC3IF_Pos

#define TIM_SR_CC3IF_Pos (3UL)

TIM SR: CC3IF (Bit 3)

## ◆ TIM_SR_CC3OF_Msk

#define TIM_SR_CC3OF_Msk (0x800UL)

TIM SR: CC3OF (Bitfield-Mask: 0x01)

## ◆ TIM_SR_CC3OF_Pos

#define TIM_SR_CC3OF_Pos (11UL)

TIM SR: CC3OF (Bit 11)

## ◆ TIM_SR_CC4IF_Msk

#define TIM_SR_CC4IF_Msk (0x10UL)

TIM SR: CC4IF (Bitfield-Mask: 0x01)

## ◆ TIM_SR_CC4IF_Pos

#define TIM_SR_CC4IF_Pos (4UL)

TIM SR: CC4IF (Bit 4)

## ◆ TIM_SR_CC4OF_Msk

#define TIM_SR_CC4OF_Msk (0x1000UL)

TIM SR: CC4OF (Bitfield-Mask: 0x01)

## ◆ TIM_SR_CC4OF_Pos

#define TIM_SR_CC4OF_Pos (12UL)

TIM SR: CC4OF (Bit 12)

## ◆ TIM_SR_COMIF_Msk

#define TIM_SR_COMIF_Msk (0x20UL)

TIM SR: COMIF (Bitfield-Mask: 0x01)

## ◆ TIM_SR_COMIF_Pos

#define TIM_SR_COMIF_Pos (5UL)

TIM SR: COMIF (Bit 5)

## ◆ TIM_SR_TIF_Msk

#define TIM_SR_TIF_Msk (0x40UL)

TIM SR: TIF (Bitfield-Mask: 0x01)

## ◆ TIM_SR_TIF_Pos

#define TIM_SR_TIF_Pos (6UL)

TIM SR: TIF (Bit 6)

## ◆ TIM_SR_UIF_Msk

#define TIM_SR_UIF_Msk (0x1UL)

TIM SR: UIF (Bitfield-Mask: 0x01)

## ◆ TIM_SR_UIF_Pos

#define TIM_SR_UIF_Pos (0UL)

TIM SR: UIF (Bit 0)

## ◆ UART_BAUDCR_BRG_Msk

#define UART_BAUDCR_BRG_Msk (0xFFFFUL)

UART BAUDCR: BRG (Bitfield-Mask: 0xFFFF)

## ◆ UART_BAUDCR_BRG_Pos

#define UART_BAUDCR_BRG_Pos (0UL)

UART BAUDCR: BRG (Bit 0)

## ◆ UART_BAUDCR_NOREF_Msk

#define UART_BAUDCR_NOREF_Msk (0x80000000UL)

UART BAUDCR: NOREF (Bitfield-Mask: 0x01)

## ◆ UART_BAUDCR_NOREF_Pos

#define UART_BAUDCR_NOREF_Pos (31UL)

UART BAUDCR: NOREF (Bit 31)

## ◆ UART_BAUDCR_SELF_BRG_Msk

#define UART_BAUDCR_SELF_BRG_Msk (0x10000UL)

UART BAUDCR: SELF_BRG (Bitfield-Mask: 0x01)

## ◆ UART_BAUDCR_SELF_BRG_Pos

#define UART_BAUDCR_SELF_BRG_Pos (16UL)

UART BAUDCR: SELF_BRG (Bit 16)

## ◆ UART_INTCLR_FECLR_Msk

#define UART_INTCLR_FECLR_Msk (0x4UL)

UART INTCLR: FECLR (Bitfield-Mask: 0x01)

## ◆ UART_INTCLR_FECLR_Pos

#define UART_INTCLR_FECLR_Pos (2UL)

UART INTCLR: FECLR (Bit 2)

## ◆ UART_INTCLR_RICLR_Msk

#define UART_INTCLR_RICLR_Msk (0x1UL)

UART INTCLR: RICLR (Bitfield-Mask: 0x01)

## ◆ UART_INTCLR_RICLR_Pos

#define UART_INTCLR_RICLR_Pos (0UL)

UART INTCLR: RICLR (Bit 0)

## ◆ UART_INTCLR_TICLR_Msk

#define UART_INTCLR_TICLR_Msk (0x2UL)

UART INTCLR: TICLR (Bitfield-Mask: 0x01)

## ◆ UART_INTCLR_TICLR_Pos

#define UART_INTCLR_TICLR_Pos (1UL)

UART INTCLR: TICLR (Bit 1)

## ◆ UART_INTSR_FE_Msk

#define UART_INTSR_FE_Msk (0x4UL)

UART INTSR: FE (Bitfield-Mask: 0x01)

## ◆ UART_INTSR_FE_Pos

#define UART_INTSR_FE_Pos (2UL)

UART INTSR: FE (Bit 2)

## ◆ UART_INTSR_RI_Msk

#define UART_INTSR_RI_Msk (0x1UL)

UART INTSR: RI (Bitfield-Mask: 0x01)

## ◆ UART_INTSR_RI_Pos

#define UART_INTSR_RI_Pos (0UL)

UART INTSR: RI (Bit 0)

## ◆ UART_INTSR_TI_Msk

#define UART_INTSR_TI_Msk (0x2UL)

UART INTSR: TI (Bitfield-Mask: 0x01)

## ◆ UART_INTSR_TI_Pos

#define UART_INTSR_TI_Pos (1UL)

UART INTSR: TI (Bit 1)

## ◆ UART_IRDACR_IREN_Msk

#define UART_IRDACR_IREN_Msk (0x100UL)

UART IRDACR: IREN (Bitfield-Mask: 0x01)

## ◆ UART_IRDACR_IREN_Pos

#define UART_IRDACR_IREN_Pos (8UL)

UART IRDACR: IREN (Bit 8)

## ◆ UART_IRDACR_IRLPMODE_Msk

#define UART_IRDACR_IRLPMODE_Msk (0x800UL)

UART IRDACR: IRLPMODE (Bitfield-Mask: 0x01)

## ◆ UART_IRDACR_IRLPMODE_Pos

#define UART_IRDACR_IRLPMODE_Pos (11UL)

UART IRDACR: IRLPMODE (Bit 11)

## ◆ UART_IRDACR_IRRXINV_Msk

#define UART_IRDACR_IRRXINV_Msk (0x400UL)

UART IRDACR: IRRXINV (Bitfield-Mask: 0x01)

## ◆ UART_IRDACR_IRRXINV_Pos

#define UART_IRDACR_IRRXINV_Pos (10UL)

UART IRDACR: IRRXINV (Bit 10)

## ◆ UART_IRDACR_IRTXINV_Msk

#define UART_IRDACR_IRTXINV_Msk (0x200UL)

UART IRDACR: IRTXINV (Bitfield-Mask: 0x01)

## ◆ UART_IRDACR_IRTXINV_Pos

#define UART_IRDACR_IRTXINV_Pos (9UL)

UART IRDACR: IRTXINV (Bit 9)

## ◆ UART_IRDACR_PSC_Msk

#define UART_IRDACR_PSC_Msk (0xFFUL)

UART IRDACR: PSC (Bitfield-Mask: 0xFF)

## ◆ UART_IRDACR_PSC_Pos

#define UART_IRDACR_PSC_Pos (0UL)

UART IRDACR: PSC (Bit 0)

## ◆ UART_SADDR_SADDR_Msk

#define UART_SADDR_SADDR_Msk (0xFFUL)

UART SADDR: SADDR (Bitfield-Mask: 0xFF)

## ◆ UART_SADDR_SADDR_Pos

#define UART_SADDR_SADDR_Pos (0UL)

UART SADDR: SADDR (Bit 0)

## ◆ UART_SADEN_SADEN_Msk

#define UART_SADEN_SADEN_Msk (0xFFUL)

UART SADEN: SADEN (Bitfield-Mask: 0xFF)

## ◆ UART_SADEN_SADEN_Pos

#define UART_SADEN_SADEN_Pos (0UL)

UART SADEN: SADEN (Bit 0)

## ◆ UART_SBUF_SBUF_Msk

#define UART_SBUF_SBUF_Msk (0xFFUL)

UART SBUF: SBUF (Bitfield-Mask: 0xFF)

## ◆ UART_SBUF_SBUF_Pos

#define UART_SBUF_SBUF_Pos (0UL)

UART SBUF: SBUF (Bit 0)

## ◆ UART_SCON_DBAUD_Msk

#define UART_SCON_DBAUD_Msk (0x200UL)

UART SCON: DBAUD (Bitfield-Mask: 0x01)

## ◆ UART_SCON_DBAUD_Pos

#define UART_SCON_DBAUD_Pos (9UL)

UART SCON: DBAUD (Bit 9)

## ◆ UART_SCON_FEEN_Msk

#define UART_SCON_FEEN_Msk (0x100UL)

UART SCON: FEEN (Bitfield-Mask: 0x01)

## ◆ UART_SCON_FEEN_Pos

#define UART_SCON_FEEN_Pos (8UL)

UART SCON: FEEN (Bit 8)

## ◆ UART_SCON_RB8_Msk

#define UART_SCON_RB8_Msk (0x4UL)

UART SCON: RB8 (Bitfield-Mask: 0x01)

## ◆ UART_SCON_RB8_Pos

#define UART_SCON_RB8_Pos (2UL)

UART SCON: RB8 (Bit 2)

## ◆ UART_SCON_REN_Msk

#define UART_SCON_REN_Msk (0x10UL)

UART SCON: REN (Bitfield-Mask: 0x01)

## ◆ UART_SCON_REN_Pos

#define UART_SCON_REN_Pos (4UL)

UART SCON: REN (Bit 4)

## ◆ UART_SCON_RIEN_Msk

#define UART_SCON_RIEN_Msk (0x1UL)

UART SCON: RIEN (Bitfield-Mask: 0x01)

## ◆ UART_SCON_RIEN_Pos

#define UART_SCON_RIEN_Pos (0UL)

UART SCON: RIEN (Bit 0)

## ◆ UART_SCON_SM0_SM1_Msk

#define UART_SCON_SM0_SM1_Msk (0xC0UL)

UART SCON: SM0_SM1 (Bitfield-Mask: 0x03)

## ◆ UART_SCON_SM0_SM1_Pos

#define UART_SCON_SM0_SM1_Pos (6UL)

UART SCON: SM0_SM1 (Bit 6)

## ◆ UART_SCON_SM2_Msk

#define UART_SCON_SM2_Msk (0x20UL)

UART SCON: SM2 (Bitfield-Mask: 0x01)

## ◆ UART_SCON_SM2_Pos

#define UART_SCON_SM2_Pos (5UL)

UART SCON: SM2 (Bit 5)

## ◆ UART_SCON_TB8_Msk

#define UART_SCON_TB8_Msk (0x8UL)

UART SCON: TB8 (Bitfield-Mask: 0x01)

## ◆ UART_SCON_TB8_Pos

#define UART_SCON_TB8_Pos (3UL)

UART SCON: TB8 (Bit 3)

## ◆ UART_SCON_TIEN_Msk

#define UART_SCON_TIEN_Msk (0x2UL)

UART SCON: TIEN (Bitfield-Mask: 0x01)

## ◆ UART_SCON_TIEN_Pos

#define UART_SCON_TIEN_Pos (1UL)

UART SCON: TIEN (Bit 1)

## ◆ UID_BASE

#define UID_BASE ((uint32_t)0x180000F0UL)

Unique device ID register base address

## ◆ VCMP_CR0_NINSEL_Msk

#define VCMP_CR0_NINSEL_Msk (0xCUL)

VCMP CR0: NINSEL (Bitfield-Mask: 0x03)

## ◆ VCMP_CR0_NINSEL_Pos

#define VCMP_CR0_NINSEL_Pos (2UL)

VCMP CR0: NINSEL (Bit 2)

## ◆ VCMP_CR0_PINSEL_Msk

#define VCMP_CR0_PINSEL_Msk (0x3UL)

VCMP CR0: PINSEL (Bitfield-Mask: 0x03)

## ◆ VCMP_CR0_PINSEL_Pos

#define VCMP_CR0_PINSEL_Pos (0UL)

VCMP CR0: PINSEL (Bit 0)

## ◆ VCMP_CR0_VCAPDIV_EN_Msk

#define VCMP_CR0_VCAPDIV_EN_Msk (0x40UL)

VCMP CR0: VCAPDIV_EN (Bitfield-Mask: 0x01)

## ◆ VCMP_CR0_VCAPDIV_EN_Pos

#define VCMP_CR0_VCAPDIV_EN_Pos (6UL)

VCMP CR0: VCAPDIV_EN (Bit 6)

## ◆ VCMP_CR0_VCAPDIV_Msk

#define VCMP_CR0_VCAPDIV_Msk (0x30UL)

VCMP CR0: VCAPDIV (Bitfield-Mask: 0x03)

## ◆ VCMP_CR0_VCAPDIV_Pos

#define VCMP_CR0_VCAPDIV_Pos (4UL)

VCMP CR0: VCAPDIV (Bit 4)

## ◆ VCMP_CR1_FALLINTEN_Msk

#define VCMP_CR1_FALLINTEN_Msk (0x1000UL)

VCMP CR1: FALLINTEN (Bitfield-Mask: 0x01)

## ◆ VCMP_CR1_FALLINTEN_Pos

#define VCMP_CR1_FALLINTEN_Pos (12UL)

VCMP CR1: FALLINTEN (Bit 12)

## ◆ VCMP_CR1_FLT_NUM_Msk

#define VCMP_CR1_FLT_NUM_Msk (0xFFFF0000UL)

VCMP CR1: FLT_NUM (Bitfield-Mask: 0xFFFF)

## ◆ VCMP_CR1_FLT_NUM_Pos

#define VCMP_CR1_FLT_NUM_Pos (16UL)

VCMP CR1: FLT_NUM (Bit 16)

## ◆ VCMP_CR1_FLTEN_Msk

#define VCMP_CR1_FLTEN_Msk (0x100UL)

VCMP CR1: FLTEN (Bitfield-Mask: 0x01)

## ◆ VCMP_CR1_FLTEN_Pos

#define VCMP_CR1_FLTEN_Pos (8UL)

VCMP CR1: FLTEN (Bit 8)

## ◆ VCMP_CR1_HIGHINTEN_Msk

#define VCMP_CR1_HIGHINTEN_Msk (0x4000UL)

VCMP CR1: HIGHINTEN (Bitfield-Mask: 0x01)

## ◆ VCMP_CR1_HIGHINTEN_Pos

#define VCMP_CR1_HIGHINTEN_Pos (14UL)

VCMP CR1: HIGHINTEN (Bit 14)

## ◆ VCMP_CR1_INT_EN_Msk

#define VCMP_CR1_INT_EN_Msk (0x8000UL)

VCMP CR1: INT_EN (Bitfield-Mask: 0x01)

## ◆ VCMP_CR1_INT_EN_Pos

#define VCMP_CR1_INT_EN_Pos (15UL)

VCMP CR1: INT_EN (Bit 15)

## ◆ VCMP_CR1_RISEINTEN_Msk

#define VCMP_CR1_RISEINTEN_Msk (0x2000UL)

VCMP CR1: RISEINTEN (Bitfield-Mask: 0x01)

## ◆ VCMP_CR1_RISEINTEN_Pos

#define VCMP_CR1_RISEINTEN_Pos (13UL)

VCMP CR1: RISEINTEN (Bit 13)

## ◆ VCMP_CR1_VCEN_Msk

#define VCMP_CR1_VCEN_Msk (0x1UL)

VCMP CR1: VCEN (Bitfield-Mask: 0x01)

## ◆ VCMP_CR1_VCEN_Pos

#define VCMP_CR1_VCEN_Pos (0UL)

VCMP CR1: VCEN (Bit 0)

## ◆ VCMP_CR1_VCMP_FLTCLK_SEL_Msk

#define VCMP_CR1_VCMP_FLTCLK_SEL_Msk (0xCUL)

VCMP CR1: VCMP_FLTCLK_SEL (Bitfield-Mask: 0x03)

## ◆ VCMP_CR1_VCMP_FLTCLK_SEL_Pos

#define VCMP_CR1_VCMP_FLTCLK_SEL_Pos (2UL)

VCMP CR1: VCMP_FLTCLK_SEL (Bit 2)

## ◆ VCMP_OUTCFG_INV_PAD_Msk

#define VCMP_OUTCFG_INV_PAD_Msk (0x40000UL)

VCMP OUTCFG: INV_PAD (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_INV_PAD_Pos

#define VCMP_OUTCFG_INV_PAD_Pos (18UL)

VCMP OUTCFG: INV_PAD (Bit 18)

## ◆ VCMP_OUTCFG_INV_PCA_Msk

#define VCMP_OUTCFG_INV_PCA_Msk (0x40UL)

VCMP OUTCFG: INV_PCA (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_INV_PCA_Pos

#define VCMP_OUTCFG_INV_PCA_Pos (6UL)

VCMP OUTCFG: INV_PCA (Bit 6)

## ◆ VCMP_OUTCFG_INV_TIM1CH1_Msk

#define VCMP_OUTCFG_INV_TIM1CH1_Msk (0x200UL)

VCMP OUTCFG: INV_TIM1CH1 (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_INV_TIM1CH1_Pos

#define VCMP_OUTCFG_INV_TIM1CH1_Pos (9UL)

VCMP OUTCFG: INV_TIM1CH1 (Bit 9)

## ◆ VCMP_OUTCFG_INV_TIM1CH2_Msk

#define VCMP_OUTCFG_INV_TIM1CH2_Msk (0x800UL)

VCMP OUTCFG: INV_TIM1CH2 (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_INV_TIM1CH2_Pos

#define VCMP_OUTCFG_INV_TIM1CH2_Pos (11UL)

VCMP OUTCFG: INV_TIM1CH2 (Bit 11)

## ◆ VCMP_OUTCFG_INV_TIM1CH3_Msk

#define VCMP_OUTCFG_INV_TIM1CH3_Msk (0x2000UL)

VCMP OUTCFG: INV_TIM1CH3 (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_INV_TIM1CH3_Pos

#define VCMP_OUTCFG_INV_TIM1CH3_Pos (13UL)

VCMP OUTCFG: INV_TIM1CH3 (Bit 13)

## ◆ VCMP_OUTCFG_INV_TIM1CH4_Msk

#define VCMP_OUTCFG_INV_TIM1CH4_Msk (0x8000UL)

VCMP OUTCFG: INV_TIM1CH4 (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_INV_TIM1CH4_Pos

#define VCMP_OUTCFG_INV_TIM1CH4_Pos (15UL)

VCMP OUTCFG: INV_TIM1CH4 (Bit 15)

## ◆ VCMP_OUTCFG_INV_TIMX_Msk

#define VCMP_OUTCFG_INV_TIMX_Msk (0x1UL)

VCMP OUTCFG: INV_TIMX (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_INV_TIMX_Pos

#define VCMP_OUTCFG_INV_TIMX_Pos (0UL)

VCMP OUTCFG: INV_TIMX (Bit 0)

## ◆ VCMP_OUTCFG_LPTIM_EN_Msk

#define VCMP_OUTCFG_LPTIM_EN_Msk (0x10UL)

VCMP OUTCFG: LPTIM_EN (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_LPTIM_EN_Pos

#define VCMP_OUTCFG_LPTIM_EN_Pos (4UL)

VCMP OUTCFG: LPTIM_EN (Bit 4)

## ◆ VCMP_OUTCFG_LPTIMEXT_EN_Msk

#define VCMP_OUTCFG_LPTIMEXT_EN_Msk (0x20UL)

VCMP OUTCFG: LPTIMEXT_EN (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_LPTIMEXT_EN_Pos

#define VCMP_OUTCFG_LPTIMEXT_EN_Pos (5UL)

VCMP OUTCFG: LPTIMEXT_EN (Bit 5)

## ◆ VCMP_OUTCFG_PCACAP0_EN_Msk

#define VCMP_OUTCFG_PCACAP0_EN_Msk (0x80UL)

VCMP OUTCFG: PCACAP0_EN (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_PCACAP0_EN_Pos

#define VCMP_OUTCFG_PCACAP0_EN_Pos (7UL)

VCMP OUTCFG: PCACAP0_EN (Bit 7)

## ◆ VCMP_OUTCFG_PCAECI_EN_Msk

#define VCMP_OUTCFG_PCAECI_EN_Msk (0x100UL)

VCMP OUTCFG: PCAECI_EN (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_PCAECI_EN_Pos

#define VCMP_OUTCFG_PCAECI_EN_Pos (8UL)

VCMP OUTCFG: PCAECI_EN (Bit 8)

## ◆ VCMP_OUTCFG_TIM10_EN_Msk

#define VCMP_OUTCFG_TIM10_EN_Msk (0x2UL)

VCMP OUTCFG: TIM10_EN (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_TIM10_EN_Pos

#define VCMP_OUTCFG_TIM10_EN_Pos (1UL)

VCMP OUTCFG: TIM10_EN (Bit 1)

## ◆ VCMP_OUTCFG_TIM11_EN_Msk

#define VCMP_OUTCFG_TIM11_EN_Msk (0x4UL)

VCMP OUTCFG: TIM11_EN (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_TIM11_EN_Pos

#define VCMP_OUTCFG_TIM11_EN_Pos (2UL)

VCMP OUTCFG: TIM11_EN (Bit 2)

## ◆ VCMP_OUTCFG_TIM1BKE_Msk

#define VCMP_OUTCFG_TIM1BKE_Msk (0x20000UL)

VCMP OUTCFG: TIM1BKE (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_TIM1BKE_Pos

#define VCMP_OUTCFG_TIM1BKE_Pos (17UL)

VCMP OUTCFG: TIM1BKE (Bit 17)

## ◆ VCMP_OUTCFG_TIM1CH1_EN_Msk

#define VCMP_OUTCFG_TIM1CH1_EN_Msk (0x400UL)

VCMP OUTCFG: TIM1CH1_EN (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_TIM1CH1_EN_Pos

#define VCMP_OUTCFG_TIM1CH1_EN_Pos (10UL)

VCMP OUTCFG: TIM1CH1_EN (Bit 10)

## ◆ VCMP_OUTCFG_TIM1CH2_EN_Msk

#define VCMP_OUTCFG_TIM1CH2_EN_Msk (0x1000UL)

VCMP OUTCFG: TIM1CH2_EN (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_TIM1CH2_EN_Pos

#define VCMP_OUTCFG_TIM1CH2_EN_Pos (12UL)

VCMP OUTCFG: TIM1CH2_EN (Bit 12)

## ◆ VCMP_OUTCFG_TIM1CH3_EN_Msk

#define VCMP_OUTCFG_TIM1CH3_EN_Msk (0x4000UL)

VCMP OUTCFG: TIM1CH3_EN (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_TIM1CH3_EN_Pos

#define VCMP_OUTCFG_TIM1CH3_EN_Pos (14UL)

VCMP OUTCFG: TIM1CH3_EN (Bit 14)

## ◆ VCMP_OUTCFG_TIM1CH4_EN_Msk

#define VCMP_OUTCFG_TIM1CH4_EN_Msk (0x10000UL)

VCMP OUTCFG: TIM1CH4_EN (Bitfield-Mask: 0x01)

## ◆ VCMP_OUTCFG_TIM1CH4_EN_Pos

#define VCMP_OUTCFG_TIM1CH4_EN_Pos (16UL)

VCMP OUTCFG: TIM1CH4_EN (Bit 16)

## ◆ VCMP_SR_INTF_Msk

#define VCMP_SR_INTF_Msk (0x1UL)

VCMP SR: INTF (Bitfield-Mask: 0x01)

## ◆ VCMP_SR_INTF_Pos

#define VCMP_SR_INTF_Pos (0UL)

VCMP SR: INTF (Bit 0)

## ◆ VCMP_SR_VCMP_FLOUT_Msk

#define VCMP_SR_VCMP_FLOUT_Msk (0x2UL)

VCMP SR: VCMP_FLOUT (Bitfield-Mask: 0x01)

## ◆ VCMP_SR_VCMP_FLOUT_Pos

#define VCMP_SR_VCMP_FLOUT_Pos (1UL)

VCMP SR: VCMP_FLOUT (Bit 1)

## ◆ WWDG_CNTVAL_WWDGCNT_Msk

#define WWDG_CNTVAL_WWDGCNT_Msk (0xFFUL)

WWDG CNTVAL: WWDGCNT (Bitfield-Mask: 0xFF)

## ◆ WWDG_CNTVAL_WWDGCNT_Pos

#define WWDG_CNTVAL_WWDGCNT_Pos (0UL)

WWDG CNTVAL: WWDGCNT (Bit 0)

## ◆ WWDG_CR_PRSC_Msk

#define WWDG_CR_PRSC_Msk (0xFFFFF00UL)

WWDG CR: PRSC (Bitfield-Mask: 0xFFFFF)

## ◆ WWDG_CR_PRSC_Pos

#define WWDG_CR_PRSC_Pos (8UL)

WWDG CR: PRSC (Bit 8)

## ◆ WWDG_CR_WINCMP_Msk

#define WWDG_CR_WINCMP_Msk (0xFFUL)

WWDG CR: WINCMP (Bitfield-Mask: 0xFF)

## ◆ WWDG_CR_WINCMP_Pos

#define WWDG_CR_WINCMP_Pos (0UL)

WWDG CR: WINCMP (Bit 0)

## ◆ WWDG_CR_WWDGEN_Msk

#define WWDG_CR_WWDGEN_Msk (0x10000000UL)

WWDG CR: WWDGEN (Bitfield-Mask: 0x01)

## ◆ WWDG_CR_WWDGEN_Pos

#define WWDG_CR_WWDGEN_Pos (28UL)

WWDG CR: WWDGEN (Bit 28)

## ◆ WWDG_INTCLR_INTCLR_Msk

#define WWDG_INTCLR_INTCLR_Msk (0x1UL)

WWDG INTCLR: INTCLR (Bitfield-Mask: 0x01)

## ◆ WWDG_INTCLR_INTCLR_Pos

#define WWDG_INTCLR_INTCLR_Pos (0UL)

WWDG INTCLR: INTCLR (Bit 0)

## ◆ WWDG_INTEN_WWDGIEN_Msk

#define WWDG_INTEN_WWDGIEN_Msk (0x1UL)

WWDG INTEN: WWDGIEN (Bitfield-Mask: 0x01)

## ◆ WWDG_INTEN_WWDGIEN_Pos

#define WWDG_INTEN_WWDGIEN_Pos (0UL)

WWDG INTEN: WWDGIEN (Bit 0)

## ◆ WWDG_RLOAD_RLOAD_Msk

#define WWDG_RLOAD_RLOAD_Msk (0xFFUL)

WWDG RLOAD: RLOAD (Bitfield-Mask: 0xFF)

## ◆ WWDG_RLOAD_RLOAD_Pos

#define WWDG_RLOAD_RLOAD_Pos (0UL)

WWDG RLOAD: RLOAD (Bit 0)

## ◆ WWDG_SR_WWDGIF_Msk

#define WWDG_SR_WWDGIF_Msk (0x1UL)

WWDG SR: WWDGIF (Bitfield-Mask: 0x01)

## ◆ WWDG_SR_WWDGIF_Pos

#define WWDG_SR_WWDGIF_Pos (0UL)

WWDG SR: WWDGIF (Bit 0)