WB32L003 Standard Peripherals Firmware Library

Functions
wb32l003_spi.c File Reference

This file provides all the SPI firmware functions. More...

`#include "wb32l003_spi.h"`
`#include "wb32l003_rcc.h"`

## Functions
void | SPI_DeInit (SPI_TypeDef *SPIx)
| Deinitializes the SPIx peripheral registers to their default reset values. More...
void | SPI_Init (SPI_TypeDef *SPIx, SPI_InitTypeDef *SPI_InitStruct)
| Initializes the SPIx peripheral according to the specified parameters in the SPI_InitStruct. More...
void | SPI_Cmd (SPI_TypeDef *SPIx, FunctionalState NewState)
| Enables or disables the specified SPI peripheral. More...
void | SPI_NSSConfig (SPI_TypeDef *SPIx, FunctionalState NewState)
| Enables or disables the specified slave select line. More...
uint8_t | SPI_ReadData (SPI_TypeDef *SPIx)
| Read one data from DATA register. More...
void | SPI_WriteData (SPI_TypeDef *SPIx, uint8_t Data)
| Write one data to DATA register. More...
FlagStatus | SPI_GetFlagStatus (SPI_TypeDef *SPIx, uint8_t SPI_FLAG)
| Checks whether the specified SPIx flag is set or not. More...

## Detailed Description

This file provides all the SPI firmware functions.

Author
  Westberry Application Team

Version
  V0.0.4

Date
  23-April-2023