WB32L003 Standard Peripherals Firmware Library

ADC multi-channels sample example

      ****************** (C) COPYRIGHT 2023 Westberry Technology *******************
      * @file    ADC/ADC_MultiChannels/readme.txt
      * @author  Westberry Application Team
      * @version V0.0.4
      * @date    23-April-2023
      * @brief   Description of the ADC ADC_MultiChannels example.
      ******************************************************************************
      * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
      * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
      * TIME. AS A RESULT, WESTBERRY SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
      * INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM
      * THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
      * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
      ******************************************************************************

例程描述

本例程演示如何使用ADC非循环模式下的多通道连续转换功能。

本例程系统时钟工作在24Mhz。

串口1按照如下配置：

- 波特率：115200
- 数据位：8

ADC被配置为对5个通道进行采样（采样通道为ADC通道0 ~ 通道4，分别对应管脚PC6, PC3, PC4, PD2, PD3），
每个通道会被连续采样10次，采样结果会被打印在串口1中。

目录内容

- ADC/ADC_MultiChannels/ADC_MultiChannels.uvprojx MDK5工程文件
- ADC/ADC_MultiChannels/ADC_MultiChannels.uvoptx MDK5工程配置文件
- ADC/ADC_MultiChannels/JLinkSettings.ini Jlink配置文件
- ADC/ADC_MultiChannels/main.c 主程序

硬件和软件环境

- 硬件平台搭建
  - 芯片管脚按如下连接：
    - UART1 (PD5, PD6) 连接到串口

如何使用？

为了使程序工作，您必须执行以下操作 :

- 使用 MDK5 打开此例程文件夹中的 ADC_MultiChannels.uvprojx 工程
- 重新编译该工程并下载到目标存储器中

- 运行此例程

  ###
  © COPYRIGHT 2023 Westberry Technology