WB32L003 Standard Peripherals Firmware Library

UART_Printf example

      ****************** (C) COPYRIGHT 2023 Westberry Technology *******************
      * @file    UART/UART_Printf/readme.txt
      * @author  Westberry Application Team
      * @version V0.0.4
      * @date    23-April-2023
      * @brief   Description of the UART UART_Printf example.
      ******************************************************************************
      * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
      * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
      * TIME. AS A RESULT, WESTBERRY SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
      * INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM
      * THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
      * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
      ******************************************************************************

例程描述

本例程演示如何将标准输入输出重定向到UART1。

本例程系统时钟工作在24Mhz。

实现输入输出重定向功能的代码在 \Utilities\Common\Retarget_uart1.c 中。

UART1 配置如下：

- 波特率： 115200
- 数据位： 8

目录内容

- UART/UART_Printf/UART_Printf.uvprojx MDK5工程文件
- UART/UART_Printf/UART_Printf.uvoptx MDK5工程配置文件
- UART/UART_Printf/JLinkSettings.ini Jlink配置文件
- UART/UART_Printf/main.c 主程序

硬件和软件环境

- 硬件平台搭建
  - 芯片管脚连接如下：
    - UART1(PD5, PD6) 管脚连接到 PC 串口

如何使用？

为了使程序工作，您必须执行以下操作 :

- 使用 MDK5 打开此例程文件夹中的 UART_Printf.uvprojx 工程
- 重新编译该工程并下载到目标存储器中

- 运行此例程

  ###
  © COPYRIGHT 2023 Westberry Technology