WB32L003 Standard Peripherals Firmware Library

wb32l003_tim.h
浏览该文件的文档.
1
10 /* Define to prevent recursive inclusion -------------------------------------*/
11 #ifndef __WB32L003_TIM_H
12 #define __WB32L003_TIM_H
13
14 #ifdef __cplusplus
15 extern "C" {
16 #endif
17
18 /* Includes ------------------------------------------------------------------*/
19 #include "wb32l003.h"
20
29 /* Exported types ------------------------------------------------------------*/
30
34 typedef struct
35 {
36 uint16_t TIM_Prescaler;
39 uint16_t TIM_CounterMode;
42 uint16_t TIM_Period;
46 uint16_t TIM_ClockDivision;
49 uint8_t TIM_RepetitionCounter;
57 } TIM_TimeBaseInitTypeDef;
58
59
63 typedef struct
64 {
65 uint16_t TIM_OCMode;
68 uint16_t TIM_OutputState;
71 uint16_t TIM_OutputNState;
75 uint16_t TIM_Pulse;
78 uint16_t TIM_OCPolarity;
81 uint16_t TIM_OCNPolarity;
85 uint16_t TIM_OCIdleState;
89 uint16_t TIM_OCNIdleState;
92 } TIM_OCInitTypeDef;
93
94
98 typedef struct
99 {
100
101 uint16_t TIM_Channel;
104 uint16_t TIM_ICPolarity;
107 uint16_t TIM_ICSelection;
110 uint16_t TIM_ICPrescaler;
113 uint16_t TIM_ICFilter;
115 } TIM_ICInitTypeDef;
116
117
122 typedef struct
123 {
124
125 uint16_t TIM_OSSRState;
128 uint16_t TIM_OSSIState;
131 uint16_t TIM_LOCKLevel;
134 uint16_t TIM_DeadTime;
138 uint16_t TIM_Break;
141 uint16_t TIM_BreakPolarity;
144 uint16_t TIM_AutomaticOutput;
146 } TIM_BDTRInitTypeDef;
147
148 /* Exported Constants --------------------------------------------------------*/
149
154 #define IS_TIM_ALL_PERIPH(PERIPH) (((PERIPH) == TIM1) || \
155 ((PERIPH) == TIM2))
156
157 /* LIST1: TIM 1 */
158 #define IS_TIM_LIST1_PERIPH(PERIPH) (((PERIPH) == TIM1))
159
160 /* LIST2: TIM 1 */
161 #define IS_TIM_LIST2_PERIPH(PERIPH) (((PERIPH) == TIM1))
162
163 /* LIST3: TIM 1, 2 */
164 #define IS_TIM_LIST3_PERIPH(PERIPH) (((PERIPH) == TIM1) || \
165 ((PERIPH) == TIM2))
166
167 /* LIST4: TIM 1, 2 */
168 #define IS_TIM_LIST4_PERIPH(PERIPH) (((PERIPH) == TIM1) || \
169 ((PERIPH) == TIM2))
170
171 /* LIST5: TIM 1, 2 */
172 #define IS_TIM_LIST5_PERIPH(PERIPH) (((PERIPH) == TIM1) || \
173 ((PERIPH) == TIM2))
174
175 /* LIST6: TIM 1, 2 */
176 #define IS_TIM_LIST6_PERIPH(PERIPH) (((PERIPH) == TIM1) || \
177 ((PERIPH) == TIM2))
178
179 /* LIST7: TIM 1, 2 */
180 #define IS_TIM_LIST7_PERIPH(PERIPH) (((PERIPH) == TIM1) || \
181 ((PERIPH) == TIM2))
182
183 /* LIST8: TIM 1, 2 */
184 #define IS_TIM_LIST8_PERIPH(PERIPH) (((PERIPH) == TIM1) || \
185 ((PERIPH) == TIM2))
186
187 /* LIST9: TIM 1, 2 */
188 #define IS_TIM_LIST9_PERIPH(PERIPH) (((PERIPH) == TIM1) || \
189 ((PERIPH) == TIM2))
190
191
195 #define TIM_OCMode_Timing ((uint16_t)0x0000)
196 #define TIM_OCMode_Active ((uint16_t)0x0010)
197 #define TIM_OCMode_Inactive ((uint16_t)0x0020)
198 #define TIM_OCMode_Toggle ((uint16_t)0x0030)
199 #define TIM_OCMode_PWM1 ((uint16_t)0x0060)
200 #define TIM_OCMode_PWM2 ((uint16_t)0x0070)
201 #define IS_TIM_OC_MODE(MODE) (((MODE) == TIM_OCMode_Timing) || \
202 ((MODE) == TIM_OCMode_Active) || \
203 ((MODE) == TIM_OCMode_Inactive) || \
204 ((MODE) == TIM_OCMode_Toggle)|| \
205 ((MODE) == TIM_OCMode_PWM1) || \
206 ((MODE) == TIM_OCMode_PWM2))
207 #define IS_TIM_OCM(MODE) (((MODE) == TIM_OCMode_Timing) || \
208 ((MODE) == TIM_OCMode_Active) || \
209 ((MODE) == TIM_OCMode_Inactive) || \
210 ((MODE) == TIM_OCMode_Toggle)|| \
211 ((MODE) == TIM_OCMode_PWM1) || \
212 ((MODE) == TIM_OCMode_PWM2) || \
213 ((MODE) == TIM_ForcedAction_Active) || \
214 ((MODE) == TIM_ForcedAction_InActive))
215
223 #define TIM_OPMode_Single ((uint16_t)0x0008)
224 #define TIM_OPMode_Repetitive ((uint16_t)0x0000)
225 #define IS_TIM_OPM_MODE(MODE) (((MODE) == TIM_OPMode_Single) || \
226 ((MODE) == TIM_OPMode_Repetitive))
227
235 #define TIM_Channel_1 ((uint16_t)0x0000)
236 #define TIM_Channel_2 ((uint16_t)0x0004)
237 #define TIM_Channel_3 ((uint16_t)0x0008)
238 #define TIM_Channel_4 ((uint16_t)0x000C)
239 #define IS_TIM_CHANNEL(CHANNEL) (((CHANNEL) == TIM_Channel_1) || \
240 ((CHANNEL) == TIM_Channel_2) || \
241 ((CHANNEL) == TIM_Channel_3) || \
242 ((CHANNEL) == TIM_Channel_4))
243 #define IS_TIM_PWMI_CHANNEL(CHANNEL) (((CHANNEL) == TIM_Channel_1) || \
244 ((CHANNEL) == TIM_Channel_2))
245 #define IS_TIM_COMPLEMENTARY_CHANNEL(CHANNEL) (((CHANNEL) == TIM_Channel_1) || \
246 ((CHANNEL) == TIM_Channel_2) || \
247 ((CHANNEL) == TIM_Channel_3))
248
256 #define TIM_CKD_DIV1 ((uint16_t)0x0000)
257 #define TIM_CKD_DIV2 ((uint16_t)0x0100)
258 #define TIM_CKD_DIV4 ((uint16_t)0x0200)
259 #define IS_TIM_CKD_DIV(DIV) (((DIV) == TIM_CKD_DIV1) || \
260 ((DIV) == TIM_CKD_DIV2) || \
261 ((DIV) == TIM_CKD_DIV4))
262
270 #define TIM_CounterMode_Up ((uint16_t)0x0000)
271 #define TIM_CounterMode_Down ((uint16_t)0x0010)
272 #define TIM_CounterMode_CenterAligned1 ((uint16_t)0x0020)
273 #define TIM_CounterMode_CenterAligned2 ((uint16_t)0x0040)
274 #define TIM_CounterMode_CenterAligned3 ((uint16_t)0x0060)
275 #define IS_TIM_COUNTER_MODE(MODE) (((MODE) == TIM_CounterMode_Up) || \
276 ((MODE) == TIM_CounterMode_Down) || \
277 ((MODE) == TIM_CounterMode_CenterAligned1) || \
278 ((MODE) == TIM_CounterMode_CenterAligned2) || \
279 ((MODE) == TIM_CounterMode_CenterAligned3))
280
288 #define TIM_OCPolarity_High ((uint16_t)0x0000)
289 #define TIM_OCPolarity_Low ((uint16_t)0x0002)
290 #define IS_TIM_OC_POLARITY(POLARITY) (((POLARITY) == TIM_OCPolarity_High) || \
291 ((POLARITY) == TIM_OCPolarity_Low))
292
300 #define TIM_OCNPolarity_High ((uint16_t)0x0000)
301 #define TIM_OCNPolarity_Low ((uint16_t)0x0008)
302 #define IS_TIM_OCN_POLARITY(POLARITY) (((POLARITY) == TIM_OCNPolarity_High) || \
303 ((POLARITY) == TIM_OCNPolarity_Low))
304
312 #define TIM_OutputState_Disable ((uint16_t)0x0000)
313 #define TIM_OutputState_Enable ((uint16_t)0x0001)
314 #define IS_TIM_OUTPUT_STATE(STATE) (((STATE) == TIM_OutputState_Disable) || \
315 ((STATE) == TIM_OutputState_Enable))
316
324 #define TIM_OutputNState_Disable ((uint16_t)0x0000)
325 #define TIM_OutputNState_Enable ((uint16_t)0x0004)
326 #define IS_TIM_OUTPUTN_STATE(STATE) (((STATE) == TIM_OutputNState_Disable) || \
327 ((STATE) == TIM_OutputNState_Enable))
328
336 #define TIM_CCx_Enable ((uint16_t)0x0001)
337 #define TIM_CCx_Disable ((uint16_t)0x0000)
338 #define IS_TIM_CCX(CCX) (((CCX) == TIM_CCx_Enable) || \
339 ((CCX) == TIM_CCx_Disable))
340
348 #define TIM_CCxN_Enable ((uint16_t)0x0004)
349 #define TIM_CCxN_Disable ((uint16_t)0x0000)
350 #define IS_TIM_CCXN(CCXN) (((CCXN) == TIM_CCxN_Enable) || \
351 ((CCXN) == TIM_CCxN_Disable))
352
360 #define TIM_Break_Enable ((uint16_t)0x1000)
361 #define TIM_Break_Disable ((uint16_t)0x0000)
362 #define IS_TIM_BREAK_STATE(STATE) (((STATE) == TIM_Break_Enable) || \
363 ((STATE) == TIM_Break_Disable))
364
372 #define TIM_BreakPolarity_Low ((uint16_t)0x0000)
373 #define TIM_BreakPolarity_High ((uint16_t)0x2000)
374 #define IS_TIM_BREAK_POLARITY(POLARITY) (((POLARITY) == TIM_BreakPolarity_Low) || \
375 ((POLARITY) == TIM_BreakPolarity_High))
376
384 #define TIM_AutomaticOutput_Enable ((uint16_t)0x4000)
385 #define TIM_AutomaticOutput_Disable ((uint16_t)0x0000)
386 #define IS_TIM_AUTOMATIC_OUTPUT_STATE(STATE) (((STATE) == TIM_AutomaticOutput_Enable) || \
387 ((STATE) == TIM_AutomaticOutput_Disable))
388
396 #define TIM_LOCKLevel_OFF ((uint16_t)0x0000)
397 #define TIM_LOCKLevel_1 ((uint16_t)0x0100)
398 #define TIM_LOCKLevel_2 ((uint16_t)0x0200)
399 #define TIM_LOCKLevel_3 ((uint16_t)0x0300)
400 #define IS_TIM_LOCK_LEVEL(LEVEL) (((LEVEL) == TIM_LOCKLevel_OFF) || \
401 ((LEVEL) == TIM_LOCKLevel_1) || \
402 ((LEVEL) == TIM_LOCKLevel_2) || \
403 ((LEVEL) == TIM_LOCKLevel_3))
404
412 #define TIM_OSSIState_Enable ((uint16_t)0x0400)
413 #define TIM_OSSIState_Disable ((uint16_t)0x0000)
414 #define IS_TIM_OSSI_STATE(STATE) (((STATE) == TIM_OSSIState_Enable) || \
415 ((STATE) == TIM_OSSIState_Disable))
416
424 #define TIM_OSSRState_Enable ((uint16_t)0x0800)
425 #define TIM_OSSRState_Disable ((uint16_t)0x0000)
426 #define IS_TIM_OSSR_STATE(STATE) (((STATE) == TIM_OSSRState_Enable) || \
427 ((STATE) == TIM_OSSRState_Disable))
428
436 #define TIM_OCIdleState_Set ((uint16_t)0x0100)
437 #define TIM_OCIdleState_Reset ((uint16_t)0x0000)
438 #define IS_TIM_OCIDLE_STATE(STATE) (((STATE) == TIM_OCIdleState_Set) || \
439 ((STATE) == TIM_OCIdleState_Reset))
440
448 #define TIM_OCNIdleState_Set ((uint16_t)0x0200)
449 #define TIM_OCNIdleState_Reset ((uint16_t)0x0000)
450 #define IS_TIM_OCNIDLE_STATE(STATE) (((STATE) == TIM_OCNIdleState_Set) || \
451 ((STATE) == TIM_OCNIdleState_Reset))
452
460 #define TIM_ICPolarity_Rising ((uint16_t)0x0000)
461 #define TIM_ICPolarity_Falling ((uint16_t)0x0002)
462 #define TIM_ICPolarity_BothEdge ((uint16_t)0x000A)
463 #define IS_TIM_IC_POLARITY(POLARITY) (((POLARITY) == TIM_ICPolarity_Rising) || \
464 ((POLARITY) == TIM_ICPolarity_Falling))
465 #define IS_TIM_IC_POLARITY_LITE(POLARITY) (((POLARITY) == TIM_ICPolarity_Rising) || \
466 ((POLARITY) == TIM_ICPolarity_Falling)|| \
467 ((POLARITY) == TIM_ICPolarity_BothEdge))
468
475 #define TIM_ICSelection_DirectTI ((uint16_t)0x0001)
477 #define TIM_ICSelection_IndirectTI ((uint16_t)0x0002)
479 #define TIM_ICSelection_TRC ((uint16_t)0x0003)
480 #define IS_TIM_IC_SELECTION(SELECTION) (((SELECTION) == TIM_ICSelection_DirectTI) || \
481 ((SELECTION) == TIM_ICSelection_IndirectTI) || \
482 ((SELECTION) == TIM_ICSelection_TRC))
483
491 #define TIM_ICPSC_DIV1 ((uint16_t)0x0000)
492 #define TIM_ICPSC_DIV2 ((uint16_t)0x0004)
493 #define TIM_ICPSC_DIV4 ((uint16_t)0x0008)
494 #define TIM_ICPSC_DIV8 ((uint16_t)0x000C)
495 #define IS_TIM_IC_PRESCALER(PRESCALER) (((PRESCALER) == TIM_ICPSC_DIV1) || \
496 ((PRESCALER) == TIM_ICPSC_DIV2) || \
497 ((PRESCALER) == TIM_ICPSC_DIV4) || \
498 ((PRESCALER) == TIM_ICPSC_DIV8))
499
507 #define TIM_IT_Update ((uint16_t)0x0001)
508 #define TIM_IT_CC1 ((uint16_t)0x0002)
509 #define TIM_IT_CC2 ((uint16_t)0x0004)
510 #define TIM_IT_CC3 ((uint16_t)0x0008)
511 #define TIM_IT_CC4 ((uint16_t)0x0010)
512 #define TIM_IT_COM ((uint16_t)0x0020)
513 #define TIM_IT_Trigger ((uint16_t)0x0040)
514 #define TIM_IT_Break ((uint16_t)0x0080)
515 #define IS_TIM_IT(IT) ((((IT) & (uint16_t)0xFF00) == 0x0000) && ((IT) != 0x0000))
516
517 #define IS_TIM_GET_IT(IT) (((IT) == TIM_IT_Update) || \
518 ((IT) == TIM_IT_CC1) || \
519 ((IT) == TIM_IT_CC2) || \
520 ((IT) == TIM_IT_CC3) || \
521 ((IT) == TIM_IT_CC4) || \
522 ((IT) == TIM_IT_COM) || \
523 ((IT) == TIM_IT_Trigger) || \
524 ((IT) == TIM_IT_Break))
525
533 #define TIM_ExtTRGPSC_OFF ((uint16_t)0x0000)
534 #define TIM_ExtTRGPSC_DIV2 ((uint16_t)0x1000)
535 #define TIM_ExtTRGPSC_DIV4 ((uint16_t)0x2000)
536 #define TIM_ExtTRGPSC_DIV8 ((uint16_t)0x3000)
537 #define IS_TIM_EXT_PRESCALER(PRESCALER) (((PRESCALER) == TIM_ExtTRGPSC_OFF) || \
538 ((PRESCALER) == TIM_ExtTRGPSC_DIV2) || \
539 ((PRESCALER) == TIM_ExtTRGPSC_DIV4) || \
540 ((PRESCALER) == TIM_ExtTRGPSC_DIV8))
541
549 #define TIM_TS_ITR0 ((uint16_t)0x0000)
550 #define TIM_TS_ITR1 ((uint16_t)0x0010)
551 #define TIM_TS_ITR2 ((uint16_t)0x0020)
552 #define TIM_TS_ITR3 ((uint16_t)0x0030)
553 #define TIM_TS_TI1F_ED ((uint16_t)0x0040)
554 #define TIM_TS_TI1FP1 ((uint16_t)0x0050)
555 #define TIM_TS_TI2FP2 ((uint16_t)0x0060)
556 #define TIM_TS_ETRF ((uint16_t)0x0070)
557 #define IS_TIM_TRIGGER_SELECTION(SELECTION) (((SELECTION) == TIM_TS_ITR0) || \
558 ((SELECTION) == TIM_TS_ITR1) || \
559 ((SELECTION) == TIM_TS_ITR2) || \
560 ((SELECTION) == TIM_TS_ITR3) || \
561 ((SELECTION) == TIM_TS_TI1F_ED) || \
562 ((SELECTION) == TIM_TS_TI1FP1) || \
563 ((SELECTION) == TIM_TS_TI2FP2) || \
564 ((SELECTION) == TIM_TS_ETRF))
565 #define IS_TIM_INTERNAL_TRIGGER_SELECTION(SELECTION) (((SELECTION) == TIM_TS_ITR0) || \
566 ((SELECTION) == TIM_TS_ITR1) || \
567 ((SELECTION) == TIM_TS_ITR2) || \
568 ((SELECTION) == TIM_TS_ITR3))
569
577 #define TIM_TIxExternalCLK1Source_TI1 ((uint16_t)0x0050)
578 #define TIM_TIxExternalCLK1Source_TI2 ((uint16_t)0x0060)
579 #define TIM_TIxExternalCLK1Source_TI1ED ((uint16_t)0x0040)
580 #define IS_TIM_TIXCLK_SOURCE(SOURCE) (((SOURCE) == TIM_TIxExternalCLK1Source_TI1) || \
581 ((SOURCE) == TIM_TIxExternalCLK1Source_TI2) || \
582 ((SOURCE) == TIM_TIxExternalCLK1Source_TI1ED))
583
590 #define TIM_ExtTRGPolarity_Inverted ((uint16_t)0x8000)
591 #define TIM_ExtTRGPolarity_NonInverted ((uint16_t)0x0000)
592 #define IS_TIM_EXT_POLARITY(POLARITY) (((POLARITY) == TIM_ExtTRGPolarity_Inverted) || \
593 ((POLARITY) == TIM_ExtTRGPolarity_NonInverted))
594
602 #define TIM_PSCReloadMode_Update ((uint16_t)0x0000)
603 #define TIM_PSCReloadMode_Immediate ((uint16_t)0x0001)
604 #define IS_TIM_PRESCALER_RELOAD(RELOAD) (((RELOAD) == TIM_PSCReloadMode_Update) || \
605 ((RELOAD) == TIM_PSCReloadMode_Immediate))
606
614 #define TIM_ForcedAction_Active ((uint16_t)0x0050)
615 #define TIM_ForcedAction_InActive ((uint16_t)0x0040)
616 #define IS_TIM_FORCED_ACTION(ACTION) (((ACTION) == TIM_ForcedAction_Active) || \
617 ((ACTION) == TIM_ForcedAction_InActive))
618
626 #define TIM_EncoderMode_TI1 ((uint16_t)0x0001)
627 #define TIM_EncoderMode_TI2 ((uint16_t)0x0002)
628 #define TIM_EncoderMode_TI12 ((uint16_t)0x0003)
629 #define IS_TIM_ENCODER_MODE(MODE) (((MODE) == TIM_EncoderMode_TI1) || \
630 ((MODE) == TIM_EncoderMode_TI2) || \
631 ((MODE) == TIM_EncoderMode_TI12))
632
640 #define TIM_EventSource_Update ((uint16_t)0x0001)
641 #define TIM_EventSource_CC1 ((uint16_t)0x0002)
642 #define TIM_EventSource_CC2 ((uint16_t)0x0004)
643 #define TIM_EventSource_CC3 ((uint16_t)0x0008)
644 #define TIM_EventSource_CC4 ((uint16_t)0x0010)
645 #define TIM_EventSource_COM ((uint16_t)0x0020)
646 #define TIM_EventSource_Trigger ((uint16_t)0x0040)
647 #define TIM_EventSource_Break ((uint16_t)0x0080)
648 #define IS_TIM_EVENT_SOURCE(SOURCE) ((((SOURCE) & (uint16_t)0xFF00) == 0x0000) && ((SOURCE) != 0x0000))
649
657 #define TIM_UpdateSource_Global ((uint16_t)0x0000)
660 #define TIM_UpdateSource_Regular ((uint16_t)0x0001)
661 #define IS_TIM_UPDATE_SOURCE(SOURCE) (((SOURCE) == TIM_UpdateSource_Global) || \
662 ((SOURCE) == TIM_UpdateSource_Regular))
663
671 #define TIM_OCPreload_Enable ((uint16_t)0x0008)
672 #define TIM_OCPreload_Disable ((uint16_t)0x0000)
673 #define IS_TIM_OCPRELOAD_STATE(STATE) (((STATE) == TIM_OCPreload_Enable) || \
674 ((STATE) == TIM_OCPreload_Disable))
675
683 #define TIM_OCFast_Enable ((uint16_t)0x0004)
684 #define TIM_OCFast_Disable ((uint16_t)0x0000)
685 #define IS_TIM_OCFAST_STATE(STATE) (((STATE) == TIM_OCFast_Enable) || \
686 ((STATE) == TIM_OCFast_Disable))
687
695 #define TIM_OCClear_Enable ((uint16_t)0x0080)
696 #define TIM_OCClear_Disable ((uint16_t)0x0000)
697 #define IS_TIM_OCCLEAR_STATE(STATE) (((STATE) == TIM_OCClear_Enable) || \
698 ((STATE) == TIM_OCClear_Disable))
699
706 #define TIM_TRGOSource_Reset ((uint16_t)0x0000)
707 #define TIM_TRGOSource_Enable ((uint16_t)0x0010)
708 #define TIM_TRGOSource_Update ((uint16_t)0x0020)
709 #define TIM_TRGOSource_OC1 ((uint16_t)0x0030)
710 #define TIM_TRGOSource_OC1Ref ((uint16_t)0x0040)
711 #define TIM_TRGOSource_OC2Ref ((uint16_t)0x0050)
712 #define TIM_TRGOSource_OC3Ref ((uint16_t)0x0060)
713 #define TIM_TRGOSource_OC4Ref ((uint16_t)0x0070)
714 #define IS_TIM_TRGO_SOURCE(SOURCE) (((SOURCE) == TIM_TRGOSource_Reset) || \
715 ((SOURCE) == TIM_TRGOSource_Enable) || \
716 ((SOURCE) == TIM_TRGOSource_Update) || \
717 ((SOURCE) == TIM_TRGOSource_OC1) || \
718 ((SOURCE) == TIM_TRGOSource_OC1Ref) || \
719 ((SOURCE) == TIM_TRGOSource_OC2Ref) || \
720 ((SOURCE) == TIM_TRGOSource_OC3Ref) || \
721 ((SOURCE) == TIM_TRGOSource_OC4Ref))
722
730 #define TIM_SlaveMode_Reset ((uint16_t)0x0004)
731 #define TIM_SlaveMode_Gated ((uint16_t)0x0005)
732 #define TIM_SlaveMode_Trigger ((uint16_t)0x0006)
733 #define TIM_SlaveMode_External1 ((uint16_t)0x0007)
734 #define IS_TIM_SLAVE_MODE(MODE) (((MODE) == TIM_SlaveMode_Reset) || \
735 ((MODE) == TIM_SlaveMode_Gated) || \
736 ((MODE) == TIM_SlaveMode_Trigger) || \
737 ((MODE) == TIM_SlaveMode_External1))
738
746 #define TIM_MasterSlaveMode_Enable ((uint16_t)0x0080)
747 #define TIM_MasterSlaveMode_Disable ((uint16_t)0x0000)
748 #define IS_TIM_MSM_STATE(STATE) (((STATE) == TIM_MasterSlaveMode_Enable) || \
749 ((STATE) == TIM_MasterSlaveMode_Disable))
750
758 #define TIM_FLAG_Update ((uint16_t)0x0001)
759 #define TIM_FLAG_CC1 ((uint16_t)0x0002)
760 #define TIM_FLAG_CC2 ((uint16_t)0x0004)
761 #define TIM_FLAG_CC3 ((uint16_t)0x0008)
762 #define TIM_FLAG_CC4 ((uint16_t)0x0010)
763 #define TIM_FLAG_COM ((uint16_t)0x0020)
764 #define TIM_FLAG_Trigger ((uint16_t)0x0040)
765 #define TIM_FLAG_Break ((uint16_t)0x0080)
766 #define TIM_FLAG_CC1OF ((uint16_t)0x0200)
767 #define TIM_FLAG_CC2OF ((uint16_t)0x0400)
768 #define TIM_FLAG_CC3OF ((uint16_t)0x0800)
769 #define TIM_FLAG_CC4OF ((uint16_t)0x1000)
770 #define IS_TIM_GET_FLAG(FLAG) (((FLAG) == TIM_FLAG_Update) || \
771 ((FLAG) == TIM_FLAG_CC1) || \
772 ((FLAG) == TIM_FLAG_CC2) || \
773 ((FLAG) == TIM_FLAG_CC3) || \
774 ((FLAG) == TIM_FLAG_CC4) || \
775 ((FLAG) == TIM_FLAG_COM) || \
776 ((FLAG) == TIM_FLAG_Trigger) || \
777 ((FLAG) == TIM_FLAG_Break) || \
778 ((FLAG) == TIM_FLAG_CC1OF) || \
779 ((FLAG) == TIM_FLAG_CC2OF) || \
780 ((FLAG) == TIM_FLAG_CC3OF) || \
781 ((FLAG) == TIM_FLAG_CC4OF))
782
783
784 #define IS_TIM_CLEAR_FLAG(TIM_FLAG) ((((TIM_FLAG) & (uint16_t)0xE100) == 0x0000) && ((TIM_FLAG) != 0x0000))
785
793 #define IS_TIM_IC_FILTER(ICFILTER) ((ICFILTER) <= 0xF)
794
802 #define IS_TIM_EXT_FILTER(EXTFILTER) ((EXTFILTER) <= 0xF)
803
812 /* Exported macro ------------------------------------------------------------*/
813 /* Exported functions --------------------------------------------------------*/
814
815 void TIM_DeInit(TIM_TypeDef* TIMx);
816 void TIM_TimeBaseInit(TIM_TypeDef* TIMx, TIM_TimeBaseInitTypeDef* TIM_TimeBaseInitStruct);
817 void TIM_OC1Init(TIM_TypeDef* TIMx, TIM_OCInitTypeDef* TIM_OCInitStruct);
818 void TIM_OC2Init(TIM_TypeDef* TIMx, TIM_OCInitTypeDef* TIM_OCInitStruct);
819 void TIM_OC3Init(TIM_TypeDef* TIMx, TIM_OCInitTypeDef* TIM_OCInitStruct);
820 void TIM_OC4Init(TIM_TypeDef* TIMx, TIM_OCInitTypeDef* TIM_OCInitStruct);
821 void TIM_ICInit(TIM_TypeDef* TIMx, TIM_ICInitTypeDef* TIM_ICInitStruct);
822 void TIM_PWMIConfig(TIM_TypeDef* TIMx, TIM_ICInitTypeDef* TIM_ICInitStruct);
823 void TIM_BDTRConfig(TIM_TypeDef* TIMx, TIM_BDTRInitTypeDef *TIM_BDTRInitStruct);
824 void TIM_TimeBaseStructInit(TIM_TimeBaseInitTypeDef* TIM_TimeBaseInitStruct);
825 void TIM_OCStructInit(TIM_OCInitTypeDef* TIM_OCInitStruct);
826 void TIM_ICStructInit(TIM_ICInitTypeDef* TIM_ICInitStruct);
827 void TIM_BDTRStructInit(TIM_BDTRInitTypeDef* TIM_BDTRInitStruct);
828 void TIM_Cmd(TIM_TypeDef* TIMx, FunctionalState NewState);
829 void TIM_CtrlPWMOutputs(TIM_TypeDef* TIMx, FunctionalState NewState);
830 void TIM_ITConfig(TIM_TypeDef* TIMx, uint16_t TIM_IT, FunctionalState NewState);
831 void TIM_GenerateEvent(TIM_TypeDef* TIMx, uint16_t TIM_EventSource);
832 void TIM_InternalClockConfig(TIM_TypeDef* TIMx);
833 void TIM_ITRxExternalClockConfig(TIM_TypeDef* TIMx, uint16_t TIM_InputTriggerSource);
834 void TIM_TIxExternalClockConfig(TIM_TypeDef* TIMx, uint16_t TIM_TIxExternalCLKSource,
835 uint16_t TIM_ICPolarity, uint16_t ICFilter);
836 void TIM_ETRClockMode1Config(TIM_TypeDef* TIMx, uint16_t TIM_ExtTRGPrescaler, uint16_t TIM_ExtTRGPolarity,
837 uint16_t ExtTRGFilter);
838 void TIM_ETRClockMode2Config(TIM_TypeDef* TIMx, uint16_t TIM_ExtTRGPrescaler,
839 uint16_t TIM_ExtTRGPolarity, uint16_t ExtTRGFilter);
840 void TIM_ETRConfig(TIM_TypeDef* TIMx, uint16_t TIM_ExtTRGPrescaler, uint16_t TIM_ExtTRGPolarity,
841 uint16_t ExtTRGFilter);
842 void TIM_PrescalerConfig(TIM_TypeDef* TIMx, uint16_t Prescaler, uint16_t TIM_PSCReloadMode);
843 void TIM_CounterModeConfig(TIM_TypeDef* TIMx, uint16_t TIM_CounterMode);
844 void TIM_SelectInputTrigger(TIM_TypeDef* TIMx, uint16_t TIM_InputTriggerSource);
845 void TIM_EncoderInterfaceConfig(TIM_TypeDef* TIMx, uint16_t TIM_EncoderMode,
846 uint16_t TIM_IC1Polarity, uint16_t TIM_IC2Polarity);
847 void TIM_ForcedOC1Config(TIM_TypeDef* TIMx, uint16_t TIM_ForcedAction);
848 void TIM_ForcedOC2Config(TIM_TypeDef* TIMx, uint16_t TIM_ForcedAction);
849 void TIM_ForcedOC3Config(TIM_TypeDef* TIMx, uint16_t TIM_ForcedAction);
850 void TIM_ForcedOC4Config(TIM_TypeDef* TIMx, uint16_t TIM_ForcedAction);
851 void TIM_ARRPreloadConfig(TIM_TypeDef* TIMx, FunctionalState NewState);
852 void TIM_SelectCOM(TIM_TypeDef* TIMx, FunctionalState NewState);
853 void TIM_CCPreloadControl(TIM_TypeDef* TIMx, FunctionalState NewState);
854 void TIM_OC1PreloadConfig(TIM_TypeDef* TIMx, uint16_t TIM_OCPreload);
855 void TIM_OC2PreloadConfig(TIM_TypeDef* TIMx, uint16_t TIM_OCPreload);
856 void TIM_OC3PreloadConfig(TIM_TypeDef* TIMx, uint16_t TIM_OCPreload);
857 void TIM_OC4PreloadConfig(TIM_TypeDef* TIMx, uint16_t TIM_OCPreload);
858 void TIM_OC1FastConfig(TIM_TypeDef* TIMx, uint16_t TIM_OCFast);
859 void TIM_OC2FastConfig(TIM_TypeDef* TIMx, uint16_t TIM_OCFast);
860 void TIM_OC3FastConfig(TIM_TypeDef* TIMx, uint16_t TIM_OCFast);
861 void TIM_OC4FastConfig(TIM_TypeDef* TIMx, uint16_t TIM_OCFast);
862 void TIM_ClearOC1Ref(TIM_TypeDef* TIMx, uint16_t TIM_OCClear);
863 void TIM_ClearOC2Ref(TIM_TypeDef* TIMx, uint16_t TIM_OCClear);
864 void TIM_ClearOC3Ref(TIM_TypeDef* TIMx, uint16_t TIM_OCClear);
865 void TIM_ClearOC4Ref(TIM_TypeDef* TIMx, uint16_t TIM_OCClear);
866 void TIM_OC1PolarityConfig(TIM_TypeDef* TIMx, uint16_t TIM_OCPolarity);
867 void TIM_OC1NPolarityConfig(TIM_TypeDef* TIMx, uint16_t TIM_OCNPolarity);
868 void TIM_OC2PolarityConfig(TIM_TypeDef* TIMx, uint16_t TIM_OCPolarity);
869 void TIM_OC2NPolarityConfig(TIM_TypeDef* TIMx, uint16_t TIM_OCNPolarity);
870 void TIM_OC3PolarityConfig(TIM_TypeDef* TIMx, uint16_t TIM_OCPolarity);
871 void TIM_OC3NPolarityConfig(TIM_TypeDef* TIMx, uint16_t TIM_OCNPolarity);
872 void TIM_OC4PolarityConfig(TIM_TypeDef* TIMx, uint16_t TIM_OCPolarity);
873 void TIM_CCxCmd(TIM_TypeDef* TIMx, uint16_t TIM_Channel, uint16_t TIM_CCx);
874 void TIM_CCxNCmd(TIM_TypeDef* TIMx, uint16_t TIM_Channel, uint16_t TIM_CCxN);
875 void TIM_SelectOCxM(TIM_TypeDef* TIMx, uint16_t TIM_Channel, uint16_t TIM_OCMode);
876 void TIM_UpdateDisableConfig(TIM_TypeDef* TIMx, FunctionalState NewState);
877 void TIM_UpdateRequestConfig(TIM_TypeDef* TIMx, uint16_t TIM_UpdateSource);
878 void TIM_SelectHallSensor(TIM_TypeDef* TIMx, FunctionalState NewState);
879 void TIM_SelectOnePulseMode(TIM_TypeDef* TIMx, uint16_t TIM_OPMode);
880 void TIM_SelectOutputTrigger(TIM_TypeDef* TIMx, uint16_t TIM_TRGOSource);
881 void TIM_SelectSlaveMode(TIM_TypeDef* TIMx, uint16_t TIM_SlaveMode);
882 void TIM_SelectMasterSlaveMode(TIM_TypeDef* TIMx, uint16_t TIM_MasterSlaveMode);
883 void TIM_SetCounter(TIM_TypeDef* TIMx, uint16_t Counter);
884 void TIM_SetAutoreload(TIM_TypeDef* TIMx, uint16_t Autoreload);
885 void TIM_SetCompare1(TIM_TypeDef* TIMx, uint16_t Compare1);
886 void TIM_SetCompare2(TIM_TypeDef* TIMx, uint16_t Compare2);
887 void TIM_SetCompare3(TIM_TypeDef* TIMx, uint16_t Compare3);
888 void TIM_SetCompare4(TIM_TypeDef* TIMx, uint16_t Compare4);
889 void TIM_SetIC1Prescaler(TIM_TypeDef* TIMx, uint16_t TIM_ICPSC);
890 void TIM_SetIC2Prescaler(TIM_TypeDef* TIMx, uint16_t TIM_ICPSC);
891 void TIM_SetIC3Prescaler(TIM_TypeDef* TIMx, uint16_t TIM_ICPSC);
892 void TIM_SetIC4Prescaler(TIM_TypeDef* TIMx, uint16_t TIM_ICPSC);
893 void TIM_SetClockDivision(TIM_TypeDef* TIMx, uint16_t TIM_CKD);
894 uint16_t TIM_GetCapture1(TIM_TypeDef* TIMx);
895 uint16_t TIM_GetCapture2(TIM_TypeDef* TIMx);
896 uint16_t TIM_GetCapture3(TIM_TypeDef* TIMx);
897 uint16_t TIM_GetCapture4(TIM_TypeDef* TIMx);
898 uint16_t TIM_GetCounter(TIM_TypeDef* TIMx);
899 uint16_t TIM_GetPrescaler(TIM_TypeDef* TIMx);
900 FlagStatus TIM_GetFlagStatus(TIM_TypeDef* TIMx, uint16_t TIM_FLAG);
901 void TIM_ClearFlag(TIM_TypeDef* TIMx, uint16_t TIM_FLAG);
902 ITStatus TIM_GetITStatus(TIM_TypeDef* TIMx, uint16_t TIM_IT);
903 void TIM_ClearITPendingBit(TIM_TypeDef* TIMx, uint16_t TIM_IT);
904
913 #ifdef __cplusplus
914 }
915 #endif
916
917 #endif /*__WB32L003_TIM_H */
TIM_BDTRInitTypeDef::TIM_Break
uint16_t TIM_Break
Definition: wb32l003_tim.h:138
TIM_GetCapture4
uint16_t TIM_GetCapture4(TIM_TypeDef *TIMx)
Gets the TIMx Input Capture 4 value.
Definition: wb32l003_tim.c:2260
TIM_SelectHallSensor
void TIM_SelectHallSensor(TIM_TypeDef *TIMx, FunctionalState NewState)
Enables or disables the TIMx's Hall sensor interface.
Definition: wb32l003_tim.c:1912
TIM_CtrlPWMOutputs
void TIM_CtrlPWMOutputs(TIM_TypeDef *TIMx, FunctionalState NewState)
Enables or disables the TIM peripheral Main Outputs.
Definition: wb32l003_tim.c:694
TIM_BDTRInitTypeDef::TIM_BreakPolarity
uint16_t TIM_BreakPolarity
Definition: wb32l003_tim.h:141
TIM_SetCompare3
void TIM_SetCompare3(TIM_TypeDef *TIMx, uint16_t Compare3)
Sets the TIMx Capture Compare3 Register value
Definition: wb32l003_tim.c:2084
TIM_Cmd
void TIM_Cmd(TIM_TypeDef *TIMx, FunctionalState NewState)
Enables or disables the specified TIM peripheral.
Definition: wb32l003_tim.c:669
TIM_BDTRInitTypeDef::TIM_DeadTime
uint16_t TIM_DeadTime
Definition: wb32l003_tim.h:134
TIM_ClearOC4Ref
void TIM_ClearOC4Ref(TIM_TypeDef *TIMx, uint16_t TIM_OCClear)
Clears or safeguards the OCREF4 signal on an external event
Definition: wb32l003_tim.c:1550
TIM_OC3FastConfig
void TIM_OC3FastConfig(TIM_TypeDef *TIMx, uint16_t TIM_OCFast)
Configures the TIMx Output Compare 3 Fast feature.
Definition: wb32l003_tim.c:1426
TIM_TimeBaseInitTypeDef::TIM_Prescaler
uint16_t TIM_Prescaler
Definition: wb32l003_tim.h:36
TIM_GetPrescaler
uint16_t TIM_GetPrescaler(TIM_TypeDef *TIMx)
Gets the TIMx Prescaler value.
Definition: wb32l003_tim.c:2286
TIM_SetIC2Prescaler
void TIM_SetIC2Prescaler(TIM_TypeDef *TIMx, uint16_t TIM_ICPSC)
Sets the TIMx Input Capture 2 prescaler.
Definition: wb32l003_tim.c:2139
TIM_SetIC3Prescaler
void TIM_SetIC3Prescaler(TIM_TypeDef *TIMx, uint16_t TIM_ICPSC)
Sets the TIMx Input Capture 3 prescaler.
Definition: wb32l003_tim.c:2161
TIM_OC3PolarityConfig
void TIM_OC3PolarityConfig(TIM_TypeDef *TIMx, uint16_t TIM_OCPolarity)
Configures the TIMx channel 3 polarity.
Definition: wb32l003_tim.c:1668
TIM_ICInitTypeDef::TIM_ICPolarity
uint16_t TIM_ICPolarity
Definition: wb32l003_tim.h:104
TIM_BDTRInitTypeDef::TIM_OSSRState
uint16_t TIM_OSSRState
Definition: wb32l003_tim.h:125
TIM_OCStructInit
void TIM_OCStructInit(TIM_OCInitTypeDef *TIM_OCInitStruct)
Fills each TIM_OCInitStruct member with its default value.
Definition: wb32l003_tim.c:615
TIM_OC3Init
void TIM_OC3Init(TIM_TypeDef *TIMx, TIM_OCInitTypeDef *TIM_OCInitStruct)
Initializes the TIMx Channel3 according to the specified parameters in the TIM_OCInitStruct.
Definition: wb32l003_tim.c:308
TIM_ClearOC1Ref
void TIM_ClearOC1Ref(TIM_TypeDef *TIMx, uint16_t TIM_OCClear)
Clears or safeguards the OCREF1 signal on an external event
Definition: wb32l003_tim.c:1476
TIM_SelectOnePulseMode
void TIM_SelectOnePulseMode(TIM_TypeDef *TIMx, uint16_t TIM_OPMode)
Selects the TIMx's One Pulse Mode.
Definition: wb32l003_tim.c:1938
TIM_SetCounter
void TIM_SetCounter(TIM_TypeDef *TIMx, uint16_t Counter)
Sets the TIMx Counter Register value
Definition: wb32l003_tim.c:2028
TIM_OC3PreloadConfig
void TIM_OC3PreloadConfig(TIM_TypeDef *TIMx, uint16_t TIM_OCPreload)
Enables or disables the TIMx peripheral Preload register on CCR3.
Definition: wb32l003_tim.c:1327
TIM_OC2NPolarityConfig
void TIM_OC2NPolarityConfig(TIM_TypeDef *TIMx, uint16_t TIM_OCNPolarity)
Configures the TIMx Channel 2N polarity.
Definition: wb32l003_tim.c:1644
TIM_ITRxExternalClockConfig
void TIM_ITRxExternalClockConfig(TIM_TypeDef *TIMx, uint16_t TIM_InputTriggerSource)
Configures the TIMx Internal Trigger as External Clock
Definition: wb32l003_tim.c:802
TIM_SelectCOM
void TIM_SelectCOM(TIM_TypeDef *TIMx, FunctionalState NewState)
Selects the TIM peripheral Commutation event.
Definition: wb32l003_tim.c:1227
TIM_SetCompare1
void TIM_SetCompare1(TIM_TypeDef *TIMx, uint16_t Compare1)
Sets the TIMx Capture Compare1 Register value
Definition: wb32l003_tim.c:2056
TIM_OC4FastConfig
void TIM_OC4FastConfig(TIM_TypeDef *TIMx, uint16_t TIM_OCFast)
Configures the TIMx Output Compare 4 Fast feature.
Definition: wb32l003_tim.c:1451
TIM_ForcedOC3Config
void TIM_ForcedOC3Config(TIM_TypeDef *TIMx, uint16_t TIM_ForcedAction)
Forces the TIMx output 3 waveform to active or inactive level.
Definition: wb32l003_tim.c:1157
TIM_ETRConfig
void TIM_ETRConfig(TIM_TypeDef *TIMx, uint16_t TIM_ExtTRGPrescaler, uint16_t TIM_ExtTRGPolarity, uint16_t ExtTRGFilter)
Configures the TIMx External Trigger (ETR).
Definition: wb32l003_tim.c:942
TIM_ARRPreloadConfig
void TIM_ARRPreloadConfig(TIM_TypeDef *TIMx, FunctionalState NewState)
Enables or disables TIMx peripheral Preload register on ARR.
Definition: wb32l003_tim.c:1203
TIM_CCxCmd
void TIM_CCxCmd(TIM_TypeDef *TIMx, uint16_t TIM_Channel, uint16_t TIM_CCx)
Enables or disables the TIM Capture Compare Channel x.
Definition: wb32l003_tim.c:1743
TIM_ETRClockMode2Config
void TIM_ETRClockMode2Config(TIM_TypeDef *TIMx, uint16_t TIM_ExtTRGPrescaler, uint16_t TIM_ExtTRGPolarity, uint16_t ExtTRGFilter)
Configures the External clock Mode2
Definition: wb32l003_tim.c:911
TIM_ForcedOC2Config
void TIM_ForcedOC2Config(TIM_TypeDef *TIMx, uint16_t TIM_ForcedAction)
Forces the TIMx output 2 waveform to active or inactive level.
Definition: wb32l003_tim.c:1133
TIM_PrescalerConfig
void TIM_PrescalerConfig(TIM_TypeDef *TIMx, uint16_t Prescaler, uint16_t TIM_PSCReloadMode)
Configures the TIMx Prescaler.
Definition: wb32l003_tim.c:970
TIM_OCInitTypeDef::TIM_OCNPolarity
uint16_t TIM_OCNPolarity
Definition: wb32l003_tim.h:81
TIM_OCInitTypeDef::TIM_OCNIdleState
uint16_t TIM_OCNIdleState
Definition: wb32l003_tim.h:89
TIM_OC1Init
void TIM_OC1Init(TIM_TypeDef *TIMx, TIM_OCInitTypeDef *TIM_OCInitStruct)
Initializes the TIMx Channel1 according to the specified parameters in the TIM_OCInitStruct.
Definition: wb32l003_tim.c:144
TIM_TimeBaseInitTypeDef::TIM_ClockDivision
uint16_t TIM_ClockDivision
Definition: wb32l003_tim.h:46
TIM_OC2Init
void TIM_OC2Init(TIM_TypeDef *TIMx, TIM_OCInitTypeDef *TIM_OCInitStruct)
Initializes the TIMx Channel2 according to the specified parameters in the TIM_OCInitStruct.
Definition: wb32l003_tim.c:226
TIM_ICStructInit
void TIM_ICStructInit(TIM_ICInitTypeDef *TIM_ICInitStruct)
Fills each TIM_ICInitStruct member with its default value.
Definition: wb32l003_tim.c:634
TIM_ICInitTypeDef::TIM_ICPrescaler
uint16_t TIM_ICPrescaler
Definition: wb32l003_tim.h:110
TIM_ETRClockMode1Config
void TIM_ETRClockMode1Config(TIM_TypeDef *TIMx, uint16_t TIM_ExtTRGPrescaler, uint16_t TIM_ExtTRGPolarity, uint16_t ExtTRGFilter)
Configures the External clock Mode1
Definition: wb32l003_tim.c:869
TIM_UpdateDisableConfig
void TIM_UpdateDisableConfig(TIM_TypeDef *TIMx, FunctionalState NewState)
Enables or Disables the TIMx Update event.
Definition: wb32l003_tim.c:1861
TIM_ForcedOC1Config
void TIM_ForcedOC1Config(TIM_TypeDef *TIMx, uint16_t TIM_ForcedAction)
Forces the TIMx output 1 waveform to active or inactive level.
Definition: wb32l003_tim.c:1109
TIM_ICInit
void TIM_ICInit(TIM_TypeDef *TIMx, TIM_ICInitTypeDef *TIM_ICInitStruct)
Initializes the TIM peripheral according to the specified parameters in the TIM_ICInitStruct.
Definition: wb32l003_tim.c:451
TIM_BDTRInitTypeDef::TIM_OSSIState
uint16_t TIM_OSSIState
Definition: wb32l003_tim.h:128
TIM_ClearFlag
void TIM_ClearFlag(TIM_TypeDef *TIMx, uint16_t TIM_FLAG)
Clears the TIMx's pending flags.
Definition: wb32l003_tim.c:2358
TIM_GetCapture3
uint16_t TIM_GetCapture3(TIM_TypeDef *TIMx)
Gets the TIMx Input Capture 3 value.
Definition: wb32l003_tim.c:2247
TIM_SetIC4Prescaler
void TIM_SetIC4Prescaler(TIM_TypeDef *TIMx, uint16_t TIM_ICPSC)
Sets the TIMx Input Capture 4 prescaler.
Definition: wb32l003_tim.c:2183
TIM_ClearOC3Ref
void TIM_ClearOC3Ref(TIM_TypeDef *TIMx, uint16_t TIM_OCClear)
Clears or safeguards the OCREF3 signal on an external event
Definition: wb32l003_tim.c:1526
TIM_OCInitTypeDef
TIM Output Compare Init structure definition
Definition: wb32l003_tim.h:63
TIM_BDTRConfig
void TIM_BDTRConfig(TIM_TypeDef *TIMx, TIM_BDTRInitTypeDef *TIM_BDTRInitStruct)
Configures the: Break feature, dead time, Lock level, the OSSI, the OSSR State and the AOE(automatic ...
Definition: wb32l003_tim.c:575
TIM_GetCapture2
uint16_t TIM_GetCapture2(TIM_TypeDef *TIMx)
Gets the TIMx Input Capture 2 value.
Definition: wb32l003_tim.c:2234
TIM_TimeBaseInitTypeDef
TIM Time Base Init structure definition
Definition: wb32l003_tim.h:34
TIM_CCPreloadControl
void TIM_CCPreloadControl(TIM_TypeDef *TIMx, FunctionalState NewState)
Sets or Resets the TIM peripheral Capture Compare Preload Control bit.
Definition: wb32l003_tim.c:1252
TIM_SelectMasterSlaveMode
void TIM_SelectMasterSlaveMode(TIM_TypeDef *TIMx, uint16_t TIM_MasterSlaveMode)
Sets or Resets the TIMx Master/Slave Mode.
Definition: wb32l003_tim.c:2010
TIM_ClearOC2Ref
void TIM_ClearOC2Ref(TIM_TypeDef *TIMx, uint16_t TIM_OCClear)
Clears or safeguards the OCREF2 signal on an external event
Definition: wb32l003_tim.c:1502
TIM_SetCompare4
void TIM_SetCompare4(TIM_TypeDef *TIMx, uint16_t Compare4)
Sets the TIMx Capture Compare4 Register value
Definition: wb32l003_tim.c:2098
TIM_GetFlagStatus
FlagStatus TIM_GetFlagStatus(TIM_TypeDef *TIMx, uint16_t TIM_FLAG)
Checks whether the specified TIM flag is set or not.
Definition: wb32l003_tim.c:2317
TIM_EncoderInterfaceConfig
void TIM_EncoderInterfaceConfig(TIM_TypeDef *TIMx, uint16_t TIM_EncoderMode, uint16_t TIM_IC1Polarity, uint16_t TIM_IC2Polarity)
Configures the TIMx Encoder Interface.
Definition: wb32l003_tim.c:1058
TIM_SetIC1Prescaler
void TIM_SetIC1Prescaler(TIM_TypeDef *TIMx, uint16_t TIM_ICPSC)
Sets the TIMx Input Capture 1 prescaler.
Definition: wb32l003_tim.c:2117
TIM_SetClockDivision
void TIM_SetClockDivision(TIM_TypeDef *TIMx, uint16_t TIM_CKD)
Sets the TIMx Clock Division value.
Definition: wb32l003_tim.c:2205
TIM_TypeDef
Definition: wb32l003.h:480
TIM_GetCapture1
uint16_t TIM_GetCapture1(TIM_TypeDef *TIMx)
Gets the TIMx Input Capture 1 value.
Definition: wb32l003_tim.c:2221
TIM_OC1PreloadConfig
void TIM_OC1PreloadConfig(TIM_TypeDef *TIMx, uint16_t TIM_OCPreload)
Enables or disables the TIMx peripheral Preload register on CCR1.
Definition: wb32l003_tim.c:1278
TIM_ICInitTypeDef::TIM_Channel
uint16_t TIM_Channel
Definition: wb32l003_tim.h:101
TIM_SelectOCxM
void TIM_SelectOCxM(TIM_TypeDef *TIMx, uint16_t TIM_Channel, uint16_t TIM_OCMode)
Selects the TIM Output Compare Mode.
Definition: wb32l003_tim.c:1814
TIM_ClearITPendingBit
void TIM_ClearITPendingBit(TIM_TypeDef *TIMx, uint16_t TIM_IT)
Clears the TIMx's interrupt pending bits.
Definition: wb32l003_tim.c:2428
TIM_OC1NPolarityConfig
void TIM_OC1NPolarityConfig(TIM_TypeDef *TIMx, uint16_t TIM_OCNPolarity)
Configures the TIMx Channel 1N polarity.
Definition: wb32l003_tim.c:1597
TIM_TimeBaseInitTypeDef::TIM_Period
uint16_t TIM_Period
Definition: wb32l003_tim.h:42
TIM_SetCompare2
void TIM_SetCompare2(TIM_TypeDef *TIMx, uint16_t Compare2)
Sets the TIMx Capture Compare2 Register value
Definition: wb32l003_tim.c:2070
TIM_OCInitTypeDef::TIM_OCMode
uint16_t TIM_OCMode
Definition: wb32l003_tim.h:65
TIM_SetAutoreload
void TIM_SetAutoreload(TIM_TypeDef *TIMx, uint16_t Autoreload)
Sets the TIMx Autoreload Register value
Definition: wb32l003_tim.c:2042
TIM_GenerateEvent
void TIM_GenerateEvent(TIM_TypeDef *TIMx, uint16_t TIM_EventSource)
Configures the TIMx event to be generate by software.
Definition: wb32l003_tim.c:767
TIM_BDTRInitTypeDef::TIM_LOCKLevel
uint16_t TIM_LOCKLevel
Definition: wb32l003_tim.h:131
TIM_ICInitTypeDef::TIM_ICSelection
uint16_t TIM_ICSelection
Definition: wb32l003_tim.h:107
TIM_UpdateRequestConfig
void TIM_UpdateRequestConfig(TIM_TypeDef *TIMx, uint16_t TIM_UpdateSource)
Configures the TIMx Update Request Interrupt source.
Definition: wb32l003_tim.c:1888
TIM_OCInitTypeDef::TIM_OCPolarity
uint16_t TIM_OCPolarity
Definition: wb32l003_tim.h:78
TIM_OC1PolarityConfig
void TIM_OC1PolarityConfig(TIM_TypeDef *TIMx, uint16_t TIM_OCPolarity)
Configures the TIMx channel 1 polarity.
Definition: wb32l003_tim.c:1574
TIM_OC4PolarityConfig
void TIM_OC4PolarityConfig(TIM_TypeDef *TIMx, uint16_t TIM_OCPolarity)
Configures the TIMx channel 4 polarity.
Definition: wb32l003_tim.c:1716
TIM_TIxExternalClockConfig
void TIM_TIxExternalClockConfig(TIM_TypeDef *TIMx, uint16_t TIM_TIxExternalCLKSource, uint16_t TIM_ICPolarity, uint16_t ICFilter)
Configures the TIMx Trigger as External Clock
Definition: wb32l003_tim.c:829
TIM_CounterModeConfig
void TIM_CounterModeConfig(TIM_TypeDef *TIMx, uint16_t TIM_CounterMode)
Specifies the TIMx Counter Mode to be used.
Definition: wb32l003_tim.c:993
TIM_TimeBaseInit
void TIM_TimeBaseInit(TIM_TypeDef *TIMx, TIM_TimeBaseInitTypeDef *TIM_TimeBaseInitStruct)
Initializes the TIMx Time Base Unit peripheral according to the specified parameters in the TIM_TimeB...
Definition: wb32l003_tim.c:95
TIM_CCxNCmd
void TIM_CCxNCmd(TIM_TypeDef *TIMx, uint16_t TIM_Channel, uint16_t TIM_CCxN)
Enables or disables the TIM Capture Compare Channel xN.
Definition: wb32l003_tim.c:1773
TIM_GetITStatus
ITStatus TIM_GetITStatus(TIM_TypeDef *TIMx, uint16_t TIM_IT)
Checks whether the TIM interrupt has occurred or not.
Definition: wb32l003_tim.c:2387
TIM_ForcedOC4Config
void TIM_ForcedOC4Config(TIM_TypeDef *TIMx, uint16_t TIM_ForcedAction)
Forces the TIMx output 4 waveform to active or inactive level.
Definition: wb32l003_tim.c:1181
TIM_SelectInputTrigger
void TIM_SelectInputTrigger(TIM_TypeDef *TIMx, uint16_t TIM_InputTriggerSource)
Selects the Input Trigger source
Definition: wb32l003_tim.c:1023
TIM_ICInitTypeDef
TIM Input Capture Init structure definition
Definition: wb32l003_tim.h:98
TIM_SelectSlaveMode
void TIM_SelectSlaveMode(TIM_TypeDef *TIMx, uint16_t TIM_SlaveMode)
Selects the TIMx Slave Mode.
Definition: wb32l003_tim.c:1989
TIM_BDTRStructInit
void TIM_BDTRStructInit(TIM_BDTRInitTypeDef *TIM_BDTRInitStruct)
Fills each TIM_BDTRInitStruct member with its default value.
Definition: wb32l003_tim.c:650
TIM_OC2PolarityConfig
void TIM_OC2PolarityConfig(TIM_TypeDef *TIMx, uint16_t TIM_OCPolarity)
Configures the TIMx channel 2 polarity.
Definition: wb32l003_tim.c:1621
TIM_OCInitTypeDef::TIM_Pulse
uint16_t TIM_Pulse
Definition: wb32l003_tim.h:75
TIM_DeInit
void TIM_DeInit(TIM_TypeDef *TIMx)
Deinitializes the TIMx peripheral registers to their default reset values.
Definition: wb32l003_tim.c:69
TIM_OCInitTypeDef::TIM_OutputState
uint16_t TIM_OutputState
Definition: wb32l003_tim.h:68
TIM_OC1FastConfig
void TIM_OC1FastConfig(TIM_TypeDef *TIMx, uint16_t TIM_OCFast)
Configures the TIMx Output Compare 1 Fast feature.
Definition: wb32l003_tim.c:1375
TIM_OCInitTypeDef::TIM_OCIdleState
uint16_t TIM_OCIdleState
Definition: wb32l003_tim.h:85
TIM_BDTRInitTypeDef::TIM_AutomaticOutput
uint16_t TIM_AutomaticOutput
Definition: wb32l003_tim.h:144
TIM_TimeBaseStructInit
void TIM_TimeBaseStructInit(TIM_TimeBaseInitTypeDef *TIM_TimeBaseInitStruct)
Fills each TIM_TimeBaseInitStruct member with its default value.
Definition: wb32l003_tim.c:599
TIM_ITConfig
void TIM_ITConfig(TIM_TypeDef *TIMx, uint16_t TIM_IT, FunctionalState NewState)
Enables or disables the specified TIM interrupts.
Definition: wb32l003_tim.c:732
TIM_SelectOutputTrigger
void TIM_SelectOutputTrigger(TIM_TypeDef *TIMx, uint16_t TIM_TRGOSource)
Selects the TIMx Trigger Output Mode.
Definition: wb32l003_tim.c:1966
TIM_TimeBaseInitTypeDef::TIM_CounterMode
uint16_t TIM_CounterMode
Definition: wb32l003_tim.h:39
TIM_InternalClockConfig
void TIM_InternalClockConfig(TIM_TypeDef *TIMx)
Configures the TIMx internal Clock
Definition: wb32l003_tim.c:783
TIM_OC2PreloadConfig
void TIM_OC2PreloadConfig(TIM_TypeDef *TIMx, uint16_t TIM_OCPreload)
Enables or disables the TIMx peripheral Preload register on CCR2.
Definition: wb32l003_tim.c:1303
TIM_OC2FastConfig
void TIM_OC2FastConfig(TIM_TypeDef *TIMx, uint16_t TIM_OCFast)
Configures the TIMx Output Compare 2 Fast feature.
Definition: wb32l003_tim.c:1401
TIM_OCInitTypeDef::TIM_OutputNState
uint16_t TIM_OutputNState
Definition: wb32l003_tim.h:71
TIM_GetCounter
uint16_t TIM_GetCounter(TIM_TypeDef *TIMx)
Gets the TIMx Counter value.
Definition: wb32l003_tim.c:2273
TIM_ICInitTypeDef::TIM_ICFilter
uint16_t TIM_ICFilter
Definition: wb32l003_tim.h:113
TIM_OC4PreloadConfig
void TIM_OC4PreloadConfig(TIM_TypeDef *TIMx, uint16_t TIM_OCPreload)
Enables or disables the TIMx peripheral Preload register on CCR4.
Definition: wb32l003_tim.c:1351
TIM_OC3NPolarityConfig
void TIM_OC3NPolarityConfig(TIM_TypeDef *TIMx, uint16_t TIM_OCNPolarity)
Configures the TIMx Channel 3N polarity.
Definition: wb32l003_tim.c:1691
TIM_BDTRInitTypeDef
BDTR structure definition
Definition: wb32l003_tim.h:122
TIM_TimeBaseInitTypeDef::TIM_RepetitionCounter
uint8_t TIM_RepetitionCounter
Definition: wb32l003_tim.h:49
TIM_PWMIConfig
void TIM_PWMIConfig(TIM_TypeDef *TIMx, TIM_ICInitTypeDef *TIM_ICInitStruct)
Configures the TIM peripheral according to the specified parameters in the TIM_ICInitStruct to measur...
Definition: wb32l003_tim.c:517
TIM_OC4Init
void TIM_OC4Init(TIM_TypeDef *TIMx, TIM_OCInitTypeDef *TIM_OCInitStruct)
Initializes the TIMx Channel4 according to the specified parameters in the TIM_OCInitStruct.
Definition: wb32l003_tim.c:387