# Static Call Graph for image .\Objects\TIM1_7PWM_Output.axf

#<CALLGRAPH># ARM Linker, 5060960: Last Updated: Wed Dec 06 09:55:16 2023

### Maximum Stack Usage = 36 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

SystemInit ⇒ SetSysClock ⇒ SetSysClockToHSI ⇒ RCC_HSIConfig

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- SVC_Handler ⇒ SVC_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - AWK_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - CLKTRIM_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - FLASH_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - GPIOA_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - GPIOB_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - GPIOC_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - GPIOD_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - HardFault_Handler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - I2C_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - IWDG_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - LPTIM_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - LPUART_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - LVD_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - NMI_Handler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - OWIRE_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - PCA_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - PendSV_Handler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - RTC_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - Reset_Handler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - SPI_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - SVC_Handler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - SysTick_Handler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - SystemInit from system_fe82160.o(i.SystemInit) referenced from startup_fe82160.o(.text)
  - TIM10_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - TIM11_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - TIM1_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - TIM2_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - UART1_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - UART2_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - VCMP_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - WWDG_IRQHandler from startup_fe82160.o(.text) referenced from startup_fe82160.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_fe82160.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 52 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_fini_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000011))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000012))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 16 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ TIM_OC4Init
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_fe82160.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_fe82160.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_fe82160.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_fe82160.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_fe82160.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_fe82160.o(RESET)

  AWK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  CLKTRIM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  GPIOA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  GPIOB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  GPIOC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  GPIOD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  I2C_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  IWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  LPTIM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  LPUART_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  LVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  OWIRE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  PCA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  SPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  TIM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  VCMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Address Reference Count : 1]

  - startup_fe82160.o(RESET)

  __user_initial_stackheap (Thumb, 10 bytes, Stack size 0 bytes, startup_fe82160.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 0 bytes, aeabi_sdiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 20 bytes, Stack size 0 bytes, aeabi_sdiv.o(.text))
  [Called By]

  - >> SystemCoreClockUpdate

  __aeabi_idiv (Thumb, 0 bytes, Stack size 8 bytes, aeabi_sdiv.o(.text), UNUSED)

  __aeabi_idivmod (Thumb, 326 bytes, Stack size 8 bytes, aeabi_sdiv.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 62 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 16 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  - >> _call_atexit_fns (Weak Reference)
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  GPIO_Init (Thumb, 168 bytes, Stack size 16 bytes, fe82160_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = GPIO_Init
  [Called By]
  - >> main

  __semihosting_library_function (Thumb, 0 bytes, Stack size 16 bytes, indicate_semi.o(.text), UNUSED)

  RCC_AHBCLKConfig (Thumb, 8 bytes, Stack size 0 bytes, fe82160_rcc.o(i.RCC_AHBCLKConfig))
  [Called By]

  - >> SetSysClockToHSI

  RCC_AHBPeriphClockCmd (Thumb, 28 bytes, Stack size 0 bytes, fe82160_rcc.o(i.RCC_AHBPeriphClockCmd))
  [Called By]

  - >> main

  RCC_APBCLKConfig (Thumb, 8 bytes, Stack size 0 bytes, fe82160_rcc.o(i.RCC_APBCLKConfig))
  [Called By]

  - >> SetSysClockToHSI

  RCC_APBPeriphClockCmd (Thumb, 28 bytes, Stack size 0 bytes, fe82160_rcc.o(i.RCC_APBPeriphClockCmd))
  [Called By]

  - >> main

  RCC_APBPeriphResetCmd (Thumb, 40 bytes, Stack size 0 bytes, fe82160_rcc.o(i.RCC_APBPeriphResetCmd))
  [Called By]

  - >> TIM_DeInit

  RCC_HSIConfig (Thumb, 194 bytes, Stack size 12 bytes, fe82160_rcc.o(i.RCC_HSIConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_HSIConfig
  [Called By]
  - >> SetSysClockToHSI

  RCC_SYSCLKConfig (Thumb, 38 bytes, Stack size 0 bytes, fe82160_rcc.o(i.RCC_SYSCLKConfig))
  [Called By]

  - >> SetSysClockToHSI

  SystemCoreClockUpdate (Thumb, 228 bytes, Stack size 8 bytes, system_fe82160.o(i.SystemCoreClockUpdate))
  [Stack]

  - Max Depth = 8
  - Call Chain = SystemCoreClockUpdate
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> main

  SystemInit (Thumb, 56 bytes, Stack size 8 bytes, system_fe82160.o(i.SystemInit))
  [Stack]

  - Max Depth = 36
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockToHSI ⇒ RCC_HSIConfig
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_fe82160.o(.text)

  TIM_ARRPreloadConfig (Thumb, 24 bytes, Stack size 0 bytes, fe82160_tim.o(i.TIM_ARRPreloadConfig))
  [Called By]

  - >> main

  TIM_Cmd (Thumb, 24 bytes, Stack size 0 bytes, fe82160_tim.o(i.TIM_Cmd))
  [Called By]

  - >> main

  TIM_CtrlPWMOutputs (Thumb, 26 bytes, Stack size 0 bytes, fe82160_tim.o(i.TIM_CtrlPWMOutputs))
  [Called By]

  - >> main

  TIM_DeInit (Thumb, 52 bytes, Stack size 8 bytes, fe82160_tim.o(i.TIM_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_DeInit
  [Calls]
  - >> RCC_APBPeriphResetCmd
  [Called By]
  - >> main

  TIM_OC1Init (Thumb, 106 bytes, Stack size 16 bytes, fe82160_tim.o(i.TIM_OC1Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = TIM_OC1Init
  [Called By]
  - >> main

  TIM_OC1PreloadConfig (Thumb, 22 bytes, Stack size 0 bytes, fe82160_tim.o(i.TIM_OC1PreloadConfig))
  [Called By]

  - >> main

  TIM_OC2Init (Thumb, 136 bytes, Stack size 16 bytes, fe82160_tim.o(i.TIM_OC2Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = TIM_OC2Init
  [Called By]
  - >> main

  TIM_OC2PreloadConfig (Thumb, 22 bytes, Stack size 0 bytes, fe82160_tim.o(i.TIM_OC2PreloadConfig))
  [Called By]

  - >> main

  TIM_OC3Init (Thumb, 130 bytes, Stack size 16 bytes, fe82160_tim.o(i.TIM_OC3Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = TIM_OC3Init
  [Called By]
  - >> main

  TIM_OC3PreloadConfig (Thumb, 22 bytes, Stack size 0 bytes, fe82160_tim.o(i.TIM_OC3PreloadConfig))
  [Called By]

  - >> main

  TIM_OC4Init (Thumb, 94 bytes, Stack size 16 bytes, fe82160_tim.o(i.TIM_OC4Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = TIM_OC4Init
  [Called By]
  - >> main

  TIM_OC4PreloadConfig (Thumb, 22 bytes, Stack size 0 bytes, fe82160_tim.o(i.TIM_OC4PreloadConfig))
  [Called By]

  - >> main

  TIM_TimeBaseInit (Thumb, 60 bytes, Stack size 0 bytes, fe82160_tim.o(i.TIM_TimeBaseInit))
  [Called By]

  - >> main

  main (Thumb, 224 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 16
  - Call Chain = main ⇒ TIM_OC4Init
  [Calls]
  - >> TIM_TimeBaseInit
  - >> TIM_OC4PreloadConfig
  - >> TIM_OC4Init
  - >> TIM_OC3PreloadConfig
  - >> TIM_OC3Init
  - >> TIM_OC2PreloadConfig
  - >> TIM_OC2Init
  - >> TIM_OC1PreloadConfig
  - >> TIM_OC1Init
  - >> TIM_DeInit
  - >> TIM_CtrlPWMOutputs
  - >> TIM_Cmd
  - >> TIM_ARRPreloadConfig
  - >> RCC_APBPeriphClockCmd
  - >> RCC_AHBPeriphClockCmd
  - >> GPIO_Init
  - >> SystemCoreClockUpdate
  [Called By]
  - >> __rt_entry_main

  ### Local Symbols

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_fe82160.o(i.SetSysClock))
  [Stack]

  - Max Depth = 28
  - Call Chain = SetSysClock ⇒ SetSysClockToHSI ⇒ RCC_HSIConfig
  [Calls]
  - >> SetSysClockToHSI
  [Called By]
  - >> SystemInit

  SetSysClockToHSI (Thumb, 66 bytes, Stack size 8 bytes, system_fe82160.o(i.SetSysClockToHSI))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClockToHSI ⇒ RCC_HSIConfig
  [Calls]
  - >> RCC_SYSCLKConfig
  - >> RCC_HSIConfig
  - >> RCC_APBCLKConfig
  - >> RCC_AHBCLKConfig
  [Called By]
  - >> SetSysClock

  ### Undefined Global Symbols

  _call_atexit_fns (ARM, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> exit