WB32L003 Standard Peripherals Firmware Library

Data Fields
LVD_InitTypeDef Struct Reference
WB32L003_StdPeriph_Driver » LVD

LVD Configuration Structure definition. More...

`#include <wb32l003_lvd.h>`

## Data Fields
uint32_t | FltClkSel
uint32_t | VoltageLevel
uint32_t | TriggerSel
uint32_t | Action
uint32_t | FltNum

## Detailed Description

LVD Configuration Structure definition.

Note
  This structure is for LVD

## Field Documentation

## ◆ Action

uint32_t Action

Specifies low voltage detection action. This parameter can be a value of LVD_Action_After_Detection

## ◆ FltClkSel

uint32_t FltClkSel

Specifies filter clock. This parameter can be a value of LVD_Filter_Clock_Selection

## ◆ FltNum

uint32_t FltNum

Specifies the filter number for digital filter. This parameter can be a value between 0x0000 to 0xFFFF

## ◆ TriggerSel

uint32_t TriggerSel

Specifies trigger selection for LVD. This parameter can be a value of LVD_Trigger_Selection

## ◆ VoltageLevel

uint32_t VoltageLevel

Specifies voltage level for LVD. This parameter can be a value of LVD_Voltage_Level

The documentation for this struct was generated from the following file:

- wb32l003_lvd.h