WB32L003 Standard Peripherals Firmware Library

Macros
FLASH_Interrupt_definition
WB32L003_StdPeriph_Driver » FLASH » FLASH_Exported_Constants

## Macros
#define | FLASH_IT_ALARM_ERASE_PROTADDR (FLASH_IFR_IF1 | FLASH_CR_IE_1)
#define | FLASH_IT_ALARM_ERASE_PCADDR (FLASH_IFR_IF0 | FLASH_CR_IE_0)

## Detailed Description

## Macro Definition Documentation

## ◆ FLASH_IT_ALARM_ERASE_PCADDR

#define FLASH_IT_ALARM_ERASE_PCADDR (FLASH_IFR_IF0 | FLASH_CR_IE_0)

The address to be erased is PC interrupt flag

## ◆ FLASH_IT_ALARM_ERASE_PROTADDR

#define FLASH_IT_ALARM_ERASE_PROTADDR (FLASH_IFR_IF1 | FLASH_CR_IE_1)

The address to be erased is protectd interrupt flag