WB32L003 Standard Peripherals Firmware Library

Functions
MISC_Exported_Functions
WB32L003_StdPeriph_Driver » MISC

## Functions
void | SysTick_CLKSourceConfig (uint32_t SysTick_CLKSource)
| Configures the SysTick clock source. More...
void | SysTick_DelayNticks (uint32_t Ticks)
| Delay n ticks. More...
void | SysTick_DelayUs (uint32_t Us)
| Delay n Us. More...
void | SysTick_DelayMs (uint32_t Ms)
| Delay n Ms. More...

## Detailed Description

## Function Documentation

## ◆ SysTick_CLKSourceConfig()

void SysTick_CLKSourceConfig | ( | uint32_t | SysTick_CLKSource | ) |

Configures the SysTick clock source.

Parameters

  SysTick_CLKSource | specifies the SysTick clock source. This parameter can be one of the following values: SysTick_CLKSource_HCLK_Div4: AHB clock divided by 4 selected as SysTick clock source. SysTick_CLKSource_HCLK: AHB clock selected as SysTick clock source.

Return values

  None |

## ◆ SysTick_DelayMs()

void SysTick_DelayMs | ( | uint32_t | Ms | ) |

Delay n Ms.

Parameters

  Ms | Number of Ms to delay.

Note
  None

Return values

  None |

## ◆ SysTick_DelayNticks()

void SysTick_DelayNticks | ( | uint32_t | Ticks | ) |

Delay n ticks.

Parameters

  Ticks | Number of ticks to delay.

Note
  Since SysTick_LOAD is a 24-bit register, the n_ticks must be less than 16777216.

Return values

  None |

## ◆ SysTick_DelayUs()

void SysTick_DelayUs | ( | uint32_t | Us | ) |

Delay n Us.

Parameters

  Us | Number of Us to delay.

Note
  None

Return values

  None |