WB32L003 Standard Peripherals Firmware Library

TIM10_Timing example

      ****************** (C) COPYRIGHT 2023 Westberry Technology *******************
      * @file    TIM10/TIM10_Timing/readme.txt
      * @author  Westberry Application Team
      * @version V0.0.4
      * @date    23-April-2023
      * @brief   Description of the TIM10 TIM10_Timing example.
      ******************************************************************************
      * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
      * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
      * TIME. AS A RESULT, WESTBERRY SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
      * INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM
      * THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
      * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
      ******************************************************************************

Example Description

This example describes how to se the Timing function of TIM10.

In this example, Main clock is configured at 24MHz.

In this routine, TIM10 enables the timing function and adopts the reloading
counting mode. The reloading value is 65295. When the counting value reaches 65535,
interrupt is generated and PC4 pin is flipped, and the waveform with a flipping speed
of 100K is output on PC4 pin.

Directory contents

- TIM10/TIM10_Timing/TIM10_Timing.uvprojx MDK5 project file
- TIM10/TIM10_Timing/TIM10_Timing.uvoptx MDK5 project options file
- TIM10/TIM10_Timing/JLinkSettings.ini Jlink settings file
- TIM10/TIM10_Timing/main.c Main program

Hardware and Software environment

- Hardware environment
  - The chip pins are connected as follows：
    - PC4 pin is connection to oscilloscope

How to use it ?

In order to make the program work, you must do the following :

- Open TIM10_Timing.uvprojx from this example folder by Keil MDK5
- Rebuild all files and load your image into target memory

- Run the example

  ###
  © COPYRIGHT 2023 Westberry Technology