WB32L003 Standard Peripherals Firmware Library

Data Fields
RTC_DateTypeDef Struct Reference
WB32L003_StdPeriph_Driver » RTC

RTC Date structure definition. More...

`#include <wb32l003_rtc.h>`

## Data Fields
uint32_t | RTC_Year
uint8_t | RTC_Month
uint8_t | RTC_Date
uint8_t | RTC_WeekDay
uint8_t | RTC_Cen

## Detailed Description

RTC Date structure definition.

## Field Documentation

## ◆ RTC_Cen

uint8_t RTC_Cen

Specifies the RTC Date century.

## ◆ RTC_Date

uint8_t RTC_Date

Specifies the RTC Date. This parameter must be a number between Min_Data = 1 and Max_Data = 31

## ◆ RTC_Month

uint8_t RTC_Month

Specifies the RTC Date Month (in BCD format). This parameter can be a value of RTC_Month_Date_Definitions

## ◆ RTC_WeekDay

uint8_t RTC_WeekDay

Specifies the RTC Date WeekDay. This parameter can be a value of RTC_WeekDay_Definitions

## ◆ RTC_Year

uint32_t RTC_Year

Specifies the RTC Date Year. This parameter must be a number between Min_Data = 00 and Max_Data = 99

The documentation for this struct was generated from the following file:

- wb32l003_rtc.h