WB32L003 Standard Peripherals Firmware Library

RTC_Calendar_DeepSleep_LSI example

      ****************** (C) COPYRIGHT 2023 Westberry Technology *******************
      * @file    RTC/RTC_Calendar_DeepSleep_LSI/readme.txt
      * @author  Westberry Application Team
      * @version V0.0.4
      * @date    23-April-2023
      * @brief   Description of the RTC RTC_Calendar_DeepSleep_LSI example.
      ******************************************************************************
      * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
      * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
      * TIME. AS A RESULT, WESTBERRY SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
      * INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM
      * THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
      * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
      ******************************************************************************

Example Description

This example describes how to use the RTC peripheral in deep sleep mode. As an application example, it demonstrates how to setup the RTC peripheral, entry sleep and generate interrupt.

In this example, Main clock is configured at 32.768KHz.

Directory contents

- RTC/RTC_Calendar_DeepSleep_LSI/RTC_Calendar_DeepSleep_LSI.uvprojx MDK5 project file
- RTC/RTC_Calendar_DeepSleep_LSI/RTC_Calendar_DeepSleep_LSI.uvoptx MDK5 project options file
- RTC/RTC_Calendar_DeepSleep_LSI/JLinkSettings.ini Jlink settings file
- RTC/RTC_Calendar_DeepSleep_LSI/main.c Main program
- RTC/RTC_Calendar_DeepSleep_LSI/rtc.c rtc.c file
- RTC/RTC_Calendar_DeepSleep_LSI/rtc.h rtc.h header file

Hardware and Software environment

- Hardware environment
  - UART connect to UART tool

How to use it ?

In order to make the program work, you must do the following :

- Open RTC_Calendar_DeepSleep_LSI.uvprojx from this example folder by Keil MDK5
- Rebuild all files and load your image into target memory

- Run the example

  ###
  © COPYRIGHT 2023 Westberry Technology