WB32L003 Standard Peripherals Firmware Library

LPUART_Sleep example

      ****************** (C) COPYRIGHT 2023 Westberry Technology *******************
      * @file    LPUART/LPUART_Sleep/readme.txt
      * @author  Westberry Application Team
      * @version V0.0.4
      * @date    23-April-2023
      * @brief   Description of the LPUART LPUART_Sleep example.
      ******************************************************************************
      * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
      * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
      * TIME. AS A RESULT, WESTBERRY SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
      * INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM
      * THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
      * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
      ******************************************************************************

例程描述

本例程演示LPUART在低功耗Sleep模式下如何工作。

本例程系统时钟工作在24Mhz。

LPUART在低功耗模式下由SCLK提供通信的时钟，可以正常进行数据收发，通信产生的中断可以将
MCU从低功耗模式唤醒，本例程开始时会进行中断数据接收，之后进入Sleep模式，接收到外部发
送的数据时唤醒MCU，打印提示信息，接收到10个字节时将收到的数据使用LPUART打印。

例程运行效果为芯片复位之后进入低功耗模式，使用上位机发送数据将芯片唤醒，之后会打印提
示信息，当接收到10个数据时将收到的数据发送给上位机。

LPUART1 配置如下：

- 波特率： 93750
- 数据位： 8
- 启用Sleep模式

目录内容

- LPUART/LPUART_Sleep/LPUART_Sleep.uvprojx MDK5工程文件
- LPUART/LPUART_Sleep/LPUART_Sleep.uvoptx MDK5工程配置文件
- LPUART/LPUART_Sleep/JLinkSettings.ini Jlink配置文件
- LPUART/LPUART_Sleep/main.c 主程序

硬件和软件环境

- 硬件平台搭建
  - 芯片管脚连接如下：
    - LPUART(PC5, PD5) 连接到PC

如何使用？

为了使程序工作，您必须执行以下操作 :

- 使用 MDK5 打开此例程文件夹中的 LPUART_Sleep.uvprojx 工程
- 重新编译该工程并下载到目标存储器中

- 运行此例程

  ###
  © COPYRIGHT 2023 Westberry Technology