WB32L003 Standard Peripherals Firmware Library

宏定义 | 函数
wb32l003_wwdg.h 文件参考

This file contains all the functions prototypes for the WWDG firmware library. 更多...

`#include "wb32l003.h"`

浏览源代码.

## 宏定义
#define | WWDG_PRESCALER_MIN ((uint32_t)0x00000000U)
#define | WWDG_PRESCALER_MAX ((uint32_t)0x000FFFFFU)
#define | WWDG_WINDOW_MIN ((uint8_t)0x00000010U)
#define | WWDG_WINDOW_MAX ((uint8_t)0x000000FFU)
#define | WWDG_RELOAD_MIN ((uint8_t)0x00000020U)
#define | WWDG_RELOAD_MAX ((uint8_t)0x000000FFU)
#define | IS_WWDG_PRESCALER_VALUE(VALUE) ((VALUE) <= WWDG_PRESCALER_MAX)
#define | IS_WWDG_WINDOW_VALUE(VALUE)
#define | IS_WWDG_RELOAD_VALUE(VALUE)

## 函数
void | WWDG_DeInit (void)
| Deinitializes the WWDG peripheral registers to their default reset values. 更多...
void | WWDG_SetPrescaler (uint32_t WWDG_Prescaler)
| Sets the WWDG Prescaler. 更多...
void | WWDG_SetWindowValue (uint8_t WindowValue)
| Sets the WWDG window value. 更多...
void | WWDG_IT_Cmd (FunctionalState NewState)
| Enables or disable the WWDG's interrupt. 更多...
void | WWDG_SetCounter (uint8_t Counter)
| Sets the WWDG counter value. 更多...
void | WWDG_Cmd (FunctionalState NewState)
| Enables or disables the WWDG peripheral. 更多...
FlagStatus | WWDG_GetFlagStatus (void)
| Checks whether the Early Wakeup interrupt flag is set or not. 更多...
void | WWDG_ClearFlag (void)
| Clears Early Wakeup interrupt flag. 更多...

## 详细描述

This file contains all the functions prototypes for the WWDG firmware library.

作者
  Westberry Application Team

版本
  V0.0.4

日期
  23-April-2023