WB32L003 Standard Peripherals Firmware Library

宏定义
LPTIM_Gate_Level_Selection
WB32L003_StdPeriph_Driver » LPTIM » LPTIM_Exported_Constants

## 宏定义
#define | LPTIM_GATELEVEL_LOW (LPTIM_CR_GATE_P)
#define | LPTIM_GATELEVEL_HIGH 0x00000000U
#define | IS_LPTIM_GATE_LEVEL(GATE_LEVEL)

## 详细描述

## 宏定义说明

## ◆ IS_LPTIM_GATE_LEVEL

#define IS_LPTIM_GATE_LEVEL | ( |  | GATE_LEVEL | ) |

值:
(((GATE_LEVEL) == LPTIM_GATELEVEL_LOW) || \
((GATE_LEVEL) == LPTIM_GATELEVEL_HIGH))
LPTIM_GATELEVEL_LOW
#define LPTIM_GATELEVEL_LOW
Definition: wb32l003_lptim.h:79
LPTIM_GATELEVEL_HIGH
#define LPTIM_GATELEVEL_HIGH
Definition: wb32l003_lptim.h:80

## ◆ LPTIM_GATELEVEL_HIGH

#define LPTIM_GATELEVEL_HIGH 0x00000000U

Specify gatelevel high for gate input

## ◆ LPTIM_GATELEVEL_LOW

#define LPTIM_GATELEVEL_LOW (LPTIM_CR_GATE_P)

Specify gatelevel low for gate input