WB32L003 Standard Peripherals Firmware Library

Macros | Functions
wb32l003_wwdg.h File Reference

This file contains all the functions prototypes for the WWDG firmware library. More...

`#include "wb32l003.h"`

Go to the source code of this file.

## Macros
#define | WWDG_PRESCALER_MIN ((uint32_t)0x00000000U)
#define | WWDG_PRESCALER_MAX ((uint32_t)0x000FFFFFU)
#define | WWDG_WINDOW_MIN ((uint8_t)0x00000010U)
#define | WWDG_WINDOW_MAX ((uint8_t)0x000000FFU)
#define | WWDG_RELOAD_MIN ((uint8_t)0x00000020U)
#define | WWDG_RELOAD_MAX ((uint8_t)0x000000FFU)
#define | IS_WWDG_PRESCALER_VALUE(VALUE) ((VALUE) <= WWDG_PRESCALER_MAX)
#define | IS_WWDG_WINDOW_VALUE(VALUE)
#define | IS_WWDG_RELOAD_VALUE(VALUE)

## Functions
void | WWDG_DeInit (void)
| Deinitializes the WWDG peripheral registers to their default reset values. More...
void | WWDG_SetPrescaler (uint32_t WWDG_Prescaler)
| Sets the WWDG Prescaler. More...
void | WWDG_SetWindowValue (uint8_t WindowValue)
| Sets the WWDG window value. More...
void | WWDG_IT_Cmd (FunctionalState NewState)
| Enables or disable the WWDG's interrupt. More...
void | WWDG_SetCounter (uint8_t Counter)
| Sets the WWDG counter value. More...
void | WWDG_Cmd (FunctionalState NewState)
| Enables or disables the WWDG peripheral. More...
FlagStatus | WWDG_GetFlagStatus (void)
| Checks whether the Early Wakeup interrupt flag is set or not. More...
void | WWDG_ClearFlag (void)
| Clears Early Wakeup interrupt flag. More...

## Detailed Description

This file contains all the functions prototypes for the WWDG firmware library.

Author
  Westberry Application Team

Version
  V0.0.4

Date
  23-April-2023