WB32L003 Standard Peripherals Firmware Library

Data Fields
SysTick_Type Struct Reference
Defines and Type Definitions » System Tick Timer (SysTick)

Structure type to access the System Timer (SysTick). More...

`#include <core_cm0plus.h>`

## Data Fields
__IOM uint32_t | CTRL
__IOM uint32_t | LOAD
__IOM uint32_t | VAL
__IM uint32_t | CALIB

## Detailed Description

Structure type to access the System Timer (SysTick).

## Field Documentation

## ◆ CALIB

__IM uint32_t CALIB

Offset: 0x00C (R/ ) SysTick Calibration Register

## ◆ CTRL

__IOM uint32_t CTRL

Offset: 0x000 (R/W) SysTick Control and Status Register

## ◆ LOAD

__IOM uint32_t LOAD

Offset: 0x004 (R/W) SysTick Reload Value Register

## ◆ VAL

__IOM uint32_t VAL

Offset: 0x008 (R/W) SysTick Current Value Register

The documentation for this struct was generated from the following file:

- core_cm0plus.h